> LTE TAI Management Database Configuration Mode Commands
> The LTE TAI Management Database Configuration Mode is used to create and manage the LTE TAI management database configuration for LTE polices configured on this system.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> tai-mgmt-obj
> Creates new, or removes/enters existing, LTE Tracking Area Identifier (TAI) object configurations.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] tai-mgmt-obj object_name [ -noconfirm ]
> no
> Removes a configured TAI management object from the TAI management database.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> object_name
> Specifies the name of the TAI management object and enters the LTE TAI Management Object Configuration Mode. object_name must be from 1 to 64 alpha and/or numeric characters.
> Usage
> Use this command to enter the LTE TAI Management Object Configuration Mode for an existing object or for a newly defined object. This command is also used to remove an existing object.
> Entering this command results in the following prompt:
> [context_name]hostname(tai-mgmt-obj)#
> LTE TAI Management Object Configuration Mode commands are defined in the LTE TAI Management Object Configuration Mode Commands chapter.
> Example
> The following command creates a TAI management object called tai-obj3 and enters the LTE TAI Management Oject Configuration Mode:
> tai-mgmt-obj tai-obj3

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883