> CSCFINTF Schema Statistics
> The CSCFINTF schema provides operational statistics that can be used for monitoring and troubleshooting the following products: SCM
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the CSCFINTF Schema

> Variables | Description | Data Type
> vpnname | VPN Name This is a key variable. | String
> vpnid | VPN ID This is a key variable. | Int32
> svcname | Service Name This is a key variable. | String
> svcid | Service ID This is a key variable. | Int32
> peer-ipaddr | Peer Ip-address | String
> peer-domain | Peer Domain Name | String
> regreqrx | Total number of Register requests received. | Int64
> regreqtx | Total number of Register requests transmitted. | Int64
> invreqrx | Total number of Invite requests received. | Int64
> invreqtx | Total number of Invite requests transmitted. | Int64
> ackreqrx | Total number of ACK requests received. | Int64
> ackreqtx | Total number of ACK requests transmitted. | Int64
> byereqrx | Total number of Bye requests received. | Int64
> byereqtx | Total number of Bye requests transmitted. | Int64
> cancreqrx | Total number of Cancel requests received. | Int64
> cancreqtx | Total number of Cancel requests transmitted. | Int64
> optreqrx | Total number of Options requests received. | Int64
> optreqtx | Total number of Options requests transmitted. | Int64
> prackreqrx | Total number of PRACK requests received. | Int64
> prackreqtx | Total number of PRACK requests transmitted. | Int64
> subreqrx | Total number of Subscribe requests received. | Int64
> subreqtx | Total number of Subscribe requests transmitted. | Int64
> notreqrx | Total number of Notify requests received. | Int64
> notreqtx | Total number of Notify requests transmitted. | Int64
> refreqrx | Total number of Refer requests received. | Int64
> refreqtx | Total number of Refer requests transmitted. | Int64
> inforeqrx | Total number of Info requests received. | Int64
> inforeqtx | Total number of Info requests transmitted. | Int64
> updreqrx | Total number of Update requests received. | Int64
> updreqtx | Total number of Update requests transmitted. | Int64
> msgreqrx | Total number of Message requests received. | Int64
> msgreqtx | Total number of Message requests transmitted. | Int64
> pubreqrx | Total number of Publish requests received. | Int64
> pubreqtx | Total number of Publish requests transmitted. | Int64
> tryrsprx | Total number of Trying responses received. | Int64
> tryrsptx | Total number of Trying responses transmitted. | Int64
> rngrsprx | Total number of Ringing responses received. | Int64
> rngrsptx | Total number of Ringing responses transmitted. | Int64
> fwdrsprx | Total number of Forwarded responses received. | Int64
> fwdrsptx | Total number of Forwarded responses transmitted. | Int64
> quersprx | Total number of Queued responses received. | Int64
> quersptx | Total number of Queued responses transmitted. | Int64
> prgrsprx | Total number of Progress responses received. | Int64
> prgrsptx | Total number of Progress responses transmitted. | Int64
> 200-rsprx | Total number of 200 OK responses received. | Int64
> 200-rsptx | Total number of 200 OK responses transmitted. | Int64
> 202-rsprx | Total number of 202 Accepted responses received. | Int64
> 202-rsptx | Total number of 202 Accepted responses transmitted. | Int64
> mchrsprx | Total number of Multiple Choices responses received. | Int64
> mchrsptx | Total number of Multiple Choices responses transmitted. | Int64
> mpersprx | Total number of Moved Permanently responses received. | Int64
> mpersptx | Total number of Moved Permanently responses transmitted. | Int64
> mtersprx | Total number of Moved Temporarily responses received. | Int64
> mtersptx | Total number of Moved Temporarily responses transmitted. | Int64
> upxrsprx | Total number of Use Proxy responses received. | Int64
> upxrsptx | Total number of Use Proxy responses transmitted. | Int64
> altrsprx | Total number of Alternative Service responses received. | Int64
> altrsptx | Total number of Alternative Service responses transmitted. | Int64
> brqerrrx | Total number of BadRequest errors received. | Int64
> brqerrtx | Total number of BadRequest errors transmitted. | Int64
> uauerrrx | Total number of UnAuthorized errors received. | Int64
> uauerrtx | Total number of UnAuthorized errors transmitted. | Int64
> prerrrx | Total number of Payment Required Errors received. | Int64
> prerrtx | Total number of Payment Required Errors transmitted. | Int64
> forerrrx | Total number of Forbidden errors received. | Int64
> forerrtx | Total number of Forbidden errors transmitted. | Int64
> nfderrrx | Total number of NotFound errors received. | Int64
> nfderrtx | Total number of NotFound errors transmitted. | Int64
> mnaerrrx | Total number of MethodNotAllowed errors received. | Int64
> mnaerrtx | Total number of MethodNotAllowed errors transmitted. | Int64
> nac406errrx | Total number of NotAcceptable(406) errors received. | Int64
> nac406errtx | Total number of NotAcceptable(406) errors transmitted. | Int64
> parerrrx | Total number of ProxyAuthRequired errors received. | Int64
> parerrtx | Total number of ProxyAuthRequired errors transmitted. | Int64
> rtoerrrx | Total number of RequestTimeout errors received. | Int64
> rtoerrtx | Total number of RequestTimeout errors transmitted. | Int64
> conferrrx | Total number of Conflict Errors received. | Int64
> conferrtx | Total number of Conflict Errors transmitted. | Int64
> lrerrrx | Total number of Length Required Errors received. | Int64
> lrerrtx | Total number of Length Required Errors transmitted. | Int64
> gonerrrx | Total number of Gone errors received. | Int64
> gonerrtx | Total number of Gone errors transmitted. | Int64
> crferrrx | Total number of ConditionalRequestFail errors received. | Int64
> crferrtx | Total number of ConditionalRequestFail errors transmitted. | Int64
> relerrrx | Total number of RequestEntityTooLarge errors received. | Int64
> relerrtx | Total number of RequestEntityTooLarge errors transmitted. | Int64
> rulerrrx | Total number of RequestURITooLong errors received. | Int64
> rulerrtx | Total number of RequestURITooLong errors transmitted. | Int64
> umterrrx | Total number of UnsupportedMediaType errors received. | Int64
> umterrtx | Total number of UnsupportedMediaType errors transmitted. | Int64
> uuserrrx | Total number of Unsupported URI Scheme errors received. | Int64
> uuserrtx | Total number of Unsupported URI Scheme errors transmitted. | Int64
> bexerrrx | Total number of BadExtension errors received. | Int64
> bexerrtx | Total number of BadExtension errors transmitted. | Int64
> exrerrrx | Total number of Extension Required errors received. | Int64
> exrerrtx | Total number of Extension Required errors transmitted. | Int64
> sitserrrx | Total number of Session Interval Too Small errors received. | Int64
> sitserrtx | Total number of Session Interval Too Small errors transmitted. | Int64
> itberrrx | Total number of Interval Too Brief errors received. | Int64
> itberrtx | Total number of Interval Too Brief errors transmitted. | Int64
> fhloerrrx | Total number of First Hop Lack Outbound errors received. | Int64
> fhloerrtx | Total number of First Hop Lack Outbound errors transmitted. | Int64
> blierrrx | Total number of Bad Location Information errors received. | Int64
> blierrtx | Total number of Bad Location Information errors transmitted. | Int64
> tnaerrrx | Total number of TempNotAvailable errors received. | Int64
> tnaerrtx | Total number of TempNotAvailable errors transmitted. | Int64
> tdnerrrx | Total number of Transaction Does Not Exist errors received. | Int64
> tdnerrtx | Total number of Transaction Does Not Exist errors transmitted. | Int64
> ldterrrx | Total number of LoopDetected errors received. | Int64
> ldterrtx | Total number of LoopDetected errors transmitted. | Int64
> tmherrrx | Total number of TooManyHops errors received. | Int64
> tmherrtx | Total number of TooManyHops errors transmitted. | Int64
> adierrrx | Total number of AddrIncomplete errors received. | Int64
> adierrtx | Total number of AddrIncomplete errors transmitted. | Int64
> amberrrx | Total number of Ambiguous errors received. | Int64
> amberrtx | Total number of Ambiguous errors transmitted. | Int64
> bhrerrrx | Total number of BusyHere errors received. | Int64
> bhrerrtx | Total number of BusyHere errors transmitted. | Int64
> rqcerrrx | Total number of RequestCancel errors received. | Int64
> rqcerrtx | Total number of RequestCancel errors transmitted. | Int64
> namerrrx | Total number of NotAcceptableMedia errors received. | Int64
> namerrtx | Total number of NotAcceptableMedia errors transmitted. | Int64
> beerrrx | Total number of BusyEverywhere errors received. | Int64
> beerrtx | Total number of BusyEverywhere errors transmitted. | Int64
> trperrrx | Total number of Request Pending errors received. | Int64
> trperrtx | Total number of Request Pending errors transmitted. | Int64
> udperrrx | Total number of Undecipherable errors received. | Int64
> udperrtx | Total number of Undecipherable errors transmitted. | Int64
> sarerrrx | Total number of sec-agree Required errors received. | Int64
> sarerrtx | Total number of Sec-agree Required errors transmitted. | Int64
> ineerrrx | Total number of InternalError errors received. | Int64
> ineerrtx | Total number of InternalError errors transmitted. | Int64
> nimerrrx | Total number of NotImplemented errors received. | Int64
> nimerrtx | Total number of NotImplemented errors transmitted. | Int64
> bgterrrx | Total number of BadGateway errors received. | Int64
> bgterrtx | Total number of BadGateway errors transmitted. | Int64
> suaerrrx | Total number of ServiceUnavailable errors received. | Int64
> suaerrtx | Total number of ServiceUnavailable errors transmitted. | Int64
> gtterrrx | Total number of GatewayTimeout errors received. | Int64
> gtterrtx | Total number of GatewayTimeout errors transmitted. | Int64
> bsverrrx | Total number of BadSipVersion errors received. | Int64
> bsverrtx | Total number of BadSipVersion errors transmitted. | Int64
> mtlerrrx | Total number of Message Too Large errors received. | Int64
> mtlerrtx | Total number of Message Too Large errors transmitted. | Int64
> pcferrrx | Total number of Precondition Failure errors received. | Int64
> pcferrtx | Total number of Precondition Failure errors transmitted. | Int64
> bewerrrx | Total number of BusyEverywhere errors received. | Int64
> bewerrtx | Total number of BusyEverywhere errors transmitted. | Int64
> decerrrx | Total number of Decline errors received. | Int64
> decerrtx | Total number of Decline errors transmitted. | Int64
> neaerrrx | Total number of NotExistAnywhere errors received. | Int64
> neaerrtx | Total number of NotExistAnywhere errors transmitted. | Int64
> nac606errrx | Total number of NotAcceptable(606) errors received. | Int64
> nac606errtx | Total number of NotAcceptable(606) errors transmitted. | Int64
> mo-call-succ-rate | Mobile Originating calls success rate. | Float
> mt-call-succ-rate | Mobile Terminating calls success rate. | Float
> mo-voice-call-succ-rate | Mobile Originating VOICE calls success rate. | Float
> mt-voice-call-succ-rate | Mobile Terminating VOICE calls success rate. | Float
> mo-video-call-succ-rate | Mobile Originating VIDEO calls success rate. | Float
> mt-video-call-succ-rate | Mobile Terminating VIDEO calls success rate. | Float
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883