> show nw-reachability server all
> show nw-reachability server Command Output Descriptions

> Field | Description
> Server | The name that was configured for this server in the current context.
> remote-addr | The IP address to which ping packets are sent in order to determine network reachability.
> local-addr | The IP address that is used as the source address of ping packets sent to the reachability server.
> state | The state of the network reachability server. Either Up or Down. Up: The server is responding to ping packets. Down: The server is not responding to ping packets.
> Total Network Reachability Servers: | The total number of network reachability servers that are configured in the current context.
> Up: | The number of network reachability servers that are responding.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883