> CSCF Translation Configuration Mode Commands
> The CSCF Translation Configuration Mode is used to configure session re-addressing within the system.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> after
> Places the CSCF translation entry at the bottom or end of the translation list. Use this command in conjunction with the uri-readdress command.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> after
> Usage
> Add this command before the uri-readdress command to place the entry at the end of the translation list.
> before
> Places the CSCF translation entry at the top or beginning of the translation list. Use this command in conjunction with the uri-readdress command.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> before
> Usage
> Add this command before the uri-readdress command to place the entry at the beginning of the translation list.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> uri-readdress
> Configures readdress criteria for URI translations.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> uri-readdress type trans_type [ log ] { base-criteria criteria } [ filter-criteria1 criteria ] [ filter-criteria2 criteria ]
> no uri-readdress type trans_type { base-criteria criteria } [ filter-criteria1 criteria ] [ filter-criteria2 criteria ]
> type trans_type
> Specifies that the translation list (trans_type) entry is to be identified as one of the following:
> blocking-cid: Identifies the translation list entry type as “call ID blocking”.
> cancel-blocking-cid: Identifies the translation list entry type as “cancel call ID blocking”.
> cancel-cid: Identifies the translation list entry type as “cancel call ID display”.
> cancel-cw: Identifies the translation list entry type as “cancel call-waiting”.
> cfbl-off: Identifies the translation list entry type as “call forward busy line off”.
> cfbl-on: Identifies the translation list entry type as “call forward busy line on”.
> cfna-off: Identifies the translation list entry type as “call forward no answer off”.
> cfna-on: Identifies the translation list entry type as “call forward no answer on”.
> cfu-off: Identifies the translation list entry type as “call forward unconditional off”.
> cfu-on: Identifies the translation list entry type as “call forward unconditional on”.
> cid: Identifies the translation list entry type as “call ID display”.
> cw-off: Identifies the translation list entry type as “call-waiting off”.
> cw-on: Identifies the translation list entry type as “call-waiting on”.
> directory-assistance: Identifies the translation list entry type as “directory assistance”.
> emergency: Identifies the translation list entry type as “emergency”.
> international: Identifies the translation list entry type as “international”.
> local: Identifies the translation list entry type as “local”.
> long-distance: Identifies the translation list entry type as “long-distance”.
> none: Identifies the translation list entry type as “any”.
> operator-assistance: Identifies the translation list entry type as “operator assistance”.
> premium-service: Identifies the translation list entry type as “premium service”.
> service: Identifies the translation list entry type as “special service”.
> tollfree: Identifies the translation list entry type as “toll free”.
> log
> Enables logging for CSCF sessions meeting the readdress criteria for URI translations.
> base-criteria criteria
> Specifies the base criteria that packets will be compared against. The following criteria is supported:

> • | any: Filters all CSCF sessions.

> • | destination aor aor: Filters sessions based on the destination AoR. aor must be an existing AoR from 1 to 79 characters in length.

> Important: AoR regular expressions are supported. Refer to the SCM Engineering Rules Appendix in the Session Control Manager Administration Guide for more information about regular expressions.

> • | plmn-id mcc mcc_code mnc mnc_code: Filters sessions based on the mobile country and network codes. mcc_code must be a three-digit integer from 200 to 999. mnc_code must be either a two or three-digit integer from 00 to 999 or any (any MNC code).

> • | source address ip_address: Filters sessions based on source IP address. ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

> • | source aor aor: Filters sessions based on the source AoR. aor must be an existing AoR from 1 to 79 characters in length.

> filter-criteria1 criteria
> Specifies the filter criteria that packets that have passed the base criteria will be compared against. The following criteria is supported:

> • | any: Filters all CSCF sessions.

> • | destination aor aor: Filters sessions based on the destination AoR. aor must be an existing AoR from 1 to 79 characters in length.

> Important: AoR regular expressions are supported. Refer to the SCM Engineering Rules Appendix in the Session Control Manager Administration Guide for more information about regular expressions.

> • | plmn-id mcc mcc_code mnc mnc_code: Filters sessions based on the mobile country and network codes. mcc_code must be a three-digit integer from 200 to 999. mnc_code must be either a two or three-digit integer from 00 to 999 or any (any MNC code).

> • | source address ip_address: Filters sessions based on source IP address. ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

> • | source aor aor: Filters sessions based on the source AoR. aor must be an existing AoR from 1 to 79 characters in length.

> filter-criteria2 criteria
> Specifies the filter criteria that packets that have passed the base criteria and filter criteria1 will be compared against. The following criteria is supported:

> • | any: Filters all CSCF sessions.

> • | destination aor aor: Filters sessions based on the destination AoR. aor must be an existing AoR from 1 to 79 characters in length.

> Important: AoR regular expressions are supported. Refer to the SCM Engineering Rules Appendix in the Session Control Manager Administration Guide for more information about regular expressions.

> • | plmn-id mcc mcc_code mnc mnc_code: Filters sessions based on the mobile country and network codes. mcc_code must be a three-digit integer from 200 to 999. mnc_code must be either a two or three-digit integer from 00 to 999 or any (any MNC code).

> • | source address ip_address: Filters sessions based on source IP address. ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

> • | source aor aor: Filters sessions based on the source AoR. aor must be an existing AoR from 1 to 79 characters in length.

> no uri-readdress type trans_type { base-criteria criteria } [ filter-criteria1 criteria ] [ filter-criteria2 criteria ]
> Remove the readdress configuration.
> Usage
> Use this command to readdress URIs based on specified criteria and enters the URI Readdress Configuration Mode. Readdressing can be used for:

> • | Mobility: When roaming in a visited domain.

> • | Service Aliases: Resolving well-known addresses via SIP-AS.

> • | Number Translation: Adding or deleting prefixes such as +1 to/from PSTN numbers.

> • | Voice VPNs: Using inter-office extensions to dial remote offices.

> Entering this command results in the following prompt:
> [context_name]hostname(config-uri-readdress)#
> URI readdress commands are defined in the CSCF URI Readdress Configuration Mode Commands chapter of this reference.
> Example
> The following command readdresses sessions to a domain named service.com, filters sessions with a base criteria of the source address (1.2.3.4) and a filter criteria of the destination AoR ($.@test.com):
> uri-readdress type service base-criteria source address 1.2.3.4 filter-criteria1 destination aor $.@test.com

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883