> show mag-service
> This chapter includes the show mag-service command output tables.
> show mag-service statistics
> show mag-service statistics Command Output Descriptions

> Field | Description
> Binding Update Sent
> Total | The total number of all binding updates sent by this system or the specified service.
> Init Request Xmit | The total number of initial request transmit binding updates sent by this system or the specified service.
> Init Request Re-Xmit | The total number of initial request retransmit binding updates sent by this system or the specified service.
> Renew Request Xmit | The total number of renew request transmit binding updates sent by this system or the specified service.
> Renew Request Re-Xmit | The total number of renew request retransmit binding updates sent by this system or the specified service.
> Dereg Request Xmit | The total number of deregistration request transmit binding updates sent by this system or the specified service.
> Dereg Request Re-Xmit | The total number of deregistration request retransmit binding updates sent by this system or the specified service.
> Binding Acknowledgement Rcvd
> Total | The total number of all binding acknowledgements received by this system or the specified service.
> Errors | The total number of all binding acknowledgements, with errors, received by this system or the specified service.
> Accepted | The total number of all binding acknowledgements received, and accepted by this system or the specified service.
> Denied | The total number of all binding acknowledgements received, but denied by this system or the specified service.
> Init Reply Rcvd | The total number of all binding acknowledgements - initial reply received by this system or the specified service.
> Renew Reply Rcvd | The total number of all binding acknowledgements - renew reply received by this system or the specified service.
> Dereg Reply Rcvd | The total number of all binding acknowledgements - deregistration reply received by this system or the specified service.
> Denied by LMA
> Insufficient Resources | The total number of binding updates sent by this system or the specified service but denied by the LMA due to insufficient resources.
> Mismatched ID | The total number of binding updates sent by this system or the specified service but denied by the LMA due to mismatched IDs.
> MN Auth Failure | The total number of binding updates sent by this system or the specified service but denied by the LMA due to mobile node authorization failures.
> Admin Prohibited | The total number of binding updates sent by this system or the specified service but denied by the LMA due to admin prohibited conditions.
> Msg ID Required | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing message IDs.
> DAD Failed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to DAD failures.
> Not Home Subnet | The total number of binding updates sent by this system or the specified service but denied by the LMA due to incorrect home subnet.
> Sequence Out Of Window | The total number of binding updates sent by this system or the specified service but denied by the LMA due to sequence out of window conditions.
> Reg Type Change Disallowed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to registration type change disallowed.
> Unspecified Reason | The total number of binding updates sent by this system or the specified service but denied by the LMA due to unspecified reasons.
> Service-Authorization Failed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to failed service authorizations.
> Proxy Reg Not Enabled | The total number of binding updates sent by this system or the specified service but denied by the LMA due to proxy registration not being enabled.
> Timestamp Mismatch | The total number of binding updates sent by this system or the specified service but denied by the LMA due to timestamp mismatches.
> Timestamp Lower Than Expected | The total number of binding updates sent by this system or the specified service but denied by the LMA due to lower than expected timestamps.
> Missing MN-ID Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing mobile node ID options.
> Missing HNP Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing HNP options.
> Missing Access Tech Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing access technology options.
> Missing Handoff Ind Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing handoff indication options.
> Not Authorized For HNP | The total number of binding updates sent by this system or the specified service but denied by the LMA due to not being authorized for HNP.
> Not LMA For Mobile | The total number of binding updates sent by this system or the specified service but denied by the LMA due incorrect LMA for mobility.
> Not Authorized For Proxy Reg | The total number of binding updates sent by this system or the specified service but denied by the LMA due to not being authorized for proxy registration.
> BCE Prefix Do Not Match | The total number of binding updates sent by this system or the specified service but denied by the LMA due to BCE prefix mismatches.
> Binding Acknowledgement Error Reason
> Missing HNP | The total number of binding acknowledgements with missing HNP errors received by this system or the specified service.
> Missing NAI | The total number of binding acknowledgements with missing NAI errors received by this system or the specified service.
> Home Address Conflict | The total number of binding acknowledgements with home address conflict errors received by this system or the specified service.
> Matching Request Not Found | The total number of binding acknowledgements with matching requests not found errors received by this system or the specified service.
> Badly Formed | The total number of binding acknowledgements with badly formed message errors received by this system or the specified service.
> Binding Revocation
> Sent | The total number of binding revocations sent by this system or the specified service.
> Retries Sent | The total number of binding revocation retries sent by this system or the specified service.
> Ack Rcvd | The total number of binding revocation acknowledgements received by this system or the specified service.
> Not Acknowledged | The total number of binding revocations sent, but not acknowledged, by this system or the specified service.
> Rcvd | The total number of binding revocations received by this system or the specified service.
> Ack Sent | The total number of binding revocation acknowledgements sent by this system or the specified service.
> Received Binding Revocation Trigger Reasons
> Unspecified | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Unspecified” revocation trigger reason.
> Administrative Reason | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Administrative Reason” revocation trigger reason.
> Inter-MAG Handoff-Same ATT | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Inter-MAG Handoff-Same ATT” revocation trigger reason.
> Inter-MAG - Unknown Handoff | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Inter-MAG - Unknown Handoff” revocation trigger reason.
> Inter-MAG Handoff-Diff ATT | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Inter-MAG Handoff-Diff ATT” revocation trigger reason.
> Per-Peer Policy | The total number of Binding Revocation Indication (BRI) messages received by the MAG with a “Per-Peer Policy” revocation trigger reason.
> Revoking Node Local Policy | The total number of Binding Revocation Indication (BRI) messages received by the MAG with a “Revoking Node Local Policy” revocation trigger reason.
> User Initiated Session Term | The total number of Binding Revocation Indication (BRI) messages received by the MAG with a “User Initiated Session Term” revocation trigger reason.
> Access Network Session Term | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Access Network Session Term” revocation trigger reason.
> Out-of Sync BCE State | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Out-of Sync BCE State” revocation trigger reason.
> Unknown | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Unknown” revocation trigger reason.
> Sent Revocation ACK Status
> Success | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Success” status.
> Partial-Success | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Partial-Success” status.
> Binding-Does-Not-Exist | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Binding-Does-Not-Exist” status.
> No IPv4-HoA-Bind | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “No IPv4-HoA-Bind” status.
> Global-Revoc-Not-Authorized | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Global-Revoc-Not-Authorized” status.
> Revoc-MN-ID-Required | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Revoc-MN-ID-Required” status.
> Revoc-Failed-MN-Attached | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Revoc-Failed-MN-Attached” status.
> Trigger-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Trigger-Not-Supported” status.
> Proxy-Bind-Rev-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Proxy-Bind-Rev-Not-Supported” status.
> Revoc-Func-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Revoc-Func-Not-Supported” status.
> Unknown | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with an “Unknown” status.
> Binding Revocation Indication Discarded
> Total | The total number of binding revocation acknowledgements received and discarded by this system or the specified service.
> Session Not Found | The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by this system or the specified service.
> Badly Formed Request | The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by this system or the specified service.
> Decode Error | The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by this system or the specified service.
> Checksum Error | The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by this system or the specified service.
> Invalid Message Type | The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by this system or the specified service.
> No Memory | The total number of binding revocation acknowledgements received and discarded, due to insufficient memory, by this system or the specified service.
> Tunnel Data Received
> Total Packets | The total number of tunnel packets received by this system or the specified service.
> 6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel packets received by this system or the specified service. The total number of IPv4-in-IPv6 tunnel packets received by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel packets received by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel packets received by this system or the specified service.
> Total Bytes | The total number of tunnel bytes received by this system or the specified service.
> 6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel bytes received by this system or the specified service. The total number of IPv4-in-IPv6 tunnel bytes received by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel bytes received by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel bytes received by this system or the specified service.
> Errors
> Protocol Type Error | The total number of protocol type data errors received by this system or the specified service.
> Invalid Pkt Length | The total number of invalid packet length data errors received by this system or the specified service.
> No Session Found | The total number of no session found data errors received by this system or the specified service.
> Tunnel Data Sent
> Total Packets | The total number of tunnel packets sent by this system or the specified service.
> 6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel packets sent by this system or the specified service. The total number of IPv4-in-IPv6 tunnel packets sent by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel packets sent by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel packets sent by this system or the specified service.
> Total Bytes | The total number of tunnel bytes sent by this system or the specified service.
> 6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel bytes sent by this system or the specified service. The total number of IPv4-in-IPv6 tunnel bytes sent by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel bytes sent by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel bytes sent by this system or the specified service.
> Total Disconnects/Failures |
> Lifetime expiry | The total number of disconnects due to lifetime expiry initiated by this system or the specified service.
> Access Initiated Term | The total number of disconnects due to deregistrations initiated by this system or the specified service.
> Admin Drops | The total number of disconnects due to admin drops initiated by this system or the specified service.
> Other Reasons | The total number of disconnects due to “other reasons” initiated by this system or the specified service.
> LMA Revocations | The total number of disconnects due to LMA revocations received by this system or the specified service.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883