> show linecard
> This chapter describes the outputs of the show linecard command.
> show linecard table
> show linecard table Command Output Descriptions

> Field | Description
> Slot | DIsplays the chassis slot number and type. The slot type represents the type of card(s) that the slot supports. Possible slot types are: Slots 17 through 23, 26 through 39, and slots 42 through 48: Supports Ethernet 10/100, Ethernet 1000 linecard, four-port Quad Gig-E (QGLC) line card (ASR 5000 only) 10 Gigabit Ethernet Line Card (XGLC) is a full-length line card. Only upper slots 17 through 23 and 26 through 32 are used when referring to this card.Slots 24 and 25: Support the Switch Processor Input/Output (SPIO) card
> Card Type | Displays the type of card installed. The possible card types supported for this release are: Ethernet 10/100 Line CardEthernet 1000 Line Card (QGLC)10 Gig Ethernet Line Card (XGLC)Switch Processor Input/Output CardDS3 Line Card
> # Ports | Displays the maximum number of physical ports supported per card. The Ethernet 10/100 Line Card supports 8 ports.The Ethernet 1000 Line Card supports 1 port.The Quad Gig-E (QGLC) Line Card supports 4 portsThe 10 Gig Ethernet Line Card (XGLC) supports 1 portThe Switch Processor Input/Output Card supports 2 ports.The DS3 Line Card supports 3 ports.
> Oper State | Displays the operational state of the card. The possible operational states are: Active: Indicates that the card is an active component that will be used to process subscriber data sessions.Standby: Indicates that the card is a redundant component. Redundant components will become active through manual configuration or automatically should a failure occur.Offline: Indicates that the card is installed but is not ready to process subscriber data sessions. This could be due to the fact that it is not completely installed (i.e. the card interlock switch is not locked, refer to the System Installation Guide for information on installing cards in the system) or that its processes have been halted.
> SPOF | Displays whether or not the component is a single point of failure (SPOF) in the system. If the component is an SPOF, then a Yes will appear in this column. If not, a No will be displayed.
> Attach | Displays the PACs/PSC/PSC2s and SPCs/SMCs that the line cards are being associated with.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883