> Starent Chassis MIB
> The following figure displays the hierarchical structure of the management information base (MIB) for the core platform
> MIB Textual Conventions
> The following are the supported MIB Objects and Notifications. Not all entries are supported on all platforms. Some may return a different output than expected.
> Object
> StarentSlotType
> Object ID
> N/A
> Syntax
> Describes the type of a slot. Each slot in the chassis is build to contain specific type(s) of cards. Only a card of one of the appropriate types can be put into a specific slot.
> Enumeration
> unknown(1)
> pactac(2)
> spc(3)
> lc(4)
> rcc(5)
> spio(6)
> Object
> StarentCardType
> Object ID
> N/A
> Description
> Describes the type of a card. Each type represents a physically different card which would have a unique part number.
> Syntax
> Integer
> Enumeration
> none(1)
> unknown(2)
> spc(3)
> pac(4)
> spio(5)
> rcc(6)
> lceth(7)
> lcgeth(8)
> lcds3
> tac(10)
> Icoc3(11)
> Icoc12(12)
> smc(13)
> psc(14)
> lcqgeth(15)
> lctgeth(16)
> vmc(17)
> vpc(18)
> vlceth1p(19)
> Object
> StarentVersionNum
> Object ID
> N/A
> Description
> Contains the system version identification string.
> Syntax
> Octet String (0.. 256)
> Object
> StarRelayState
> Object ID
> N/A
> Description
> The state of a Central Office (CO) relay.
> Syntax
> Integer
> Enumeration
> off(1)
> on(2)
> unknown(3)
> Object
> StarLongDurTimeoutAction
> Object ID
> N/A
> Description
> The action taken by the system upon detection of a long-duration session.
> Syntax
> INTEGER
> Enumeration
> unknown(0)
> detection(1)
> disconnection(2)
> notapplicable(3)
> dormantdisconnection(4)
> dormantdetection(5)
> Object
> StarShortName
> Object ID
> N/A
> Description
> short identification string. Follows the same conventions as the DisplayString TEXTUAL-CONVENTION.
> Syntax
> Octet String (1..32)
> Object
> StarShortID
> Object ID
> N/A
> Description
> An abbreviated form for identifying a service, composed of the first 8 characters of the context name, and the first 8 characters of a service name, separated by (:)
> Syntax
> OCTET STRING(1..17)
> Object
> StarMediumID
> Object ID
> N/A
> Description
> An abbreviated form for identifying a context-specific object, composed of the first 8 characters of the context name, and the first 16 characters of the object name, separated by (:)
> Syntax
> OCTET STRING (SIZE (1..25))
> Object
> StarQOSTPAction
> Object ID
> N/A
> Description
> Traffic Policing Action
> Syntax
> INTEGER
> Enumeration
> unknown(0)
> notapplicable(1)
> transmit(2)
> drop(3)
> loweripprecedence(4)
> Object
> StarOSPFNeighborState
> Object ID
> N/A
> Description
> OSPF Neighbor State
> Syntax
> INTEGER
> Enumeration
> unknown(0),
> down(1),
> attempt(2),
> init(3),
> twoway(4),
> exstart(5),
> exchange(6),
> loading(7),
> full(8)
> starentMIB(8164).starentMIBObjects(1).starentChassis(1)
> Object
> starChassisCriticalCO
> Object ID
> enterprises.8164.1.1.1
> Description
> The current state of the Critical Central Office (CO) relay.
> Syntax
> StarRelayState
> Access
> Read-only
> Object
> starChassisMajorCO
> Object ID
> enterprises.8164.1.1.2
> Description
> The current state of the Major Central Office (CO) relay.
> Syntax
> StarRelayState
> Access
> Read-only
> Object
> starChassisMinorCO
> Object ID
> enterprises.8164.1.1.3
> Description
> The current state of the Minor Central Office (CO) relay.
> Syntax
> StarRelayState
> Access
> Read-only
> Object
> starChassisAction
> Object ID
> enterprises.8164.1.1.5
> Description
> Trigger to perform certain system-wide operations. noaction (1) performs no operation. It is the normal value received when this attribute is read. testled (2) triggers a test of all of the LEDs in the system. aco (3) triggers the Alarm Cut-Off, which shuts off all of the Central Office (CO) audible/visual relays. reset (4) triggers a system-wide restart. It will completely disrupt service on the device.
> Syntax
> Integer
> Access
> Read-write
> Enumeration
> noaction(1)
> testled(2)
> aco(3)
> reset(4)
> Object
> starTimeTicks
> Object ID
> enterprises.8164.1.1.6
> Description
> The number of system clock ticks since the last system Epoch. One system clock tick is 10 milliseconds.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starChassisAudibleAlarm
> Object ID
> enterprises.8164.1.1.7
> Description
> The current state of the chassis Audible Alarm.
> Syntax
> StarRelayState
> Access
> Read-only
> Object
> starChassisUTCTime
> Object ID
> enterprises.8164.1.1.8
> Description
> The current time on the chassis, in UTC format
> Syntax
> DateAndTime
> Access
> Read-only
> Object
> starChassisLocalTime
> Object ID
> enterprises.8164.1.1.9
> Description
> The current time on the chassis, converted to the local time zone
> Syntax
> DateAndTime
> Access
> Read-only
> Object
> starChassisType
> Object ID
> enterprises.8164.1.1.10
> Description
> The physical chassis type
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(0)
> ST16(1)
> ST40(2)
> XT2(3)
> st20(4)
> Object
> starChassisDescription
> Object ID
> enterprises.8164.1.1.11
> Description
> Chassis description
> Syntax
> DisplayString
> Access
> Read-Only
> Object
> starChassisSWRevision
> Object ID
> enterprises.8164.1.1.12
> Description
> Software revision
> Syntax
> DisplayString
> Access
> Read-Only
> Object
> starChassisPeakMemoryUsage
> Object ID
> enterprises.8164.1.1.13
> Description
> The system level peak memory usage, in kilobytes, rounded down (i.e. 1023 bytes = 0kilobytes)
> Syntax
> Integer32(1..2097152)
> Access
> Read-Only
> starentMIB(8164).starentMIBObjects(1).starentSlots(2)
> Object
> starSlotTable
> Object ID
> enterprises.8164.1.2.1
> Description
> A table containing information on all of the slots.
> Syntax
> Sequence of StarSlotEntry
> Access
> Not-accessible
> Object
> starSlotEntry
> Object ID
> enterprises.8164.1.2.1.1
> Description
> Information about a particular slot.
> Syntax
> StarSlotEntry
> Access
> Not-accessible
> Sequence
> starSlotNum
> starSlotType
> starCardType
> starCardOperState
> starCardAdminState
> starCardRevision
> starCardLastStateChange
> starCardMode
> starCardDesiredMode
> starCardPacStandbyPriority
> starCardLock
> starCardHaltIssued
> starCardRebootPending
> starCardUsable
> starCardSinglePOF
> starCardAttachment
> starCardTemperature
> starSlotVoltage1dot5
> starSlotVoltage1dot5LowThresh
> starSlotVoltage1dot5HighThresh
> starSlotVoltage1dot8
> starSlotVoltage1dot8LowThresh
> starSlotVoltage1dot8HighThresh
> starSlotVoltage2dot5
> starSlotVoltage2dot5LowThresh
> starSlotVoltage2dot5HighThresh
> starSlotVoltage3dot3
> starSlotVoltage3dot3LowThresh
> starSlotVoltage3dot3HighThresh
> starSlotVoltage5dot0
> starSlotVoltage5dot0LowThresh
> starSlotVoltage5dot0HighThresh
> starSlotNumPorts
> starSlotVoltageState
> starSlotNumCpu
> starSlotNum
> Object ID
> enterprises.8164.1.2.1.1.1
> Description
> The slot number.
> Syntax
> Integer32(1..48)
> Access
> Not-accessible
> Object
> starSlotType
> Object ID
> enterprises.8164.1.2.1.1.2
> Description
> The type of the slot.
> Syntax
> StarentSlotType
> Access
> Read-only
> Object
> starCardType
> Object ID
> enterprises.8164.1.2.1.1.3
> Description
> The type of the card which is plugged into a slot.
> Syntax
> StarentCardType
> Access
> Read-only
> Object
> starCardOperState
> Object ID
> enterprises.8164.1.2.1.1.4
> Description
> The current operational state of the card.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(1)
> empty(2)
> offline(3)
> booting(4)
> ready(5)
> standby(6)
> active(7)
> migratefrom(8)
> migrateto(9)
> Object
> starCardAdminState
> Object ID
> enterprises.8164.1.2.1.1.5
> Description
> The current administrative state of the card.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(1)
> enabled(2)
> disabled(3)
> Object
> starCardRevision
> Object ID
> enterprises.8164.1.2.1.1.6
> Description
> The revision number of the card that is physically present in this slot.
> Syntax
> StarentVersionNum
> Access
> Read-only
> Object
> starCardLastStateChange
> Object ID
> enterprises.8164.1.2.1.1.7
> Description
> The time when the last state change occurred for this row. A manager could poll this variable to determine if information has changed.
> Syntax
> DateAndTime
> Access
> Read-only
> Object
> starCardMode
> Object ID
> enterprises.8164.1.2.1.1.8
> Description
> The desired mode of the card. This field is applicable only to slots which can contain PAC/PSC and TAC cards. The active(4) value is obsolete and has been replaces with activepac(5) and activetac(6).
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(1)
> notapplicable(2)
> standby(3)
> active(4)
> activepac(5)
> activetac(6)
> activepsc(7)
> activevpc(8)
> Object
> starCardPacStandbyPriority
> Object ID
> enterprises.8164.1.2.1.1.9
> Description
> Specifies the standby priority of the packet accelerator card.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starCardHaltIssued
> Object ID
> enterprises.8164.1.2.1.1.10
> Description
> Only applicable to SPC cards.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> notapplicable(1)
> yes(2)
> no(3)
> Object
> starCardLock
> Object ID
> enterprises.8164.1.2.1.1.11
> Description
> Identifies if the card lock is currently engaged. A value of locked(2) means that the lock is engaged, and thus the card could not be removed from the chassis. A value of unlocked(3) means that the lock is not engaged, and an operator could remove the card from the chassis. A value of unknown(1) should represent that there is no card physically in the slot.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(1)
> locked(2)
> unlocked(3)
> Object
> starCardRebootPending
> Object ID
> enterprises.8164.1.2.1.1.12
> Description
> Identifies if a reboot operation is currently pending for this card.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> no(1)
> yes(2)
> Object
> starCardUsable
> Object ID
> enterprises.8164.1.2.1.1.13
> Description
> Indicates if the card is currently usable.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> no(1)
> yes(2)
> Object
> starCardSinglePOF
> Object ID
> enterprises.8164.1.2.1.1.14
> Description
> Identifies if this card represents a single point of failure (POF). A value of no(1) indicates that this card is supported by a redundant card which can take over in the event of a failure. A value of yes(2) indicates that this card does not have a redundant partner, and that a failure of this card could result in service interruption.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> notapplicable(1)
> no(2)
> yes(3)
> Object
> starCardAttachment
> Object ID
> enterprises.8164.1.2.1.1.15
> Description
> Identifies if the card is currently attached to another card (a PAC/PSC attached to a line card, or visa versa, for example)
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> connected(1)
> unconnected(2)
> Object
> starCardTemperature
> Object ID
> enterprises.8164.1.2.1.1.16
> Description
> The temperature, in degrees Celsius, as measured on the card. A value of 0 indicates that the temperature cannot be read, or that the card is not present. The maximum measurable temperature is 70 C.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSlotVoltage1dot5
> Object ID
> enterprises.8164.1.2.1.1.20
> Description
> The current voltage, in millivolts, of the nominal 1.5V power supply. The working range for this card is the range defined by variables starSlotVoltage1dot5LowThresh and starSlotVoltage1dot5HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage1dot5LowThresh
> Object ID
> enterprises.8164.1.2.1.1.21
> Description
> The voltage level, in millivolts, which is the lowest allowable value for the nominal 1.5V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage1dot5HighThresh
> Object ID
> enterprises.8164.1.2.1.1.22
> Description
> The voltage level, in millivolts, which is the highest allowable value for the nominal 1.5V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage1dot8
> Object ID
> enterprises.8164.1.2.1.1.23
> Description
> The current voltage, in millivolts, of the nominal 1.8V power supply. The working range for this card is the range defined by variables starSlotVoltage1dot8LowThresh and starSlotVoltage1dot8HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification
> Object
> starSlotVoltage1dot8LowThresh
> Object ID
> enterprises.8164.1.2.1.1.24
> Description
> The voltage level, in millivolts, which is the lowest allowable value for the nominal 1.8V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage1dot8HighThresh
> Object ID
> enterprises.8164.1.2.1.1.25
> Description
> The voltage level, in millivolts, which is the highest allowable value for the nominal 1.8V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage2dot5
> Object ID
> enterprises.8164.1.2.1.1.26
> Description
> The current voltage, in millivolts, of the nominal 2.5V power supply. The working range for this card is the range defined by variables starSlotVoltage2dot5LowThresh and starSlotVoltage2dot5HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage2dot5LowThresh
> Object ID
> enterprises.8164.1.2.1.1.27
> Description
> The voltage level, in millivolts, which is the lowest allowable value for the nominal 2.5V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage2dot5HighThresh
> Object ID
> enterprises.8164.1.2.1.1.28
> Description
> The voltage level, in millivolts, which is the highest allowable value for the nominal 2.5V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage3dot3
> Object ID
> enterprises.8164.1.2.1.1.29
> Description
> The current voltage, in millivolts, of the nominal 3.3V power supply. The working range for this card is the range defined by variables starSlotVoltage3dot3LowThresh and starSlotVoltage3dot3HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage3dot3LowThresh
> Object ID
> enterprises.8164.1.2.1.1.30
> Description
> The voltage level, in millivolts, which is the lowest allowable value for the nominal 3.3V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage3dot3HighThresh
> Object ID
> enterprises.8164.1.2.1.1.31
> Description
> The voltage level, in millivolts, which is the highest allowable value for the nominal 3.3V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage5dot0
> Object ID
> enterprises.8164.1.2.1.1.32
> Description
> The current voltage, in millivolts, of the nominal 5.0V power supply. The working range for this card is the range defined by variables starSlotVoltage5dot0LowThresh and starSlotVoltage5dot0HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage5dot0LowThresh
> Object ID
> enterprises.8164.1.2.1.1.33
> Description
> The voltage level, in millivolts, which is the lowest allowable value for the nominal 5.0V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.
> Object
> starSlotVoltage5dot0HighThresh
> Object ID
> enterprises.8164.1.2.1.1.34
> Description
> The voltage level, in millivolts, which is the highest allowable value for the nominal 5.0V power supply. A value of 0 indicates that there is no card present.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification
> Object
> starSlotNumPorts
> Object ID
> enterprises.8164.1.2.1.1.35
> Description
> Number of data ports on this card. This value will be 0 for cards that no not contain ports, such as SPC/PAC/TAC cards, or for slots which do not contain a card.
> Syntax
> Gauge32
> Access
> Read-only
> Important: This alarm is obsolete.
> Object
> starSlotAction
> Object ID
> enterprises.8164.1.2.1.1.36
> Description
> Trigger to perform certain slot operations. noaction(1) performs no operation. It is the normal value received when this attribute is read. reset(2) causes the slot to be reset.
> Syntax
> Integer
> Access
> Read-write
> Enumeration
> noaction(1)
> reset(2)
> Object
> starSlotVoltageState
> Object ID
> enterprises.8164.1.2.1.1.37
> Description
> The state of the voltage supplies on the card. A value of unknown(0) means that the state cannot be identified; normal(1) represents a properly functioning card; outofrange(2) indicates that one or more voltage sources are not within their specified operating range.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(0)
> normal(1)
> outfrange(2)
> Object
> starSlotNumCpu
> Object ID
> enterprises.8164.1.2.1.1.38
> Description
> The number of general purpose CPU on this card.
> Syntax
> Integer32
> Access
> Read-only
> Object
> starSlotPartNumber
> Object ID
> enterprises.8164.1.2.1.1.39
> Description
> The part number of this card.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSlotPartRevision
> Object ID
> enterprises.8164.1.2.1.1.40
> Description
> The revision number of this card.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSlotSerialNumber
> Object ID
> enterprises.8164.1.2.1.1.41
> Description
> The serial number of this card.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSlotCLEICode
> Object ID
> enterprises.8164.1.2.1.1.42
> Description
> The CLEI code of this card.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSlotCiscoModelName
> Object ID
> enterprises.8164.1.2.1.1.43
> Description
> Cisco-defined Product Identifier (PID). The PID is an alphanumeric identifier used to identify specific Cisco product hardware, and may be up to 18 characters in length.
> starSlotCiscoModelName will be blank (zero characters) if no PID is available.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSlotCiscoHardwareRev
> Object ID
> enterprises.8164.1.2.1.1.44
> Description
> Cisco-defined Version Identifier (VID). The VID is used to track the version of the Customer-Orderable Cisco Product Identifier (PID) [starSlotCiscoModelName]. The data convention for VID is 'V' followed by a two digit number. VID numbering typically begins at 'V01' but can be initiated at a higher value.
> starSlotCiscoModelName will be blank (zero characters) if no PID is available.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSlotCiscoSerialNumber
> Object ID
> enterprises.8164.1.2.1.1.45
> Description
> Cisco-defined Serial Number (SN). The SN is an 11 character identifier used in conjunction with the Cisco Product Identifier (PID) [starSlotCiscoModelName] to identify a unique product or Field Replaceable Unit (FRU) of a product.
> starSlotCiscoSerialNumber will be blank (zero characters) if no VID is available.
> Syntax
> DisplayString
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentSlotMapping(3)
> Object
> starSlotMappingTable
> Object ID
> enterprises.8164.1.3.1
> Description
> A table identifying all of the slot mappings.
> Syntax
> Sequence of StarSlotMappingEntry
> Access
> Not-accessible
> Object
> starSlotMappingEntry
> Object ID
> enterprises.8164.1.3.1.1
> Description
> Information about a particular slot mapping.
> Syntax
> StarSlotMappingEntry
> Access
> Not-accessible
> Sequence
> starSlotMappingNum Index
> starSlotMappingType
> starSlotMappingRCCNum
> starSlotMappingToSlot
> Object
> starSlotMappingNum
> Object ID
> enterprises.8164.1.3.1.1.1
> Description
> The slot number. This always represents a slot in the back of the chassis.
> Syntax
> Integer32(17..48)
> Access
> Not-accessible
> Object
> starSlotMappingType
> Object ID
> enterprises.8164.1.3.1.1.2
> Description
> The type of the slot mapping. The value none(1) represents that there is no mapping, which typically represents that there is no card present in this slot.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(1)
> none(2)
> direct(3)
> rcc(4)
> cross(5)
> Object
> starSlotMappingRCCNum
> Object ID
> enterprises.8164.1.3.1.1.3
> Description
> Identifies which RCC card is responsible for this mapping. This value is only valid if the value of starSlotMappingType is rcc(3).
> Syntax
> Integer32(0..2)
> Access
> Read-only
> Object
> starSlotMappingToSlot
> Object ID
> enterprises.8164.1.3.1.1.4
> Description
> The slot number this slot is mapped to. This always represents a slot in the front of the chassis.
> Syntax
> Integer32(1..16)
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentFans(4)
> Object
> starFanTable
> Object ID
> enterprises.8164.1.4.1
> Description
> A table containing information on all of the fan controllers.
> Syntax
> Sequence of StarFanEntry
> Access
> Not-accessible
> Object
> starFanEntry
> Object ID
> enterprises.8164.1.4.1.1
> Description
> Information about a particular fan controller.
> Syntax
> StarFanEntry
> Access
> Not-accessible
> Sequence
> starFanNum Index
> starFanLocation
> starFanStatus
> starFanSpeed
> Object
> starFanNum
> Object ID
> enterprises.8164.1.4.1.1.1
> Description
> The fan controller number.
> Syntax
> Integer32(1..2)
> Access
> Not-accessible
> Object
> starFanLocation
> Object ID
> enterprises.8164.1.4.1.1.2
> Description
> The physical location of the fan controller.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> upper(1)
> lower(2)
> Object
> starFanStatus
> Object ID
> enterprises.8164.1.4.1.1.3
> Description
> A bitmask representing the status of the fan tray. A normal, properly functioning fan tray would show 0x101 (257 decimal), meaning it is present (0x100) and all fans are working (0x1).
> Syntax
> Integer32
> Access
> Read-only
> Enumeration
> 0x01 All Fans Good
> 0x02 Multiple Fans Bad
> 0x04 Single Fan Bad
> 0x08 HB Error
> 0x10 COM A Error
> 0x20 COM B Error
> 0x40 COMM Error
> 0x80 Not Present
> 0x100 Present
> 0x200 Filter Clogged
> 0x400 State Unknown
> Object
> starFanSpeed
> Object ID
> enterprises.8164.1.4.1.1.4
> Description
> The speed of the fans controlled by this fan controller. The values represent the percentage that the speed is running relative to the maximum possible speed, speed100(12)
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(1)
> speed50(2)
> speed55(3)
> speed60(4)
> speed65(5)
> speed70(6)
> speed75(7)
> speed80(8)
> speed85(9)
> speed90(10)
> speed95(11)
> speed100(12)
> starentMIB(8164).starentMIBObjects(1).starentLogs(5)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starLogTable
> Object ID
> enterprises.8164.1.5.1
> Description
> A table containing information about all of the system logs.
> Syntax
> Sequence of StarLogEntry
> Access
> Not-accessible
> Object
> starLogEntry
> Object ID
> enterprises.8164.1.5.1.1
> Description
> Information about a particular system log.
> Syntax
> StarLogEntry
> Access
> Not-accessible
> Sequence
> starLogName Index
> starLogCurSize
> starLogMaxSize
> starLogText
> Object
> starLogName
> Object ID
> enterprises.8164.1.5.1.1.1
> Description
> The name of the system log.
> Syntax
> StarShortName
> Access
> Not-accessible
> Object
> starLogCurSize
> Object ID
> enterprises.8164.1.5.1.1.2
> Description
> The size, in bytes, of this log.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starLogMaxSize
> Object ID
> enterprises.8164.1.5.1.1.3
> Description
> The maximum size, in bytes, of this log.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starLogText
> Object ID
> enterprises.8164.1.5.1.1.4
> Description
> For use in LogMsg trap.
> Syntax
> Octet String (SIZE (1..512))
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentAlertMan(8)
> starentFeedback(1)
> Object
> starMaxAlertsPerTime
> Object ID
> enterprises.8164.1.8.1.1
> Description
> The maximum number of SNMP Traps which will be sent within the time period specified by starWindowTime.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starWindowTime
> Object ID
> enterprises.8164.1.8.1.2
> Description
> The amount of time, in seconds, within which no more than starMaxAlertsPerTime SNMP Traps will be sent.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starAlertSendingEnabled
> Object ID
> enterprises.8164.1.8.1.3
> Description
> Shows if SNMP traps are currently enabled or disabled. Traps are disabled when more than starMaxAlertsPerTime traps are sent within the starWindowTime time period. A value of true(1) indicates that traps will still be sent. A value of false(2) indicates that traps are no longer being generated
> Syntax
> TruthValue
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentPower(9)
> Object
> starPowerTable
> Object ID
> enterprises.8164.1.9.1
> Description
> A table containing information about all power filters.
> Syntax
> Sequence of StarPowerEntry
> Access
> Not-accessible
> Object
> starPowerEntry
> Object ID
> enterprises.8164.1.9.1.1
> Description
> Information about a particular power filter.
> Syntax
> StarPowerEntry
> Access
> Not-accessible
> Sequence
> starPowerNumber Index
> starPowerState
> Object
> starPowerNumber
> Object ID
> enterprises.8164.1.9.1.1.1
> Description
> The identifying number for this power filter.
> Syntax
> Integer
> Access
> Not-accessible
> Enumeration
> powerA(1)
> powerB(2)
> Object
> starPowerState
> Object ID
> enterprises.8164.1.9.1.1.2
> Description
> The state of the power filter. The value active(1) means that the power filter is present and operational. The value failed(2) means that the power filter is present, but not operational. The value not-present(3) means that the power filter is not physically present in the system.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> active(1)
> failed(2)
> notpresent(3)
> starentMIB(8164).starentMIBObjects(1).starentCPU(10)
> Object
> starCPUTable
> Object ID
> enterprises.8164.1.10.1
> Description
> A table containing information about all CPUs
> Syntax
> Sequence of StarCPUEntry
> Access
> Not-accessible
> Object
> starCPUEntry
> Object ID
> enterprises.8164.1.10.1.1
> Description
> Information about a particular CPU.
> Syntax
> StarCPUEntry
> Access
> Not-accessible
> Sequence
> starCPUSlot Index
> starCPUNumber Index
> starCPUUser
> starCPUSystem
> starCPUIdle
> starCPUIO
> starCPURQ
> starCPULoad1Min
> starCPULoad5Min
> starCPULoad15Min
> starCPUMemTotal
> starCPUMemUsed
> starCPUNumProcesses
> starCPUMemCached
> Object
> starCPUSlot
> Object ID
> enterprises.8164.1.10.1.1.1
> Description
> The slot number of the card holding this CPU.
> Syntax
> Integer32(1..16)
> Access
> Not-accessible
> Object
> starCPUNumber
> Object ID
> enterprises.8164.1.10.1.1.2
> Description
> The CPU number within this card. Numbers begin at 0.
> Syntax
> Integer32(0..3)
> Access
> Not-accessible
> Object
> starCPUUser
> Object ID
> enterprises.8164.1.10.1.1.3
> Description
> Percentage of the CPU spent running user processes. starCPUUser is the percentage value times 100; for example, 2.3% would be represented as 230
> Syntax
> Integer32(1..10000)
> Access
> Read-only
> Object
> starCPUSystem
> Object ID
> enterprises.8164.1.10.1.1.4
> Description
> Percentage of the CPU spent running system processes. starCPUSystem is the percentage value times 100; for example, 2.3% would be represented as 230.
> Syntax
> Integer32(1..10000)
> Access
> Read-only
> Object
> starCPUIdle
> Object ID
> enterprises.8164.1.10.1.1.6
> Description
> Percentage of the CPU spent idle. starCPUIdle is the percentage value times 100; for example, 2.3% would be represented as 230.
> Syntax
> Integer32(1..10000)
> Access
> Read-only
> Object
> starCPUIO
> Object ID
> enterprises.8164.1.10.1.1.7
> Description
> Percentage of the CPU spent running Input/Output processes. starCPUIO is the percentage value times 100; for example, 2.3% would be represented as 230.
> Syntax
> Integer32(1..10000)
> Access
> Read-only
> Object
> starCPURQ
> Object ID
> enterprises.8164.1.10.1.1.8
> Description
> Percentage of the CPU spent running IRQ processes. starCPURQ is the percentage value times 100; for example, 2.3% would be represented as 230.
> Syntax
> Integer32(1..10000)
> Access
> Read-only
> Object
> starCPULoad1Min
> Object ID
> enterprises.8164.1.10.1.1.11
> Description
> The average CPU load over the last minute. The CPU load is defined to be the number of processes who are ready to run. starCPULoad1Min is the average number of processes times 100; for example, 2.45 would be represented as 245.
> Syntax
> Integer32(1..1000000000)
> Access
> Read-only
> Object
> starCPULoad5Min
> Object ID
> enterprises.8164.1.10.1.1.12
> Description
> The average CPU load over the last 5 minutes. The CPU load is defined to be the number of processes who are ready to run. starCPULoad5Min is the average number of processes times 100; for example, 2.45 would be represented as 245.
> Syntax
> Integer32(1..1000000000)
> Access
> Read-only
> Object
> starCPULoad15Min
> Object ID
> enterprises.8164.1.10.1.1.13
> Description
> The average CPU load over the last 15 minutes. The CPU load is defined to be the number of processes who are ready to run. starCPULoad15Min is the average number of processes times 100; for example, 2.45 would be represented as 245.
> Syntax
> Integer32(1..1000000000)
> Access
> Read-only
> Object
> starCPUMemTotal
> Object ID
> enterprises.8164.1.10.1.1.14
> Description
> The total amount of memory dedicated to this CPU, in kilobytes.
> Syntax
> Integer32(1..2097152)
> Access
> Read-only
> Object
> starCPUMemUsed
> Object ID
> enterprises.8164.1.10.1.1.15
> Description
> The total amount of memory consumed by this CPU, in kilobytes.
> Syntax
> Integer32(1..2097152)
> Access
> Read-only
> Object
> starCPUNumProcesses
> Object ID
> enterprises.8164.1.10.1.1.16
> Description
> The total number of processes which exist on this CPU.
> Syntax
> Integer32(1..4096)
> Access
> Read-only
> Object
> starCPUMemCached
> Object ID
> enterprises.8164.1.10.1.1.17
> Description
> The total amount of memory consumed by the (reusable) memory cache on this CPU, in kilobytes
> Syntax
> Integer32(1..2097152)
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentNPUMgr(11)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starNPUMgrTable
> Object ID
> enterprises.8164.1.11.1
> Description
> A table containing information about all NPU Managers.
> Syntax
> Sequence of StarNPUMgrEntry
> Access
> Not-accessible
> Object
> starNPUMgrEntry
> Object ID
> enterprises.8164.1.11.1.1
> Description
> Information about a particular NPU Manager.
> Syntax
> StarNPUMgrEntry
> Access
> Not-accessible
> Sequence
> starNPUMgrNumber
> Object
> starNPUMgrNumber
> Object ID
> enterprises.8164.1.11.1.1.1
> Description
> The identity of this NPU.
> Syntax
> Integer32(1..65535)
> Access
> Not-accessible
> starentMIB(8164).starentMIBObjects(1).starentSessInP(12)
> Object
> starSessInProgCalls
> Object ID
> enterprises.8164.1.12.1
> Description
> The number of sessions currently in progress.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgActiveCalls
> Object ID
> enterprises.8164.1.12.2
> Description
> The number of sessions with active calls.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgDormantCalls
> Object ID
> enterprises.8164.1.12.3
> Description
> The number of sessions associated with dormant calls.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgArrived
> Object ID
> enterprises.8164.1.12.4
> Description
> The number of sessions in the arrived state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgLCPNeg
> Object ID
> enterprises.8164.1.12.5
> Description
> The number of sessions in the link control protocol negotiation state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgLCPUp
> Object ID
> enterprises.8164.1.12.6
> Description
> The number of sessions in the link control protocol up state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgAuthenticating
> Object ID
> enterprises.8164.1.12.7
> Description
> The number of sessions in the authenticating state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgAuthenticated
> Object ID
> enterprises.8164.1.12.8
> Description
> The number of sessions in the authenticated state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgIPCPUp
> Object ID
> enterprises.8164.1.12.9
> Description
> The number of sessions in the IP control protocol up state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgSIPConn
> Object ID
> enterprises.8164.1.12.10
> Description
> The number of sessions in the Simple IP connected state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgMIPConn
> Object ID
> enterprises.8164.1.12.11
> Description
> The number of sessions in the Mobile IP connected state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessInProgDisc
> Object ID
> enterprises.8164.1.12.12
> Description
> The number of sessions in the disconnecting state.
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentSessMgr(13)
> Object
> starSessMgrCount
> Object ID
> enterprises.8164.1.13.1
> Description
> The total number of session manager instances.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlArrived
> Object ID
> enterprises.8164.1.13.2
> Description
> The total number of requested sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlRejected
> Object ID
> enterprises.8164.1.13.3
> Description
> The total number of rejected sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlConnected
> Object ID
> enterprises.8164.1.13.4
> Description
> The total number of sessions which were connected.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlAuthSucc
> Object ID
> enterprises.8164.1.13.5
> Description
> The total number of sessions where authentication was successful.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlAuthFail
> Object ID
> enterprises.8164.1.13.6
> Description
> The total number of sessions which failed authentication.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlLCPUp
> Object ID
> enterprises.8164.1.13.7
> Description
> The total number of sessions in the link control protocol in the up state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlIPCPUp
> Object ID
> enterprises.8164.1.13.8
> Description
> The total number of sessions in the IP control protocol up state.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlSrcViol
> Object ID
> enterprises.8164.1.13.9
> Description
> The total number of sessions which had an invalid source.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlKeepFail
> Object ID
> enterprises.8164.1.13.10
> Description
> The total number of sessions which had a keep alive failure.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessTtlOctForwarded
> Object ID
> enterprises.8164.1.13.11
> Description
> The total number of octets forwarded (data + control).
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlRPRegAccept
> Object ID
> enterprises.8164.1.13.12
> Description
> The total number of Initial RRQ Accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessTtlRPRegAcceptInterPDSN
> Object ID
> enterprises.8164.1.13.13
> Description
> The total number of Inter PDSN Handoff RRQ Accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPCurrSessions
> Object ID
> enterprises.8164.1.13.14
> Description
> The current number of PPP sessions
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessTtlTxBytes
> Object ID
> enterprises.8164.1.13.15
> Description
> The total number of bytes transmitted from mobiles
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlRxBytes
> Object ID
> enterprises.8164.1.13.16
> Description
> he total number of bytes received by mobiles
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlSIPTxBytes
> Object ID
> enterprises.8164.1.13.17
> Description
> The total number of bytes transmitted from mobiles using SIP
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlSIPRxBytes
> Object ID
> enterprises.8164.1.13.18
> Description
> The total number of bytes received by mobiles using SIP
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlMIPTxBytes
> Object ID
> enterprises.8164.1.13.19
> Description
> The total number of bytes transmitted from mobiles using MIP
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlMIPRxBytes
> Object ID
> enterprises.8164.1.13.20
> Description
> The total number of bytes received by mobiles using MIP
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starSessTtlOctForwardedGB
> Object ID
> enterprises.8164.1.13.21
> Description
> The total number of octets forwarded (data + control)
> Syntax
> Counter32
> Units
> Gigabytes
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentAAAMgr(14)
> Object
> starAAAMgrCount
> Object ID
> enterprises.8164.1.14.1
> Description
> The total number of AAA manager instances.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAATtlRequests
> Object ID
> enterprises.8164.1.14.2
> Description
> The total number of AAA requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAATtlAuthRequests
> Object ID
> enterprises.8164.1.14.3
> Description
> The total number of AAA authentication requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAATtlAcctRequests
> Object ID
> enterprises.8164.1.14.4
> Description
> The total number of AAA accounting requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAACurRequests
> Object ID
> enterprises.8164.1.14.5
> Description
> The current number of AAA requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAACurAuthRequests
> Object ID
> enterprises.8164.1.14.6
> Description
> The current number of AAA authentication requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAACurAcctRequests
> Object ID
> enterprises.8164.1.14.7
> Description
> The current number of AAA accounting requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAATtlAcctSess
> Object ID
> enterprises.8164.1.14.8
> Description
> The total number of AAA accounting sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAACurAcctSess
> Object ID
> enterprises.8164.1.14.9
> Description
> The current number of accounting sessions
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAATtlAuthSuccess
> Object ID
> enterprises.8164.1.14.10
> Description
> The total number of AAA authentication successes.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starAAATtlAuthFailure
> Object ID
> enterprises.8164.1.14.11
> Description
> The total number of AAA authentication failures.
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentA11Mgr(15)
> Object
> starA11MgrCount
> Object ID
> enterprises.8164.1.15.1
> Description
> The total number of A11 manager instances.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starA11TtlArrived
> Object ID
> enterprises.8164.1.15.2
> Description
> The total number of A11 session requests.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starA11TtlRejected
> Object ID
> enterprises.8164.1.15.3
> Description
> The total number of rejected A11 sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starA11TtlDemultiplexed
> Object ID
> enterprises.8164.1.15.4
> Description
> The total number of demultiplexed A11 sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starA11TtlDereg
> Object ID
> enterprises.8164.1.15.5
> Description
> The total number of A11 deregistrations.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starA11CurActive
> Object ID
> enterprises.8164.1.15.6
> Description
> The current number of active A11 sessions.
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentHAMgr(16)
> Object
> starHAMgrCount
> Object ID
> enterprises.8164.1.16.1
> Description
> The total number of home agent manager instances.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starHATtlArrived
> Object ID
> enterprises.8164.1.16.2
> Description
> The total number of home agent session requests.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starHATtlRejected
> Object ID
> enterprises.8164.1.16.3
> Description
> The total number of rejected home agent sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starHATtlDemultiplexed
> Object ID
> enterprises.8164.1.16.4
> Description
> The total number of demultiplexed home agent sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starHATtlDereg
> Object ID
> enterprises.8164.1.16.5
> Description
> The total number of home agent deregistrations.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starHACurActive
> Object ID
> enterprises.8164.1.16.6
> Description
> The current number of active home agent sessions.
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentFAMgr(17)
> Object
> starFAMgrCount
> Object ID
> enterprises.8164.1.17.1
> Description
> The total number of foreign agent manager instances.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starFATtlArrived
> Object ID
> enterprises.8164.1.17.2
> Description
> The total number of foreign agent session requests.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starFATtlRejected
> Object ID
> enterprises.8164.1.17.3
> Description
> The total number of rejected foreign agent sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starFATtlDemultiplexed
> Object ID
> enterprises.8164.1.17.4
> Description
> The total number of demultiplexed foreign agent sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starFATtlDereg
> Object ID
> enterprises.8164.1.17.5
> Description
> The total number of foreign agent deregistrations.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starFACurActive
> Object ID
> enterprises.8164.1.17.6
> Description
> The current number of active foreign agent sessions.
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentService(18)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starServiceTable
> Object ID
> enterprises.8164.1.18.1
> Description
> A table containing information about all of the service managers.
> Syntax
> Sequence of StarSvcEntry
> Access
> Not-accessible
> Object
> starServiceEntry
> Object ID
> enterprises.8164.1.18.1.1
> Description
> Information about a particular service manager.
> Syntax
> StarSvcEntry
> Access
> Not-accessible
> Sequence
> starServiceVpnID Index
> starServiceSvcID Index
> starServiceVpnName
> starServiceServName
> starServiceSubLimit
> starServiceSubCurrent
> starServiceType
> starServiceFAIpAddr
> starServiceHAIpAddr
> Object
> starServiceVpnId
> Object ID
> enterprises.8164.1.18.1.1.1
> Description
> The internal identification of the VPN (context).
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starServiceSvcID
> Object ID
> enterprises.8164.1.18.1.1.2
> Description
> The internal identification of the service, unique to the associated context.
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starServiceVpnName
> Object ID
> enterprises.8164.1.18.1.1.3
> Description
> The name of the VPN (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starServiceServName
> Object ID
> enterprises.8164.1.18.1.1.4
> Description
> The name of the service.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starServiceSubLimit
> Object ID
> enterprises.8164.1.18.1.1.5
> Description
> The configured subscriber limit.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starServiceSubCurrent
> Object ID
> enterprises.8164.1.18.1.1.6
> Description
> Current subscriber limit.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starServiceType
> Object ID
> enterprises.8164.1.18.1.1.7
> Description
> Service type.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(1)
> pdsn(2)
> ggsn(3)
> ha(4)
> fa(5)
> l2tpserver(6)
> lac(7)
> lns(8)
> closedrp(9
> ecs(10)
> cscf(11)
> ipsg(12)
> evdoreva(13)
> pdif(15)
> asnpc(16)
> mipv6ha(17)
> phsgw(18)
> phspc(19)
> sgw(20)
> pgw(21)
> mag(22)
> gprs(23)
> hsgw(24)
> sgsn(25)
> mme(26)
> pdg(27)
> standalonefa(28)
> imsue(29)
> fng(30)
> pccpolicy(31)
> pccquota(32)
> pccaf(33)
> Object
> starServiceFAIpAddr
> Object ID
> enterprises.8164.1.18.1.1.8
> Description
> The IP address for an FA service. Where unknown or not applicable this will contain all zeroes.
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starServiceHAIpAddr
> Object ID
> enterprises.8164.1.18.1.1.9
> Description
> The IP address for an HA service. Where unknown or not applicable this will contain all zeroes.
> Syntax
> IpAddress
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentCLIMgr(19)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starCLITable
> Object ID
> enterprises.8164.1.19.1
> Description
> A table containing information about all interactive CLI sessions.
> Syntax
> Sequence of StarSvcEntry
> Access
> Not-accessible
> Object
> starCLIEntry
> Object ID
> enterprises.8164.1.19.1.1
> Description
> Information about a particular CLI session.
> Syntax
> StarSvcEntry
> Access
> Not-accessible
> Sequence
> starCLIID
> starCLIUsername
> starCLITtyname
> starCLIPrivs
> starCLIType
> starCLIRemoteIpAddr
> starCLIContext
> Object
> starCLIID
> Object ID
> enterprises.8164.1.19.1.1.1
> Description
> The internal identify of the CLI session.
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starCLIUsername
> Object ID
> enterprises.8164.1.19.1.1.2
> Description
> The name of the user logged into the CLI sessions or ‘unknown’ if not known.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starCLITtyname
> Object ID
> enterprises.8164.1.19.1.1.3
> Description
> The name of the TTY device used for the CLI session.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starCLIPrivs
> Object ID
> enterprises.8164.1.19.1.1.4
> Description
> The CLI session privilege level.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starCLIType
> Object ID
> enterprises.8164.1.19.1.1.5
> Description
> The CLI type; commandline(1) represents the normal interactive command line; ftp(2) represents an incoming FTP session.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> commandline(1)
> ftp(2)
> Object
> starCLIRemoteIPAddr
> Object ID
> enterprises.8164.1.19.1.1.6
> Description
> The remote IP address used to access this CLI session. Where unknown or not applicable (such as access through a serial port) this will be 0.
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starCLIContext
> Object ID
> enterprises.8164.1.19.1.1.7
> Description
> The context (VPN) currently being viewed or managed by the CLI session.
> Syntax
> DisplayString
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentTaskMgr(20)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starTaskTable
> Object ID
> enterprises.8164.1.20.1
> Description
> A table containing information about all of the active tasks.
> Syntax
> Sequence of StarSvcEntry
> Access
> Not-accessible
> Object
> starTaskEntry
> Object ID
> enterprises.8164.1.20.1.1
> Description
> Information about a particular task.
> Syntax
> StarSvcEntry
> Access
> Not-accessible
> Sequence
> starTaskFacility Index
> starTaskInstance Index
> starTaskFacilityName
> starTaskCard
> starTaskCPU
> Object
> starTaskFacility
> Object ID
> enterprises.8164.1.20.1.1.1
> Description
> The internal identify of the facility.
> Syntax
> Unsigned32
> Access
> Not-accessible
> Object
> starTaskInstance
> Object ID
> enterprises.8164.1.20.1.1.2
> Description
> The unique internal instance identifier for the task without a given facility.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starTaskFacilityName
> Object ID
> enterprises.8164.1.20.1.1.3
> Description
> The name of the facility the task is associated with.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starTaskCard
> Object ID
> enterprises.8164.1.20.1.1.4
> Description
> The slot number of the card where the task is located.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starTaskCPU
> Object ID
> enterprises.8164.1.20.1.1.5
> Description
> The CPU number where the task is running.
> Syntax
> Unsigned32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentPPP(21)
> Object
> starPPPStatTable
> Object ID
> enterprises.8164.1.21.1
> Description
> A table containing PPP statistics.
> Syntax
> Sequence of StarPPPStatEntry
> Access
> Not-accessible
> Object
> starPPPStatEntry
> Object ID
> enterprises.8164.1.21.1.1
> Description
> The statistics for an individual entry for a PPP context and service.
> Syntax
> StarPPPStatEntry
> Access
> Not-accessible
> Sequence
> starPPPStatVpnID
> starPPPStatSvcID Index (Implied)
> starPPPStatVpnName
> starPPPStatServName
> starPPPStatInit
> starPPPStatReneg
> starPPPStatSuccess
> starPPPStatFailed
> starPPPStatReleased
> starPPPStatReleasedLocal
> starPPPStatReleasedRemote
> starPPPStatLcpFailMaxRetry
> starPPPStatLcpFailOption
> starPPPStatIpcpFailMaxRetry
> starPPPStatIpcpFailOption
> starPPPStatCcpFail
> starPPPStatAuthFail
> starPPPStatLcpEntered
> starPPPStatAuthEntered
> starPPPStatIpcpEntered
> starPPPStatRenegPdsn
> starPPPStatRenegMobil
> starPPPStatRenegAddrMismatch
> starPPPStatRenegOther
> starPPPStatChapAuthAttempt
> starPPPStatPapAuthAttempt
> starPPPStatMSChapAuthAttempt
> starPPPStatChapAuthFail
> starPPPStatPapAuthFail
> starPPPStatMSChapAuthFail
> starPPPStatStacComp
> starPPPStatMppcComp
> starPPPStatDeflComp
> starPPPStatFscErrs
> starPPPStatUnknProto
> starPPPStatBadAddr
> starPPPStatBadCtrl
> starPPPStatVjComp
> starPPPStatDiscLcpRemote
> starPPPStatDiscRpRemote
> starPPPStatDiscAdmin
> starPPPStatDiscIdleTimeout
> starPPPStatDiscAbsTimeout
> starPPPStatDiscPPPKeepalive
> starPPPStatDiscNoResource
> starPPPStatDiscMisc
> starPPPStatFailedReneg
> starPPPStatLcpFailUnknown
> starPPPStatIpcpFailUnknown
> starPPPStatAuthAbort
> starPPPStatLowerLayerDisc
> starPPPStatLcpSuccess
> starPPPStatAuthSuccess
> starPPPStatRenegLowerLayerHandoff
> starPPPStatRenegParamUpdate
> starPPPStatChapAuthSuccess
> starPPPStatPapAuthSuccess
> starPPPStatMSChapAuthSuccess
> starPPPStatChapAuthAbort
> starPPPStatPapAuthAbort
> starPPPStatMSChapAuthAbort
> starPPPStatSessSkipAuth
> starPPPStatNegComp
> starPPPStatCCPNegFailComp
> starPPPStatDiscLocalLowerLayer
> starPPPStatDiscAddFlowFail
> starPPPStatDiscMaxRetriesLCP
> starPPPStatDiscMaxRetriesIPCP
> starPPPStatDiscMaxSetupTimer
> starPPPStatDiscInvalidDestVpn
> starPPPStatDiscOptNegFailLCP
> starPPPStatDiscOptNegFailIPCP
> arPPPStatDiscNoRemoteIpAddr
> starPPPStatDiscCallTypeDetectFail
> starPPPStatDiscRemoteDiscUpLayer
> starPPPStatDiscLongDuraTimeout
> starPPPStatDiscAuthFail
> starPPPStatLCPEchoTotalReq
> starPPPStatLCPEchoReqResent
> starPPPStatLCPEchoRepRecved
> starPPPStatLCPEchoReqTimeout
> starPPPStatRecvErrBadCtrlField
> starPPPStatRecvErrBadPacketLen
> starPPPStatRemoteTerm
> starPPPStatMiscFail
> Object
> starPPPStatVpnID
> Object ID
> enterprises.8164.1.21.1.1.1
> Description
> The internal identification of the PPP VPN (context).
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starPPPStatSvcID
> Object ID
> enterprises.8164.1.21.1.1.2
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).
> Syntax
> StarShortID
> Access
> Not-accessible
> Object
> starPPPStatVpnName
> Object ID
> enterprises.8164.1.21.1.1.3
> Description
> The name of the PPP VPN (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPPPStatServName
> Object ID
> enterprises.8164.1.21.1.1.4
> Description
> The name of the PPP service.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPPPStatInit
> Object ID
> enterprises.8164.1.21.1.1.5
> Description
> The number of initialized PPP sessions for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatReneg
> Object ID
> enterprises.8164.1.21.1.1.6
> Description
> The number of PPP session renegotiations for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatSuccess
> Object ID
> enterprises.8164.1.21.1.1.7
> Description
> The number of PPP session negotiation successes for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatFailed
> Object ID
> enterprises.8164.1.21.1.1.8
> Description
> The number of PPP session negotiation failures for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatReleased
> Object ID
> enterprises.8164.1.21.1.1.9
> Description
> The number of PPP sessions released for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatReleasedLocal
> Object ID
> enterprises.8164.1.21.1.1.10
> Description
> The number of PPP sessions where the release was initiated locally for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatReleasedRemote
> Object ID
> enterprises.8164.1.21.1.1.11
> Description
> The number of PPP session where the release was initiated remotely for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLcpFailMaxRetry
> Object ID
> enterprises.8164.1.21.1.1.12
> Description
> The number of PPP sessions which failed to bring up the link control protocol due to excessive retries for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLcpFailOption
> Object ID
> enterprises.8164.1.21.1.1.13
> Description
> The number of PPP sessions which failed to bring up the Link Control Protocol (LCP) due to an invalid option being received for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatIpcpFailMaxRetry
> Object ID
> enterprises.8164.1.21.1.1.14
> Description
> The number of PPP sessions which failed to start the IP Control Protocol (IPCP) due to excessive retries for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatIpcpFailOption
> Object ID
> enterprises.8164.1.21.1.1.15
> Description
> The number of PPP sessions which failed to start the IP Control Protocol due to an invalid option being received for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatCcpFail
> Object ID
> enterprises.8164.1.21.1.1.16
> Description
> The number of PPP sessions which failed to initialize the CCP.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatAuthFail
> Object ID
> enterprises.8164.1.21.1.1.17
> Description
> The number of PPP sessions which failed authentication for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLcpEntered
> Object ID
> enterprises.8164.1.21.1.1.18
> Description
> The number of PPP sessions which successfully initialized the Link Control Protocol.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatAuthEntered
> Object ID
> enterprises.8164.1.21.1.1.19
> Description
> The number of PPP sessions which were successfully authenticated.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatIpcpEntered
> Object ID
> enterprises.8164.1.21.1.1.20
> Description
> The number of PPP sessions which successfully initialized the IP Control Protocol.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRenegPdsn
> Object ID
> enterprises.8164.1.21.1.1.21
> Description
> The number of PPP sessions which re-negotiated the PDSN service access.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRenegMobil
> Object ID
> enterprises.8164.1.21.1.1.22
> Description
> The number of PPP sessions which re-negotiated the Mobile IP service access.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRenegAddrMismatch
> Object ID
> enterprises.8164.1.21.1.1.23
> Description
> The number of PPP sessions which had an IP address mismatch during re-negotiation.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRenegOther
> Object ID
> enterprises.8164.1.21.1.1.24
> Description
> The number of PPP sessions which failed renegotiation for reasons other than IP address mismatch.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatChapAuthAttempt
> Object ID
> enterprises.8164.1.21.1.1.25
> Description
> The number of PPP CHAP authentication attempts for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatPapAuthAttempt
> Object ID
> enterprises.8164.1.21.1.1.26
> Description
> The number of PPP PAP authentication attempts for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatMSChapAuthAttempt
> Object ID
> enterprises.8164.1.21.1.1.27
> Description
> The number of PPP MSCHAP authentication attempts for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatChapAuthFail
> Object ID
> enterprises.8164.1.21.1.1.28
> Description
> The number of PPP CHAP authentication attempt failures for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatPapAuthFail
> Object ID
> enterprises.8164.1.21.1.1.29
> Description
> The number of PPP PAP authentication failures for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatMSChapAuthFail
> Object ID
> enterprises.8164.1.21.1.1.30
> Description
> The number of PPP MSCHAP authentication failures for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatStacComp
> Object ID
> enterprises.8164.1.21.1.1.31
> Description
> The number of PPP sessions which had STAC compression enabled for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatMppcComp
> Object ID
> enterprises.8164.1.21.1.1.32
> Description
> The number of PPP sessions which had MPPC compression enabled for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDeflComp
> Object ID
> enterprises.8164.1.21.1.1.33
> Description
> The number of PPP sessions which had DEFLATE compression enabled for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatFscErrs
> Object ID
> enterprises.8164.1.21.1.1.34
> Description
> The number of PPP forward sequence control errors in messaging.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatUnknProto
> Object ID
> enterprises.8164.1.21.1.1.35
> Description
> The number of PPP sessions which failed due to an unknown protocol received for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatBadAddr
> Object ID
> enterprises.8164.1.21.1.1.36
> Description
> The number of PPP sessions which failed due to a bad address being received for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatBadCtrl
> Object ID
> enterprises.8164.1.21.1.1.37
> Description
> The number of PPP sessions in which a bad control sequence was received.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatVjComp
> Object ID
> enterprises.8164.1.21.1.1.38
> Description
> The number of PPP sessions which had VJ header compression enabled for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscLcpRemote
> Object ID
> enterprises.8164.1.21.1.1.39
> Description
> The number of PPP sessions which were disconnected via the link control protocol from the remote end for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscRpRemote
> Object ID
> enterprises.8164.1.21.1.1.40
> Description
> The number of PPP sessions which were disconnected by the remote via the R-P interface for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscAdmin
> Object ID
> enterprises.8164.1.21.1.1.41
> Description
> The number of PPP sessions which were disconnected by a local administrator for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscIdleTimeout
> Object ID
> enterprises.8164.1.21.1.1.42
> Description
> The number of PPP sessions disconnected due to session idle timer expiration for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscAbsTimeout
> Object ID
> enterprises.8164.1.21.1.1.43
> Description
> The number of PPP sessions disconnected due to the session absolute timer expiration for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscPPPKeepalive
> Object ID
> enterprises.8164.1.21.1.1.44
> Description
> The number of PPP sessions disconnected due to PPP keep alive failure for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscNoResource
> Object ID
> enterprises.8164.1.21.1.1.45
> Description
> The number of PPP sessions disconnected due to local resource shortage for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscMisc
> Object ID
> enterprises.8164.1.21.1.1.46
> Description
> The number of PPP sessions disconnected due to any cause which does not match any other existing disconnect statistic for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatFailedReneg
> Object ID
> enterprises.8164.1.21.1.1.47
> Description
> The number of failed PPP renegotiations the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLcpFailUnknown
> Object ID
> enterprises.8164.1.21.1.1.48
> Description
> The number of failed PPP LCP that are due to unknown reasons for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatIpcpFailUnknown
> Object ID
> enterprises.8164.1.21.1.1.49
> Description
> The number of failed PPP IPCP that are due to unknown reasons for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatAuthAbort
> Object ID
> enterprises.8164.1.21.1.1.50
> Description
> The number of aborted PPP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLowerLayerDisc
> Object ID
> enterprises.8164.1.21.1.1.51
> Description
> The number of Failed PPP session due to RP disconnect for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLcpSuccess
> Object ID
> enterprises.8164.1.21.1.1.52
> Description
> The number of successful PPP LCPs for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatAuthSuccess
> Object ID
> enterprises.8164.1.21.1.1.53
> Description
> The number of successful PPP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRenegLowerLayerHandoff
> Object ID
> enterprises.8164.1.21.1.1.54
> Description
> The number of PPP renegotiations for RP handoff for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRenegParamUpdate
> Object ID
> enterprises.8164.1.21.1.1.55
> Description
> The number of PPP renegotiations for parameter update for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatChapAuthSuccess
> Object ID
> enterprises.8164.1.21.1.1.56
> Description
> The number of successful PPP CHAP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatPapAuthSuccess
> Object ID
> enterprises.8164.1.21.1.1.57
> Description
> The number of successful PPP PAP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatMSChapAuthSuccess
> Object ID
> enterprises.8164.1.21.1.1.58
> Description
> The number of successful PPP MSCHAP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatChapAuthAbort
> Object ID
> enterprises.8164.1.21.1.1.59
> Description
> The number of aborted PPP CHAP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatPapAuthAbort
> Object ID
> enterprises.8164.1.21.1.1.60
> Description
> The number of aborted PPP PAP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatMSChapAuthAbort
> Object ID
> enterprises.8164.1.21.1.1.61
> Description
> The number of aborted PPP MSCHAP authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatSessSkipAuth
> Object ID
> enterprises.8164.1.21.1.1.62
> Description
> The number of PPP sessions that skipped authentications for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatNegComp
> Object ID
> enterprises.8164.1.21.1.1.63
> Description
> The number of PPP sessions that negotiated compressions for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatCCPNegFailComp
> Object ID
> enterprises.8164.1.21.1.1.64
> Description
> The number of PPP sessions that failed compression negotiation for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscLocalLowerLayer
> Object ID
> enterprises.8164.1.21.1.1.65
> Description
> The number of disconnected PPP sessions due to local RP disconnect for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscAddFlowFail
> Object ID
> enterprises.8164.1.21.1.1.66
> Description
> The number of disconnected PPP sessions due to failure in adding new flow for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscMaxRetriesLCP
> Object ID
> enterprises.8164.1.21.1.1.67
> Description
> The number of disconnected PPP sessions due to max retries for LCP for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscMaxRetriesIPCP
> Object ID
> enterprises.8164.1.21.1.1.68
> Description
> The number of disconnected PPP sessions due to max retries for IPCP for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscMaxSetupTimer
> Object ID
> enterprises.8164.1.21.1.1.69
> Description
> The number of disconnected PPP sessions due to max setup time out for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscInvalidDestVpn
> Object ID
> enterprises.8164.1.21.1.1.70
> Description
> The number of disconnected PPP sessions due to invalid destination VPN for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscOptNegFailLCP
> Object ID
> enterprises.8164.1.21.1.1.71
> Description
> The number of disconnected PPP sessions due to invalid destination VPN for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscOptNegFailIPCP
> Object ID
> enterprises.8164.1.21.1.1.72
> Description
> The number of disconnected PPP sessions due to failed IPCP option negotiation for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscNoRemoteIpAddr
> Object ID
> enterprises.8164.1.21.1.1.73
> Description
> The number of disconnected PPP sessions due to no remote IP address for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscCallTypeDetectFail
> Object ID
> enterprises.8164.1.21.1.1.74
> Description
> The number of disconnected PPP sessions due to failure detecting call type for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscRemoteDiscUpLayer
> Object ID
> enterprises.8164.1.21.1.1.75
> Description
> The number of disconnected PPP sessions due to failure detecting call type for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscLongDuraTimeout
> Object ID
> enterprises.8164.1.21.1.1.76
> Description
> The number of disconnected PPP sessions due to long duration time out for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatDiscAuthFail
> Object ID
> enterprises.8164.1.21.1.1.77
> Description
> The number of disconnected PPP sessions due to failed authentication for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLCPEchoTotalReq
> Object ID
> enterprises.8164.1.21.1.1.78
> Description
> The total number of PPP LCP echo requests for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLCPEchoReqResent
> Object ID
> enterprises.8164.1.21.1.1.79
> Description
> The total number of PPP LCP echo requests resent for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLCPEchoRepRecved
> Object ID
> enterprises.8164.1.21.1.1.80
> Description
> The total number of PPP LCP echo replies received for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatLCPEchoReqTimeout
> Object ID
> enterprises.8164.1.21.1.1.81
> Description
> The total number of PPP LCP echo requests time out for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRecvErrBadCtrlField
> Object ID
> enterprises.8164.1.21.1.1.82
> Description
> The total number of received PPP error due to bad control fields for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRecvErrBadPacketLen
> Object ID
> enterprises.8164.1.21.1.1.83
> Description
> The total number of received PPP error due to bad packet length for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatRemoteTerm
> Object ID
> enterprises.8164.1.21.1.1.84
> Description
> The total number of PPP remote terminations for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPPPStatMiscFail
> Object ID
> enterprises.8164.1.21.1.1.85
> Description
> The number of miscellaneous PPP failures for the associated VPN service.
> Syntax
> Counter32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentMIPHA(22)
> Object
> starMIPHAStatTable
> Object ID
> enterprises.8164.1.22.1
> Description
> A table containing MIP home agent statistics.
> Syntax
> Sequence of starMIPHAStatEntry
> Access
> Not-accessible
> Object
> starMIPHAStatEntry
> Object ID
> enterprises.8164.1.22.1.1
> Description
> The Mobile IP home agent statistics for a specific VPN (context) and service.
> Syntax
> starMIPHAStatEntry
> Access
> Not-accessible
> Sequence
> starMIPHAStatVpnID
> starMIPHAStatSvcID Index (Implied)
> starMIPHAStatVpnName
> starMIPHAStatServName
> starMIPHADisconnects
> starMIPHAExpiry
> starMIPHADereg
> starMIPHAAdminDrop
> starMIPHARegRecvTotal
> starMIPHARegRecvInitial
> starMIPHARegRecvRenew
> starMIPHARegRecvDereg
> starMIPHARegAcceptTotal
> starMIPHARegAcceptReg,
> starMIPHARegAcceptRenew
> starMIPHARegAcceptDereg
> starMIPHARegDeniedTotal
> starMIPHARegDeniedInitial
> starMIPHARegDeniedRenew
> starMIPHARegDeniedDereg
> starMIPHARegReplyTotal
> starMIPHARegReplyAcceptReg
> starMIPHARegReplyAcceptDereg
> starMIPHARegReplyDenied
> starMIPHARegReplyBadReq
> starMIPHARegReplyMismatchID
> starMIPHARegReplyAdminProhib
> starMIPHARegReplyUnspecErr,
> starMIPHARegReplyNoResource
> starMIPHARegReplyMnAuthFail
> starMIPHARegReplyFAAuthFail
> starMIPHARegReplySimulBind
> starMIPHARegReplyUnknownHA
> starMIPHARegReplyRevTunUnavail
> starMIPHARegReplyRevTunMand
> starMIPHARegReplyEncapUnavail
> starMIPHARegReplySendError
> starMIPHAStatFARevocations
> starMIPHAStatRegAcceptHO
> starMIPHAStatRegDeniedHO
> starMIPHAStatRegDiscardTotal
> Object
> starMIPHAStatVpnID
> Object ID
> enterprises.8164.1.22.1.1.1
> Description
> The internal identification of the home agent Mobile IP VPN (context).
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starMIPHAStatSvcID
> Object ID
> enterprises.8164.1.22.1.1.2
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).
> Syntax
> StarShortID
> Access
> Not-accessible
> Object
> starMIPHAStatVpnName
> Object ID
> enterprises.8164.1.22.1.1.3
> Description
> The name of the VPN (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starMIPHAStatServName
> Object ID
> enterprises.8164.1.22.1.1.4
> Description
> The Mobile IP home agent service name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starMIPHAStatDisconnects
> Object ID
> enterprises.8164.1.22.1.1.5
> Description
> The number of session disconnects for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatExpiry
> Object ID
> enterprises.8164.1.22.1.1.6
> Description
> The number of session expirations for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatDereg
> Object ID
> enterprises.8164.1.22.1.1.7
> Description
> The number of session deregistrations for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatAdminDrop
> Object ID
> enterprises.8164.1.22.1.1.8
> Description
> The number of session disconnects due to administrator actions for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegRecvTotal
> Object ID
> enterprises.8164.1.22.1.1.9
> Description
> The number of session registrations received for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegRecvInitial
> Object ID
> enterprises.8164.1.22.1.1.10
> Description
> The number of initial session registrations received for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegRecvRenew
> Object ID
> enterprises.8164.1.22.1.1.11
> Description
> The number of session registration renewals received for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegRecvDereg
> Object ID
> enterprises.8164.1.22.1.1.12
> Description
> The number of session deregistrations received for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegAcceptTotal
> Object ID
> enterprises.8164.1.22.1.1.13
> Description
> The number of session registrations accepted for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegAcceptReg
> Object ID
> enterprises.8164.1.22.1.1.14
> Description
> The number of session registrations accepted for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegAcceptRenew
> Object ID
> enterprises.8164.1.22.1.1.15
> Description
> The number of session registration renewals accepted for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegAcceptDereg
> Object ID
> enterprises.8164.1.22.1.1.16
> Description
> The number of session deregistrations accepted for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegDeniedTotal
> Object ID
> enterprises.8164.1.22.1.1.17
> Description
> The number of session registrations denied for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegDeniedInitial
> Object ID
> enterprises.8164.1.22.1.1.18
> Description
> The number of session initial registrations denied for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegDeniedRenew
> Object ID
> enterprises.8164.1.22.1.1.19
> Description
> The number of session registration renewals denied for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegDeniedDereg
> Object ID
> enterprises.8164.1.22.1.1.20
> Description
> The number of session deregistrations denied for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyTotal
> Object ID
> enterprises.8164.1.22.1.1.21
> Description
> The total number of session registration replies for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyAcceptReg
> Object ID
> enterprises.8164.1.22.1.1.22
> Description
> The number of session registration replies accepted indicating registration for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyAcceptDereg
> Object ID
> enterprises.8164.1.22.1.1.23
> Description
> The number of session registration replies accepted indicating deregistration for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyDenied
> Object ID
> enterprises.8164.1.22.1.1.24
> Description
> The number of session registration replies which were denied for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyBadReq
> Object ID
> enterprises.8164.1.22.1.1.25
> Description
> The number of session registration replies indicating a bad request for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyMismatchID
> Object ID
> enterprises.8164.1.22.1.1.26
> Description
> The number of session registration replies indicating an ID mismatch for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyAdminProhib
> Object ID
> enterprises.8164.1.22.1.1.27
> Description
> The number of session registration replies indicating administrator prohibition for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyUnspecErr
> Object ID
> enterprises.8164.1.22.1.1.28
> Description
> The number of session registration replies with an unspecified error for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyNoResource
> Object ID
> enterprises.8164.1.22.1.1.29
> Description
> The number of session registration replies indicating no resources for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyMnAuthFail
> Object ID
> enterprises.8164.1.22.1.1.30
> Description
> The number of session registration replies indicating mobile number authentication failure for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyFAAuthFail
> Object ID
> enterprises.8164.1.22.1.1.31
> Description
> The number of session registration replies indicating a foreign agent authentication failure for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplySimulBind
> Object ID
> enterprises.8164.1.22.1.1.32
> Description
> The number of session registration replies indicating a simultaneous bind condition for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyUnknownHA
> Object ID
> enterprises.8164.1.22.1.1.33
> Description
> The number of session registration replies indicating unknown home agent for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyRevTunUnavail
> Object ID
> enterprises.8164.1.22.1.1.34
> Description
> The number of session registration replies indicating no reverse tunnel available for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyRevTunMand
> Object ID
> enterprises.8164.1.22.1.1.35
> Description
> The number of session registration replies indicating reverse tunneling is mandatory for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplyEncapUnavail
> Object ID
> enterprises.8164.1.22.1.1.36
> Description
> The number of session registration replies indicating IP encapsulation was not available for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegReplySendError
> Object ID
> enterprises.8164.1.22.1.1.37
> Description
> The number of session registration replies indicating a send error occurred for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatFARevocations
> Object ID
> enterprises.8164.1.22.1.1.38
> Description
> The number of FA revocations for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegAcceptHO
> Object ID
> enterprises.8164.1.22.1.1.39
> Description
> The number of hand over session registrations accepted for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegDeniedHO
> Object ID
> enterprises.8164.1.22.1.1.40
> Description
> The number of hand over session registrations denied for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPHAStatRegDiscardTotal
> Object ID
> enterprises.8164.1.22.1.1.41
> Description
> The number of session registrations discarded for the associated Mobile IP home agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentMIPFA(23)
> Object
> starMIPFAStatTable
> Object ID
> enterprises.8164.1.23.1
> Description
> A table containing the Mobile IP Foreign Agent statistics.
> Syntax
> Sequence of starMIPFAStatEntry
> Access
> Not-accessible
> Description
> A table containing MIP FA statistics
> Object
> starMIPFAStatEntry
> Object ID
> enterprises.8164.1.23.1.1.
> Description
> The statistics for a specific foreign agent Mobile IP VPN (context) service.
> Syntax
> starMIPFAStatEntry
> Access
> Not-accessible
> Sequence
> starMIPFAStatVpnID
> starMIPFAStatSvcID Index (Implied)
> starMIPFAStatVpnName
> starMIPFAStatServName
> starMIPFAAdvertSend
> starMIPFADiscExpiry
> starMIPFADiscDereg
> starMIPFADiscAdmin
> starMIPFAAuthAttempt
> starMIPFAAuthSuccess
> starMIPFAAuthFailure
> starMIPFARegRecvTotal
> starMIPFARegRecvInitial
> starMIPFARegRecvRenewal
> starMIPFARegRecvDereg
> starMIPFARegAcceptTotal
> starMIPFARegAcceptInitial
> starMIPFARegAcceptRenewal
> starMIPFARegAcceptDereg
> starMIPFARegDenTotal
> starMIPFARegDenInitial
> starMIPFARegDenRenewal
> starMIPFARegDenDereg
> starMIPFARegDiscardTotal
> starMIPFARegDiscardInitial
> starMIPFARegDiscardRenewal
> starMIPFARegDiscardDereg
> starMIPFARegRelayedTotal
> starMIPFARegRelayedInitial
> starMIPFARegRelayedRenewal
> starMIPFARegRelayedDereg
> starMIPFARegAuthFailTotal
> starMIPFARegAuthFailInitial
> starMIPFARegAuthFailRenewal
> starMIPFARegAuthFailDereg
> starMIPFARegDenPDSNTotal
> starMIPFARegDenPDSNInitial
> starMIPFARegDenPDSNRenewal
> starMIPFARegDenPDSNDereg
> starMIPFARegDenHATotal
> starMIPFARegDenHAInitial
> starMIPFARegDenHARenewal
> starMIPFARegDenHADereg
> starMIPFARegDenPDSNUnspec
> starMIPFARegDenPDSNTimeout
> starMIPFARegDenPDSNAdmin
> starMIPFARegDenPDSNResources
> starMIPFARegDenPDSNMnAuth
> starMIPFARegDenPDSNHAAuth
> starMIPFARegDenPDSNTooLong
> starMIPFARegDenPDSNBadReq
> starMIPFARegDenPDSNEncapUnav
> starMIPFARegDenPDSNRevTunUnav
> starMIPFARegDenPDSNRevTunMand
> starMIPFARegDenHAFAAuth
> starMIPFARegDenHABadReq
> starMIPFARegDenHAMismatchID
> starMIPFARegDenHASimulBind
> starMIPFARegDenHAUnknownHA
> starMIPFARegDenHARevRunUnavail
> starMIPFARegRplRcvTotal
> starMIPFARegRplRcvTotalRly
> starMIPFARegRplRcvErrors
> starMIPFARegRplRcvInitial
> starMIPFARegRplRcvInitialRly
> starMIPFARegRplRcvRenewal
> starMIPFARegRplRcvRenewalRly
> starMIPFARegRplRcvDereg
> starMIPFARegRplRcvDeregRly
> starMIPFARegRplSentTotal
> starMIPFARegRplSentAcceptReg
> starMIPFARegRplSentAcceptDereg
> starMIPFARegRplSentBadReq
> starMIPFARegRplSentTooLong
> starMIPFARegRplSentMnAuthFail
> starMIPFARegRplSentHAAuthFail
> starMIPFARegRplSentAdminProhib
> starMIPFARegRplSentNoResources
> starMIPFARegRplSentRevTunUnavail
> starMIPFARegRplSentRevTunMand
> starMIPFARegRplSentSendErrors
> starMIPFAStatRegDenPDSNBadReply
> starMIPFAStatRegDenPDSNMissNAI
> starMIPFAStatRegDenPDSNMissHomeAgent
> starMIPFAStatRegDenPDSNMissHomeAddr
> starMIPFAStatRegDenPDSNUnknChallenge
> starMIPFAStatRegDenPDSNMissChallenge
> starMIPFAStatRegDenPDSNStaleChallenge
> starMIPFAStatRegDenPDSNMNTooDistant
> starMIPFAStatRegDenPDSNStyleUnavail
> starMIPFAStatRegDenPDSNHANetUnreach
> starMIPFAStatRegDenPDSNHAHostUnreach
> starMIPFAStatRegDenPDSNHAPortUnreach
> starMIPFAStatRegDenPDSNHAUnreach
> starMIPFAStatRegDenPDSNInvCOA
> starMIPFAStatRegReqSentInitTotal
> starMIPFAStatRegReqSentInitResend
> starMIPFAStatRegReqSentRenewTotal
> starMIPFAStatRegReqSentRenewResend
> starMIPFAStatRegReqSentDeregTotal
> starMIPFAStatRegReqSentDeregResend
> starMIPFAStatRegRplSentMNTooDistant
> starMIPFAStatRegRplSentInvCOA
> starMIPFAStatRegRplSentHANetUnreach
> starMIPFAStatRegRplSentHAHostUnreach
> starMIPFAStatRegRplSentHAPortUnreach
> starMIPFAStatRegRplSentHAUnreach
> starMIPFAStatRegRplSentRegTimeout
> starMIPFAStatRegRplSentMissNAI
> starMIPFAStatRegRplSentMissHomeAgent
> starMIPFAStatRegRplSentMissHomeAddr
> starMIPFAStatRegRplSentUnknChallenge
> starMIPFAStatRegRplSentMissChallenge
> starMIPFAStatRegRplSentStaleChallenge
> starMIPFAStatRegRplSentBadReply
> Object
> starMIPFAStatVpnID
> Object ID
> enterprises.8164.1.23.1.1.1
> Description
> Internal identification of the foreign agent Mobile IP VPN (context).
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starMIPFAStatSvcID
> Object ID
> enterprises.8164.1.23.1.1.2
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).
> Syntax
> StarShortID
> Access
> Not-accessible
> Object
> starMIPFAStatVpnName
> Object ID
> enterprises.8164.1.23.1.1.3
> Description
> The foreign agent mobile IP VPN (context) name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starMIPFAStatServName
> Object ID
> enterprises.8164.1.23.1.1.4
> Description
> The Mobile IP foreign agent service name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starMIPFAStatAdvertSend
> Object ID
> enterprises.8164.1.23.1.1.5
> Description
> The number of advertisements sent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatDiscExpiry
> Object ID
> enterprises.8164.1.23.1.1.6
> Description
> The number of session disconnects due to expiration for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatDiscDereg
> Object ID
> enterprises.8164.1.23.1.1.7
> Description
> The number of session disconnects due to deregistration requests for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatDiscAdmin
> Object ID
> enterprises.8164.1.23.1.1.8
> Description
> The number of session disconnects due to administrator action for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatAuthAttempt
> Object ID
> enterprises.8164.1.23.1.1.9
> Description
> The number of session authentication attempts for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatAuthSuccess
> Object ID
> enterprises.8164.1.23.1.1.10
> Description
> The number of session authentication successes for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatAuthFailure
> Object ID
> enterprises.8164.1.23.1.1.11
> Description
> The number of session authentication failures for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRecvTotal
> Object ID
> enterprises.8164.1.23.1.1.12
> Description
> The total number of session registrations received for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRecvInitial
> Object ID
> enterprises.8164.1.23.1.1.13
> Description
> The number of initial session registrations received for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRecvRenewal
> Object ID
> enterprises.8164.1.23.1.1.14
> Description
> The number of session registration renewals for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRecvDereg
> Object ID
> enterprises.8164.1.23.1.1.15
> Description
> The number of session deregistrations for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAcceptTotal
> Object ID
> enterprises.8164.1.23.1.1.16
> Description
> The total number of session registrations accepted for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAcceptInitial
> Object ID
> enterprises.8164.1.23.1.1.17
> Description
> The number of initial session registrations accepted for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAcceptRenewal
> Object ID
> enterprises.8164.1.23.1.1.18
> Description
> The number of session registration renewals accepted for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAcceptDereg
> Object ID
> enterprises.8164.1.23.1.1.19
> Description
> The number of session deregistrations accepted for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenTotal
> Object ID
> enterprises.8164.1.23.1.1.20
> Description
> The total number of session registrations denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenInitial
> Object ID
> enterprises.8164.1.23.1.1.21
> Description
> The number of initial session registrations denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenRenewal
> Object ID
> enterprises.8164.1.23.1.1.22
> Description
> The number of session registration renewals denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenDereg
> Object ID
> enterprises.8164.1.23.1.1.23
> Description
> The number of session deregistrations denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDiscardTotal
> Object ID
> enterprises.8164.1.23.1.1.24
> Description
> The total number of session registrations discarded for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDiscardInitial
> Object ID
> enterprises.8164.1.23.1.1.25
> Description
> The number of initial session registrations discarded for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDiscardRenewal
> Object ID
> enterprises.8164.1.23.1.1.26
> Description
> The number of session registration renewals discarded for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDiscardDereg
> Object ID
> enterprises.8164.1.23.1.1.27
> Description
> The number of session deregistrations discarded for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRelayedTotal
> Object ID
> enterprises.8164.1.23.1.1.28
> Description
> The total number of session registrations relayed for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRelayedInitial
> Object ID
> enterprises.8164.1.23.1.1.29
> Description
> The number of initial session registrations relayed for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRelayedRenewal
> Object ID
> enterprises.8164.1.23.1.1.30
> Description
> The number of session registration renewals relayed for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRelayedDereg
> Object ID
> enterprises.8164.1.23.1.1.31
> Description
> The number of session deregistrations relayed for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAuthFailTotal
> Object ID
> enterprises.8164.1.23.1.1.32
> Description
> The total number of session registration authentication failures for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAuthFailInitial
> Object ID
> enterprises.8164.1.23.1.1.33
> Description
> The number of initial session registration failures for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAuthFailRenewal
> Object ID
> enterprises.8164.1.23.1.1.34
> Description
> The number of session registration renewal failures for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegAuthFailDereg
> Object ID
> enterprises.8164.1.23.1.1.35
> Description
> The number of session deregistration authentication failures for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNTotal
> Object ID
> enterprises.8164.1.23.1.1.36
> Description
> The total number of PDSN session registrations denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNInitial
> Object ID
> enterprises.8164.1.23.1.1.37
> Description
> The number of initial PDSN session registrations denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNRenewal
> Object ID
> enterprises.8164.1.23.1.1.38
> Description
> The number of PDSN session registration renewals denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNDereg
> Object ID
> enterprises.8164.1.23.1.1.39
> Description
> The number of PDSN session deregistrations denied for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHATotal
> Object ID
> enterprises.8164.1.23.1.1.40
> Description
> The total number of session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHAInitial
> Object ID
> enterprises.8164.1.23.1.1.41
> Description
> The number of initial session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHARenewal
> Object ID
> enterprises.8164.1.23.1.1.42
> Description
> The number of session registration renewals denied by the home agent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHADereg
> Object ID
> enterprises.8164.1.23.1.1.43
> Description
> The number of session deregistrations denied by the home agent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNUnspec
> Object ID
> enterprises.8164.1.23.1.1.44
> Description
> The number of PDSN session registrations denied for an unspecified reason for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNTimeout
> Object ID
> enterprises.8164.1.23.1.1.45
> Description
> The number of PDSN session registrations denied due to timer expiration for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNAdmin
> Object ID
> enterprises.8164.1.23.1.1.46
> Description
> The number of PDSN session registration denied due administrator prohibition for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNResources
> Object ID
> enterprises.8164.1.23.1.1.47
> Description
> The number of PDSN session registrations denied due to no resources for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNMnAuth
> Object ID
> enterprises.8164.1.23.1.1.48
> Description
> The number of PDSN session registrations denied due to mobile number authentication failure for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNHAAuth
> Object ID
> enterprises.8164.1.23.1.1.49
> Description
> The number of PDSN session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNTooLong
> Object ID
> enterprises.8164.1.23.1.1.50
> Description
> The number of PDSN session registrations denied due to a life too lone indication for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNBadReq
> Object ID
> enterprises.8164.1.23.1.1.51
> Description
> The number of PDSN session registration denied due to a bad request indication for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNEncapUnav
> Object ID
> enterprises.8164.1.23.1.1.52
> Description
> The number of PDSN session registration denied due to no IP encapsulation available for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDeniedPDSNRevTunUnav
> Object ID
> enterprises.8164.1.23.1.1.53
> Description
> The number of PDSN session registrations denied due to no reverse tunnel available for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNRevTunMand
> Object ID
> enterprises.8164.1.23.1.1.54
> Description
> The number of PDSN session registration denied due to reverse tunneling being mandatory for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHAFAAuth
> Object ID
> enterprises.8164.1.23.1.1.55
> Description
> The number of session registrations denied by the home agent due to authentication failure for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHABadReq
> Object ID
> enterprises.8164.1.23.1.1.56
> Description
> The number of session registration denied by the home agent due to the request being invalid for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHAMismatchID
> Object ID
> enterprises.8164.1.23.1.1.57
> Description
> The number of session registrations denied by the home agent due to an ID mismatch for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHASimulBind
> Object ID
> enterprises.8164.1.23.1.1.58
> Description
> The number of session registrations denied by the home agent due to a simultaneous bind attempt for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHAUnknownHA
> Object ID
> enterprises.8164.1.23.1.1.59
> Description
> The number of session registrations denied by the home agent for an unknown reason for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenHARevRunUnavail
> Object ID
> enterprises.8164.1.23.1.1.60
> Description
> The number of session registrations denied by the home agent due to no reverse tunnel being available for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvTotal
> Object ID
> enterprises.8164.1.23.1.1.61
> Description
> The total number of session registration replies received for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvTotalRly
> Object ID
> enterprises.8164.1.23.1.1.62
> Description
> The total number of session registration replies relayed for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvErrors
> Object ID
> enterprises.8164.1.23.1.1.63
> Description
> The number of session registration replies received indicating errors for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvInitial
> Object ID
> enterprises.8164.1.23.1.1.64
> Description
> The number of initial session registration replies received for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvInitialRly
> Object ID
> enterprises.8164.1.23.1.1.65
> Description
> The number of initial session registration replies relayed for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvRenewal
> Object ID
> enterprises.8164.1.23.1.1.66
> Description
> The number of session registration renewal replies received for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvRenewalRly
> Object ID
> enterprises.8164.1.23.1.1.67
> Description
> The number of session registration replies relayed received for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvDereg
> Object ID
> enterprises.8164.1.23.1.1.68
> Description
> The number of session registration replies received indicating deregistration for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplRcvDeregRly
> Object ID
> enterprises.8164.1.23.1.1.69
> Description
> The number of session registration replies relayed indicating deregistration for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentTotal
> Object ID
> enterprises.8164.1.23.1.1.70
> Description
> The total number of session registration replies sent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentAcceptReg
> Object ID
> enterprises.8164.1.23.1.1.71
> Description
> The number of session registration replies which were sent and accepted for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentAcceptDereg
> Object ID
> enterprises.8164.1.23.1.1.72
> Description
> The number of session registration replies which were sent and accepted indicating deregistration for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentBadReq
> Object ID
> enterprises.8164.1.23.1.1.73
> Description
> The number of session registration replies which were sent indicating the request was invalid for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentTooLong
> Object ID
> enterprises.8164.1.23.1.1.74
> Description
> The number of session registration replies which were sent indicating life too long for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentMnAuthFail
> Object ID
> enterprises.8164.1.23.1.1.75
> Description
> The number of session registration replies which were sent indicating mobile number authentication failure for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentHAAuthFail
> Object ID
> enterprises.8164.1.23.1.1.76
> Description
> The number of session registration replies which were sent indicating for home agent authentication failure the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentAdminProhib
> Object ID
> enterprises.8164.1.23.1.1.77
> Description
> The number of session registration replies which were sent indicating prohibited by the administrator for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentNoResources
> Object ID
> enterprises.8164.1.23.1.1.78
> Description
> The number of session registration replies which were sent indicating no resources available for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentRevTunUnavail
> Object ID
> enterprises.8164.1.23.1.1.79
> Description
> The number of session registration replies which were sent indicating no reverse tunnel available for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentRevTunMand
> Object ID
> enterprises.8164.1.23.1.1.80
> Description
> The number of session registration replies which were sent indicating reverse tunneling was mandatory for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentSendErrors
> Object ID
> enterprises.8164.1.23.1.1.81
> Description
> The number of session registration replies which were sent indicating there were errors in transmission for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNBadReply
> Object ID
> enterprises.8164.1.23.1.1.82
> Description
> The number of session registrations denied by PDSN due to bad reply from HA for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNMissNAI
> Object ID
> enterprises.8164.1.23.1.1.83
> Description
> The number of session registrations denied by PDSN due to missing NAI for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNMissHomeAgent
> Object ID
> enterprises.8164.1.23.1.1.84
> Description
> The number of session registrations denied by PDSN due to missing home agent for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNMissHomeAddr
> Object ID
> enterprises.8164.1.23.1.1.85
> Description
> The number of session registrations denied by PDSN due to missing home address for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNUnknChallenge
> Object ID
> enterprises.8164.1.23.1.1.86
> Description
> The number of session registrations denied by PDSN due to unknown challenge for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNMissChallenge
> Object ID
> enterprises.8164.1.23.1.1.87
> Description
> The number of session registrations denied by PDSN due to missing challenge for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNStaleChallenge
> Object ID
> enterprises.8164.1.23.1.1.88
> Description
> The number of session registrations denied by PDSN due to stale challenge for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNMNTooDistant
> Object ID
> enterprises.8164.1.23.1.1.89
> Description
> The number of session registrations denied by PDSN due to MN too distant for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNStyleUnavail
> Object ID
> enterprises.8164.1.23.1.1.90
> Description
> The number of session registration denied by PDSN due to style not available for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNHANetUnreach
> Object ID
> enterprises.8164.1.23.1.1.91
> Description
> The number of session registrations denied by PDSN due to HA network unreachable for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNHAHostUnreach
> Object ID
> enterprises.8164.1.23.1.1.92
> Description
> The number of session registrations denied by PDSN due to HA host unreachable for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNHAPortUnreach
> Object ID
> enterprises.8164.1.23.1.1.93
> Description
> The number of session registrations denied by PDSN due to HA port unreachable for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNHAUnreach
> Object ID
> enterprises.8164.1.23.1.1.94
> Description
> The number of session registrations denied by PDSN due to HA unreachable for miscellaneous reasons for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegDenPDSNInvCOA
> Object ID
> enterprises.8164.1.23.1.1.95
> Description
> The number of session registrations denied by PDSN due to invalid COA for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegReqSentInitTotal
> Object ID
> enterprises.8164.1.23.1.1.96
> Description
> The number of initial session registrations for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegReqSentInitResend
> Object ID
> enterprises.8164.1.23.1.1.97
> Description
> The number of initial session registrations retried for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegReqSentRenewTotal
> Object ID
> enterprises.8164.1.23.1.1.98
> Description
> The number of renewal session registrations for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegReqSentRenewResend
> Object ID
> enterprises.8164.1.23.1.1.99
> Description
> The number of renewal session registrations retried for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegReqSentDeregTotal
> Object ID
> enterprises.8164.1.23.1.1.100
> Description
> The number of session deregistrations for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegReqSentDeregResend
> Object ID
> enterprises.8164.1.23.1.1.101
> Description
> The number of session deregistrations retried for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentMNTooDistant
> Object ID
> enterprises.8164.1.23.1.1.102
> Description
> The number of session registration reply that indicate MN too distant for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentInvCOA
> Object ID
> enterprises.8164.1.23.1.1.103
> Description
> The number of session registration reply that indicate invalid COA for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentHANetUnreach
> Object ID
> enterprises.8164.1.23.1.1.104
> Description
> The number of session registration reply that indicate HA network unreachable for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentHAHostUnreach
> Object ID
> enterprises.8164.1.23.1.1.105
> Description
> The number of session registration reply that indicate HA host unreachable for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentHAPortUnreach
> Object ID
> enterprises.8164.1.23.1.1.106
> Description
> The number of session registration reply that indicate HA port unreachable for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentHAUnreach
> Object ID
> enterprises.8164.1.23.1.1.107
> Description
> The number of session registration reply that indicate HA unreachable due to miscellaneous reasons for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentRegTimeout
> Object ID
> enterprises.8164.1.23.1.1.108
> Description
> The number of session registration reply that indicate registration time out for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentMissNAI
> Object ID
> enterprises.8164.1.23.1.1.109
> Description
> The number of session registration reply that indicate NAI missing for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentMissHomeAgent
> Object ID
> enterprises.8164.1.23.1.1.110
> Description
> The number of session registration reply that indicate HA missing for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentMissHomeAddr
> Object ID
> enterprises.8164.1.23.1.1.111
> Description
> The number of session registration reply that indicate home address missing for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentUnknChallenge
> Object ID
> enterprises.8164.1.23.1.1.112
> Description
> The number of session registration reply that indicate unknown challenge for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentMissChallenge
> Object ID
> enterprises.8164.1.23.1.1.113
> Description
> The number of session registration reply that indicate challenge missing for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentStaleChallenge
> Object ID
> enterprises.8164.1.23.1.1.114
> Description
> The number of session registration reply that indicate stale challenge for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starMIPFAStatRegRplSentBadReply
> Object ID
> enterprises.8164.1.23.1.1.115
> Description
> The number of session registration reply that indicate bad reply for the associated Mobile IP foreign agent VPN service.
> Syntax
> Counter32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentRP(24)
> Object
> starRPStatTable
> Object ID
> enterprises.8164.1.24.1
> Description
> A table containing the R-P interface statistics.
> Syntax
> Sequence of starMIPFAStatEntry
> Access
> Not-accessible
> Description
> A table containing MIP FA statistics
> Object
> starRPStatEntry
> Object ID
> enterprises.8164.1.24.1.1
> Description
> The statistics for a specific R-P VPN (context) service.
> Syntax
> starRPStatEntry
> Access
> Not-accessible
> Sequence
> starRPStatVpnID
> starRPStatSvcID Index (Implied)
> starRPStatVpnName
> starRPStatServName
> starRPRegRecvTotal
> starRPRegAcceptTotal
> starRPRegDeniedTotal
> starRPRegDiscardTotal
> starRPRegAcceptInitial
> starRPRegAcceptIntraPDSN
> starRPRegAcceptInterPDSN
> starRPRegDeniedInitial
> starRPRegAcceptRenew
> starRPRegDeniedRenew
> starRPRegAcceptDereg
> starRPRegDeniedDereg
> starRPRegSendError
> starRPRegHashError
> starRPRegDecodeError
> starRPRegUnhandled
> starRPRegAirlinkSeqError
> starRPRegDenyUnspec
> starRPRegDenyAdminProhib
> starRPRegDenyNoResource
> starRPRegDenyAuth
> starRPRegDenyMismatchID
> starRPRegDenyBadRequest
> starRPRegDenyUnknownPDSN
> starRPRegDenyRevTunUnav
> starRPRegDenyRevTunReq
> starRPRegDenyUnrecogVend
> starRPRegUpdTotal
> starRPRegUpdAccept
> starRPRegUpdDenied
> starRPRegUpdUnack
> starRPRegUpdTrans
> starRPRegUpdRetrans
> starRPRegUpdReceived
> starRPRegUpdDiscard
> starRPRegUpdSendError
> starRPRegUpdUplyrInit
> starRPRegUpdOther
> starRPRegUpdHandoff
> starRPRegUpdDenyUnspec
> starRPRegUpdDenyAdminProhib
> starRPRegUpdDenyAuth
> starRPRegUpdDenyMismatchID
> starRPRegUpdDenyBadRequest
> starRPSecViolations
> starRPSecBadAuth
> starRPSecBadID
> starRPSecBadSpi
> starRPSecMissingMnHAAuth
> starRPSecMissingRegUpdate
> starRPRegRecvInitial
> starRPRegAcceptActvStartIntraPDSN
> starRPRegAcceptActvStopIntraPDSN
> starRPRegRecvRenew
> starRPRegActvStartRenew
> starRPRegActvStopRenew
> starRPRegRecvDereg
> starRPRegAcceptActvStopDereg
> starRPDiscSessAbsent
> starRPDiscNoMemory
> starRPDiscMalformed
> starRPDiscAuthFail
> starRPDiscInternalBounce
> starRPDiscInpuQueueExceeded
> starRPDiscMismatchedId
> starRPDiscInvPacketLen
> starRPDiscMisc
> Object
> starRPStatVpnID
> Object ID
> enterprises.8164.1.24.1.1.1
> Description
> The internal identification of the R-P VPN (context).
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starRPStatSvcID
> Object ID
> enterprises.8164.1.24.1.1.2
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).
> Syntax
> StarShortID
> Access
> Not-accessible
> Object
> starRPStatVpnName
> Object ID
> enterprises.8164.1.24.1.1.3
> Description
> The R-P VPN (context) name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starRPStatServName
> Object ID
> enterprises.8164.1.24.1.1.4
> Description
> The R-P service name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starRPRegRecvTotal
> Object ID
> enterprises.8164.1.24.1.1.5
> Description
> The total number of session registrations received for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptTotal
> Object ID
> enterprises.8164.1.24.1.1.6
> Description
> The total number of session registrations accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDeniedTotal
> Object ID
> enterprises.8164.1.24.1.1.7
> Description
> The total number of session registrations denied for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDiscardTotal
> Object ID
> enterprises.8164.1.24.1.1.8
> Description
> The total number of session registrations discarded for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptInitial
> Object ID
> enterprises.8164.1.24.1.1.9
> Description
> The total number of initial session registrations accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptIntraPDSN
> Object ID
> enterprises.8164.1.24.1.1.10
> Description
> The number of Intra-PDSN session registrations accepted for the associated R-P VPN service.
> Syntax
> Gauge32
> Access
> Read-only
> Important: Status of this alarm is obsolete.
> Object
> starRPRegAcceptInterPDSN
> Object ID
> enterprises.8164.1.24.1.1.11
> Description
> The number of Inter-PDSN session registrations accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDeniedInitial
> Object ID
> enterprises.8164.1.24.1.1.12
> Description
> The number of initial session registrations denied for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptRenew
> Object ID
> enterprises.8164.1.24.1.1.13
> Description
> The number of session registration renewals accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDeniedRenew
> Object ID
> enterprises.8164.1.24.1.1.14
> Description
> The number of session registration renewals denied for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptDereg
> Object ID
> enterprises.8164.1.24.1.1.15
> Description
> The number of session deregistrations accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDeniedDereg
> Object ID
> enterprises.8164.1.24.1.1.16
> Description
> The number of session deregistrations denied accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegSendError
> Object ID
> enterprises.8164.1.24.1.1.17
> Description
> The number of session registrations with errors in transmission for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegHashError
> Object ID
> enterprises.8164.1.24.1.1.18
> Description
> The number of session registrations with hash errors for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDecodeError
> Object ID
> enterprises.8164.1.24.1.1.19
> Description
> The number of session registrations with decode errors for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUnhandled
> Object ID
> enterprises.8164.1.24.1.1.20
> Description
> The number of session registrations not processed for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAirlinkSeqError
> Object ID
> enterprises.8164.1.24.1.1.21
> Description
> The number of session registrations with air link sequence errors for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyUnspec
> Object ID
> enterprises.8164.1.24.1.1.22
> Description
> The number of session registrations denied for an unspecified reason for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyAdminProhib
> Object ID
> enterprises.8164.1.24.1.1.23
> Description
> The number of session registrations denied due to administrator prohibition for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyNoResource
> Object ID
> enterprises.8164.1.24.1.1.24
> Description
> The number of session registrations denied due to no resources available for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyAuth
> Object ID
> enterprises.8164.1.24.1.1.25
> Description
> The number of session registrations denied due to authentication failure for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyMismatchID
> Object ID
> enterprises.8164.1.24.1.1.26
> Description
> The number of session registrations denied due to an ID mismatch for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyBadRequest
> Object ID
> enterprises.8164.1.24.1.1.27
> Description
> The number of session registrations denied due to the request being invalid for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyUnknownPDSN
> Object ID
> enterprises.8164.1.24.1.1.28
> Description
> The number of session registrations denied due to the packet data service not being recognized for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyRevTunUnav
> Object ID
> enterprises.8164.1.24.1.1.29
> Description
> The number of session registrations denied due to no reverse tunnel being available for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyRevTunReq
> Object ID
> enterprises.8164.1.24.1.1.30
> Description
> The number of session registrations denied due to reverse tunneling being mandatory for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegDenyUnrecogVend
> Object ID
> enterprises.8164.1.24.1.1.31
> Description
> The number of session registrations denied due to the vendor not being recognized for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdTotal
> Object ID
> enterprises.8164.1.24.1.1.32
> Description
> The total number of session registration updates for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdAccept
> Object ID
> enterprises.8164.1.24.1.1.33
> Description
> The number of session registration updates which were accepted for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDenied
> Object ID
> enterprises.8164.1.24.1.1.34
> Description
> The number of session registration updates denied for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdUnack
> Object ID
> enterprises.8164.1.24.1.1.35
> Description
> The number of session registration updates which were not acknowledged for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdTrans
> Object ID
> enterprises.8164.1.24.1.1.36
> Description
> The number of session registration updates sent for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdRetrans
> Object ID
> enterprises.8164.1.24.1.1.37
> Description
> The number of session registration updates resent for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdReceived
> Object ID
> enterprises.8164.1.24.1.1.38
> Description
> The number of session registration updates received for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDiscard
> Object ID
> enterprises.8164.1.24.1.1.39
> Description
> The number of session registration updates discarded for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdSendError
> Object ID
> enterprises.8164.1.24.1.1.40
> Description
> The number of session registration updates with errors in transmission for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdUplyrInit
> Object ID
> enterprises.8164.1.24.1.1.41
> Description
> The number of session registration updates with up-link re-initializations.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdOther
> Object ID
> enterprises.8164.1.24.1.1.42
> Description
> The number of session registration updates with a reason of ‘other’ for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdHandoff
> Object ID
> enterprises.8164.1.24.1.1.43
> Description
> The number of session registration updates due to a mobile hand-off for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDenyUnspec
> Object ID
> enterprises.8164.1.24.1.1.44
> Description
> The number of session registration updates denied for an unspecified reason for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDenyAdminProhib
> Object ID
> enterprises.8164.1.24.1.1.45
> Description
> The number of session registration updates denied due to administrator prohibition for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDenyAuth
> Object ID
> enterprises.8164.1.24.1.1.46
> Description
> The number of session registration updates denied due to authentication failure for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDenyMismatchID
> Object ID
> enterprises.8164.1.24.1.1.47
> Description
> The number of session registration updates denied due to an ID mismatch for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegUpdDenyBadRequest
> Object ID
> enterprises.8164.1.24.1.1.48
> Description
> The number of session registration updates denied due to the request being invalid for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPSecViolations
> Object ID
> enterprises.8164.1.24.1.1.49
> Description
> The total number of session security violations for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPSecBadAuth
> Object ID
> enterprises.8164.1.24.1.1.50
> Description
> The total number of session security authentication violations for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPSecBadID
> Object ID
> enterprises.8164.1.24.1.1.51
> Description
> The total number of session security ID violations for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPSecBadSpi
> Object ID
> enterprises.8164.1.24.1.1.52
> Description
> The total number of session security SPI violations for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPSecMissingMnHAAuth
> Object ID
> enterprises.8164.1.24.1.1.53
> Description
> The total number of session security missing mobile number home agent authentication violations for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPSecMissingRegUpdate
> Object ID
> enterprises.8164.1.24.1.1.54
> Description
> The total number of session missing registration update violations for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegRecvInitial
> Object ID
> enterprises.8164.1.24.1.1.55
> Description
> The total number of initial session registration for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptActvStartIntraPDSN
> Object ID
> enterprises.8164.1.24.1.1.56
> Description
> The number of accepted registration request during intra-PDSN handoffs which contains active start for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptActvStopIntraPDSN
> Object ID
> enterprises.8164.1.24.1.1.57
> Description
> The number of accepted registration request during intraPDSN handoff which contains active stop for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegRecvRenew
> Object ID
> enterprises.8164.1.24.1.1.58
> Description
> The number of received renew registration request for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegActvStartRenew
> Object ID
> enterprises.8164.1.24.1.1.59
> Description
> The number of received renew registration request that contains active start for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegActvStopRenew
> Object ID
> enterprises.8164.1.24.1.1.60
> Description
> The number of received renew registration request that contains active stop for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegRecvDereg
> Object ID
> enterprises.8164.1.24.1.1.61
> Description
> The number of received deregistration request for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPRegAcceptActvStopDereg
> Object ID
> enterprises.8164.1.24.1.1.62
> Description
> The number of accepted deregistration request that contains active stop for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscSessAbsent
> Object ID
> enterprises.8164.1.24.1.1.63
> Description
> The number of registration request discarded due to no session for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscNoMemory
> Object ID
> enterprises.8164.1.24.1.1.64
> Description
> The number of registration request discarded due to no memory for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscMalformed
> Object ID
> enterprises.8164.1.24.1.1.65
> Description
> The number of registration request discarded because malformed for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscAuthFail
> Object ID
> enterprises.8164.1.24.1.1.66
> Description
> The number of registration request discarded because authentication failed for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscInternalBounce
> Object ID
> enterprises.8164.1.24.1.1.67
> Description
> The number of registration request discarded because internal bounce for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscInpuQueueExceeded
> Object ID
> enterprises.8164.1.24.1.1.68
> Description
> The number of registration request discarded because internal queue exceeded for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscMismatchedId
> Object ID
> enterprises.8164.1.24.1.1.69
> Description
> The number of registration request discarded because mismatched ID for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscInvPacketLen
> Object ID
> enterprises.8164.1.24.1.1.70
> Description
> The number of registration request discarded because invalid packet length for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscMisc
> Object ID
> enterprises.8164.1.24.1.1.71
> Description
> The number of registration request discarded due to misc. reasons for the associated R-P VPN service.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRP1xTxBytes
> Object ID
> enterprises.8164.1.24.1.1.72
> Description
> The number of 1x bytes transmitted, in megabytes.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDiscMisc
> Object ID
> enterprises.8164.1.24.1.1.73
> Description
> The number of 1x bytes received, in megabytes.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRP1xTxPackets
> Object ID
> enterprises.8164.1.24.1.1.74
> Description
> The number of 1x packets transmitted, in thousands.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRP1xRxPackets
> Object ID
> enterprises.8164.1.24.1.1.75
> Description
> The number of 1x packets received, in thousands.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDoTxBytes
> Object ID
> enterprises.8164.1.24.1.1.76
> Description
> The number of Do bytes transmitted, in megabytes.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDoRxBytes
> Object ID
> enterprises.8164.1.24.1.1.77
> Description
> The number of Do bytes received, in megabytes.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDoTxPackets
> Object ID
> enterprises.8164.1.24.1.1.78
> Description
> The number of Do packets transmitted, in thousands.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starRPDoRxPackets
> Object ID
> enterprises.8164.1.24.1.1.79
> Description
> The number of Do packets received, in thousands.
> Syntax
> Counter32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentSubscriber(26)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starSubTable
> Object ID
> enterprises.8164.1.26.1
> Description
> A table containing subscriber information.
> Syntax
> SEQUENCE OF starSubEntry
> Access
> Not-accessible
> Object
> starSubEntry
> Object ID
> enterprises.8164.1.26.1.1
> Description
> Information for a specific Subscriber.
> Syntax
> starSubEntry
> Access
> Not-accessible
> Sequence
> starSubContext
> starSubMSID Index
> starSubName Index
> starSubTimerDuration
> starSubLongDurTimeoutAction
> starSubSetupTime
> starSubHomeAddr
> starSubHomeAddrv6
> Object
> starSubContext
> Object ID
> enterprises.8164.1.26.1.1.1
> Description
> The context the subscriber is in.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSubMSID
> Object ID
> enterprises.8164.1.26.1.1.2
> Description
> The MSID of the subscriber.
> Syntax
> OCTET STRING (SIZE (1..16))
> Access
> Not-accessible
> Object
> starSubName
> Object ID
> enterprises.8164.1.26.1.1.3
> Description
> The name of the subscriber.
> Syntax
> OCTET STRING (SIZE (1..128))
> Access
> Not-accessible
> Object
> starSubTimerDuration
> Object ID
> enterprises.8164.1.26.1.1.4
> Description
> The length of the long-duration timer in seconds
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starSubLongDurTimeoutAction
> Object ID
> enterprises.8164.1.26.1.1.5
> Description
> he action taken by the system upon detection of a long-duration session.
> Syntax
> StarLongDurTimeoutAction
> Access
> Read-only
> Object
> starSubSetupTime
> Object ID
> enterprises.8164.1.26.1.1.6
> Description
> The time when the call was setup.
> Syntax
> DateAndTime
> Access
> Read-only
> Object
> starSubHomeAddr
> Object ID
> enterprises.8164.1.26.1.1.7
> Description
> The IPv4 home address.
> Syntax
> IPv4Address
> Access
> Read-only
> Object
> starSubHomeAddrv6
> Object ID
> enterprises.8164.1.26.1.1.8
> Description
> The IPv6 home address.
> Syntax
> IPv6Address
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentEISServer(27)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starEISServerTable
> Object ID
> enterprises.8164.1.27.1
> Description
> A table containing EIS Server information.
> Syntax
> SEQUENCE OF StarEISServerEntry
> Access
> Not-accessible
> Object
> starEISServerEntry
> Object ID
> enterprises.8164.1.27.1.1
> Description
> Information for a specific EIS Server.
> Syntax
> StarEISServerEntry
> Access
> Not-accessible
> Sequence
> starEISServerVPNID Index
> starEISServerAddr Index
> starEISServerVPNName
> Object
> starEISServerVPNID
> Object ID
> enterprises.8164.1.27.1.1.1
> Description
> The VPN ID for the EIS Server.
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starEISServerAddr
> Object ID
> enterprises.8164.1.27.1.1.2
> Description
> The IP Address for the EIS Server.
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starEISServerVPNName
> Object ID
> enterprises.8164.1.27.1.1.3
> Description
> The VPN Name for this EIS Server.
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starentThresholds(28)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starThreshMeasuredPct
> Object ID
> enterprises.8164.1.28.1
> Description
> The measured value of a thresholded parameter.
> Syntax
> INTEGER32(0..100)
> Access
> Accessible-for-notify
> Object
> starThreshPct
> Object ID
> enterprises.8164.1.28.2
> Description
> The configured value of a thresholded parameter.
> Syntax
> INTEGER32(0..100)
> Access
> Accessible-for-notify
> Object
> starThreshMeasuredInt
> Object ID
> enterprises.8164.1.28.3
> Description
> The measured value of a thresholded parameter.
> Syntax
> Guage32
> Access
> Accessible-for-notify
> Object
> starThreshInt
> Object ID
> enterprises.8164.1.28.4
> Description
> The configured value of a thresholded parameter.
> Syntax
> Unsigned32
> Access
> Accessible-for-notify
> Object
> starThreshMeasuredMB
> Object ID
> enterprises.8164.1.28.5
> Description
> The measured value of a thresholded parameter.
> Syntax
> Guard32
> Units
> Megabytes
> Access
> Accessible-for-notify
> Object
> starThreshMB
> Object ID
> enterprises.8164.1.28.6
> Description
> The configured value of a thresholded parameter
> Syntax
> Unsigned32
> Units
> Megabytes
> Access
> Accessible-for-notify
> Object
> starThreshMeasuredGB
> Object ID
> enterprises.8164.1.28.7
> Description
> The configured value of a thresholded parameter.
> Syntax
> Gauge32
> Units
> Gigabytes
> Access
> Accessible-for-notify
> Object
> starThreshGB
> Object ID
> enterprises.8164.1.28.8
> Description
> The configured value of a thresholded parameter.
> Syntax
> Unsigned32
> Units
> Gigabytes
> Access
> Accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starentPort(29)
> Object
> starPortTable
> Object ID
> enterprises.8164.1.29.1
> Description
> A table containing Port information.
> Syntax
> SEQUENCE OF starPortEntry
> Access
> Not-accessible
> Object
> starPortEntry
> Object ID
> enterprises.8164.1.29.1.1
> Description
> Information for a specific Port
> Syntax
> starPortEntry
> Access
> Not-accessible
> Sequence
> starPortSlot Integer32
> starPortNum integer32
> starPortType INTEGER
> starPortTypeDescr DisplayString
> starPortAdminState INTEGER
> starPortOperState INTEGER
> starPortOperMode INTEGER
> starPortLinkState INTEGER
> starRedundantPortSlot integer32
> starRedundantPortNum integer32
> starPortRXByte Counter32
> starPortTXByte Counter32
> starPortRXFrames Counter32
> starPortTXFrames Counter32
> starPortRxDiscards Counter32
> starPortTxDiscards Counter32
> starPortRxErrors Counter32
> starPortTxErrors Counter32
> Object
> starPortSlot
> Object ID
> enterprises.8164.1.29.1.1.1
> Description
> The Slot number for this port.
> Syntax
> Integer32(1..48)
> Access
> Not-accessible
> Object
> starPortNum
> Object ID
> enterprises.8164.1.29.1.1.2
> Description
> The Port number within this slot.
> Syntax
> Integer32(1..8)
> Access
> Not-accessible
> Object
> starPortType
> Object ID
> enterprises.8164.1.29.1.1.3
> Description
> The type of the port.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> none(0)
> ethernet10100(1)
> ethernet1000dualmedia(2)
> ethernet1000(3)
> ds3(4)
> oc3(5)
> oc3atm(6)
> ds3e(7)
> rs232(8)
> bits1e1(9)
> virtualEthernet(10)
> Object
> starPortTypeDescr
> Object ID
> enterprises.8164.1.29.1.1.4
> Description
> A textual representation of the starPortType attribute
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPortAdminState
> Object ID
> enterprises.8164.1.29.1.1.5
> Description
> The administrative start of the port
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> enabled(1)
> disabled(2)
> Object
> starPortOperState
> Object ID
> enterprises.8164.1.29.1.1.6
> Description
> The operation status of the port
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> up(1)
> down(2)
> notapplicable(3)
> Object
> starPortOperMode
> Object ID
> enterprises.8164.1.29.1.1.7
> Description
> The operation mode of the port
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> active(1)
> standby(2)
> Object
> starPortLinkState
> Object ID
> enterprises.8164.1.29.1.1.8
> Description
> The link status of the port
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> up(1)
> down(2)
> Object
> starRedundantPortSlot
> Object ID
> enterprises.8164.1.29.1.1.9
> Description
> The slot number of the redundant port for the current port.
> Syntax
> Integer32(1..48)
> Access
> Read-only
> Object
> starRedundantPortNum
> Object ID
> enterprises.8164.1.29.1.1.10
> Description
> The port number of the redundant port for the current port
> Syntax
> Integer32(1..8)
> Access
> Read-only
> Object
> starPortRXBytes
> Object ID
> enterprises.8164.1.29.1.1.11
> Description
> The number of bytes successfully received, in megabytes.
> For ports of type rs232(8) for bitst1e1(9) this value will always be zero.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPortTXBytes
> Object ID
> enterprises.8164.1.29.1.1.12
> Description
> The number of bytes successfully transmitted in megabytes. For ports of type rs232(8) for bitst1e1(9) this value will always be zero.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPortRXFrames
> Object ID
> enterprises.8164.1.29.1.1.13
> Description
> The number of frames successfully received, in thousands. For ports of type rs232(8) for bitst1e1(9) this value will always be zero and for ports of type oc3atm(5) and oc12atm(6) this is the count of cells received.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPortTXFrames
> Object ID
> enterprises.8164.1.29.1.1.14
> Description
> The number of frames successfully transmitted, in thousands. For ports of type rs232(8) for bitst1e1(9) this value will always be zero and for ports of type oc3atm(5) and oc12atm(6) this is the count of cells received..
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPortRxDiscards
> Object ID
> enterprises.8164.1.29.1.1.15
> Description
> The number of inbound packets which were chosen to be discarded even though no errors had been detected to prevent their being deliverable to a higher-layer protocol. One possible reason for discarding such a packet could be to free up buffer space.
> Syntax
> Counter32
> Access
> read-only
> Object
> starPortTxDiscards
> Object ID
> enterprises.8164.1.29.1.1.16
> Description
> The number of outbound packets which were chosen to be discarded even though no errors had been detected to prevent their being transmitted. One possible reason for discarding such a packet could be to free up buffer space.
> Syntax
> Counter32
> Access
> read-only
> Object
> starPortRxErrors
> Object ID
> enterprises.8164.1.29.1.1.17
> Description
> The number of inbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.
> Syntax
> Counter32
> Access
> read-only
> Object
> starPortTxErrors
> Object ID
> enterprises.8164.1.29.1.1.18
> Description
> The number of outbound packets that could not be transmitted because of errors.
> Syntax
> Counter32
> Access
> read-only
> Units
> Thousands
> starentMIB(8164).starentMIBObjects(1).starentIPPool(30)
> Object
> starIPPoolTable
> Object ID
> enterprises.8164.1.30.1
> Description
> A table containing IP Pool information.
> Syntax
> SEQUENCE OF StarIPPoolEntry
> Access
> Not-accessible
> Object
> starIPPoolEntry
> Object ID
> enterprises.8164.1.30.1.1
> Description
> Information for a specific IP Pool
> Syntax
> StarIPPoolEntry
> Access
> Not-accessible
> Sequence
> starIPPoolVpnID Gauge32
> starIPPoolID StarMediumID
> starIPPoolContext DisplayString
> starIPPoolGroup DisplayString
> starIPPoolName OCTET STRING
> starIPPoolType INTEGER
> starIPPoolState INTEGER
> starIPPoolStartAddr IpAddress
> starIPPoolMaskorEndAddr IpAddress
> starIPPoolPriority Integer32
> starIPPoolUsed Gauge32
> starIPPoolHold Gauge32
> starIPPoolRelease Gauge32
> starIPPoolFree Gauge32
> Object
> starIPPoolVpnID
> Object ID
> enterprises.8164.1.30.1.1.1
> Description
> The context ID for this pool.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starIPPoolID
> Object ID
> enterprises.8164.1.30.1.1.2
> Description
> The service identification is made up from first 16 chars of context name and first 8 chars of pool name separated by (:).
> Syntax
> StarMediumID
> Access
> Not-accessible
> Object
> starIPPoolContext
> Object ID
> enterprises.8164.1.30.1.1.3
> Description
> The context for this pool.
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starIPPoolGroup
> Object ID
> enterprises.8164.1.30.1.1.4
> Description
> The name of the group to which the IP pool belongs.
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starIPPoolName
> Object ID
> enterprises.8164.1.30.1.1.5
> Description
> The name of the IP pool.
> Syntax
> OCTET STRING (SIZE (1..32))
> Access
> Not-accessible
> Object
> starIPPoolType
> Object ID
> enterprises.8164.1.30.1.1.6
> Description
> The type of the pool.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> private(1)
> public(2)
> static(3)
> resource(4),
> nat(5)
> Object
> starIPPoolState
> Object ID
> enterprises.8164.1.30.1.1.7
> Description
> The state of the pool.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> good(1)
> pendingdelete(2)
> alarm(3)
> resize(4)
> inactive(5)
> Object
> starIPPoolStartAddr
> Object ID
> enterprises.8164.1.30.1.1.8
> Description
> The start IP address of the pool.
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starIPPoolMaskorEndAddr
> Object ID
> enterprises.8164.1.30.1.1.9
> Description
> The mask or end IP address of the pool.
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starIPPoolPriority
> Object ID
> enterprises.8164.1.30.1.1.10
> Description
> The priority of the pool.
> Syntax
> Integer32
> Access
> Read-only
> Object
> starIPPoolUsed
> Object ID
> enterprises.8164.1.30.1.1.11
> Description
> The number of IP addresses in USED state in the pool.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starIPPoolHold
> Object ID
> enterprises.8164.1.30.1.1.12
> Description
> The number of IP addresses in HOLD state in the pool.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starIPPoolRelease
> Object ID
> enterprises.8164.1.30.1.1.13
> Description
> The number of IP addresses in RELEASE state in the pool.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starIPPoolFree
> Object ID
> enterprises.8164.1.30.1.1.14
> Description
> The number of IP addresses in FREE state in the pool.
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentTrapData(31)
> Object
> starCongestionPolicy
> Object ID
> enterprises.8164.1.31.1
> Description
> The policy invoked for congestion events.
> Syntax
> INTEGER
> Access
> Not-accessible
> Objects
> reject(1)
> redirect(2)
> drop(3)
> Object
> starCongestionResourceType
> Object ID
> enterprises.8164.1.31.2
> Description
> The resource type for a congestion event.
> Syntax
> INTEGER
> Access
> Not-accessible
> Objects
> systemcpu(1)
> servicecpu(2)
> averagememory(3)
> queuesize(4)
> queuedelay(5)
> license(6)
> portutil(7)
> rxportutill(8)
> txportutil(9)
> rxperportutil(10)
> txperportutil(11)
> servicecapacity(12)
> Object
> starPTACConfig
> Object ID
> enterprises.8164.1.31.3
> Description
> The number of PACs/PSCs/TACs configured in the system.
> Syntax
> Integer32(0..14)
> Access
> Not-accessible
> Object
> starPTACActive
> Object ID
> enterprises.8164.1.31.4
> Description
> The number of PACs/PSCs/TACs active in the system.
> Syntax
> Integer32(0..14)
> Access
> Not-accessible
> Object
> starContextName
> Object ID
> enterprises.8164.1.31.5
> Description
> The name of a context configured on the system.
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starInterfaceName
> Object ID
> enterprises.8164.1.31.6
> Description
> The name of an interface.
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starPCFAddress
> Object ID
> enterprises.8164.1.31.7
> Description
> The IP address of a PCF.
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starPeerAddress
> Object ID
> enterprises.8164.1.31.8
> Description
> Peer Address
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starLicensedSessions
> Object ID
> enterprises.8164.1.31.9
> Description
> The number of sessions enabled by the software license.
> Syntax
> Unsigned32
> Access
> Accessible-for-notify
> Object
> starCurrentSessions
> Object ID
> enterprises.8164.1.31.10
> Description
> The number of current sessions in use against a software license.
> Syntax
> Gauge32
> Access
> Accessible-for-notify
> Object
> starL3Address
> Object ID
> enterprises.8164.1.31.11
> Description
> L3 Address
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starUDPPortNum
> Object ID
> enterprises.8164.1.31.12
> Description
> UDP Port Number
> Syntax
> Integer32(1..65535)
> Access
> Not-accessible
> Object
> starSRPIPAddress
> Object ID
> enterprises.8164.1.31.13
> Description
> SRP IP Address
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starBGPPeerIPAddress
> Object ID
> enterprises.8164.1.31.14
> Description
> BGP Peer IP Address
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starContFiltCFFilename
> Object ID
> enterprises.8164.1.31.15
> Description
> File name for the Optimized Content Rating Database (OPTCMDB)
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starContFiltCFErrorCode
> Object ID
> enterprises.8164.1.31.16
> Description
> Error code.
> Syntax
> Integer32
> Access
> Not-accessible
> Object
> starFetchedFromAAAMgr
> Object ID
> enterprises.8164.1.31.17
> Description
> The total number of calls fetched from AAA Manager
> Syntax
> Integer32
> Access
> Read-only
> Object
> starPriorToAudit
> Object ID
> enterprises.8164.1.31.18
> Description
> The number calls prior to audit
> Syntax
> Integer32
> Access
> Read-only
> Object
> starPassedAudit
> Object ID
> enterprises.8164.1.31.19
> Description
> The number calls prior to audit
> Syntax
> Integer32
> Access
> Read-only
> Object
> starCallsRecovered
> Object ID
> enterprises.8164.1.31.20
> Description
> The number calls recovered
> Syntax
> Integer32
> Access
> Read-only
> Object
> starA11CallLines
> Object ID
> enterprises.8164.1.31.21
> Description
> The number of A11 call lines
> Syntax
> Integer32
> Access
> Read-only
> Object
> starElapsedMs
> Object ID
> enterprises.8164.1.31.22
> Description
> The audit time elapsed in milli-seconds
> Syntax
> Integer32
> Access
> Read-only
> Object
> starCDRFilename
> Object ID
> enterprises.8164.1.31.23
> Description
> The name of a CDR (EDR/UDR) file.
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starDiameterVpnName
> Object ID
> enterprises.8164.1.31.24
> Description
> Diameter VPN (Context) Name
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starDiameterPeerAddr
> Object ID
> enterprises.8164.1.31.25
> Description
> Diameter Peer Address
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> Object
> starDiameterEndpointName
> Object ID
> enterprises.8164.1.31.26
> Description
> Diameter Endpoint Name
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starInterfaceIPAddress
> Object ID
> enterprises.8164.1.31.27
> Description
> Interface IP Address
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> Object
> starOSPFNeighborRouterID
> Object ID
> enterprises.8164.1.31.28
> Description
> Interface IP Address
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> Object
> starOSPFFromState
> Object ID
> enterprises.8164.1.31.29
> Description
> FROM state for OSPF Neighbor
> Syntax
> StarOSPFNeighborState
> Access
> Accessible-for-notify
> Object
> starOSPFToState
> Object ID
> enterprises.8164.1.31.30
> Description
> TO state for OSPF Neighbor
> Syntax
> StarOSPFNeighborState
> Access
> Accessible-for-notify
> Object
> starDiameterEncoderString
> Object ID
> enterprises.8164.1.31.31
> Description
> Diameter Cause Code String
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starDiameterECode
> Object ID
> enterprises.8164.1.31.33
> Description
> Diameter Cause code
> Syntax
> Integer
> Access
> Accessible-for-notify
> Enumeration
> notcomplete(1)
> hostnamemismatch(2)
> hostrealmismatch(3)
> securitymismatch(4)
> tlscertificateerror(5)
> tlshandshakeerror(6)
> authappidmismatch(7)
> Object
> starDiameterPeerAddrIpv6
> Object ID
> enterprises.8164.1.31.34
> Description
> Diameter Peer Address
> Syntax
> Ipv6Address
> Access
> accessible-for-notify
> Object
> starContFiltCFUpgradeFilename
> Object ID
> enterprises.8164.1.31.35
> Description
> File name for the Full or Incremental OPTCMDB
> Syntax
> DisplayString
> Access
> not-accessible
> Object
> starContFiltCFUpgradeErrorCode
> Object ID
> enterprises.8164.1.31.36
> Description
> Error code
> Syntax
> unknownerror(1)
> upgradefullfailure(2)
> upgradeincrfailure(3)
> Access
> not-accessible
> Object
> starBLUpgradeFilename
> Object ID
> enterprises.8164.1.31.37
> Description
> File name for the Full OPTBLDB
> Syntax
> DisplayString
> Access
> not-accessible
> Object
> starBLUpgradeErrorCode
> Object ID
> enterprises.8164.1.31.38
> Description
> Error code
> Syntax
> unknownerror(1)
> upgradefullfailure(2)
> Access
> not-accessible
> Object
> starDynPkgFilename
> Object ID
> enterprises.8164.1.31.39
> Description
> File name for the DynPkg
> Syntax
> DisplayString
> Access
> not-accessible
> Object
> starDynCFErrorCode
> Object ID
> enterprises.8164.1.31.40
> Description
> Error code
> Syntax
> unknownerror(1)
> notavailable(2)
> loadfailure(3)
> Access
> not-accessible
> Object
> starDynPkgUpgradeFilename
> Object ID
> enterprises.8164.1.31.41
> Description
> File name for the Full DynPkg
> Syntax
> DisplayString
> Access
> not-accessible
> Object
> starDynCFUpgradeErrorCode
> Object ID
> enterprises.8164.1.31.42
> Description
> Error code
> Syntax
> unknownerror(1)
> upgradefullfailure(2)
> Access
> not-accessible
> Object
> starCscfSessCongestionResourceType
> Object ID
> enterprises.8164.1.31.43
> Description
> Cscf Session resource type for a congestion event
> Syntax
> cpu(1)
> memory(2)
> Access
> not-accessible
> Object
> starSmgrId
> Object ID
> enterprises.8164.1.31.44
> Description
> Session Manager Instance ID
> Syntax
> Integer32
> Access
> not-accessible
> Object
> starEGTPVpnName
> Object ID
> enterprises.8164.1.31.45
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starEGTPServName
> Object ID
> enterprises.8164.1.31.46
> Description
> The name of this service
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starEGTPInterfaceType
> Object ID
> enterprises.8164.1.31.47
> Description
> Egtp interface type
> Syntax
> INTEGER
> Access
> accessible-for-notify
> Object
> starEGTPSelfPort
> Object ID
> enterprises.8164.1.31.48
> Description
> The Port number of the EGTP
> Syntax
> Gauge32
> Access
> accessible-for-notify
> Object
> starEGTPSelfAddr
> Object ID
> enterprises.8164.1.31.49
> Description
> The IP Address of the EGTP
> Syntax
> IpAddress
> Access
> accessible-for-notify
> Object
> starEGTPPeerPort
> Object ID
> enterprises.8164.1.31.50
> Description
> The Port number of the PeerNode
> Syntax
> Gauge32
> Access
> accessible-for-notify
> Object
> starEGTPPeerAddr
> Object ID
> enterprises.8164.1.31.51
> Description
> The IP Address of the PeerNode
> Syntax
> IpAddress
> Access
> accessible-for-notify
> Object
> starEGTPPeerOldRstCnt
> Object ID
> enterprises.8164.1.31.52
> Description
> EGTP peer old restart counter
> Syntax
> Gauge32
> Access
> accessible-for-notify
> Object
> starEGTPPeerNewRstCnt
> Object ID
> enterprises.8164.1.31.53
> Description
> EGTP peer new restart counter
> Syntax
> Gauge32
> Access
> accessible-for-notify
> Object
> starEGTPPeerSessCnt
> Object ID
> enterprises.8164.1.31.54
> Description
> EGTP peer session count
> Syntax
> Gauge32
> Access
> accessible-for-notify
> Object
> starEGTPFailureReason
> Object ID
> enterprises.8164.1.31.55
> Description
> Egtp path failure reason
> Syntax
> INTEGER
> Access
> accessible-for-notify
> Object
> starGSSCDRLossConfigured
> Object ID
> enterprises.8164.1.31.56
> Description
> The configured value of threshold CDR Loss at GSS
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starGSSCDRLossMeasured
> Object ID
> enterprises.8164.1.31.57
> Description
> The Measured value of CDR Loss at GSS
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starLicenseKey
> Object ID
> enterprises.8164.1.31.58
> Description
> The license key
> Syntax
> Unsigned32
> Access
> accessible-for-notifyaccessible-for-notify
> Object
> starLicenseExpiryDate
> Object ID
> enterprises.8164.1.31.59
> Description
> The license expiration date/time
> Syntax
> DateAndTime
> Access
> accessible-for-notify
> Object
> starLicenseDaysRemaining
> Object ID
> enterprises.8164.1.31.60
> Description
> The number of days remaining before the license expires
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starLicenseDaysafterExpiry
> Object ID
> enterprises.8164.1.31.61
> Description
> The number of days after the license has expired
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starNPUSlot
> Object ID
> enterprises.8164.1.31.62
> Description
> The NPU slot number
> Syntax
> Integer32
> Access
> accessible-for-notify
> Object
> starSPRServerIpAddr
> Object ID
> enterprises.8164.1.31.63
> Description
> The IP Address of the SSC Server
> Syntax
> IpAddress
> Access
> accessible-for-notify
> Object
> starMVGEndpointName
> Object ID
> enterprises.8164.1.31.66
> Description
> MVG Endpoint Name.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starMVGProtocolType
> Object ID
> enterprises.8164.1.31.68
> Description
> MVG Protocol Types.
> Syntax
> INTEGER { protocolhttp(1), protocoltcp(2), protocolicmp(3) }
> Access
> accessible-for-notify
> Object
> starMVGCauseCode
> Object ID
> enterprises.8164.1.31.69
> Description
> MVG Cause Code.
> Syntax
> INTEGER { servernotreachable(1), servicereachable(2) }
> Access
> accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starentGGSNService(32)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starGGSNSerTable
> Object ID
> enterprises.8164.1.32.1
> Description
> A table containing GGSN related information
> Syntax
> SEQUENCE OF StarGGSNSerEntry
> Access
> Not-accessible
> Object
> starGGSNSerEntry
> Object ID
> enterprises.8164.1.32.1.1
> Description
> The statistics for a specific GGSN service
> Syntax
> StarGGSNSerEntry
> Access
> Not-accessible
> Sequence
> starGGSNSerVpnID
> starGGSNSerSvcID
> starSessGGSNVpnName
> starSessGGSNServName
> starSessGGSNPeerPort
> starSessGGSNPeerAddr
> starSessGGSNImsi
> starSessGGSNSubsName
> starSessGGSNAPNName
> Object
> starGGSNSerVpnID
> Object ID
> enterprises.8164.1.32.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starGGSNSerSvcID
> Object ID
> enterprises.8164.1.32.1.1.2
> Description
> The internal identification of this service; unique within a specific context
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starSessGGSNVpnName
> Object ID
> enterprises.8164.1.32.1.1.3
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessGGSNServName
> Object ID
> enterprises.8164.1.32.1.1.4
> Description
> The name of this service
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessGGSNPeerPort
> Object ID
> enterprises.8164.1.32.1.1.5
> Description
> The Peer Port for which PATH Failure has occurred
> Syntax
> Gauge32
> Access
> Accessible-for-notify
> Object
> starSessGGSNPeerAddr
> Object ID
> enterprises.8164.1.32.1.1.6
> Description
> The Peer Address for which PATH Failure has occurred
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessGGSNImsi
> Object ID
> enterprises.8164.1.32.1.1.7
> Description
> The IMSI of the subscriber.
> Syntax
> OCTET STRING (SIZE (1..8))
> Access
> Accessible-for-notify
> Object
> starSessGGSNSubsName
> Object ID
> enterprises.8164.1.32.1.1.8
> Description
> The name of the subscriber.
> Syntax
> OCTET STRING (SIZE (1..128))
> Access
> Accessible-for-notify
> Object
> starSessGGSNAPNName
> Object ID
> enterprises.8164.1.32.1.1.9
> Description
> The name of the APN.
> Syntax
> OCTET STRING (SIZE (1..64))
> Access
> Accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starentL2TP(33)
> Object
> starL2TPTable
> Object ID
> enterprises.8164.1.33.1
> Description
> A table containing L2TP related information
> Syntax
> SEQUENCE OF starL2TPEntry
> Access
> Not-accessible
> Object
> starL2TPEntry
> Object ID
> enterprises.8164.1.33.1.1
> Description
> The statistics for a L2TP entry
> Syntax
> starL2TPEntry
> Access
> Not-accessible
> Sequence
> starL2TPLocalTunnelID
> starL2TPPeerTunnelID
> starL2TPContextName
> starL2TPServiceName
> starL2TPServiceTypeName
> starL2TPLocalAddress
> starL2TPPeerAddress
> Object
> starL2TPLocalTunnelID
> Object ID
> enterprises.8164.1.33.1.1.1
> Description
> The internal identification of the L2TP local tunnel ID
> Syntax
> Unsigned32
> Access
> Not-accessible
> Object
> starL2TPPeerTunnelID
> Object ID
> enterprises.8164.1.33.1.1.2
> Description
> The internal identification of the L2TP peer tunnel ID
> Syntax
> Unsigned32
> Access
> Not-accessible
> Object
> starL2TPContextName
> Object ID
> enterprises.8164.1.33.1.1.3
> Description
> The name of the context
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starL2TPServiceName
> Object ID
> enterprises.8164.1.33.1.1.4
> Description
> The name of the service
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starL2TPServiceTypeName
> Object ID
> enterprises.8164.1.33.1.1.5
> Description
> The name of the service type
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starL2TPLocalAddress
> Object ID
> enterprises.8164.1.33.1.1.6
> Description
> The local address of the service
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> Object
> starL2TPPeerAddress
> Object ID
> enterprises.8164.1.33.1.1.7
> Description
> The peer address of the service
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starSessSub1(34)

> 1. | Use a SET pdu to provide the keys to lookup. Set one or more of the fields starSessSub1Context, starSessSub1NAI, starSessSub1MSID, starSessSub1IpAddr.

> The SET pdu returns once the query is complete. This query can takes some time especially on large systems, so do not use small retry timers.

> 2. | Use a GET pdu to retrieve the data.

> Important: Note that in some cases, multiple subscribers might watch the given search criteria. The starSessSub1LastResult field identifies if zero, one or multiple matches were found. If multiple matches are found, data is returned for one of them.
> Object
> starSessSub1Context
> Object ID
> enterprises.8164.1.34.1
> Description
> The name of the context for this subscriber. If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.
> Syntax
> DisplayString
> Access
> Read-write
> Object
> starSessSub1NAI
> Object ID
> enterprises.8164.1.34.2
> Description
> The NAI for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.
> Syntax
> OCTET STRING (SIZE (1..128))
> Access
> Read-write
> Object
> starSessSub1MSID
> Object ID
> enterprises.8164.1.34.3
> Description
> The MSID for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.
> Syntax
> OCTET STRING (SIZE (1..16))
> Access
> Read-write
> Object
> starSessSub1IpAddr
> Object ID
> enterprises.8164.1.34.4
> Description
> The remote IP address for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.
> Syntax
> IpAddress
> Access
> Read-write
> Object
> starSessSub1LastResult
> Object ID
> enterprises.8164.1.34.5
> Description
> The result of the last search. A value of unknown(0) means that the query wasn't created properly, or that no query has been performed; error(1) indicates an internal error performing the query, this is an abnormal condition that shouldn't normally be seen; nomatch(2) means that the query did not find a matching subscriber; onematch(3) means that the query found exactly one subscriber; multimatch(4) means that more than one subscriber matched; the information for one (random) subscriber was fetched
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> error(1)
> nomatch(2)
> onematch(3)
> multimatch(4)
> Object
> starSessSub1ServiceName
> Object ID
> enterprises.8164.1.34.6
> Description
> The service name of the subscriber.
> Syntax
> OCTET STRING (SIZE (1..63))
> Access
> Read-only
> Object
> starSessSub1HAIpAddr
> Object ID
> enterprises.8164.1.34.7
> Description
> The HA IP address for FA MIP connections
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1PeerIpAddr
> Object ID
> enterprises.8164.1.34.8
> Description
> The remote IP address of the peer. The type of peer depends on the session type.
> Syntax
> IpAddress
> Access
> Read-only

> Session Type | Peer
> PDSN | PCF
> GGSN | SGSN
> HA Mobile IP/HA IPSEC | FA
> LAC | LNS
> LNS | LAC

> ‌
> Object
> starSessSub1InPackets
> Object ID
> enterprises.8164.1.34.9
> Description
> The number of incoming packets for the subscriber
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1InPacketsDropped
> Object ID
> enterprises.8164.1.34.10
> Description
> The number of incoming packets dropped for the subscriber
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1InBytes
> Object ID
> enterprises.8164.1.34.11
> Description
> The count of incoming bytes for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes
> Syntax
> Counter32
> Units
> KB
> Access
> Read-only
> Object
> starSessSub1OutPackets
> Object ID
> enterprises.8164.1.34.12
> Description
> The number of out going packets for the subscriber
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1OutPacketsDropped
> Object ID
> enterprises.8164.1.34.13
> Description
> The number of out going packets dropped for the subscriber
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1OutBytes
> Object ID
> enterprises.8164.1.34.14
> Description
> The count of outgoing bytes for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes
> Syntax
> Counter32
> Units
> KB
> Access
> Read-only
> Object
> starSessSub1Activity
> Object ID
> enterprises.8164.1.34.15
> Description
> TBD
> Syntax
> Gauge32
> Units
> %
> Access
> Read-only
> Object
> starSessSub1State
> Object ID
> enterprises.8164.1.34.16
> Description
> The state of the subscriber
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> Unknown(0)
> Connecting(1)
> Connected(2)
> Disconnecting(3)
> Object
> starSessSub1CallID
> Object ID
> enterprises.8164.1.34.17
> Description
> The internal call ID of the subscriber
> Syntax
> Integer32
> Access
> Read-only
> Object
> starSessSub1ConnectTime
> Object ID
> enterprises.8164.1.34.18
> Description
> The connect time for the subscriber, in UTC. The UNIX epoch (Jan. 1, 1970) is used if no value is available
> Syntax
> DateAndTime
> Access
> Read-only
> Object
> starSessSub1CallDuration
> Object ID
> enterprises.8164.1.34.19
> Description
> The duration of the call, in seconds
> Syntax
> Counter32
> Units
> Seconds
> Access
> Read-only
> Object
> starSessSub1TimeIdle
> Object ID
> enterprises.8164.1.34.20
> Description
> The idle time of the call, in seconds
> Syntax
> Gauge32
> Units
> Seconds
> Access
> Read-only
> Object
> starSessSub1AccessType
> Object ID
> enterprises.8164.1.34.21
> Description
> The access type for the subscriber.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> pdsnsimpleip(1)
> pdsnmobileip(2)
> hamobileip(3)
> ggsnpdptypeipv4(4)
> ggsnpdptypeppp(5)
> ggsnpdptypeipv6(6)
> lnsl2tp(7)
> haipsec(8)
> ipsg(9)
> pdsnsipmip(10)
> mipproxyfa(11)
> imsa(12)
> bcmcs(13)
> ggsnmip(14)
> ipprobe(15)
> ansgw(16)
> Object
> starSessSub1AccessTech
> Object ID
> enterprises.8164.1.34.22
> Description
> The access technology for the subscriber.
> Syntax
> INTEGER
> Access
> Read-only
> Sequence
> unknown(0)
> cdma1xrtt(1)
> cdmaevdo(2)
> cdmaother(3)
> wcdmautran(4)
> gprsgeran(5)
> gprsother(6)
> wirelesslan(7)
> ipsg(8)
> wimax(9)
> sip(10)
> other(11)
> cdmaevdoreva(12)
> pdif(13)
> phs(14)
> ehrpd(15)
> eutran(16)
> gan(17)
> hspa(18)
> Object
> starSessSub1LinkStatus
> Object ID
> enterprises.8164.1.34.23
> Description
> The link status for the subscriber.
> Syntax
> INTEGER
> Enumeration
> Read-only
> Sequence
> unknown(0)
> active(1)
> dormant(2)
> Object
> starSessSub1NetworkType
> Object ID
> enterprises.8164.1.34.24
> Description
> The network type for the subscriber.
> Syntax
> INTEGER
> Access
> Read-only
> Sequence
> unknown(0)
> ip(1)
> mobileip(2)
> l2tp(3)
> proxymobileip(4)
> ipinip(5)
> gre(6)
> ipv6inipv4(7)
> Object
> starSessSub1CarrierID
> Object ID
> enterprises.8164.1.34.25
> Description
> Carrier ID
> Syntax
> OCTET STRING (SIZE (0..6))
> Access
> Read-only
> Object
> starSessSub1ESN
> Object ID
> enterprises.8164.1.34.26
> Description
> Electronic Serial Number
> Syntax
> OCTET STRING (SIZE (0..15))
> Access
> Read-only
> Object
> starSessSub1GMTTimezoneOffset
> Object ID
> enterprises.8164.1.34.27
> Description
> Timezone offset from GMT, in seconds. This is a signed value
> Syntax
> Integer32
> Units
> Seconds
> Access
> Read-only
> Object
> starSessSub1SessMgr
> Object ID
> enterprises.8164.1.34.28
> Description
> The instance number of the session manager for this subscriber.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starSessSub1RemoteIPAddr
> Object ID
> enterprises.8164.1.34.29
> Description
> Remote IP Address
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1Card
> Object ID
> enterprises.8164.1.34.30
> Description
> The card holding the session manager for this session. Use in combination with starSessSub1CPU.
> Syntax
> Integer32(1..16)
> Access
> Read-only
> Object
> starSessSub1CPU
> Object ID
> enterprises.8164.1.34.31
> Description
> The CPU holding the session manager for this session. Use in combination with starSessSub1Card
> Syntax
> Integer32(0..3)
> Access
> Read-only
> Object
> starSessSub1TimeIdleLeft
> Object ID
> enterprises.8164.1.34.32
> Description
> The remaining idle time of the call, in seconds. A value of 0xffffffff is used if the call does not have an idle timeout
> Syntax
> Gauge32
> Units
> Seconds
> Access
> Read-only
> Object
> starSessSub1TimeLeft
> Object ID
> enterprises.8164.1.34.33
> Description
> The remaining session time of the call, in seconds. A value of 0xffffffff is used if the call does not have a session timeout
> Syntax
> Gauge32
> Units
> Seconds
> Access
> Read-only
> Object
> starSessSub1TimeLongDurLeft
> Object ID
> enterprises.8164.1.34.34
> Description
> The remaining long duration time of the call, in seconds. A value of 0xffffffff is used if the call does not have a long duration timer
> Syntax
> Gauge32
> Units
> Seconds
> Access
> Read-only
> Object
> starSessSub1LongDurAction
> Object ID
> enterprises.8164.1.34.35
> Description
> The action to take when the long duration timer is reached
> Syntax
> StarLongDurTimeoutAction
> Access
> Read-only
> Object
> starSessSub1AlwaysOn
> Object ID
> enterprises.8164.1.34.36
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> enabled(1)
> disabled(2)
> Object
> starSessSub1IPPoolName
> Object ID
> enterprises.8164.1.34.37
> Syntax
> OCTET STRING (SIZE(0..31))
> Access
> Read-only
> Object
> starSessSub1VLANID
> Object ID
> enterprises.8164.1.34.38
> Description
> 0 is returned if this is not applicable
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starSessSub1LNSIPAddr
> Object ID
> enterprises.8164.1.34.39
> Description
> Only valid if starSessSub1NetworkType is l2tp(3), otherwise 0.0.0.0
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1ProxyMIP
> Object ID
> enterprises.8164.1.34.40
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> enabled(1)
> disabled(2)
> Object
> starSessSub1GGSNMIP
> Object ID
> enterprises.8164.1.34.41
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> enabled(1)
> disabled(2)
> Object
> starSessSub1HomeAgentIpAddr
> Object ID
> enterprises.8164.1.34.42
> Description
> The IP address of the Home Agent. This value is applicable only if one of the following is true:

> • | The value of starSessSub1AccessType is pdsnmobileip(2)

> • | The value of starSessSub1ProxyMIP is enabled(1)

> • | The value of starSessSub1GGSNMIP is enabled(1)

> If not applicable, a value of 0.0.0.0 will be returned
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1LocalIPAddr
> Object ID
> enterprises.8164.1.34.43
> Description
> The Local IP address of the Home Agent. This value is applicable only if one of the following is true:

> • | The value of starSessSub1AccessType is pdsnsimpleip(1)

> • | The value of starSessSub1AccessType is ggsnpdptypeppp(5)

> • | The value of starSessSub1AccessType is lnsl2tp(7)

> If not applicable, a value of 0.0.0.0 will be returned
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1FAServiceName
> Object ID
> enterprises.8164.1.34.44
> Description
> The FA service name for the subscriber. This value is applicable only if one of the following is true:

> • | The value of starSessSub1AccessType is pdsnmobileip(2)

> • | The value of starSessSub1ProxyMIP is enabled(1)

> • | The value of starSessSub1GGSNMIP is enabled(1)

> Syntax
> OCTET STRING (SIZE (1..63))
> Access
> Read-only
> Object
> starSessSub1FAVPNName
> Object ID
> enterprises.8164.1.34.45
> Description
> The FA VPN (Context) name. This value is applicable only if one of the following is true:

> • | The value of starSessSub1AccessType is pdsnmobileip(2)

> • | The value of starSessSub1ProxyMIP is enabled(1)

> • | The value of starSessSub1GGSNMIP is enabled(1)

> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessSub1SourceVPN
> Object ID
> enterprises.8164.1.34.46
> Description
> The Source VPN (Context) name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessSub1DestVPN
> Object ID
> enterprises.8164.1.34.47
> Description
> The Destination VPN (Context) name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessSub1AAAVPN
> Object ID
> enterprises.8164.1.34.48
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessSub1AAADomain
> Object ID
> enterprises.8164.1.34.49
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessSub1AAAStart
> Object ID
> enterprises.8164.1.34.50
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1AAAStop
> Object ID
> enterprises.8164.1.34.51
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1AAAInterim
> Object ID
> enterprises.8164.1.34.52
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1AcctSessionID
> Object ID
> enterprises.8164.1.34.53
> Syntax
> OCTET STRING (SIZE(0..23))
> Access
> Read-only
> Object
> starSessSub1AAARadiusGroup
> Object ID
> enterprises.8164.1.34.54
> Syntax
> OCTET STRING (SIZE(0..63))
> Access
> Read-only
> Object
> starSessSub1AAARadiusAuthServerIPAddr
> Object ID
> enterprises.8164.1.34.55
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1AAARadiusAcctServerIPAddr
> Object ID
> enterprises.8164.1.34.56
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1NASIPAddr
> Object ID
> enterprises.8164.1.34.57
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1NexthopIPAddr
> Object ID
> enterprises.8164.1.34.58
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1ActiveInACL
> Object ID
> enterprises.8164.1.34.59
> Syntax
> OCTET STRING (SIZE(0..79))
> Access
> Read-only
> Object
> starSessSub1ActiveOutACL
> Object ID
> enterprises.8164.1.34.60
> Syntax
> OCTET STRING (SIZE(0..79))
> Access
> Read-only
> Object
> starSessSub1ECSRulebase
> Object ID
> enterprises.8164.1.34.61
> Syntax
> OCTET STRING (SIZE(0..63))
> Access
> Read-only
> Object
> starSessSub1InPlcyGrp
> Object ID
> enterprises.8164.1.34.62
> Syntax
> OCTET STRING (SIZE(0..15))
> Access
> Read-only
> Object
> starSessSub1OutPlcyGrp
> Object ID
> enterprises.8164.1.34.63
> Syntax
> OCTET STRING (SIZE(0..15))
> Access
> Read-only
> Object
> starSessSub1DownTrafPolState
> Object ID
> enterprises.8164.1.34.64
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> enabled(1)
> disabled(2)
> Object
> starSessSub1DownCommDataRate
> Object ID
> enterprises.8164.1.34.65
> Description
> Downlink committed data rate, in bps. This value is only valid if starSessSub1DownTrafPolState is enabled(1)
> Syntax
> Unsigned32
> Units
> bps
> Access
> Read-only
> Object
> starSessSub1DownPeakDataRate
> Object ID
> enterprises.8164.1.34.66
> Description
> Downlink peak data rate, in bps. This value will be 0 if the value of starSessSub1DownTrafPolState is anything other than enabled(1)
> Syntax
> Unsigned32
> Units
> bps
> Access
> Read-only
> Object
> starSessSub1DownBurstSize
> Object ID
> enterprises.8164.1.34.67
> Description
> Downlink burst size, in bytes. This value will be 0 if the value of starSessSub1DownTrafPolState is anything other than enabled(1)
> Syntax
> Unsigned32
> Units
> bytes
> Access
> Read-only
> Object
> starSessSub1DownExceedAction
> Object ID
> enterprises.8164.1.34.68
> Description
> Downlink Exceed Action. This value will be notapplicable(1) if the value of starSessSub1DownTrafPolState is anything other than enabled(1)
> Syntax
> StarQOSTPAction
> Access
> Read-only
> Object
> starSessSub1DownViolateAction
> Object ID
> enterprises.8164.1.34.69
> Description
> Downlink Violate Action. This value will be notapplicable(1) if the value of starSessSub1DownTrafPolState is anything other than enabled(1)
> Syntax
> StarQOSTPAction
> Access
> Read-only
> Object
> starSessSub1DownExceed
> Object ID
> enterprises.8164.1.34.70
> Description
> Downlink packets exceeded bandwidth parameters
> Syntax
> Counter32
> Units
> packets
> Access
> Read-only
> Object
> starSessSub1DownViolate
> Object ID
> enterprises.8164.1.34.71
> Description
> Downlink packets violated bandwidth parameters
> Syntax
> Counter32
> Units
> packets
> Access
> Read-only
> Object
> starSessSub1UpTrafPolState
> Object ID
> enterprises.8164.1.34.72
> Description
> Uplink traffic policing state
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unknown(0)
> enabled(1)
> disabled(2)
> Object
> starSessSub1UpCommDataRate
> Object ID
> enterprises.8164.1.34.73
> Description
> Uplink committed data rate, in bps. This value is only valid if starSessSub1UpTrafPolState is enabled(1)
> Syntax
> Unsigned32
> Units
> bps
> Access
> Read-only
> Object
> starSessSub1UpPeakDataRate
> Object ID
> enterprises.8164.1.34.74
> Description
> Uplink peak data rate, in bps. This value will be 0 if the value of starSessSub1UpTrafPolState is anything other than enabled(1)
> Syntax
> Unsigned32
> Units
> bps
> Access
> Read-only
> Object
> starSessSub1UpBurstSize
> Object ID
> enterprises.8164.1.34.75
> Description
> Uplink burst size, in bytes. This value will be 0 if the value of starSessSub1UpTrafPolState is anything other than enabled(1
> Syntax
> Unsigned32
> Units
> bytes
> Access
> Read-only
> Object
> starSessSub1UpExceedAction
> Object ID
> enterprises.8164.1.34.76
> Description
> Uplink Exceed Action. This value will be notapplicable(1) if the value of starSessSub1UpTrafPolState is anything other than enabled(1)
> Syntax
> StarQOSTPAction
> Access
> Read-only
> Object
> starSessSub1UpViolateAction
> Object ID
> enterprises.8164.1.34.77
> Description
> Uplink Violate Action. This value will be notapplicable(1) if the value of starSessSub1UpTrafPolState is anything other than enabled(1)
> Syntax
> StarQOSTPAction
> Access
> Read-only
> Object
> starSessSub1UpExceed
> Object ID
> enterprises.8164.1.34.78
> Description
> Uplink packets exceeded bandwidth parameters
> Syntax
> Counter32
> Units
> packets
> Access
> Read-only
> Object
> starSessSub1UpViolate
> Object ID
> enterprises.8164.1.34.79
> Description
> Uplink packets violated bandwidth parameters
> Syntax
> Counter32
> Units
> packets
> Access
> Read-only
> Object
> starSessSub1L3TunnelingState
> Object ID
> enterprises.8164.1.34.80
> Description
> Identifies if L3 tunneling is enabled. This value should be enabled(1) if starSessSub1NetworkType is ipinip(5) or gre(6).
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1L3TunLocalIPAddr
> Object ID
> enterprises.8164.1.34.81
> Description
> L3 tunnel local address. This value is valid only if starSessSub1L3TunnelState is enabled(1), other it will be 0.0.0.0.
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1L3TunRemoteIPAddr
> Object ID
> enterprises.8164.1.34.82
> Description
> L3 tunnel remote address. This value is valid only if starSessSub1L3TunnelState is enabled(1), other it will be 0.0.0.0
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1AddrViaDHCP
> Object ID
> enterprises.8164.1.34.83
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1DHCPServName
> Object ID
> enterprises.8164.1.34.84
> Description
> DHCP service name. This value is only valid if starSessSub1DHCPAddrViaDHCP is enabled(1)
> Syntax
> Octet string
> Access
> Read-only
> Object
> starSessSub1DHCPServIPAddr
> Object ID
> enterprises.8164.1.34.85
> Description
> DHCP service IP address. This value is only valid if starSessSub1DHCPAddrViaDHCP is enabled(1), otherwise it will be 0.0.0.0
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1AccessLinkIPFrag
> Object ID
> enterprises.8164.1.34.86
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1IgnoreDFBit
> Object ID
> enterprises.8164.1.34.87
> Description
> Ignore DF-bit data-tunnel
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1MIPGratARPMode
> Object ID
> enterprises.8164.1.34.88
> Description
> This field is only applicable if starSessSub1AccessType is hamobileip(3) or haipsec(8)
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrProc
> Object ID
> enterprises.8164.1.34.89
> Description
> The state of external inline server processing
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrIngrIPAddr
> Object ID
> enterprises.8164.1.34.90
> Description
> The external inline server ingress IP address. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> IP Address
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrIngrVLANTag
> Object ID
> enterprises.8164.1.34.91
> Description
> The external inline server ingress VLAN tag. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrEgrIPAddr
> Object ID
> enterprises.8164.1.34.92
> Description
> The external inline server egress IP address. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrEgrVLANTag
> Object ID
> enterprises.8164.1.34.93
> Description
> The external inline server egress VLAN tag. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrVPNName
> Object ID
> enterprises.8164.1.34.94
> Description
> The external inline server context (VPN). This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSessSub1RadAcctMode
> Object ID
> enterprises.8164.1.34.95
> Description
> Radius Accounting Mode
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1InBytesDropped
> Object ID
> enterprises.8164.1.34.96
> Description
> The count of incoming bytes dropped for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1OutBytesDropped
> Object ID
> enterprises.8164.1.34.97
> Description
> The count of outgoing bytes dropped for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1PeakBPSTx
> Object ID
> enterprises.8164.1.34.98
> Description
> Peak rate from user, in bytes per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1PeakBPSRx
> Object ID
> enterprises.8164.1.34.99
> Description
> Peak rate to user, in bytes per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1AveBPSTx
> Object ID
> enterprises.8164.1.34.100
> Description
> Average rate from user, in bytes per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1AveBPSRx
> Object ID
> enterprises.8164.1.34.101
> Description
> Average rate to user, in bytes per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1SustBPSTx
> Object ID
> enterprises.8164.1.34.102
> Description
> Sustained rate from user, in bytes per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1SustBPSRx
> Object ID
> enterprises.8164.1.34.103
> Description
> Sustained rate to user, in bytes per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1PeakPPSTx
> Object ID
> enterprises.8164.1.34.104
> Description
> Peak rate from user, in packets per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1PeakPPSRx
> Object ID
> enterprises.8164.1.34.105
> Description
> Peak rate to user, in packets per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1AvePPSTx
> Object ID
> enterprises.8164.1.34.106
> Description
> Average rate from user, in packets per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1AvePPSRx
> Object ID
> enterprises.8164.1.34.107
> Description
> Average rate to user, in packets per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1SustPPSTx
> Object ID
> enterprises.8164.1.34.108
> Description
> Sustained rate from user, in packets per second.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1SustPPSRx
> Object ID
> enterprises.8164.1.34.109
> Description
> Sustained rate to user, in packets per second
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1ActivePct
> Object ID
> enterprises.8164.1.34.110
> Description
> Link online/active percentage.
> Syntax
> Integer32(0..100)
> Access
> Read-only
> Object
> starSessSub1IPv4BadHdr
> Object ID
> enterprises.8164.1.34.111
> Description
> IPv4 Bad Headers
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4TtlExceeded
> Object ID
> enterprises.8164.1.34.112
> Description
> IPv4 Total Exceeded
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4FragSent
> Object ID
> enterprises.8164.1.34.113
> Description
> IPv4 Fragments sent
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4FragFail
> Object ID
> enterprises.8164.1.34.114
> Description
> IPv4 Could Not Fragment errors
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4InACLDrop
> Object ID
> enterprises.8164.1.34.115
> Description
> IPv4 Input ACL Drops
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4OutACLDrop
> Object ID
> enterprises.8164.1.34.116
> Description
> IPv5 Output ACL Drops
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4InCSSDownDrop
> Object ID
> enterprises.8164.1.34.117
> Description
> IPv4 Input CSS Down Drops
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4OutCSSDownDrop
> Object ID
> enterprises.8164.1.34.118
> Description
> IPv4 Output CSS Down Drops
> Syntax
> Counter-32
> Access
> Read-only
> Object
> starSessSub1IPv4OutXOFFDropPkt
> Object ID
> enterprises.8164.1.34.119
> Description
> IPv4 Output XOFF Packets Drop
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4OutXOFFDropByte
> Object ID
> enterprises.8164.1.34.120
> Description
> IPv4 Output XOFF Bytes Drop
> Syntax
> Counter-32
> Access
> Read-only
> Object
> starSessSub1IPv4SrcViol
> Object ID
> enterprises.8164.1.34.121
> Description
> IPv4 Source Violations
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4ProxyDNSRedir
> Object ID
> enterprises.8164.1.34.122
> Description
> IPv4 Proxy-DNS Redirect
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4SrcProxyDNSPThru
> Object ID
> enterprises.8164.1.34.123
> Description
> IPv4 Proxy-DNS Pass-Thru
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4ProxyDNSDrop
> Object ID
> enterprises.8164.1.34.124
> Description
> IPv4 Proxy-DNS Drop
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4SrcViolNoAcct
> Object ID
> enterprises.8164.1.34.125
> Description
> IPv4 Source Violations No Account
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4SrcViolIgnored
> Object ID
> enterprises.8164.1.34.126
> Description
> IPv4 Source Violations Ignored
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrTxPkt
> Object ID
> enterprises.8164.1.34.127
> Description
> Packets transmitted to inline server. This value is valid only if the value of starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1ExtInlSrvrRxPkt
> Object ID
> enterprises.8164.1.34.128
> Description
> Packets received from inline server. This value is valid only if the value of starSessSub1ExtInlSrvrProc is enabled(1)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPv4ICMPDropPkt
> Object ID
> enterprises.8164.1.34.129
> Description
> IPv4 ICMP Packets dropped
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1TunnelType
> Object ID
> enterprises.8164.1.34.130
> Description
> Tunnel Type
> Syntax
> Integer
> Access
> Read-only
> Object
> starSessSub1IPSECTunDownDropPkt
> Object ID
> enterprises.8164.1.34.131
> Description
> Pool IPSEC tunnel down packets dropped. This value is only valid if the value of starSessSub1TunnelType is esp(6)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1IPSECFlowID
> Object ID
> enterprises.8164.1.34.132
> Description
> IP Pool IPSEC flow id. This value is only valid if the value of starSessSub1TunnelType is esp(6)
> Syntax
> Integer32
> Access
> Read-only
> Object
> starSessSub1DormancyTotal
> Object ID
> enterprises.8164.1.34.133
> Description
> Dormancy total. This value is not valid if the value of starSessSub1AccessType is ggsnpdptypeipv4(4) or ggsnpdptypeppp(5)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1HandoffTotal
> Object ID
> enterprises.8164.1.34.134
> Description
> Handoff total. This value is not valid if the value of starSessSub1AccessType is ggsnpdptypeipv4(4) or ggsnpdptypeppp(5)
> Syntax
> Counter32
> Access
> Read-only
> Object
> starSessSub1AccessFlows
> Object ID
> enterprises.8164.1.34.135
> Description
> Access flows
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1TFT
> Object ID
> enterprises.8164.1.34.136
> Description
> Number of TFTs
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSub1NASPort
> Object ID
> enterprises.8164.1.34.137
> Description
> NAS port
> Syntax
> Integer32
> Access
> Read-only
> Object
> starSessSub1CorrID
> Object ID
> enterprises.8164.1.34.139
> Description
> ThreeGPP2-correlation-id (C2)
> Syntax
> Octet String
> Access
> Read-only
> Object
> starSessSub1L2TPPeerIPAddr
> Object ID
> enterprises.8164.1.34.140
> Description
> L2TP Peer address. This value is only valid if the value of starSessSub1NetworkType is l2tp(3)
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSessSub1IPv4EarlyPDURecv
> Object ID
> enterprises.8164.1.34.141
> Description
> IPv4 early PDU received
> Syntax
> Counter32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentNwReachServer(35)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starNwReachTable
> Object ID
> enterprises.8164.1.35.1
> Description
> A table containing Network Reachable Server information
> Syntax
> SEQUENCE OF StarNwReachEntry
> Access
> Not-accessible
> Object
> starNwReachEntry
> Object ID
> enterprises.8164.1.35.1.1
> Description
> Information for a specific Ntw Reachable Server
> Syntax
> StarNwReachEntry
> Access
> Not-accessible
> Sequence
> starNwReachName
> starNwReachSrvrAddr
> Object
> starNwReachName
> Object ID
> enterprises.8164.1.35.1.1.1
> Description
> The Name for this Network Reachable Server
> Syntax
> OCTET STRING (SIZE (1..16))
> Access
> Not-accessible
> Object
> starNwReachSrvrAddr
> Object ID
> enterprises.8164.1.35.1.1.2
> Description
> The IP Address for the Network Reachable Server
> Syntax
> IpAddress
> Access
> Not-accessible
> starentMIB(8164).starentMIBObjects(1).starentIPSEC(36)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starIPSECContextName
> Object ID
> enterprises.8164.1.36.1
> Description
> The name of a context
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starIPSECGroupName
> Object ID
> enterprises.8164.1.36.2
> Description
> The name of a crypto map
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starIPSECTunLocalIPAddr
> Object ID
> enterprises.8164.1.36.3
> Description
> The local IP Address for an IPSEC tunnel
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starIPSECTunRemoteIPAddr
> Object ID
> enterprises.8164.1.36.4
> Description
> The local IP Address for an IPSEC tunnel
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starIPSECPolicyName
> Object ID
> enterprises.8164.1.36.5
> Description
> An IPSEC policy name
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starIPSECDynPolicyType
> Object ID
> enterprises.8164.1.36.6
> Description
> An IPSEC dynamic policy type. Note that the value test(5) is used only for internal testing
> Syntax
> Integer
> Access
> Accessible-for-notify
> Enumeration
> unknown(0)
> manual(1)
> isakmp(2)
> subscribertemplate(3)
> subscribertunnel(4)
> test(5)
> dynamic(6)
> Object
> starIPSECDynPolicyPayloadType
> Object ID
> enterprises.8164.1.36.7
> Description
> An IPSEC dynamic policy payload type
> Syntax
> Integer
> Access
> Accessible-for-notify
> Object
> starIPSECLocalGateway
> Object ID
> enterprises.8164.1.36.8
> Description
> IP address of IPSec local gateway
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> Object
> starIPSECRemoteGateway
> Object ID
> enterprises.8164.1.36.9
> Description
> IP address of IPSec remote gateway
> Syntax
> IpAddress
> Access
> Accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starentSIPRoute(37)
> Object
> starSIPRouteTable
> Object ID
> enterprises.8164.1.37.1
> Description
> A table containing SIPRoute related information
> Syntax
> SEQUENCE OF StarSIPRouteEntry
> Access
> Not-accessible
> Object
> starSIPRouteEntry
> Object ID
> enterprises.8164.1.37.1.1
> Description
> The statistics for a specific SIPRoute service
> Syntax
> StarSIPRouteEntry
> Access
> Not-accessible
> Sequence
> starSIPRouteVpnID Index
> starSIPRouteVpnName Index
> starSIPRouteVmgName
> starSIPRouteAsName
> starSIPRouteDestPartyNum
> starSIPRouteReqNum
> Object
> starSIPRouteVpnID
> Object ID
> enterprises.8164.1.37.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starSIPRouteVpnName
> Object ID
> enterprises.8164.1.37.1.1.2
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteVmgName
> Object ID
> enterprises.8164.1.37.1.1.3
> Description
> The name of this VMG (context)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteAsName
> Object ID
> enterprises.8164.1.37.1.1.4
> Description
> The name of this AS (context)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteDestPartyNum
> Object ID
> enterprises.8164.1.37.1.1.5
> Description
> The dest. party number
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteReqNum
> Object ID
> enterprises.8164.1.37.1.1.6
> Description
> The request number
> Syntax
> DisplayString
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentRPServiceOption(38)
> Object
> starRPServiceOptionTable
> Object ID
> enterprises.8164.1.38.1
> Syntax
> SEQUENCE OF StarRPServiceOptionEntry
> Access
> Not-accessible
> Object
> starRPServiceOptionEntry
> Object ID
> enterprises.8164.1.38.1.1
> Syntax
> StarRPServiceOptionEntry
> Access
> Not-accessible
> Sequence
> starRPServiceOptionNum
> starRPServiceOptionCalls
> Object
> starRPServiceOptionNum
> Object ID
> enterprises.8164.1.38.1.1.1
> Syntax
> Integer32(1..255)
> Access
> Not-accessible
> Object
> starRPServiceOptionCalls
> Object ID
> enterprises.8164.1.38.1.1.2
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentPCFStats(39)
> Object
> starPCFStatTable
> Object ID
> enterprises.8164.1.39.1
> Description
> A table containing per-PCF statistics.
> Syntax
> SEQUENCE OF StarPCFStatEntry
> Access
> Not-accessible
> Object
> starPCFStatEntry
> Object ID
> enterprises.8164.1.39.1.1
> Description
> The statistics for a specific PCF.
> Syntax
> StarPCFStatsEntry
> Access
> Not-accessible
> Sequence
> starPCFStatVpnID Index
> starPCFStatIpAddr
> starPCFStatVpnName
> starPCFStatRxPkts
> starPCFStatTxPkts
> starPCFStatRxBytes
> starPCFStatTxBytes
> starPCFStatTotalSessions
> starPCFStatCurrentSessions
> starPCFStatCurrentActiveSessions
> starPCFStatCurrentDormantSessions
> starPCFStatCurrentSIPConnected
> starPCFStatCurrentMIPConnected
> starPCFStatCurrentPMIPConnected
> starPCFStatCurrentL2TPLACConnected
> starPCFStatCurrentOtherConnected
> Object
> starPCFStatVpnID
> Object ID
> enterprises.8164.1.39.1.1.1
> Description
> The internal identification of the VPN (context).
> Syntax
> Guage32
> Access
> Not-accessible
> Object
> starPCFStatIpAddr
> Object ID
> enterprises.8164.1.39.1.1.2
> Description
> The IP address of the specific PCF.
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starPCFStatVpnName
> Object ID
> enterprises.8164.1.39.1.1.3
> Description
> The name of the VPN (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPCFStatRxPkts
> Object ID
> enterprises.8164.1.39.1.1.4
> Description
> Total packets received.
> Syntax
> Counter32
> Units
> Millions
> Access
> Read-only
> Object
> starPCFStatTxPkts
> Object ID
> enterprises.8164.1.39.1.1.5
> Description
> total packets transferred.
> Syntax
> Counter32
> Units
> Millions
> Access
> Read-only
> Object
> starPCFStatRxBytes
> Object ID
> enterprises.8164.1.39.1.1.6
> Description
> Total bytes received.
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starPCFStatTxBytes
> Object ID
> enterprises.8164.1.39.1.1.7
> Description
> Total bytes send.
> Syntax
> Counter32
> Units
> Megabytes
> Access
> Read-only
> Object
> starPCFStatTotalSessions
> Object ID
> enterprises.8164.1.39.1.1.8
> Description
> Total number of sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFStatCurrentSessions
> Object ID
> enterprises.8164.1.39.1.1.9
> Description
> Total current sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentActiveSessions
> Object ID
> enterprises.8164.1.39.1.1.10
> Description
> Total number of current active sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentDormantSessions
> Object ID
> enterprises.8164.1.39.1.1.11
> Description
> Total Numbers of current dormant sessions.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentSIPConnected
> Object ID
> enterprises.8164.1.39.1.1.12
> Description
> Total number of Simple IP sessions connected.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentMIPConnected
> Object ID
> enterprises.8164.1.39.1.1.13
> Description
> Total number of Mobile IP sessions connected.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentPMIPConnected
> Object ID
> enterprises.8164.1.39.1.1.14
> Description
> Total number of Proxy Mobile IP sessions connected.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentL2TPLACConnected
> Object ID
> enterprises.8164.1.39.1.1.15
> Description
> Total number of current L2TP LAC connected.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFStatCurrentOtherConnected
> Object ID
> enterprises.8164.1.39.1.1.16
> Description
> Total number of other connections.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFTable
> Object ID
> enterprises.8164.1.39.2
> Description
> A table of per service PCF statistics
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFEntry
> Object ID
> enterprises.8164.1.39.2.1
> Description
> The statistics for a specific PCF per service
> Syntax
> StarPCFEntry
> Access
> not-accessible
> Object
> starPCFSvcID
> Object ID
> enterprises.8164.1.39.2.1.1
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:)
> Syntax
> StarShortID
> Access
> Read-only
> Object
> starPCFIpAddr
> Object ID
> enterprises.8164.1.39.2.1.2
> Description
> The PCF IP address
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starPCFVpnID
> Object ID
> enterprises.8164.1.39.2.1.3
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPCFVpnName
> Object ID
> enterprises.8164.1.39.2.1.4
> Description
> The VPN (context) name
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPCFServName
> Object ID
> enterprises.8164.1.39.2.1.5
> Description
> The name of this service.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPCFRrqRcvd
> Object ID
> enterprises.8164.1.39.2.1.6
> Description
> Number of rrq received.
> Syntax
> StarShortID
> Access
> Read-only
> Object
> starPCFRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.7
> Description
> Number of rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRrqDenied
> Object ID
> enterprises.8164.1.39.2.1.8
> Description
> Number of rrq denied
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRrqDiscarded
> Object ID
> enterprises.8164.1.39.2.1.9
> Description
> Number of rrq discarded.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFInitialRrqRcvd
> Object ID
> enterprises.8164.1.39.2.1.10
> Description
> Initial rrq received.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFInitialRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.11
> Description
> Initial rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFIntraPDSNActiveHORrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.12
> Description
> Intra PDSN active handoff rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFIntraPDSNDormantHORrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.13
> Description
> Intra PDSN dormant handoff rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFInterPDSNHORrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.14
> Description
> Inter PDSN handoff rrq accpted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFInitialRrqDenied
> Object ID
> enterprises.8164.1.39.2.1.15
> Description
> Intial rrq denied.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFInitialRrqDiscarded
> Object ID
> enterprises.8164.1.39.2.1.16
> Description
> Intial rrq discarded.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRenewRrqRcvd
> Object ID
> enterprises.8164.1.39.2.1.17
> Description
> Renew rrq received.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRenewRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.18
> Description
> Renew rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRenewActiveRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.19
> Description
> Renew active rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRenewDormantRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.20
> Description
> Renew dormant rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRenewRrqDenied
> Object ID
> enterprises.8164.1.39.2.1.21
> Description
> Renew rrq denied.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRenewRrqDiscarded
> Object ID
> enterprises.8164.1.39.2.1.22
> Description
> Renew rrq discarded.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeregRrqRcvd
> Object ID
> enterprises.8164.1.39.2.1.23
> Description
> Deregistration rrq received.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeregRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.24
> Description
> Deregistration rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeregDormantRrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.25
> Description
> Deregistration dormant rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeregRrqDenied
> Object ID
> enterprises.8164.1.39.2.1.26
> Description
> Deregistration rrq denied.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeregRrqDiscarded
> Object ID
> enterprises.8164.1.39.2.1.27
> Description
> Deregistration rrq discarded.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFIntraPDSNActiveAnidHORrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.28
> Description
> Intra PDSN active anid handoff rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFIntraPDSNDormantAnidHORrqAccepted
> Object ID
> enterprises.8164.1.39.2.1.29
> Description
> Intra PDSN dormant anidhandoff rrq accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedUnSpeReason
> Object ID
> enterprises.8164.1.39.2.1.30
> Description
> Denied unspecified reason.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedAdmProh
> Object ID
> enterprises.8164.1.39.2.1.31
> Description
> Denied admin prohibited.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedAdmProh
> Object ID
> enterprises.8164.1.39.2.1.32
> Description
> Denied insufficient resources.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedMobNodeAuthFail
> Object ID
> enterprises.8164.1.39.2.1.33
> Description
> Denied mobile node authentication failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedIdentMismatch
> Object ID
> enterprises.8164.1.39.2.1.34
> Description
> Denied identification mismatch.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedPoorFormedReq
> Object ID
> enterprises.8164.1.39.2.1.35
> Description
> Denied poor formed request.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedUnknownPDSNAddr
> Object ID
> enterprises.8164.1.39.2.1.36
> Description
> Denied unknown PDSN address.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedRevTunnelUnavail
> Object ID
> enterprises.8164.1.39.2.1.37
> Description
> Denied rev tunnel unavilable.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedRevTunnelRequire
> Object ID
> enterprises.8164.1.39.2.1.38
> Description
> Denied rev tunnel required.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedUnrecogVendorId
> Object ID
> enterprises.8164.1.39.2.1.39
> Description
> Denied unrecognized vendor id.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedSessionClosed
> Object ID
> enterprises.8164.1.39.2.1.40
> Description
> Denied session closed.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDeniedBsnSessionInfoUnavail
> Object ID
> enterprises.8164.1.39.2.1.41
> Description
> Denied bsn session information unavilable.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFegUpdTransmitted
> Object ID
> enterprises.8164.1.39.2.1.42
> Description
> Registration updates transmitted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRegUpdAccepted
> Object ID
> enterprises.8164.1.39.2.1.43
> Description
> Registration updates accepted.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRegUpdateRpLifetimeExpiry
> Object ID
> enterprises.8164.1.39.2.1.44
> Description
> Registration update rp life time expiry.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRegUpdateUpperLayerIntiated
> Object ID
> enterprises.8164.1.39.2.1.45
> Description
> Registration update upper layer intiated
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRegUpdateOtherReason
> Object ID
> enterprises.8164.1.39.2.1.46
> Description
> Registration update other reason.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRegUpdateHORelease
> Object ID
> enterprises.8164.1.39.2.1.47
> Description
> Registration update handoff release.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRegUpdateSessmgrDied
> Object ID
> enterprises.8164.1.39.2.1.48
> Description
> Registration update sessmgr denied.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFAuxA10ConnectionsSetup
> Object ID
> enterprises.8164.1.39.2.1.49
> Description
> Aux a10 connections setup.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFSessionsDenied
> Object ID
> enterprises.8164.1.39.2.1.50
> Description
> Number of sessions denied.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFSessionsInit
> Object ID
> enterprises.8164.1.39.2.1.51
> Description
> Number of sessions initiated.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFSessionsReneg
> Object ID
> enterprises.8164.1.39.2.1.52
> Description
> Number of PCF sessions renegotiated.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscLcpRemote
> Object ID
> enterprises.8164.1.39.2.1.53
> Description
> Disconnect reason lcp remote.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscRpRemote
> Object ID
> enterprises.8164.1.39.2.1.54
> Description
> Disconnect reason rp remote.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscRpLocal
> Object ID
> enterprises.8164.1.39.2.1.55
> Description
> Disconnect reason rp local.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscMaxIpcpRetr
> Object ID
> enterprises.8164.1.39.2.1.56
> Description
> Disconnect reason ppp maximum ipcp retries.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscMaxIpv6cpRetr
> Object ID
> enterprises.8164.1.39.2.1.57
> Description
> Disconnect reason max ipv6cp retries.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscMaxLcpRetr
> Object ID
> enterprises.8164.1.39.2.1.58
> Description
> Disconnect reason max lcp retries.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscAuthFail
> Object ID
> enterprises.8164.1.39.2.1.59
> Description
> Disconnect reason authentication failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscSessSetupTimeout
> Object ID
> enterprises.8164.1.39.2.1.60
> Description
> Disconnect reason session setup timeout.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscFlowAddFail
> Object ID
> enterprises.8164.1.39.2.1.61
> Description
> Disconnect reason flow add failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscInvDestContext
> Object ID
> enterprises.8164.1.39.2.1.62
> Description
> Disconnect reason invalid destination context.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscLcpOptFail
> Object ID
> enterprises.8164.1.39.2.1.63
> Description
> Disconnect reason lcp option failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscIpcpOptFail
> Object ID
> enterprises.8164.1.39.2.1.64
> Description
> Disconnect reason lcp option failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscIpv6cpOptFail
> Object ID
> enterprises.8164.1.39.2.1.65
> Description
> Disconnect reason ipv6cp option failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscNoRemIpAddr
> Object ID
> enterprises.8164.1.39.2.1.66
> Description
> Disconnect reason no ip remote ip address.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscDetectionFail
> Object ID
> enterprises.8164.1.39.2.1.67
> Description
> Disconnect reason detection failure.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFDiscMisc
> Object ID
> enterprises.8164.1.39.2.1.68
> Description
> Disconnect reason misallaneous.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFCurrentSessions
> Object ID
> enterprises.8164.1.39.2.1.69
> Description
> Current sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFSessionsSetup
> Object ID
> enterprises.8164.1.39.2.1.70
> Description
> Session setup.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFSessionsRelsese
> Object ID
> enterprises.8164.1.39.2.1.71
> Description
> Sessions release.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFCurrentRevaSessions
> Object ID
> enterprises.8164.1.39.2.1.72
> Description
> Current reva sessions.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRevaSessionsSetup
> Object ID
> enterprises.8164.1.39.2.1.73
> Description
> Reva session setup.
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPCFRevaSessionsRelsese
> Object ID
> enterprises.8164.1.39.2.1.74
> Description
> Reva session release
> Syntax
> Counter32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentSIPRouteServer(40)
> Object
> starSIPRouteServerTable
> Object ID
> enterprises.8164.1.40.1
> Description
> A table containing SIPRouteServer related information
> Syntax
> SEQUENCE OF StarSIPRouteServerEntry
> Access
> Not-accessible
> Object
> starSIPRouteServerEntry
> Object ID
> enterprises.8164.1.40.1.1
> Description
> The statistics for a specific SIPRouteServer.
> Syntax
> StarSIPRouteServerEntry
> Access
> Not-accessible
> Sequence
> starSIPRouteServerVpnID Index
> starSIPRouteServerVpnName
> starSIPRouteServerVmgName
> starSIPRouteServerAsName
> starSIPRouteServerIpAddr
> Object
> starSIPRouteServerVpnID
> Object ID
> enterprises.8164.1.40.1.1.1
> Description
> The internal identification of the VPN (context).
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starSIPRouteServerVpnName
> Object ID
> enterprises.8164.1.40.1.1.2
> Description
> The name of the VPN (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteServerVmgName
> Object ID
> enterprises.8164.1.40.1.1.3
> Description
> The name of the VMG (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteServerAsName
> Object ID
> enterprises.8164.1.40.1.1.4
> Description
> The name of the AS (context).
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSIPRouteServerIpAddr
> Object ID
> enterprises.8164.1.40.1.1.5
> Description
> The SIP Route Server IP address.
> Syntax
> IP Address in dotted decimal notation
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentVIMService(41)
> Object
> starVIMServiceTable
> Object ID
> enterprises.8164.1.41.1
> Description
> A table containing VIM's Service related information
> Syntax
> SEQUENCE OF StarVIMServiceEntry
> Access
> Not-accessible
> Object
> starVIMServiceEntry
> Object ID
> enterprises.8164.1.41.1.1
> Description
> The statistics for a specific VIM's Service
> Syntax
> StarVIMServiceEntry
> Access
> Not-accessible
> Sequence
> starVIMServiceVpnID
> starVIMServiceVpnName
> starVIMServiceInstanceId
> starVIMServiceFMDMaxCallRate
> starVIMServiceFMDContinuousLoadCount
> Object
> starVIMServiceVpnID
> Object ID
> enterprises.8164.1.41.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starVIMServiceVpnName
> Object ID
> enterprises.8164.1.41.1.1.2
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starVIMServiceInstanceId
> Object ID
> enterprises.8164.1.41.1.1.3
> Description
> The VIM Instance ID
> Syntax
> Unsigned32
> Access
> Not-accessible
> Object
> starVIMServiceFMDMaxCallRate
> Object ID
> enterprises.8164.1.41.1.1.4
> Description
> Configured FMD max call rate
> Syntax
> Unsigned32
> Units
> Calls per Minute
> Access
> Read-only
> Object
> starVIMServiceFMDContinuousLoadCount
> Object ID
> enterprises.8164.1.41.1.1.5
> Description
> Configured FMD continuous load count
> Syntax
> Unsigned32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentGSS(42)
> The GTPP Storage Server is an external entity, but the chassis reports notifications on its behalf. The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starGSSClusterName
> Object ID
> enterprises.8164.1.42.1
> Description
> The name of the Storage Server Cluster
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterNodeName
> Object ID
> enterprises.8164.1.42.2
> Description
> The name of a node within a Storage Server Cluster
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterRgName
> Object ID
> enterprises.8164.1.42.3
> Description
> The name of the Storage Server Cluster Resource Group
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterRsName
> Object ID
> enterprises.8164.1.42.4
> Description
> The name of the Storage Server Cluster Resource
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterNodeState
> Object ID
> enterprises.8164.1.42.5
> Description
> Status of the Storage Server Cluster node
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterPrevOnlineNode
> Object ID
> enterprises.8164.1.42.6
> Description
> Name of the previous node of the Storage Server Cluster which was online/active
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterFromNode
> Object ID
> enterprises.8164.1.42.7
> Description
> Information from Storage Server Cluster to node
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSClusterToNode
> Object ID
> enterprises.8164.1.42.8
> Description
> Information from node to Storage Server Cluster
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSDiskPath
> Object ID
> enterprises.8164.1.42.9
> Description
> Path information of Storage Server disk
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSTransportPath
> Object ID
> enterprises.8164.1.42.10
> Description
> Path information of Storage Server for data transportation
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSIPMPGroupName
> Object ID
> enterprises.8164.1.42.11
> Description
> Name of the IPMP group for GSS
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> Object
> starGSSInterfaceName
> Object ID
> enterprises.8164.1.42.12
> Description
> Name of the GSS interface
> Syntax
> DisplayString
> Access
> Accessible-for-notify
> starentMIB(8164).starentMIBObjects(1).starentPDIFSys(43)
> Object
> starPDIFSysStatus
> Object ID
> enterprises.8164.1.43.1
> Description
> The overall status of the chassis as a PDIF service. A value of noservice(1) means that the chassis is not configured/licensed for PDIF; active(2) indicates that at least one PDIF service is available for processing sessions; temporary(3) indicates that PDIF is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no PDIF service is currently active, but one or more PDIF services are configured
> Syntax
> INTEGER
> unknown(0)
> noservice(1)
> active(2)
> temporary(3)
> outofservice(4)
> Access
> Read-only
> Object
> starPDIFSysNumService
> Object ID
> enterprises.8164.1.43.2
> Description
> The number of PDIF services configured
> Syntax
> Unsigned32
> Units
> Services
> Access
> Read-only
> Object
> starPDIFSysSessCurrent
> Object ID
> enterprises.8164.1.43.3
> Description
> The number of current PDIF sessions for this chassis
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSysSessCurrActive
> Object ID
> enterprises.8164.1.43.4
> Description
> The number of currently active PDIF sessions for this chassis
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSysSessCurrDormant
> Object ID
> enterprises.8164.1.43.5
> Description
> The number of currently dormant PDIF sessions for this chassis
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSysSessTtlSetup
> Object ID
> enterprises.8164.1.43.6
> Description
> The cumulative total number of PDIF sessions that has been setup
> Syntax
> Counter32
> Access
> Read-only
> Object
> starPDIFSysChildSACurrent
> Object ID
> enterprises.8164.1.43.7
> Description
> Number of current PDIF child SAs for the chassis
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentPDIFService(44)
> Object
> starPDIFTable
> Object ID
> enterprises.8164.1.44.1
> Description
> A table of per-service PDIF information
> Syntax
> SEQUENCE OF StarPDIFEntry
> Access
> Not-accessible
> Object
> starPDIFEntry
> Object ID
> enterprises.8164.1.44.1.1
> Description
> The information for a PDIF service
> Syntax
> StarPDIFEntry
> Access
> Not-accessible
> Sequence
> starPDIFSvcID
> StarShortID
> starPDIFVpnID Gauge32
> starPDIFVpnName DisplayString
> starPDIFServName DisplayString
> starPDIFStatus INTEGER
> starPDIFSessCurrent Gauge32
> starPDIFSessRemain Gauge32
> starPDIFSessCurrentActive Gauge32
> starPDIFSessCurrentDormant Gauge32
> starPDIFSessCurrentIpv6Active Gauge32
> starPDIFSessCurrentIpv6Dormant Gauge32
> starPDIFSessCurrentIpv4Active Gauge32
> starPDIFSessCurrentIpv4Dormant Gauge32
> starPDIFBindIpAddress IpAddress
> starPDIFBindIpPort Integer32
> starPDIFBindSlot Integer32
> starPDIFBindPort Integer32
> Object
> starPDIFSvcID
> Object ID
> enterprises.8164.1.44.1.1.1
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).
> Syntax
> StarShortID
> Access
> Not-accessible
> Object
> starPDIFVpnID
> Object ID
> enterprises.8164.1.44.1.1.2
> Description
> The internal VPN (context) ID.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFVpnName
> Object ID
> enterprises.8164.1.44.1.1.3
> Description
> The VPN (context) name.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPDIFServName
> Object ID
> enterprises.8164.1.44.11.1.4
> Description
> The name of this service
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starPDIFStatus
> Object ID
> enterprises.8164.1.44.1.1.5
> Description
> The state of this PDIF service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.
> Syntax
> INTEGER
> unknown(0)
> inservice(1)
> outofservice(2)
> Access
> Read-only
> Object
> starPDIFSessCurrent
> Object ID
> enterprises.8164.1.44.1.1.6
> Description
> The number of current sessions for this PDIF service.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessRemain
> Object ID
> enterprises.8164.1.44.1.1.7
> Description
> A count of the remaining capacity for this PDIF service, in terms of sessions. If a session limit is configured for this PDIF service, starPDIFSessRemain will identify the difference between this limit and starPDIFSessCurrent. If no individual limit has been configured for this service, starPDIFSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starPDIFSessRemain cannot be summed across multiple services.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessCurrentActive
> Object ID
> enterprises.8164.1.44.1.1.8
> Description
> The number of currently active sessions for this PDIF service
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessCurrentDormant
> Object ID
> enterprises.8164.1.44.1.1.9
> Description
> The number of currently dormant sessions for this PDIF service
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessCurrentIpv6Active
> Object ID
> enterprises.8164.1.44.1.1.10
> Description
> The number of currently active IPv6 sessions for this PDIF service
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessCurrentIpv6Dormant
> Object ID
> enterprises.8164.1.44.1.1.11
> Description
> The number of currently dormant IPv6 sessions for this PDIF service.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessCurrentIpv4Active
> Object ID
> enterprises.8164.1.44.1.1.12
> Description
> The number of currently active IPv4 sessions for this PDIF service.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFSessCurrentIpv4Dormant
> Object ID
> enterprises.8164.1.44.1.1.13
> Description
> The number of currently dormant IPv4 sessions for this PDIF service.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starPDIFBindIpAddress
> Object ID
> enterprises.8164.1.44.1.1.14
> Description
> The bind IP address for this PDIF service
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starPDIFBindIpPort
> Object ID
> enterprises.8164.1.44.1.1.15
> Description
> The bind IP port for this PDIF service
> Syntax
> Integer32
> Access
> Read-only
> Object
> starPDIFBindSlot
> Object ID
> enterprises.8164.1.44.1.1.16
> Description
> The physical slot number for the physical port which holds the interface bound to the starPDIFBindIpAddress address.
> Syntax
> Integer32
> Access
> Read-only
> Object
> starPDIFBindPort
> Object ID
> enterprises.8164.1.44.1.1.17
> Description
> The physical port number for the physical port which holds the interface bound to the starPDIFBindIpAddress address.
> Syntax
> SYNTAX Integer32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentSGSNService(45)
> Object
> starSGSNSerTable
> Object ID
> enterprises.8164.1.45.1
> Description
> A table containing SGSN related information.
> Syntax
> SEQUENCE OF StarSGSNSerEntry
> Access
> Not-accessible
> Object
> starSGSNSerEntry
> Object ID
> enterprises.8164.1.45.1.1
> Description
> The statistics for a specific SGSN service.
> Syntax
> StarSGSNSerEntry
> Access
> Not-accessible
> Sequence
> starSGSNSerVpnID Gauge32
> starSGSNSerSvcID Gauge32
> starSessSGSNVpnName DisplayString
> starSessSGSNServName DisplayString
> starLinkM3UASs7rdId Gauge32
> starSS7Pc Gauge32
> starLinkM3UAPsId Gauge32
> Object
> starSGSNSerVpnID
> Object ID
> enterprises.8164.1.45.1.1.1
> Description
> The internal identification of the VPN (context).
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starSGSNSerSvcID
> Object ID
> enterprises.8164.1.45.1.1.2
> Description
> The internal identification of this service; unique within a specific context.
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starSessSGSNVpnName
> Object ID
> enterprises.8164.1.45.1.1.3
> Description
> The name of this VPN (context).
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessSGSNServName
> Object ID
> enterprises.8164.1.45.1.1.4
> Description
> The name of this service.
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessSGSNMcc
> Object ID
> enterprises.8164.1.45.1.1.5
> Description
> Mobile country code
> Syntax
> Octet String (size1..3))
> Access
> Read-only
> Object
> starSessSGSNMnc
> Object ID
> enterprises.8164.1.45.1.1.6
> Description
> Mobile network code
> Syntax
> Octet String (size1..3))
> Access
> Read-only
> Object
> starSessSGSNRncId
> Object ID
> enterprises.8164.1.45.1.1.7
> Description
> The RNC id
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSessSGSNHlrNum
> Object ID
> enterprises.8164.1.45.1.1.8
> Description
> The HLR id
> Syntax
> Octet String (Size(1..16))
> Access
> Read-
> starentMIB(8164).starentMIBObjects(1).starentSS7Rd(46)
> Object
> starSS7RdTable
> Object ID
> enterprises.8164.1.46.1
> Description
> Table containing SS7Rd-related information
> Syntax
> Sequence of StarSS7RdEntry
> Access
> Not-Accessible
> Object
> starSS7RdEntry
> Object ID
> enterprises.8164.1.46.1.1
> Description
> The statistics for a specific ss7rd
> Syntax
> StarSS7RdEntry
> Access
> Not-Accessible
> Sequence
> starSS7rdId Index
> starSS7Pc
> starSS7M3UAPsId
> starSS7M3UAPspId
> starSS7MTP3LinkSetId
> starSS7MTP3LinkId
> starSS7SCTPSelfAddr
> starSS7SCTPPeerAddr
> starSS7SCTPSelfPort
> starSS7SCTPPeerPort
> Object
> starSS7rdid
> Object ID
> enterprises.8164.1.46.1.1.1
> Description
> SS7 Routing Domain identification.
> Syntax
> Gauge32
> Access
> Not accessible
> Object
> starSS7Pc
> Object ID
> enterprises.8164.1.46.1.1.2
> Description
> Point Code.
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starSS7M3UAPsId
> Object ID
> enterprises.8164.1.46.1.1.3
> Description
> Peer Server identification.
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSS7M3UAPspid
> Object ID
> enterprises.8164.1.46.1.1.4
> Description
> Peer Server Process Identification
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSS7MTP3LinkSetId
> Object ID
> enterprises.8164.1.46.1.1.5
> Description
> MTP3 LinkSet Identifier
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSS7MTP3LinkId
> Object ID
> enterprises.8164.1.46.1.1.6
> Description
> MTP3 Link Identifier
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSS7SCTPSelfAddr
> Object ID
> enterprises.8164.1.46.1.1.7
> Description
> Self-End-Point IP Address
> Syntax
> IpAddress
> Access
> Read-only
> Object
> starSS7SCTPPeerAddr
> Object ID
> enterprises.8164.1.46.1.1.8
> Description
> Peer Node IP Address
> Syntax
> IpAddress
> Access
> Read-Only
> Object
> starSS7SCTPSelfPort
> Object ID
> enterprises.8164.1.46.1.1.9
> Description
> Self end-point sctp port
> Syntax
> Gauge32
> Access
> Read-Only
> Object
> starSS7SCTPPeerPort
> Object ID
> enterprises.8164.1.46.1.1.10
> Description
> Peer end-point SCTP Port
> Syntax
> Gauge32
> Access
> Read-Only
> starentMIB(8164).starentMIBObjects(1).starentSccpNw(47)
> Object
> starSccpNwTable
> Object ID
> enterprises.8164.1.47.1
> Description
> Table containing Sccp Network-related information
> Syntax
> Sequence of StarSccpNwEntry
> Access
> Not-accessible
> Object
> starSccpNwEntry
> Object ID
> enterprises.8164.1.47.1.1
> Description
> Statistics for a specific Sccp Network
> Syntax
> StarSccpNwEntry
> Access
> Not-accessible
> Sequence
> starSccpNwld Gauge32
> starSccpSsn Gauge32
> Object
> starSccpNwId
> Object ID
> enterprises.8164.1.47.1.1.1
> Description
> SCCP Network ID
> Syntax
> Gauge32
> Access
> Not accessible
> Object
> starSccpSsn
> Object ID
> enterprises.8164.1.47.1.1.2
> Description
> Sub-system number
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentSGTPService(48)
> Object
> starSGTPSerTable
> Object ID
> enterprises.8164.1.48.1
> Description
> Table containing SGTP Service-related info
> Syntax
> Sequence of StarSGTPSerEntry
> Access
> Not-accessible
> Object
> starSGTPSerEntry
> Object ID
> enterprises.8164.1.48.1.1
> Description
> Statistics for a specific SGTP Service
> Syntax
> StarSGTPSerEntry
> Access
> Not-accessible
> Sequence
> starSGTPSerVpnID Gauge32
> starSGTPSerSvcID Gauge32
> starSGTPVpnName Display String
> starSGTPServName Display String
> starSGTPSelfAddr IpAddress
> starSGTPPeerAddr IpAddress
> starSGTPSelfPort Gauge32
> starSGTPPeerPort Gauge32
> Object
> starSGTPSerVpnID
> Object ID
> enterprises.8164.1.48.1.1.1
> Description
> Internal ID of the VPN (Context)
> Syntax
> Gauge32
> Access
> Not accessible
> Object
> starSGTPSerSvcID
> Object ID
> enterprises.8164.1.48.1.1.2
> Description
> Internal service ID unique within this context
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starSGTPVpnName
> Object ID
> enterprises.8164.1.48.1.1.3
> Description
> Name of this VPN (Context)
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSGTPServName
> Object ID
> enterprises.8164.1.48.1.1.4
> Description
> Name of this service
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starSGTPSelfAddr
> Object ID
> enterprises.8164.1.48.1.1.5
> Description
> SGSN IP Address
> Syntax
> IP Address
> Access
> Read-only
> Object
> starSGTPPeerAddr
> Object ID
> enterprises.8164.1.48.1.1.6
> Description
> IP Address for the PeerNode
> Syntax
> IPAddress
> Access
> Read-only
> Object
> starSGTPSelfPort
> Object ID
> enterprises.8164.1.48.1.1.7
> Description
> The self end point SGTP port
> Syntax
> Gauge32
> Access
> Read-only
> Object
> starSGTPPeerPort
> Object ID
> enterprises.8164.1.48.1.1.8
> Description
> The peer end point SGTP port
> Syntax
> Gauge32
> Access
> Read-only
> starentMIB(8164).starentMIBObjects(1).starentIPMSServer(49)
> Object
> starIPMSServerTable
> Object ID
> enterprises.8164.1.49.1
> Description
> Table containing information on IPMS servers
> Syntax
> Sequence of StarIPMSServerEntry
> Access
> Not-accessible
> Sequence
> starIPMSServerVpnIDGauge32
> starIPMSServerAddrIpAddress
> starIPMSServerVpnNameDisplayString
> Object
> starIPMSServerEntry
> Object ID
> enterprises.8164.1.49.1.1
> Description
> Information about a particular IPMS Server.
> Syntax
> Sequence of StarIPMSServerEntry
> Access
> Not-accessible
> Sequence
> starIPMSServerVpnID Gauge32
> starIPMSServerAddr Address
> starIPMSServerVpnName DisplayString
> Object
> starIPMSServerVpnID
> Object ID
> enterprises.8164.1.49.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> Not-accessible
> Object
> starIPMSServerAddr
> Object ID
> enterprises.8164.1.49.1.1.2
> Description
> The IP address of the IPMS server within this VPN (context)
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starIPMSServerVpnName
> Object ID
> enterprises.8164.1.49.1.1.3
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentCert(50)
> Object
> starCertTable
> Object ID
> enterprises.8164.1.50.1
> Description
> Table containing information on X.509 certificates
> Syntax
> Sequence of StarCertEntry
> Access
> Not-accessible
> Object
> starCertEntry
> Object ID
> enterprises.8164.1.50.1.1
> Description
> Information on a particular X.509 Certificate
> Syntax
> StarCertEntry
> Access
> Not-accessible
> Sequence
> starCertSerialNumber Display-String
> starCertExpiryTime DateAndTime
> starCertIssuer Display-String
> Object
> starCertSerialNumber
> Object ID
> enterprises.8164.1.50.1.1.1
> Description
> Certificate serial number
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starCertExpiryTime
> Object ID
> enterprises.8164.1.50.1.1.2
> Description
> Certificate expiration date and time
> Syntax
> DateAndTime
> Access
> Read-only
> Object
> starCertIssuer
> Object ID
> enterprises.8164.1.50.1.1.3
> Description
> The certificate issuing agency
> Syntax
> DisplayString
> Access
> Read-0nly
> starentMIB(8164).starentMIBObjects(1).starentFile(51)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starFileTable
> Object ID
> enterprises.8164.1.51.1
> Description
> A table of files stored on a mass storage device
> Syntax
> SEQUENCE OF StarFileEntry
> Access
> Not-accessible
> Object
> starFileEntry
> Object ID
> enterprises.8164.1.51.1.1
> Description
> Information about a particular file on a mass storage device
> Syntax
> StarFileEntry
> Access
> Not-accessible
> Sequence
> starFileName DisplayString,
> starFileApplication INTEGER
> Object
> starFileName
> Object ID
> enterprises.8164.1.51.1.1.1
> Description
> The name (full path) of the file
> Syntax
> DisplayString
> Access
> Not-accessible
> Object
> starFileApplication
> Object ID
> enterprises.8164.1.51.1.1.2
> Description
> The application that owns this file
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> unknown(0)
> systemfile(1)
> cdrmod(2)
> starentMIB(8164).starentMIBObjects(1).starentFTPServ(52)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starFTPServTable
> Object ID
> enterprises.8164.1.52.1
> Description
> A table of FTP servers configured
> Syntax
> SEQUENCE OF StarFTPServEntry
> Access
> Not-accessible
> Object
> starFTPServEntry
> Object ID
> enterprises.8164.1.52.1.1
> Description
> Information about a particular FTP Server
> Syntax
> StarFTPServEntry
> Access
> Not-accessible
> Sequence
> starFTPServVpnID Unsigned32,
> starFTPServIpAddr IpAddress,
> starFTPServVpnName DisplayString
> Object
> starFTPServVpnID
> Object ID
> enterprises.8164.1.52.1.1.1
> Description
> The internal identification of the VPN (context) used to reach this FTP server
> Syntax
> Unsigned32
> Access
> Not-accessible
> Object
> starFTPServIpAddr
> Object ID
> enterprises.8164.1.52.1.1.2
> Description
> The IP address of the FTP server
> Syntax
> IpAddress
> Access
> Not-accessible
> Object
> starFTPServVpnName
> Object ID
> enterprises.8164.1.52.1.1.3
> Description
> The name of the VPN (context)
> Syntax
> DisplayString
> Access
> Not-accessible
> starentMIB(8164).starentMIBObjects(1).starentCSCFPeerServer(53)
> Object
> starCSCFPeerServerTable
> Object ID
> enterprises.8164.1.53.1
> Description
> A table containing PeerServer related information
> Syntax
> SEQUENCE OF StarCSCFPeerServerEntry
> Access
> Not Accessible
> Object
> starCSCFPeerServerEntry
> Object ID
> enterprises.8164.1.53.1.1
> Description
> The statistics for a specific CSCF service
> Syntax
> StarCSCFPeerServerEntry
> Access
> Not Accessible
> Sequence
> starCSCFPeerServerVpnID Gauge32,
> starCSCFPeerServerSvcID Gauge32,
> starCSCFPeerServerVpnName DisplayString,
> starCSCFPeerServerSvcName DisplayString,
> starCSCFPeerServerListName DisplayString
> Object
> starCSCFPeerServerVpnID
> Object ID
> enterprises.8164.1.53.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> Not Accessible
> Object
> starCSCFPeerServerSvcID
> Object ID
> enterprises.8164.1.53.1.1.2
> Description
> The internal identification of this CSCF service; unique
> Syntax
> Gauge32
> Access
> Not Accessible
> Object
> starCSCFPeerServerVpnName
> Object ID
> enterprises.8164.1.53.1.1.3
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> Read-Only
> Object
> starCSCFPeerServerSvcName
> Object ID
> enterprises.8164.1.53.1.1.4
> Description
> The name of this CSCF-service
> Syntax
> DisplayString
> Access
> Read-Only
> Object
> starCSCFPeerServerListName
> Object ID
> enterprises.8164.1.53.1.1.5
> Description
> The name of the cscf-peer-server
> Syntax
> DisplayString
> Object
> starCSCFPeerServerName
> Object ID
> enterprises.8164.1.53.1.1.6
> Description
> The name of the cscf-peer-server
> Syntax
> DisplayString
> Object
> starCSCFPeerServerState
> Object ID
> enterprises.8164.1.53.1.1.7
> Description
> The state of the cscf-peer-server.
> Syntax
> DisplayString
> starentMIB(8164).starentMIBObjects(1).starentSDH(54)
> Object
> starSDHTable
> Object ID
> enterprises.8164.1.54.1
> Description
> Table containing SDH information
> Syntax
> SEQUENCE OF StarSDHEntry
> Access
> Not Accessible
> Object
> starSDHEntry
> Object ID
> enterprises.8164.1.54.1.1
> Description
> Statistical data
> Syntax
> StarSDHEntry
> Access
> Not Accessible
> Sequence
> starSDHSlot Index
> starSDHPort Index
> starSDHOperState
> Object
> starSDHSlot
> Object ID
> enterprises.8164.1.54.1.1.1
> Description
> The slot number for this port
> Syntax
> Integer32(17..48)
> Access
> Not Accessible
> Object
> starSDHPort
> Object ID
> enterprises.8164.1.54.1.1.2
> Description
> The port number within this slot
> Syntax
> Integer32(1..8)
> Access
> Not Accessible
> Object
> starSDHOperState
> Object ID
> enterprises.8164.1.54.1.1.3
> Description
> A bitmask indicating the state of SDH layer SCT.
> 0x0000 Good
> 0x0001 lais
> 0x0002 linesd
> 0x0004 linesf
> 0x0010 lof
> 0x0020 los
> 0x0040 msrdi
> Syntax
> Integer32
> Access
> Read-Only
> starentMIB(8164).starentMIBObjects(1).starentSDHPath(55)
> Object
> starSDHPathTable
> Object ID
> enterprises.8164.1.55.1
> Description
> Table for SDH Path data
> Syntax
> SEQUENCE OF starSDHPathEntry
> Access
> Not Accessible
> Object
> starSDHPathEntry
> Object ID
> enterprises.8164.1.55.1.1
> Description
> Table statistical data
> Syntax
> starSDHPathEntry
> Access
> Not Accessible
> Sequence
> starSDHPathSlot Integer32
> starSDHPathPort Integer32
> starSDHPathNum Integer32
> starSDHPathOperState Integer32
> Object
> starSDHPathSlot
> Object ID
> enterprises.8164.1.55.1.1.1
> Description
> Slot number for this port
> Syntax
> Integer32(17..48)
> Access
> Not Accessible
> Object
> starSDHPathPort
> Object ID
> enterprises.8164.1.55.1.1.2
> Description
> Port number within this slot
> Syntax
> Integer32(1..8)
> Access
> Not Accessible
> Object
> starSDHPathNum
> Object ID
> enterprises.8164.1.55.1.1.3
> Description
> Path number
> Syntax
> Integer32(1..3)
> Access
> Not Accessible
> Object
> starSDHPathOperState
> Object ID
> enterprises.8164.1.55.1.1.4
> Description
> A bitmask indicating the state of SDH Path HOP
> 0x0000 Good
> 0x0001 hopathsd
> 0x0002 hopathsf
> 0x0020ppdi
> 0x0040 prdi
> 0x0080 perdi
> 0x0100 perdival
> 0x0200 perdivaloff
> Syntax
> Integer32
> Access
> Read-Only
> starentMIB(8164).starentMIBObjects(1).starentE1Trib(56)
> Object
> starE1TribTable
> Object ID
> enterprises.8164.1.56.1
> Description
> Table for E1Trib data
> Syntax
> SEQUENCE OF StarE1TribEntry
> Access
> Not Accessible
> Object
> starE1TribEntry
> Object ID
> enterprises.8164.1.56.1.1
> Description
> Statistical data for table
> Syntax
> StarE1TribEntry
> Access
> Not Accessible
> Sequence
> starE1TribSlot Index
> starE1TribPort Index
> starE1TribPath Index
> starE1TribTug2 Integer32
> starE1TribTu12 Integer32
> starE1TribOperStateLOP Integer32
> starE1TribOperState Integer32
> Object
> starE1TribSlot
> Object ID
> enterprises.8164.1.56.1.1.1
> Description
> The slot number for this port
> Syntax
> Integer32(17..48)
> Access
> Not Accessible
> Object
> starE1TribPort
> Object ID
> enterprises.8164.1.56.1.1.2
> Description
> The port number within this slot
> Syntax
> Integer32(1..8)
> Access
> Not Accessible
> Object
> starE1TribPath
> Object ID
> enterprises.8164.1.56.1.1.3
> Description
> Not shown
> Syntax
> Integer32(1..3)
> Access
> Not Accessible
> Object
> starE1TribTug2
> Object ID
> enterprises.8164.1.56.1.1.4
> Description
> Not shown
> Syntax
> Integer32(1..7)
> Access
> Not Accessible
> Object
> starE1TribTu12
> Object ID
> enterprises.8164.1.56.1.1.5
> Description
> Not shown
> Syntax
> Integer32(1..3)
> Access
> Not Accessible
> Object
> starE1TribOperStateLOP
> Object ID
> enterprises.8164.1.56.1.1.6
> Description
> A bitmask indicating the stare of SDH layer LOP
> 0x0000 Good
> 0x0001 lopathsd
> 0x0002 lopathsf
> 0x0100 erdi
> 0x0200 rdi
> 0x0400 lop
> 0x0800 ais
> 0x1000 lom
> Syntax
> Integer32
> Access
> Read Only
> Object
> starE1TribOperState
> Object ID
> enterprises.8164.1.56.1.1.7
> Description
> A bitmask indicating the state of the E1 Tributary
> 0x0000 Good
> 0x0001 inf0x0002 insmf
> 0x0004 incmf
> 0x0008 ooof
> 0x0010 raiccrc
> 0x0020 cfebe
> 0x0040 rai
> 0x0080 rmai
> 0x0100 aisd
> 0x0200 red
> 0x0400 ais
> 0x0800 ts16aisd
> Syntax
> Integer32
> Access
> Read Only
> starentMIB(8164).starentMIBObjects(1).starentGPRSLink(57)
> Object
> starGPRSLinkTable
> Object ID
> enterprises.8164.1.57.1
> Description
> A table containing GPRS Service Link related information.
> Syntax
> SEQUENCE of StarGPRSLinkEntry
> Access
> Not Accessible
> Object
> starGPRSLinkEntry
> Object ID
> enterprises.8164.1.57.1.1
> Description
> The link statistics for a specific GPRS service.
> Syntax
> StarGPRSLinkEntry
> Sequence
> starGPRSNsei Gauge32,
> starGPRSNsvci Gauge32,
> starGPRSBvci Gauge32,
> Object
> starGPRSNsei
> Object ID
> enterprises.8164.1.57.1.1.1
> Description
> Network Service Entity Identifier
> Syntax
> Gauge32
> Access
> Read-Only
> Object
> starGPRSNsvci
> Object ID
> enterprises.8164.1.57.1.1.2
> Description
> Network Service Virtual Circuit Identifier
> Syntax
> Gauge32
> Access
> Read-Only
> Object
> starGPRSBvci
> Object ID
> enterprises.8164.1.57.1.1.3
> Description
> Base Station System GPRS (General Packet Radio Service) Protocol Virtual Circuit Identifier.
> Syntax
> Gauge32
> Access
> Read-Only
> starentMIB(8164).starentMIBObjects(1).starentFractE1Trib(58)
> Object
> starFractE1TribTable
> Object ID
> enterprises.8164.1.58.1
> Description
> A table ...
> Syntax
> SEQUENCE of StarFractTribEntry
> Access
> Not Accessible
> Object
> starFractE1TribEntry
> Object ID
> enterprises.8164.1.58.1.1
> Description
> Information about a specific Entry
> Syntax
> starFractE1TribEntry
> Sequence
> starFractE1TribSlot Integer32,
> starFractE1TribPort I Integer32,
> starFractE1TribPath Integer32,
> starFractE1TribTug2 Integer32,
> starFractE1TribTu12 Integer32
> starFractE1TribBundNum Integer32,
> starFractE1TribTimeslots DisplayString
> Object
> starFractE1TribSlot
> Object ID
> enterprises.8164.1.58.1.1.1
> Description
> Slot number for this port
> Syntax
> Integer32(17..48)
> Access
> Not Accessible
> Object
> starFractE1TribPort
> Object ID
> enterprises.8164.1.58.1.1.2
> Description
> Port number within slot
> Syntax
> Integer32(1..8)
> Access
> Not Accessible
> Object
> starFractE1TribPath
> Object ID
> enterprises.8164.1.58.1.1.3
> Description
> Not shown
> Syntax
> Integer32(1..3)
> Object
> starFractE1TribTug2
> Object ID
> enterprises.8164.1.58.1.1.4
> Description
> Not shown
> Syntax
> Integer32(1..84)
> Access
> Not Accessible
> Object
> starFractE1TribTu12
> Object ID
> enterprises.8164.1.58.1.1.5
> Syntax
> Integer32(1..3)
> Access
> not-accessible
> Object
> starFractE1TribBundNum
> Object ID
> enterprises.8164.1.58.1.1.6
> Description
> Not Given
> Syntax
> Integer32(0..31)
> Access
> Not Accessible
> Object
> starFractE1TribTimeslots
> Object ID
> enterprises.8164.1.58.1.1.7
> Description
> Not Given
> Syntax
> Display/String
> Access
> Read-Only
> starentMIB(8164).starentMIBObjects(1).starentStorage(59)
> The objects in this table are not accessible via SNMP. They are intended for use within traps.
> Object
> starStorageTable
> Object ID
> enterprises.8164.1.59.1
> Description
> A table of mass storage devices
> Syntax
> SEQUENCE OF StarStorageEntry
> Access
> Not Accessible
> Object
> starStorageEntry
> Object ID
> enterprises.8164.1.59.1.1
> Description
> Information about a particular file on a mass storage device
> Syntax
> StarStorageEntry
> Access
> Not Accessible
> Sequence
> starStorageSlot Integer32,
> starStorageName DisplayString,
> starStorageDeviceType INTEGER
> Object
> starStorageSlot
> Object ID
> enterprises.8164.1.59.1.1.1
> Description
> The slot number of the card holding this storage device
> Syntax
> Integer32(1..16)
> Access
> Not Accessible
> Object
> starStorageName
> Object ID
> enterprises.8164.1.59.1.1.2
> Description
> The name of the storage device
> Syntax
> DisplayString
> Access
> Not Accessible
> Object
> starStorageDeviceType
> Object ID
> enterprises.8164.1.59.1.1.3
> Description
> The storage device type. A value of independent(1) means that the device can be accessed as a standalone device, and is not part of a raid array. A value of raid(2) means that this device is a raid array. A value of raidmember(3) means the device is part of a raid array, and thus cannot be read/written to outside of the raid array
> Syntax
> INTEGER
> Access
> Not Accessible
> Enumeration
> unknown(0),
> independent(1),
> raid(2),
> raidmember(3)
> starentMIB(8164).starentMIBObject(1).FNGSys(60)
> Object
> starFNGSysStatus
> Object ID
> 8164.1.60.1
> Description
> The overall status of the chassis as a FNG service. A value of noservice(1) means that the chassis is not configured/licensed for FNG; active(2) indicates that at least one NG service is available for processing sessions; temporary(3) indicates that FNG is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no FNG service is currently active, but one or more FNG services are configured.
> Syntax
> unknown(0)
> noservice(1)
> active(2)
> temporary(3)
> outofservice(4)
> Access
> read-only
> Object
> starFNGSysNumService
> Object ID
> 8164.1.60.2
> Description
> The number of FNG services configured
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSysSessCurrent
> Object ID
> 8164.1.60.3
> Description
> The number of current FNG sessions for this chassis
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSysSessCurrActive
> Object ID
> 8164.1.60.4
> Description
> The number of currently active FNG sessions for this chassis
> Syntax
> current
> Access
> read-only
> Object
> starFNGSysSessCurrDormant
> Object ID
> 8164.1.60.5
> Description
> The number of currently dormant FNG sessions for this chassis
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSysSessTtlSetup
> Object ID
> 8164.1.60.6
> Description
> he cumulative total number of FNG sessions that has been setup
> Syntax
> Counter32
> Access
> read-only
> Object
> starFNGSysChildSACurrent
> Object ID
> 8164.1.60.7
> Description
> The number of current FNG child SAs for this chassis
> Syntax
> Gauge32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentFNGService(61)
> Object
> starFNGTable
> Object ID
> 8164.1.61.1
> Description
> A table of per-service FNG information
> Syntax
> SEQUENCE OF StarFNGEntry
> Access
> not-accessible
> Object
> starFNGEntry
> Object ID
> 8164.1.61.1.1
> Description
> The information for a FNG service
> Syntax
> StarFNGEntry
> Access
> not-accessible
> Object
> starFNGSvcID
> Object ID
> 8164.1.61.1.1.1
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:)
> Syntax
> StarShortID
> Access
> not-accessible
> Object
> starFNGVpnID
> Object ID
> 8164.1.61.1.1.2
> Description
> The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the FNG device; in general starFNGVpnName should be used to identify the VPN (context)
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGVpnName
> Object ID
> 8164.1.61.1.1.3
> Description
> he VPN (context) name
> Syntax
> DisplayString
> Access
> read-only
> Object
> starFNGServName
> Object ID
> 8164.1.61.1.1.4
> Description
> he name of this service
> Syntax
> DisplayString
> Access
> read-only
> Object
> starFNGStatus
> Object ID
> 8164.1.61.1.1.5
> Description
> The state of this FNG service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.
> Syntax
> unknown(0)
> inservice(1)
> outofservice(2)
> Access
> read-only
> Object
> starFNGSessCurrent
> Object ID
> 8164.1.61.1.1.6
> Description
> The number of current sessions for this FNG service.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessRemain
> Object ID
> 8164.1.61.1.1.7
> Description
> A count of the remaining capacity for this FNG service, in terms of sessions. If a session limit is configured for this FNG service, starFNGSessRemain will identify the difference between this limit and starFNGSessCurrent. If no individual limit has been configured for this service, starFNGSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starFNGSessRemain cannot be summed across multiple services.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessCurrentActive
> Object ID
> 8164.1.61.1.1.8
> Description
> The number of currently active sessions for this FNG service
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessCurrentDormant
> Object ID
> 8164.1.61.1.1.9
> Description
> The number of currently dormant sessions for this FNG service.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessCurrentIpv6Active
> Object ID
> 8164.1.61.1.1.10
> Description
> The number of currently active IPv6 sessions for this FNG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessCurrentIpv6Dormant
> Object ID
> 8164.1.61.1.1.11
> Description
> The number of currently dormant IPv6 sessions for this FNG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessCurrentIpv4Active
> Object ID
> 8164.1.61.1.1.12
> Description
> The number of currently active IPv4 sessions for this FNG service. Note that all FNG sessions are currently identified as 'active', and the value for starFNGSessCurrentIPv4Dormant will always be zero.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGSessCurrentIpv4Dormant
> Object ID
> 8164.1.61.1.1.13
> Description
> The number of currently dormant IPv4 sessions for this FNG service. Note that all FNG sessions are currently identified as 'active', so the value for starFNGSessCurrentIPv4Dormant will always be zero.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starFNGBindIpAddress
> Object ID
> 8164.1.61.1.1.14
> Description
> The bind IP address for this FNG service.
> Syntax
> IpAddress
> Access
> read-only
> Object
> starFNGBindIpPort
> Object ID
> 8164.1.61.1.1.15
> Description
> The bind IP port for this FNG service.
> Syntax
> Integer32
> Access
> read-only
> Object
> starFNGBindSlot
> Object ID
> 8164.1.61.1.1.16
> Description
> he physical slot number for the physical port which holds the interface bound to the starFNGBindIpAddress address.
> Syntax
> Integer32
> Access
> read-only
> Object
> starFNGBindPort
> Object ID
> 8164.1.61.1.1.17
> Description
> The physical port number for the physical port which holds the interface bound to the starFNGBindIpAddress address.
> Syntax
> Integer32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentPDGSys(62)
> Object
> starPDGSysStatus
> Object ID
> 8164.1.62.1
> Description
> The overall status of the chassis as a PDG service. A value of noservice(1) means that the chassis is not configured/licensed for PDG; active(2) indicates that at least one PDG service is available for processing sessions; temporary(3) indicates that PDG is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no PDG service is currently active, but one or more PDG services are configured.
> Syntax
> unknown(0)
> noservice(1)
> active(2)
> temporary(3)
> outofservice(4)
> Access
> read-only
> Object
> starPDGSysNumService
> Object ID
> 8164.1.62.2
> Description
> The number of PDG services configured
> Syntax
> Unsigned32
> Access
> read-only
> Units
> Services
> Object
> starPDGSysSessCurrent
> Object ID
> 8164.1.62.3
> Description
> The number of current PDG sessions for this chassis
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSysSessCurrActive
> Object ID
> 8164.1.62.4
> Description
> he number of currently active PDG sessions for this chassis.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSysSessCurrDormant
> Object ID
> 8164.1.62.5
> Description
> The number of currently dormant PDG sessions for this chassis
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSysSessTtlSetup
> Object ID
> 8164.1.62.6
> Description
> The cumulative total number of PDG sessions that has been setup
> Syntax
> Counter32
> Access
> read-only
> Object
> starPDGSysChildSACurrent
> Object ID
> 8164.1.62.7
> Description
> The number of current PDG child SAs for this chassis
> Syntax
> Gauge32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentPDGService(63)
> Object
> starPDGTable
> Object ID
> 8164.1.63.1
> Description
> A table of per-service PDG information
> Syntax
> SEQUENCE OF StarPDGEntry
> Access
> not-accessible
> Object
> starPDGEntry
> Object ID
> 8164.1.63.1.1
> Description
> The information for a PDG service
> Syntax
> StarPDGEntry
> Access
> not-accessible
> Sequence
> starPDGSvcID
> starPDGVpnID
> starPDGVpnName
> starPDGServName
> starPDGStatus
> starPDGSessCurrent
> starPDGSessRemain
> starPDGSessCurrentActive
> starPDGSessCurrentDormant
> starPDGSessCurrentIpv6Active
> starPDGSessCurrentIpv6Dormant
> starPDGSessCurrentIpv4Active
> starPDGSessCurrentIpv4Dormant
> starPDGBindIpAddress
> starPDGBindIpPort
> Object
> starPDGSvcID
> Object ID
> 8164.1.63.1.1.1
> Description
> The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:)
> Syntax
> StarShortID
> Access
> not-accessible
> Object
> starPDGVpnID
> Object ID
> 8164.1.63.1.1.2
> Description
> The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the PDG device; in general starPDGVpnName should be used to identify the VPN (context)
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGVpnName
> Object ID
> 8164.1.63.1.1.3
> Description
> The VPN (context) name
> Syntax
> DisplayString
> Access
> read-only
> Object
> starPDGServName
> Object ID
> 8164.1.63.1.1.4
> Description
> The name of this service
> Syntax
> DisplayString
> Access
> read-only
> Object
> starPDGStatus
> Object ID
> 8164.1.63.1.1.5
> Description
> The state of this PDG service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.
> Syntax
> unknown(0)
> inservice(1)
> outofservice(2)
> Access
> read-only
> Object
> starPDGSessCurrent
> Object ID
> 8164.1.63.1.1.6
> Description
> The number of current sessions for this PDG service.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessRemain
> Object ID
> 8164.1.63.1.1.7
> Description
> A count of the remaining capacity for this PDG service, in terms of sessions. If a session limit is configured for this PDG service, starPDGSessRemain will identify the difference between this limit and starPDGSessCurrent. If no individual limit has been configured for this service, starPDGSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starPDGSessRemain cannot be summed across multiple services.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessCurrentActive
> Object ID
> 8164.1.63.1.1.8
> Description
> The number of currently active sessions for this PDG service
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessCurrentDormant
> Object ID
> 8164.1.63.1.1.9
> Description
> The number of currently dormant sessions for this PDG service
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessCurrentIpv6Active
> Object ID
> 8164.1.63.1.1.10
> Description
> The number of currently active IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessCurrentIpv6Dormant
> Object ID
> 8164.1.63.1.1.11
> Description
> The number of currently dormant IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessCurrentIpv4Active
> Object ID
> 8164.1.63.1.1.12
> Description
> The number of currently active IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', and the value for tarPDGSessCurrentIPv4Dormant will always be zero.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGSessCurrentIpv4Dormant
> Object ID
> 8164.1.63.1.1.13
> Description
> The number of currently dormant IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', so the value for starPDGSessCurrentIPv4Dormant will always be zero.
> Syntax
> Gauge32
> Access
> read-only
> Object
> starPDGBindIpAddress
> Object ID
> 8164.1.63.1.1.14
> Description
> The bind IP address for this PDG service
> Syntax
> IpAddress
> Access
> read-only
> Object
> starPDGBindIpPort
> Object ID
> 8164.1.63.1.1.15
> Description
> The bind IP port for this PDG service
> Syntax
> Integer32
> Access
> read-only
> Object
> starPDGBindSlot
> Object ID
> 8164.1.63.1.1.16
> Description
> The bind IP port for this PDG service
> Syntax
> Integer32
> Access
> read-only
> Object
> starPDGBindPort
> Object ID
> 8164.1.63.1.1.17
> Description
> The physical port number for the physical port which holds the interface bound to the starPDGBindIpAddress address.
> Syntax
> Integer32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentIPPoolGroup(64)
> Object
> starIPPoolGroupTable
> Object ID
> 8164.1.64.1
> Description
> A table containing IP Pool Group information
> Syntax
> SEQUENCE OF StarIPPoolGroupEntry
> Access
> not-accessible
> Object
> starIPPoolGroupEntry
> Object ID
> 8164.1.64.1.1
> Description
> Information for a specific IP Pool Group
> Syntax
> StarIPPoolGroupEntry
> Access
> not-accessible
> Object
> starIPPoolGroupVpnID
> Object ID
> 8164.1.63.1.1.1
> Description
> The context ID for this pool group
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starIPPoolGroupID
> Object ID
> 8164.1.64.1.1.2
> Description
> The service identification is made up from first 8 chars of context name and first 16 chars of pool group name separated by (:)
> Syntax
> StarMediumID
> Access
> not-accessible
> Object
> starIPPoolGroupName
> Object ID
> 8164.1.64.1.1.3
> Description
> The name of the IP pool group
> Syntax
> DisplayString
> Access
> read-only
> Object
> starIPPoolGroupVpnName
> Object ID
> 8164.1.64.1.1.4
> Description
> The context name string for this pool group
> Syntax
> DisplayString
> Access
> read-only
> Object
> starIPPoolGroupUsed
> Object ID
> 8164.1.64.1.1.5
> Description
> The number of IP addresses in USED state in the pool group
> Syntax
> Gauge32
> Access
> read-only
> Object
> starIPPoolGroupHold
> Object ID
> 8164.1.64.1.1.6
> Description
> The number of IP addresses in HOLD state in the pool group
> Syntax
> Gauge32
> Access
> read-only
> Object
> starIPPoolGroupRelease
> Object ID
> 8164.1.64.1.1.7
> Description
> The number of IP addresses in RELEASE state in the pool group
> Syntax
> Gauge32
> Access
> read-only
> Object
> starIPPoolGroupFree
> Object ID
> 8164.1.64.1.1.8
> Description
> The number of IP addresses in FREE state in the pool group
> Syntax
> Gauge32
> Access
> read-only
> Object
> starIPPoolGroupPctUsed
> Object ID
> 8164.1.64.1.1.9
> Description
> The context name string for this pool group
> Syntax
> Integer32(0..10000)
> Access
> read-only
> Object
> starIPPoolGroupAvail
> Object ID
> 8164.1.64.1.1.10
> Description
> The context name string for this pool group
> Syntax
> Gauge32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentHNBGWService(65)
> Object
> starHNBGWServTable
> Object ID
> 8164.1.65.1
> Description
> The statistics for a specific HNBGW service
> Syntax
> StarHNBGWSerEntry
> Access
> not-accessible
> Object
> starHNBGWSerEntry
> Object ID
> 8164.1.65.1.1
> Description
> The statistics for a specific HNBGW service
> Syntax
> StarHNBGWSerEntry
> Access
> not-accessible
> Object
> starHNBGWSerVpnID
> Object ID
> 8164.1.65.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starHNBGWSerSvcID
> Object ID
> 8164.1.65.1.1.2
> Description
> The internal identification of this service; unique within a specific context
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starSessHNBGWVpnName
> Object ID
> 8164.1.65.1.1.3
> Description
> The name of this VPN (context)
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessHNBGWServName
> Object ID
> 8164.1.65.1.1.4
> Description
> The name of this Service
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessHNBGWCsNwName
> Object ID
> 8164.1.65.1.1.5
> Description
> The name of the CS NW
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessHNBGWPsNwName
> Object ID
> 8164.1.65.1.1.6
> Description
> The name of the PS NW
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessHNBGWSgsnPtCd
> Object ID
> 8164.1.65.1.1.7
> Description
> SGSN Point Code
> Syntax
> Integer32
> Access
> read-only
> Object
> starSessHNBGWMscPtCd
> Object ID
> 8164.1.65.1.1.8
> Description
> MSC Point Code
> Syntax
> Integer32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentALCAPService(66)
> Object
> starALCAPServTable
> Object ID
> 8164.1.66.1
> Description
> A table containing ALCAP relate information.
> Syntax
> StarALCAPSerEntry
> Access
> not-accessible
> Object
> starALCAPSerEntry
> Object ID
> 8164.1.66.1.1
> Description
> The statistics for a specific ALCAP service
> Syntax
> StarALCAPSerEntry
> Access
> not-accessible
> Object
> starALCAPSerVpnID
> Object ID
> 8164.1.66.1.1.1
> Description
> The internal identification of the VPN (context)
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starALCAPSerSvcID
> Object ID
> 8164.1.66.1.1.2
> Description
> The internal identification of this service; unique within a specific context.
> Syntax
> Gauge32
> Access
> not-accessible
> Object
> starSessALCAPVpnName
> Object ID
> 8164.1.66.1.1.3
> Description
> The name of this VPN (context).
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessALCAPServName
> Object ID
> 8164.1.66.1.1.4
> Description
> The name of this Service.
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessALCAPAAL2NodeName
> Object ID
> 8164.1.66.1.1.5
> Description
> The name of the AAL2 Node.
> Syntax
> DisplayString
> Access
> read-only
> Object
> starSessALCAPPathId
> Object ID
> 8164.1.66.1.1.6
> Description
> The path id of AAL2 path.
> Syntax
> Integer32
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentPDGSys(67)
> Object
> starMMES1AssocTable
> Object ID
> 8164.1.67.1
> Description
> A table of MME S1 Associations.
> Syntax
> SEQUENCE OF StarMMES1AssocEntry
> Access
> not-accessible
> Object
> starMMES1AssocEntry
> Object ID
> 8164.1.67.1.1
> Description
> Information about a particular MME S1 Association.
> Syntax
> StarMMES1AssocEntry
> Access
> not-accessible
> Object
> starMMES1AssocSvcID
> Object ID
> 8164.1.67.1.1.1
> Description
> The service identification is made up from the first 8 characters of the VPN name and the first 16 characters of the service name seperated by (:).
> Syntax
> StarMediumID
> Access
> not-accessible
> Object
> starMMES1AssocENBID
> Object ID
> 8164.1.67.1.1.2
> Description
> The identification of the eNodeB.
> Syntax
> StarENBID
> Access
> not-accessible
> Object
> starMMES1AssocVpnName
> Object ID
> 8164.1.66.1.1.3
> Description
> The name of this VPN (context).
> Syntax
> DisplayString
> Access
> read-only
> Object
> starMMES1AssocServName
> Object ID
> 8164.1.66.1.1.4
> Description
> The name of this MME Service.
> Syntax
> DisplayString
> Access
> read-only

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883