> LTE Handover Restriction List Configuration Mode Commands
> The LTE Handover Restriction List Configuration Mode is used to create and manage the LTE handover restriction lists for LTE/SAE networks. Handover restriction lists are used to restrict user equipment (UE) from participating in specified handovers. The MME creates the handover restriction lists as part of it’s local policy and provides them to the eNobeB where the restrictions are enforced.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax exit
> Usage
> Return to the previous mode.
> forbidden
> Configures the handover restriction lists provided to eNodeBs where handover restrictions are enforced for UEs.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] forbidden { inter-rat { all | cdma2000 | geran | utran } | location-area plmnid id | tracking-area plmnid id }
> default forbidden inter-rat
> default forbidden inter-rat
> Removes the forbidden inter-rat configuration from the LTE policy.
> no
> Removes the forbidden configuration from the LTE policy.
> inter-rat { all | cdma2000 | geran | utran }
> Specifies that one or all Radio Access Technology (RAT) handovers are to be prohibited for UEs associated with the LTE policy.
> all: Specifies that all inter-RAT handovers are to be prohibited for UEs associated with the LTE policy.
> cdma2000: Specifies that all CDMA2000 handovers are to be prohibited for UEs associated with the LTE policy.
> geran: Specifies that all GSM EDGE Radio Access Network (GERAN) handovers are to be prohibited for UEs associated with the LTE policy.
> utran: Specifies that all UMTS Terrestrial Radio Access Network (UTRAN) handovers are to be prohibited for UEs associated with the LTE policy.
> location-area plmnid id
> Specifies that handovers to 3G location area codes defined through this keyword and subsequent configuration mode are to be prohibited for UEs associated with the LTE policy. Enters the LTE Forbidden Location Area Configuration Mode. id must be a valid PLMN ID and be an integer value comprising an MCC and MNC (five-digit minimum, six-digit maximum).
> Important: Up to 16 forbidden location area PLMN IDs can be configured per handover restriction list.
> Entering this command results in the following prompt:
> [context_name]hostname(forbidden_la)#
> LTE Forbidden Location Area Configuration Mode commands are defined in the LTE Forbidden Location Area Configuration Mode Commands chapter.
> tracking-area plmnid id
> Specifies that handovers to 4G tracking area codes defined through this keyword and subsequent configuration mode are to be prohibited for UEs associated with the LTE policy. Enters the LTE Forbidden Tracking Area Configuration Mode. id must be a valid PLMN ID and be an integer value comprising an MCC and MNC (five-digit minimum, six-digit maximum).
> Important: Up to 16 forbidden tracking area PLMN IDs can be configured per handover restriction list.
> Entering this command results in the following prompt:
> [context_name]hostname(forbidden_ta)#
> LTE Forbidden Tracking Area Configuration Mode commands are defined in the LTE Forbidden Tracking Area Configuration Mode Commands chapter.
> Usage
> Use this command to create the list of restricted handover types that apply to all UEs associated with the LTE policy.
> Example
> The following command prohibits UEs associated with this LTE policy from participating in a handover to a GERAN network type:
> forbidden inter-rat geran
> The following command prohibits UEs, associated with this LTE policy and a mobile network with a PLMN ID of 12345, from participating in a handover to location area codes defined in the Location Area Configuration Mode:
> forbidden location-area plmnid 12345

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883