> Exec Mode Show Commands (Q-S)
> This section includes the commands qci-qos-mapping through show system uptime.
> show qci-qos-mapping
> Displays QoS Class Identifier-Quality of Service (QCI-QoS) mapping tables configured on this system.
> Product
> HSGW, P-GW, S-GW
> Privilege
> Inspector
> Syntax
> show qci-qos-mapping table { all | name table_name } [ | { grep grep_options | more } ]
> all
> Displays information for all QCI-QoS mapping tables configured on this system.
> name table_name
> Displays information for a QCI-QoS mapping tables configured for a specific QCI-QoS table on this system.
> table_name must be an existing QCI-QoS table from 1 to 63 alphanumeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display the contents of a specific QCI-QoS mapping table or all mapping tables configured on this system.
> Example
> The following command displays the contents of a QCI-QoS mapping table named table1:
> show qci-qos-mapping table name table1
> show qos npu inter-subscriber traffic
> Displays configuration information pertaining to Network Processing Unit (NPU) QoS priority queue bandwidth allocation and sharing.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show inter-subscriber traffic { bandwidth | bandwidth-sharing }
> bandwidth
> Displays NPU QoS priority queue bandwidth allocation configuration information.
> bandwidth-sharing
> Displays NPU QoS priority queue bandwidth sharing configuration information.
> Usage
> Use this command to verify configuration information and for troubleshooting.
> When the bandwidth keyword is used, the output is a table showing the configuration status, the priority queue, and the bandwidth allocation per DSCP.
> When the bandwidth-sharing keyword is used, the output of is a table displaying the bandwidth sharing configuration per processing card slot/CP number.
> For additional information on the NPU QoS functionality, refer to the System Administration Guide.
> Important: This functionality is not supported for use with the PDSN at this time.
> show qos npu stats
> Displays Network Processing Unit (NPU) QoS statistics per priority queue for a particular processing card:
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show qos npu stats inter-subscriber traffic slot slot_num
> slot slot_num
> Specifies the chassis slot number in which the processing card for which to display statistics is installed.
> slot_num is an integer from 1 to 48 that represents the slot in which a processing card is installed. Processing cards can be installed in slots 1 through 8, and/or 10 through 16.
> Usage
> This command displays packet and byte counts per NPU QoS priority queue on a per-processing card basis.
> For additional information on the NPU QoS functionality, refer to the System Administration Guide.
> Important: This functionality is not supported for use with the PDSN at this time.
> Example
> The following command displays NPU QoS priority queue statistics for a processing card installed in chassis slot number 4:
> show qos npu stats inter-subscriber traffic slot 4
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show radius
> Displays and statistic information for RADIUS accounting and/or authentication.
> Product
> PDSN, HA, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show radius { accounting servers | authentication servers } [ detail ] [ admin-status { enabled | disabled } ] [ | { grep grep_options | more } ] [ radius group group_name [ detail ] [ | { grep grep_options | more } ] ]
> accounting servers
> Lists information for configured accounting servers and their current state.
> authentication servers
> Lists information for configured authentication servers and their current state.
> [ detail ]
> Displays historical state information for configured servers of the specified type.
> admin-status { enabled | disabled }
> Displays information for accounting and/or authentication servers with an administrative status of “enabled” or ”disabled”.
> radius group group_name
> Displays the authentication/authorization RADIUS server group information for server group group_name within the current context.
> group_name will be a string of 1 to 63 characters that specifies the name of a server group configured in a specific context for authentication/accounting.
> grep grep_options | more
> Specifies the output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Display the RADIUS server information as part of periodic monitoring of the health of the system.
> Example
> The following displays the information on configured accounting servers:
> show radius accounting server
> The following command displays detailed information for RADIUS accounting servers:
> show radius accounting servers detail
> The following command displays detailed information for RADIUS server group star1 used for authentication:
> show radius authentication servers radius group star1 detail
> The following command displays detailed information for RADIUS server group star1 used for accounting:
> show radius accounting servers radius group star1 detail
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show radius charging servers
> This command displays the RADIUS authentication and accounting servers or server group that are configured for use by charging services.
> Product
> PDSN, HA, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show radius charging servers [ radius group group_name ] [ | { grep grep_options | more } ]
> radius group group_name all
> Displays all RADIUS counter information for the specified server group configured for use by charging services.
> group_name specifies the name of server group configured in a specific context for authentication/accounting, and must be a string of 1 through 63 characters.
> grep grep_options | more
> Specifies the output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display information about RADIUS servers or server group configured for use by Charging Services.
> Example
> The following command displays RADIUS servers configured for Charging Services:
> show radius charging servers
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show radius client
> DIsplays information about the RADIUS client configured on the system.
> Product
> PDSN, HA, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show radius client status [ | { grep grep_options | more } ]
> status
> Displays a status summary for the RADIUS client.
> | { grep grep_options | more }
> Specifies the output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> The configuration of the RADIUS protocol on the system enables RADIUS client functionality.
> This command is used to view information pertaining to the status of the client.
> Example
> The following command displays detailed information pertaining to the system’s RADIUS client:
> show radius client status
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show radius counters
> Displays RADIUS server and statistic information for accounting and/or authentication.
> Product
> PDSN, HA, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show radius counters { all | radius group group_name all | server ip_address [ port number ] | summary [ all-contexts [ verbose ] ] } [ | { grep grep_options | more } ]
> counters { all | server ip_address [ port number ] }
> counters { all | server ip_address [ port number ] }: indicates the statistics for either all servers or the server specified by ip_address is to be displayed. The statistics for a specific port of the server may also be specified as number. ip_address must be specified using IPv4 dotted-decimal notation. number must be an integer from 0 through 65535.
> radius group group_name all
> Displays all RADIUS counter information for the specified server group within the current context.
> group_name specifies the name of the server group configured in a specific context for authentication/accounting, and must be a string of 1 through 63 characters.
> summary [ all-contexts [ verbose ] ]
> Displays a summary of RADIUS statistics for all the RADIUS servers configured in a specific context.
> all-contexts: Specifies that a summary of RADIUS statistics for all RADIUS servers configured in all contexts should be displayed. If verbose is also specified the information is dispayed in more detail.
> grep grep_options | more
> Specifies the output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Display the RADIUS server information as part of periodic monitoring of the health of the system.
> Example
> The following command displays detailed information pertaining to the RADIUS server group star1 with in current context:
> show radius counters radius group star1 all
> The following displays the statistics for the server with IP address 1.2.3.4, then just port 7777, followed by all services.
> show radius counters server 1.2.3.4
> show radius counters server 1.2.3.4 port 7777
> show radius counters all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show resources
> Displays the resource information by CPU or session.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show resources { cpu | session } [ | { grep grep_options | more } ]
> cpu | session
> cpu: indicates the resource information is to be displayed by CPU.
> session: indicates the resource information is to be displayed by session.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View resource utilization as part of troubleshooting systems which appear sluggish or are having excessive connection timeouts or other connection issues.
> Example
> The following display the resource information by CPU and session, respectively.
> show resources cpu
> show resources session
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show rohc counters
> This command displays RObust Header Compression (ROHC) counters for all active calls.
> Product
> PDSN, HSGW, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rohc counters [ all | callid call_id | imsi imsi_num | ip-address ip_addr | msid msid_num | username user_name ] [ | { grep grep_options | more } ]
> all
> indicates all information is to be displayed.
> callid call_id
> call_id indicates the information only for calls with Id call_id are to be displayed. call_id must be specified as a 4-byte hexadecimal number.
> imsi imsi_num
> imsi_num: Specifies an international mobile subscriber ID only for which information is to be displayed. The IMSI (International Mobile Subscriber Identity) ID is an up to 15-character field which identifies the subscriber’s home country and carrier: 3 digits of Mobile Country Code (MCC), 2 or 3 digits of Mobile Network Code (MNC), followed by the Mobile Subscriber Identification Number MSIN. Example: 123-45-678910234. May also be entered as 12345678910234.
> ip-address ip_addr
> ip_addr: Specifies a mobile subscriber IP address only for which information is to be displayed. ip_addr must be expressed in IPv4 dotted-decimal or IPv6 colon-separated notation.
> msid msid_num
> msid_num specifies a mobile subscriber ID only for which information is to be displayed. msid_num must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> username user_name
> user_name: specifies a user only for which radio-packet (R-P) interface information is to be displayed where the user is specified as user_name.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display ROHC counters for all active calls.
> Example
> The following command displays ROHC counters for all active calls:
> show rohc counters all
> show rohc statistics
> This command displays statistics and counters for RObust Header Compression (ROHC) IP header compression.
> Product
> PDSN, HSGW, and ASN-GW.
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rohc statistics [ pdsn-service service name ] [ asngw-service service name ] [ hsgw-service hsgwsvc_name ] [ | { grep grep_options | more } ]
> Important: Keywords available for this command are license-driven. For example, if a PDSN license is loaded, the pdsn-service option is visable.
> pdsn-service pdsnsvc_name
> Display ROHC statistics and counters for the specified PDSN service.
> asngw-service asngwsvc_name
> Display ROHC statistics and counters for the specified ASN-GW service.
> hsgw-service hsgwsvc_name
> Display ROHC statistics and counters for the specified HSGW service.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display ROHC statistics for all services or for a specific ASN-GW, PDSN, or HSGW.
> Example
> The following command displays ROHC statistics for the PDSN service named pdsn1:
> show rohc statistics pdsn-service pdsn1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show route-map
> This command displays entries for all route maps wintin the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show route-map [ name route-map name ] [ | { grep grep_options | more } ]
> name route-map name
> Displays information for a specified route-map. The name is a string of 1 to 79 characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to see the rules configured in all route-maps for the current context.
> Example
> The following command displays the route-map information;
> show route-map
> Refer to the match and set command descriptions in the Route-map Configuration Mode Commands chapter for descriptions of the various entries listed.
> show rp
> Displays radio-packet (R-P) interface statistics using the filtering options specified.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rp [ counters | full | summary ] { all | callid call_id | msid ms_id | peer-address peer_ip_address | username user_name } [ | { grep grep_options | more } ]
> counters | full | summary
> Provides an optional modifier to the output for the level and type of information.
> counters: indicates the R-P protocol statistics are to be displayed.
> full: indicates all available information is to be displayed.
> summary: indicates only a summary of available information is to be displayed.
> These options are not available in conjunction with the keywords statistics or service-option statistics.
> all | callid call_id | msid ms_id | peer-address peer_ip_address | username user_name
> all: indicates all R-P information is to be displayed.
> callid call_id: indicates the information only for calls with Id call_id are to be displayed. call_id must be specified as a 4-digit hexadecimal number.
> msid ms_id: specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> peer-address peer_ip_address: specifies the peer IP address, of the PCF, for which R-P information is to be displayed. peer_ip_address must be specified using IPv4 dotted-decimal notation.
> username user_name: specifies a user only for which R-P information is to be displayed where the user is specified as user_name.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the R-P interface statistics for the current context.
> Example
> The following displays the summary for all connections.
> show rp summary all
> The following outputs the R-P interface detailed information for the user user1.
> show rp full username isp1user1
> The following command displays the standard information for the call with ID FF0E11CD.
> show rp callid ff0e11cd
> The following displays the statistics summary for the R-P facility.
> show rp
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show rp service-option
> Displays the radio-packet (R-P) service option statistics using the filtering options specified.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rp service-option statistics [ number svc_option_num | pdsn-service pdsn_name ] [ | { grep grep_options | more } ]
> number svc_option_num | pdsn-service pdsn_name
> Default: display statistics for all service options numbers and associated packet data services.
> number svc_option_num: specifies the service option number for which collected statistics are to be displayed.
> pdsn-service pdsn_name: specifies the packet data service for which the collected statistics are to be displayed.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the R-P service option statistics for the current context.
> Example
> The following displays the statistics for all service options.
> show rp service-option statistics
> The following displays the statistics for service option 5.
> show rp service-option statistics number 5
> The following command displays the statistics for all service options in collected for the packet data service sampleService.
> show rp service-option statistics pdsn-service sampleService
> show rp statistics
> Displays the radio-packet (R-P) protocol statistics using the filtering options specified.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rp statistics [ hsgw-service hsgw-name | pcf-summary [ wf1 ] | pdsn-service pdsn_name | peer-address { peer_address | all } ] [ include-bcmcs ] [ verbose ] [ | { grep grep_options | more } ]
> hsgw-service hsgw_name
> hsgw-service is eHRPD Serving Gate Way service and must be followed by name of an HSGW service.
> hsgw_name is a string from 1 to 63 characters.
> pcf-summary [ wf1 ]
> pcf-summary displays a session summary of Packet Control Function (PCF) statistics.
> wf1 displays PCF statistics in wide-format number 1.
> pdsn-service pdsn_name
> pdsn_name Displays the statistics information for the specified pdsn-service. pdsn_name must be from 1 to 63 alphanumeric characters.
> peer-address { peer_address | all }

> • | peer_address:

> Displays only the statistics information for the specified peer. peer_address must be specified using IPv4 dotted-decimal notation.

> • | all:

> Displays the statistics information for the all peers. peer_address must be specified using IPv4 dotted-decimal notation.
> verbose
> Displays more detailed statistics.
> | {grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the R-P statistics for the current context.
> Example
> The following displays all collected R-P statistics.
> show rp statistics
> The following displays the R-P statistics associated with the peer address 1.2.3.4.
> show rp statistics peer-address 1.2.3.4
> The following command displays the R-P statistics for the packet data service PCFnet.
> show rp statistics pdsn-service PCFnet
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show rsvp counters
> Displays Resource Reservation Protocol (RSVP) counters using the filtering options specified.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rsvp counters [ all | callid call_id | msid ms_id | username user_name ]
> all | callid call_id | msid ms_id | username user_name
> all: indicates all RSVP information is to be displayed.
> callid call_id: indicates the information only for calls with Id call_id are to be displayed. call_id must be specified as a 4-digit hexadecimal number.
> msid ms_id: specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> username user_name: specifies a user only for which RSVP information is to be displayed where the user is specified as user_name.
> Usage
> View the RSVP counters for the current context.
> Example
> The following displays all collected rsvp counters.
> show rsvp counters all
> show rsvp statistics
> Displays the Resource Reservation Protocol (RSVP) statistics using the filtering options specified.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show rsvp counters [ pdsn-service service | sessmgr instance instance ]
> pdsn-service service | sessmgr instance instance
> pdsn-service service: indicates the statistical information is to be displayed for the specified service. pdsn_name must be from 1 to 63 alphanumeric characters.
> sessmgr instance instance: indicates the session manager instance.
> Usage
> View the RSVP statistics for the current context.
> Example
> The following displays collected rsvp statistics for a sampleService.
> show rsvp statistics pdsn-service sampleService
> show sccp-network
> This command displays SS7 Signaling Connection Control Part (SCCP) network configuration and status information.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show sccp-network { ntwk_index | all } [ status [ all | dpc ] ]
> ntwk_index
> Display configuration and status information for the SSCP network configuration with the specified network index.
> ntwk_index must be an integer from 1 through 12.
> all
> Display all available configuration and status information for all SSCP networks.
> status all
> Display all status information for specified SCCP networks.
> status dpc
> Display status information for the device in the SCCP network identified by the destination point-code (DPC).
> Usage
> Use this command to display global SCCP statistics or to display SCCP statistics for a specified service or network.
> Example
> The following command displays global SCCP statistics:
> show sccp-network all
> The following command displays information for an SCCP network configuration with the network index of 1:
> show sccp-network 1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sccp statistics
> This command displays SS7 Signaling Connection Control Part (SCCP) statistics for services that use the SCCP protocol.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sccp statistics [ iups-service iups_srvc_name | map-service map_srvc_name | sccp-network ntwk_index [ dpc dpc [ ssn ssn ] | global-title-translation { address-map instance add_map_inst | association instance assoc_inst } [ sessmgr instance sessmgr_inst ] ] [ | { grep grep_options | more } ]
> iups-service iups_srvc_name
> Display SCCP protocol statistics for the specified IuPS service in the current context.iups_name must be the name of a configured Iu-PS service from 1 through 63 characters.
> map-service map_srvc_name
> Display SCCP protocol statistics for the specified Mobile Application Part (MAP) service in the current context. map_srvc_name must be the name of a configured MAP service and must be an alphanumeric string of from 1 through 63 characters.
> sccp-network ntwk_index
> Display SCCP protocol statistics for the SSCP network configuration with the specified network index. ntwk_index must be an integer from 1 through 12.
> The following filters can be added to fine tune the display of SCCP network statistics:

> • | dpc dpc: Enter a standard pointcode address to limit the display of SCCP network statistics to those for the identified DPC.

> • | ssn ssn: Enter an integer from 1 to 255 to limit the display of SCCP network statistics to those for the identified subsystem number.

> • | global-title-translation address-map instance add_map_inst: Enter an integer from 1 to 4096 to limit the display of SCCP network statistics to those for the identified GTT address-map.

> • | global-title-translation association instance assoc_inst: Enter an integer from 1 to 16 to limit the display of SCCP network statistics to those for the identified GTT association.

> • | sessmgr instance sessmgr_inst: Enter an integer from 1 to 384 to limit the display of SCCP network statistics to those for the identified session manager.

> Usage
> Use this command to display global SCCP statistics or to display SCCP statistics for a specified service or SCCP network.
> Example
> The following command displays global SCCP statistics:
> show sccp statistics
> The following command displays SCCP statistics for the IuPS service named iups-serv1:
> show sccp statistics iups-service iups-serv1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sctp-param-template
> Displays configuration information for Stream Control Transmission Protocol (SCTP) parameter templates configured on this system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show sctp-param-template { all | name template_name } [ | { grep grep_options | more } ]
> all
> Displays configuration information for all SCTP parameter templates configured on this system.
> name template_name
> Displays configuration information for a specific SCTP parameter template configured on this system. template_name must be an existing SCTP parameter template from 1 to 63 alphanumeric characters.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified. For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in the CLI Overview chapter.
> Usage
> Use this command to view configuration information for SCTP parameter templates on this system.
> Example
> The following command displays configured parameters for an SCTP parameter template named sctp_pt3:
> show sctp-param-template name sctp_pt3
> show session counters historical
> Displays historical information for session-related counters based on data collected in bulk statistics.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show session counters historical { all | arrived | callops | connected | disconnected | failed | handoff | rejected | renewal } [ all-intervals | recent-intervals ] [ cumulative | incremental ] [ graph | table ]
> all
> Displays data for all counters either as a single, wide table or as multiple graphs.
> arrived
> Displays only data for “total calls arrived” counters. This is based on the “sess-ttlarrived” statistic in the system schema.
> callops
> Displays data for all call operations. This is a calculated value based on the following formula:
> (arrived + rejected + disconnected + failed + handoffs + renewals)
> connected
> Displays only data for “total calls connected” counters. This is based on the “sess-ttlconnected” statistic in the system schema.
> disconnected
> Displays only data for “total calls disconnected” counters. This is based on the “sess-ttldisconn” statistic in the system schema.
> failed
> Displays only data for “total calls failed” counters. This is based on the “sess-ttlfailed” statistic in the system schema.
> handoff
> Displays only data for “total handoffs” counters. This is based on the “sess-ttlhandoff” statistic in the system schema.
> rejected
> Displays only data for “total calls rejected” counters. This is based on the “sess-ttlrejected” statistic in the system schema.
> renewal
> Displays only data for “total renewal” counters. This is based on the “sess-ttlrenewal” statistic in the system schema.
> all-intervals
> Displays all available historical information from all samples. This this filter is used by default.
> recent-intervals
> Displays historical information for only recent samples.
> cumulative
> Displays total data for all samples up to and including the last one. In this view, values increase over time.
> incremental
> Displays data changes for each specific sample. The data for each sample is the amount of change since the previous sample. This filter is used by default.
> graph
> Displays data in graphical form.
> table
> Displays data in tabular form. This is the default view.
> Usage
> This command provides the ability to track key session-related statistic information over time. This information can be used as part of system performance monitoring and capacity planning.
> Important: The information provided in the output of this command requires that bulk statistics funtionality be enabled on the system. Refer to the System Administration Guide for more information on configuring/enabling bulk statistics support.
> The output of this command displays historical data collected at various sample intervals. The interval length is 15 minutes and is not user-configurable. Up to 192 samples (2 days’ worth of data) are maintained.
> Important: Data collection is “best-effort” over these intervals. Data is preserved on system management card switchovers. As with all counters, certain session failures can cause inaccuracies with counters, including counters which appear to go backwards.
> Each sample is identified by a timestamp that displays the approximate time the data was gathered. It is in the format YYYY:MM:DD:hh:mm:ss.
> Data acquired during the sample may be marked with an “S” appended to the end of the timestamp or to the counter value. The “S” indicates that the data is suspect (potentially bad). Occurrences of this result from events like changes to the real time clock, which can cause an interval to be an atypical length. Instances of suspect data should be rare. Additionally, there may be occasions in which a sample may be marked as “invalid”. “invalid” identifies bad data, a situation that could result when the polling has not run long enough, or because of an unexpected error retrieving data.
> Since baseline values must be obtained prior to collecting interval samples, the first interval of data will not be available until up to twice the interval period.
> Example
> The following command displays cumulative total calls arrived information for the most recent intervals and displays the output in graphical format:
> show session counters historical arrived recent-intervals cummulative graph
> The following command displays historical data for all counters for all intervals and displays the output in tabular format:
> show session counters historical all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show session counters pcf-summary
> Displays the Packet Control Function (PCF) summary which include the number of calls, call types, and Tx/Rx packets/octets statistics.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show session counters pcf-summary [ call-types | data | wf1 [ pcf pcf_address | [ | { grep grep_options | more } ] ] ]
> call-types
> Displays the number of calls and the types of calls.
> data
> Displays the number of successful calls and Tx/Rx packets/octets statistics.
> pcf pcf_address
> Displays the given PCF summary for a particular address.
> wf1
> Displays the PCF summary in a single very wide line.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display a summary of all PCFs.
> Example
> show session counters pcf-summary
> show session disconnect-reasons
> Displays a list of the reasons for call disconnects and the number of calls disconnected for each reason.
> Product
> All
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show session disconnect-reasons [ gprs-only | sgsn-only | mme-only | verbose ] [ | { grep grep_options | more } ] ]
> gprs-only
> Only supported on the SGSN.
> This keyword limits the display to session disconnect reasons for the SGSN’s 2G MM and PDP context disconnects.
> sgsn-only
> Only supported on the SGSN.
> This keyword limits the display to session disconnect reasons for the SGSN’s 3G MM and PDP context disconnects.
> mme-only
> This keyword filters to the list of the session disconnect reasons for MME call disconnects.
> verbose
> List all disconnect reasons even if the values are zero (0).
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference .
> Usage
> Use this command to display a list of the reasons why calls were disconnected.
> Example
> To view session disconnect statistics, enter the following command:
> show session disconnect-reasons
> To view a list of the disconnect reasons with verbose output, enter the following command:
> show session disconnect-reasons verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show session duration
> Displays session duration information for the current context filtered by the options specified.
> Product
> All
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show session duration [ session_filter ] [ | { grep grep_options | more } ]
> session_filter
> Indicates name of the sessions/services/AGWs whose session duration information is to be filtered and displayed. This consist of following:

> • | asn-peer-address ip_address: Indicates that only the session information for the ASN GW peer whose IP address is specified by ip_address is to be displayed. ip_address must be specified using IPv4 dotted-decimal notation.

> • | asngw-service service_name: Indicates that only the session information for the ASN GW service whose name is specified by service_name is to be displayed.

> • | asnpc-peer-address ip_address: Indicates that only the session information for the Access Service Network Paging Controller (ASN PC) peer whose IP address is specified by ip_address is to be displayed. ip_address must be specified using IPv4 dotted-decimal notation.

> • | asnpc-service service_name: Indicates that only the session information for the ASN PC service whose name is specified by service_name is to be displayed.

> • | apn apn_name: Indicates that only session information for the specified Access Point Name (APN) will be displayed. apn_name specifies the name of a configured APN that can be from 1 to 63 alphanumeric characters and is case sensitive.

> • | cscf-service service_name:Indicates that only session information for the specified Call Session Control Function (CSCF) service will be displayed. service_name must be an existing CSCF service from 1 to 63 alphanumeric characters.

> Important: CSCF SIP calls under progress only. Registrations will not be considered a call.

> • | dhcp-server dhcp_address: Indicates that only session information for the specified Dynamic Host Configuration Protocol (DHCP) server will be displayed. dhcp_address is the name of the DHCP server and must be expressed in IPv4 dotted-decimal notation.

> • | fa fa_address: Indicates only the session information for the foreign agent (FA) whose IP address is specified by fa_address is to be displayed. fa_address must be specified using IPv4 dotted-decimal notation.

> • | fa-service fa_name: Indicates only the session information for the foreign agent service specified by fa_name is to have information displayed.

> • | ggsn-service ggsn_name: Indicates that only session information for the specified GGSN service will be displayed. ggsn_name specifies the name of a configured GGSN service that can be from 1 to 63 alphanumeric characters and is case sensitive.

> • | gprs-only: Limits the display to the session information for the SGSN’s 2G MM and PDP contexts.

> • | ha ha_address: Indicates only the session information for the home agent whose IP address is specified by ha_address is to be displayed. ha_address must be specified using IPv4 dotted-decimal notation.

> • | ha-service ha_name: Indicates only the session information for the home agent (HA) service specified by ha_name is to be displayed.

> • | hnbgw-only: Indicates only the session information for the HNB-GW service related sessions instances (such as HNB, IuPS, IuCS) to be displayed.

> • | hsgw-service service_name: Indicates only the session information for the HSGW service specified by the service_name is to be displayed. service_name must be an existing HSGW service from 1 to 63 alphanumeric characters.

> • | lma-service service_name: Indicates only the session information for the Local Mobility Anchor (LMA) service specified by the service_name is to be displayed. service_name must be an existing LMA service from 1 to 63 alphanumeric characters.

> • | mme-service service_name: Indicates only the session information for the Mobility Management Entity (MME) service specified by the service_name is to be displayed. service_name must be an existing MME service from 1 to 63 alphanumeric characters.

> • | mag-service service_name: Indicates only the session information for the Mobile Access Gateway (MAG) service specified by the service_name is to be displayed. service_name must be an existing MAG service and be from 1 to 63 alphanumeric characters.

> • | pcf pcf_address: Indicates only the session information for the packet control function with IP address pcf_address is to be displayed. pcf_address must be specified usingIPv4 dotted-decimal notation.

> • | pdsn-service pdsn_name: Indicates only the session information for the packet data service specified by pdsn_name is to have information displayed.

> Important: If no PCF address or PDSN service is specified the session information for all sessions is displayed.

> • | sgsn-address sgsn-address: Indicates that only session information for the specified SGSN will be displayed. sgsn_address is the IP address of the SGSN and must be expressed in dotted decimal notation.

> • | sgsn-only: Limits the display to the session information for the SGSN’s 3G MM and PDP contexts.

> • | sgw-service service_name: Indicates only the session information for the S-GW service specified by the service_name is to be displayed. service_name must be an existing S-GW service and be from 1 to 63 alphanumeric characters.

> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the session information to troubleshooting subscriber problems and for general monitoring for orphaned sessions.
> Example
> The following commands display the duration for the session connected to the packet control function with address 1.2.3.4, packet data service sampleService, and for all sessions, respectively.
> show session duration pcf 1.2.3.4
> show session duration pdsn-service sampleService
> show session duration
> show session progress
> Displays session progress information for the current context filtered by the options specified.
> Product
> All
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show session progress [ asn-peer-address ip_address | asngw-service service_name | asnpc-service service_name | asnpc-peer-address ip_address | apn apn_name | cscf-service service_name | dhcp-server dhcp_address | fa fa_address | fa-service fa_name | ggsn-service ggsn_name | ha ha_adress | ha-service ha_name | hsgw-servie service_name | lma-service service_name | mag-service service_name | mme-address mme_address | pcf { pcf_address | all } | pdsn-service pdsn_name | pdsnclosedrp-service | pgw-address ip_address | sgsn-address sgsn_address | sgw-service service_name ] [ | { grep grep_options | more } ]
> progress [ asn-peer-address ip_address | asngw-service service_name | asnpc-service service_name | asnpc-peer-address ip_address | apn apn_name | cscf-service service_name | dhcp-server dhcp_address | fa fa_address | fa-service fa_name | ggsn-service ggsn_name | ha ha_adress | ha-service ha_name | hsgw-servie service_name | lma-service service_name | mag-service service_name | mme-address mme_address | pcf { pcf_address | all } | pdsn-service pdsn_name | pdsnclosedrp-service | pgw-address ip_address | sgsn-address sgsn_address | sgw-service service_name ]
> progress: indicates session progress information is to be displayed.

> • | asn-peer-address ip_address: Indicates that only the session information for the Access Service network-Gateway (ASN-GW) peer whose IP address specified by ip_address is to be displayed. ip_address must be specified using IPv4 dotted-decimal notation.

> • | asngw-service service_name: Indicates that only the session information for the ASN-GW service whose name is specified by service_name is to be displayed.

> • | asnpc-service service_name: Indicates that only the session information for the Access Service Network Paging Conntroller (ASN PC) service whose name is specified by service_name is to be displayed.

> • | asnpc-peer-address ip_address: Indicates that only the session information for the ASN PC peer whose IP address specified by ip_address is to be displayed. ip_address must be specified using IPv4 dotted-decimal notation.

> • | apn apn_name: Indicates that only session information for the specified Access Point Name (APN) will be displayed. apn_name specifies the name of a configured APN that can be from 1 to 63 alphanumeric characters and is case sensitive.

> • | cscf-service service_name:Indicates that only session information for the specified Call Session Control Function (CSCF) service will be displayed. service_name must be an existing CSCF service from 1 to 63 alphanumeric characters.

> Important: CSCF SIP calls under progress only. Registrations will not be considered a call.

> • | dhcp-server dhcp_address: Indicates that only session information for the specified Dynamic Host Configuration Protocol (DHCP) server will be displayed. dhcp_address is the name or IP address (IPv4 dotted-decimal notation) of the DHCP server.

> • | fa fa_address: indicates only the session information for the foreign agent (FA) whose IP address is specified by fa_address is to be displayed. fa_address must be specified using IPv4 dotted-decimal notation.

> • | fa-service fa_name: indicates only the session information for the foreign agent (FA) service specified by fa_name is to have information displayed.

> • | ggsn-service ggsn_name: Indicates that only session information for the specified GGSN service will be displayed. ggsn_name specifies the name of a configured GGSN service that can be from 1 to 63 alphanumeric characters and is case sensitive.

> • | ha ha_adress: indicates only the session information for the home agent (HA) whose IP address is specified by ha_address is to be displayed. ha_address must be specified using IPv4 dotted-decimal notation.

> • | ha-service ha_name: indicates only the session information for the home agent service specified by ha_name is to have information displayed.

> • | hsgw-service service_name: Indicates only the session progress information for the HSGW service specified by the service_name is to be displayed. service_name must be an existing HSGW service and be from 1 to 63 alphanumeric characters.

> • | lma-service service_name: Indicates only the session progress information for the Local Mobility Anchor (LMA) service specified by the service_name is to be displayed. service_name must be an existing LMA service and be from 1 to 63 alphanumeric characters.

> • | mag-service service_name: Indicates only the session progress information for the Mobile Access Gateway (MAG) service specified by the service_name is to be displayed. service_name must be an existing MAG service and be from 1 to 63 alphanumeric characters.

> • | mme-address mme_address: Indicates only the session information for the foreign agent (FA) whose IP address is specified by mme_address is to be displayed. mme_address must be specified using IPv4 dotted-decimal notation.

> • | pcf pcf_address: Indicates only the session information for the packet control function with IP address pcf_address is to be displayed. pcf_address must be specified using IPv4 dotted-decimal notation.

> • | pcf all: indicates the session information for the packet control function for all PCF addresses.

> • | pdsn-service pdsn_name: indicates only the session information for the packet data service specified by pdsn_name is to be displayed.

> Important: If no PCF address or PDSN service is specified the session information for all sessions is displayed.

> • | pgw-address ip_address: Indicates only session progress information for the P-GW with an IP address specified by ip_address is to be displayed. ip_address must be specified using IPv4 dotted-decimal notation.

> • | sgsn-address sgsn-address: Indicates that only session information for the specified SGSN will be displayed. sgsn_address is the IP address of the SGSN and expressed in IPv4 dotted-decimal notation.

> • | sgw-service service_name: Indicates only the session progress information for the S-GW service specified by the service_name is to be displayed. service_name must be an existing S-GW service from 1 to 63 alphanumeric characters.

> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the session information to troubleshooting subscriber problems and for general monitoring for orphaned sessions.
> Example
> The following commands display the status information for the session connected to the packet control function with address 1.2.3.4, packet data service sampleService, and for all sessions, respectively.
> show session progress pcf 1.2.3.4
> show session progress pdsn-service sampleService
> show session progress
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show session recovery status
> Displays session recovery status information for the current context filtered by the options specified.
> Product
> All
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show session recovery status [ verbose ] [ | { grep grep_options | more } ]
> recovery status
> Displays the current status of the system’s ability to recover from a hardware or software fault that requires the recovery of home agent-based Mobile IP session(s).
> verbose
> Includes per-CPU Session Recovery status.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the session information for troubleshooting subscriber problems and for general monitoring for orphaned sessions.
> Example
> To display the session recovery status information, enter the following command:
> show session recovery status
> Adding the optional verbose keyword to this command provides more details.
> show session recovery status verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show session setuptime
> Displays session setup time information for all sessions or sessions associated with the specified Access Gateway (AGW).
> Product
> All
> Privilege
> Operator
> Syntax
> show session setuptime [ hnbgw-only | pcf pcf_address | gprs-only | sgsn-address sgsn_address| sgsn-only ] [ | { grep grep_options | more } ]
> [ hnbgw-only | mme-only | pcf pcf_address | gprs-only | sgsn-address sgsn_address | sgsn-only ]
> Displays the call setup times aggregated into basic ranges of time.

> • | hnbgw-only: Filters and displays the call setup information for HNB-GW calls only.

> • | pcf pcf_address: displays call setup data for the packet control function whose IP address is specified as pcf_address. pcf_address must be specified using IPv4 dotted-decimal notation. The call setup times for all PCFs is displayed when no specified PCF is specified.

> • | gprs-only: Displays 2G call setup data for the for the SGSN for the MM and PDP contexts.

> • | sgsn-address sgsn_address: Displays call setup times for the specified SGSN. sgsn_address is the IP address of the SGSN and must be expressed in IPv4 dotted-decimal notation. This keyword is used by the GGSN.

> • | sgsn-only: Displays 3G call setup data for the for the SGSN for the MM and PDP contexts.

> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View the session information to troubleshooting subscriber problems and for general monitoring for orphaned sessions.
> When no keywords are specified, the information shown is cumulative for all sessions that have been facilitated by the system.
> Example
> The following command shows setup time statistics for all sessions from the PCF at IP address 192.168.10.3:
> show session setuptime pcf 192.168.10.3
> show session subsystem
> Displays session information for system subsystems. If no keywords are specified, information for all subsystems is displayed.
> Product
> All
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show session subsystem [ full | facility facility [ all | instance id ] ] [ verbose ] [ | { grep grep_options | more }]
> [ full | facility facility [ all | instance id ] ]

> • | full: Indicates that a full statistics summary of all subsystems is to be displayed.

> • | facility facility: Specifies the facility for which subsystem statistics is to be displayed where facility is specified as one of:

> • | a11mgr: A11 Manager

> • | aaamgr: Accounting and Authentication Manager

> • | aaaproxy: AAA Proxy Manager

> • | asngwmgr: ASN Gateway Manager

> • | asnpcmgr: ASN Paging/Location-Registry Manager

> • | cscfmgr: SIP CSCF Manager

> • | dgmbmgr: Diameter Gmb Application Manager

> • | diamproxy: Diameter Proxy Application Manager

> • | egtpegmgr: EGTP Egress Demux Manager

> • | egtpinmgr: EGTP Ingress Demux Manager

> • | famgr: Foreign Agent Manager

> • | gtpumgr: GTPUMGR Demux Manager

> • | gtpcmgr: GTPC Manager

> • | hamgr: Home Agent Manager

> • | hnbmgr: HNBGW HNB Manager

> • | imsimgr: SGSN IMSI Manager

> • | ipsgmgr: IP Services Gateway Manager

> • | l2tpdemux: L2TP Demux Manager

> • | l2tpmgr: L2TP Manager

> • | linkmgr: SGSN/SS7 Master Manager

> • | magmgr: Mobile Access Gateway Manager

> • | megadiammgr: Mega Diameter Manager

> • | mmedemux: MME Demux Manager logging facility

> • | mmemgr: MME Manager logging facility

> • | mmgr: SGSN/SS7 Master Manager

> • | phsgwmgr: PHS Gateway Manager

> • | phspcmgr: PHS Paging Controller Manager

> • | sessmgr: Session Manager

> • | sgtpcmgr: SGSN GTPC Manager

> • | all | instance id: the keyword all indicates all instances of the specified facility are to be displayed whereas the keyword instance specifies a specific instance for which information is to be displayed where id must be specified as an instance ID in the range 0 through 4294967295. If all or instance is not specified summary statistics are displayed.

> verbose
> Displays everything the show session subsystem command displays with the exception that the Setup Time statistics are reported in 100 millisecond increments from <100 ms up to 9600 ms.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> View the session information to troubleshooting subscriber problems and for general monitoring for orphaned sessions.
> If this command is entered with no keywords, the information displayed is cumulative for all sessions facilitated by the system.
> Example
> The following commands display the statistics information summarized for all sessions, then for the famgr facility (all sessions), and finally only for the session ID 127589 for the hamgr subsystem.
> show session subsystem full
> show session subsystem facility a11mgr all
> show session subsystem facility aaamgr all
> show session subsystem facility asngwmgr all
> show session subsystem facility famgr all
> show session subsystem facility hamgr all
> show session subsystem facility sessmgr all
> show session subsystem facility aaaproxy all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show session trace
> Displays status and statistics for the session trace application.
> Product
> GGSN, MME, P-GW, S-GW
> Privilege
> Inspector
> Syntax
> show session trace { statistics | subscriber network-element { ggsn | mme | pgw | sgw } trace-ref value | tce-address ip_address tce-index num | tce-summary | trace-summary } [ | { grep grep_options | more } ]
> statistics
> Displays summary statistics for the session trace subsystem.
> subscriber network-element { ggsn | mme | pgw | sgw } trace-ref value
> Displays status and statistics for a specified session trace using the network element type; GGSN, MME, P-GW, and S-GW, and the trace reference. value must be a valid trace reference of 12 characters.
> tce-address ip_address tce-index num
> Displays status and statistics for a specified Trace Collection Entity (TCE) connection. ip_address must be a valid existing collection entity IPv4 address in dotted-decimal notation.
> tce-summary
> Displays a summary of all active TCE connections.
> trace-summary
> Displays a summary of all active session traces.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display status and statistics for the session trace application.
> Example
> The following command displays status and statistics for a subscriber session trace on a P-GW with a trace reference of 32223398765:
> show session trace subscriber network-element pgw trace-ref 32223398765
> The following command displays status and statistics for a subscriber session trace on an MME with a trace reference of 32221234567:
> show session trace subscriber network-element mme trace-ref 32223398765
> The following command displays status and statistics for a subscriber session trace on an GGSN with a trace reference of 1203398765:
> show session trace subscriber network-element ggsn trace-ref 1203398765
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sgs-service
> Displays information and statistics about Visitor Location Register (VLR) SGs interface services configured on this system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show sgs-service { all | name name | statistics { all | name name } | vlr-status [ service-name name ] [ vlr-name name ] [ full ]
> all
> Displays information about all SGs interface services configured on this system.
> name name
> Displays information about a specific SGs service configured on this system. name must be an existing SGs service from 1 to 63 alphanumeric characters.
> statistics { all | name name }
> Displays statistics for SGs services configured on this system.
> all: Displays statistics for al SGs services configured on this system.
> name name: Displays statistics for a specific SGs service configured on this system.name must be an existing SGs service and be from 1 to 63 alphanumeric characters.
> vlr-status [ service-name name ] [ vlr-name name ] [ full ]
> Displays status information about VLRs configured in SGs services on this system.
> service-name name: Displays names and states of VLRs configured in a specific SGs service on this system. name must be an existing SGs service and be from 1 to 63 alphanumeric characters.
> vlr-name name: Displays the name and state of a specific VLR configured in SGs services on this system. name must be an existing VLR name from 1 to 63 alphanumeric characters.
> full: Displays additional information about VLRs configured in SGs services on this system. Additional information includes ports, addresses and peer IDs.
> Usage
> Use this command to display information and statistics about SGs services configured on this system.
> Example
> The following command displays statistics for an SGs service named sgs3:
> show sgs-service name sgs3
> The following command displays VLR status information for a configured VLR named vlr-main:
> show sgs-service vlr-status vlr-name vlr-main
> show sgsn-operator-policy
> This command has been deprecated. Refer to the show operator-policy command.
> show sgsn
> This command displays session manager (SessMGR) statistics specific to the SGSN service.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sgsn sessmgr { all | instance smgr_inst }
> all
> Displays all SessMGR statistics specific to the system’s SGSN services.
> instance smgr_inst
> Displays the statistics for a specific session manager instance of the SGSN service.
> smgr_inst must be an integer between 1 and 10000000.
> Usage
> Use this command to display information for SGSN services.
> Example
> The following command displays SGSN SessMGR statistics for all SGSN services on the system:
> show sgsn sessmgr all
> show sgsn-fast-path
> This command displays information related to SGSN fast-path.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sgsn-fast-path statistics [ all | smgr-instance smgr_inst ] [ | { grep grep_options | more } ]
> all
> Displays fast-path statistics for all session managers.
> smgr-instance smgr_inst
> Displays the fast-path statistics for a specific session manager instance.
> smgr_inst must be an integer between 1 and 65535.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display statistics for SGSN fast-path configurations.
> Example
> The following command displays fast-path statistics for all SGSN session managers :
> show sgsn sessmgr all
> show sgsn-map-app
> This command displays collected statistics for the SGSN Mobile Application Part (MAP).
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sgsn-map-app statistics [ | { grep grep_options | more } ]
> all
> Displays collected statistics for the SGSN MAP application.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display statistics for the SGSN MAP application.
> Example
> The following command displays SGSN MAP statistics :
> show sgsn-map-app statistics
> show sgsn-mode
> This command displays the SGSN global configuration.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sgsn-mode[ | { grep grep_options | more } ]
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display the configuration created with the commands in the SGSN global configuration mode.
> Example
> The following command displays the SGSN global configuration:
> show sgsn-mode
> show sgsn-pool
> This command displays collected pooling statistics for either GPRS services or SGSN services.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sgsn-pool statistics { gprs-service srvc_name | sgsn-service srvc_name} { nri-value nri_value | peer-non-broadcast-lac lac rac rac | target-load-in-progress [ smgr-instance smgr_instance | target-nri target_nri ] | target-offloaded-to-peer [ target-nri target_nri ] } [ | { grep grep_options | more } ]
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display the collected statistics for pooling in either GPRS or SGSN services. The outputs can be filtered to focus the statistics displayed.
> Example
> The following command displays the :
> show sgsn-pool statistics sgsn-service sgsn1 nri-value 3
> show sgsn-service
> This command displays information about the configured SGSN services in the current context.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sgsn-servie { all | name srvc_name }
> all
> Displays information for all SGSN services in the current context.
> name srvc_name
> Displays information for the specified SGSN service in the current context. srvc_name must be the name of a configured SGSN service and must be an alphanumeric string from 1 to 63 characters.
> Usage
> Use this command to display information for SGSN services.
> Example
> The following command displays information for all SGSN services in the current context:
> show sgsn-service all
> The following command displays information for an SGSN service in the current context that is named sgsn1:
> show sgsn-service name sgsn1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sgtp-service
> This command displays information about the configured SGSN GPRS Tunnelling Protocol (SGTP) services in the current context, including GTP-C and GTP-U operational configuration.
> Product
> SGSN
> PDG/TTG
> MME
> Privilege
> Inspector
> Syntax
> show sgtp-service { all [ gtpu-table ] | ggsn-table [ smgr-instance smgr_instance ] | mbms-bearers | name srvc_name [ gtpu-table ] | sgsn-table }
> all [ gtpu-table ]
> Displays configuration information for all of the SGTP services defined for the current context.
> gtpu-table applies a filter to limit the output to GTPU information for all SGTP services.
> ggsn-table [ smgr-instance srvc_name ]
> Displays GGSN information configured for the SGTP service(s) in the current context.
> smgr-instance srvc_name enter an integer from 1 to 384 to limit the GGSN output to information for a specific session manager.
> mbms-bearers
> This keyword is specific to the SGSN and is not yet supported.
> name srvc_name [ gtpu-table ]
> Displays information for the specified SGTP service in the current context. srvc_name must be an alphanumeric string from 1 to 63 characters in length that identifies a configured SGTP service.
> gtpu-table applies a filter to limit the output to GTPU information for a specific SGTP service.
> sgsn-table
> Displays SGSN information configured for the SGTP service(s) in the current context.
> Usage
> Use this command to control the display of SGTP services information.
> Example
> The following command displays information for all SGTP services in the current context:
> show sgtp-service all
> The following command displays the GGSN information in SGTP services in the current context:
> show sgtp-service ggsn-table
> The following command displays the SGSN information in SGTP services in the current context:
> show sgtp-service sgsn-table
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sgtpc statistics
> This command displays all statistics, for SGSN GPRS Tunnelling Protocol (SGTP) interface parameters, collected since the last restart or last use of a clear command.
> Product
> SGSN
> PDG/TTG
> MME
> Privilege
> Inspector
> Syntax
> show sgtpc statistics [ all | gsn-address ipv4_address | sgtp-service sgtp_srvc_name ] [ verbose ][ | { grep grep_options | more } ]
> all
> Displays configuration information for all of the SGTP services defined for the current context.
> gsn-address ipv4_address
> ipv4_address Displays statistics for a specific SGSN identified by its IP address expressed in IPv4 dotted-decimal notation.
> Note this must be an existing and active interface.
> sgtp-service sgtp_srvc_name
> Displays statistics for the specified SGTP service in the current context.
> sgtp_srvc_name must be the name of a previously configured and active SGTP service and must be an alphanumeric string from 1 to 63 characters.
> verbose
> Causes the system to displays more detailed level of statistics.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display information for SGSN services.
> Example
> The following command displays statistics for the SGTP service named sgtp1:
> show sgtpc statistics sgtp-service sgtp1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sgtpu statistics
> This command displays all transmission and reception statistics for pre-defined and active GTP-U interfaces collected since the last restart or last use of a clear command.
> Product
> SGSN
> PDG/TTG
> Privilege
> Inspector
> Syntax
> show sgtpu statistics [ ggsn-address ipv4_address | gprs-service gprs_srvc_name nsei nse_id | iups-bind-address ipv4_address| iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name ][ | { grep grep_options | more } ]
> ggsn-address ipv4_address
> ipv4_address enter the IP adddress of a GGSN in IPv4 dotted-decimal to display statistics for that specific GGSN.
> gprs-service gprs_srvc_name nsei nse_id
> Displays NSEI-based GTPU statistics associated with the specified GPRS service in the current context.
> gprs_srvc_name must be the name of a previously configured and active GPRS service and must be an alphanumeric string from 1 to 63 characters.
> nse_id must be an integer from 0 to 65535.
> iups-bind-address ipv4_address
> ipv4_address enter the IP addresz of a specific Iu GTPU interface in IPv4 dotted-decimal notation as a filter for the SGSN GPRS Tunnelling Protocol (SGTP) statistics.
> iups-service iups_srvc_name
> Displays statistics for the specified IuPS service in the current context.
> iups_srvc_name must be the name of a previously configured and active IuPS service and must be an alphanumeric string from 1 to 63 characters.
> rnc-address ipv4_address
> ipv4_address Displays statistics for a specific Radio Network Controller (RNC) identified by its IP address expressed in IPv4 dotted-decimal notation.
> sgtp-service sgtp_srvc_name
> Displays statistics for the specified SGTP service in the current context.
> sgtp_srvc_name must be the name of a previously configured and active SGTP service and must be an alphanumeric string from 1 to 63 characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating the Command Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display statistics for the SGTPU interface.
> Example
> The following command displays GPTP-U statistics for the traffic between an SGSN and a connected RNC.
> show sgtpu statistics rnc-address 123.1.2.3
> show sgw-service
> Displays configuration settings and/or service statistics for Serving Gateway (S-GW) services on this system.
> Product
> S-GW
> Privilege
> Inspector
> Syntax
> show sgw-service { all | name service_name | statistics { all | name service_name } } [ | { grep grep_options | more } ]
> all
> Displays configuration information for all S-GW services configured on this system.
> name service_name
> Displays configuration information for a specific S-GW service configured on this system.
> service_name must be an existing S-GW servicee from 1 to 63 alphanumeric characters.
> statistics { all | name service_name }
> Displays statistics for all S-GW services on this system or for a specified service. service_name must be an existing S-GW service from 1 to 63 alphanumerics characters.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to view configuration settings and/or service statistics for S-GW services on this system.
> Example
> The following command displays service statistics for the S-GW service named sgw1:
> show sgw-service statistics name sgw1
> show sms statistics
> This command displays traffic statistics for the Short Message Service (SMS).
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sms statistics [ gprs-only | sgsn-only ] [ name map_srvc ] [ verbose ] [ | { grep grep_options | more } ]
> gprs-only
> This keyword limits the display to GPRS access type SMS statistics.
> sgsn-only
> This keyword limits the display to UMTS access type SMS statistics.
> name map_srvc
> map_srvc must be a string of 1 to 63 alphanumeric characters that identifies a configured MAP service.
> verbose
> Causes the system to displays more detailed level of statistics.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display traffic statistics for the SMS services.
> Example
> Use the following command to display SMS statistics for 3G traffic:
> show sms statistics sgsn-only
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show sndcp statistics
> This command displays statistics for the packet traffic going through the Subnetwork Dependent Convergence Protocol (SNDCP) layer.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show sndcp statistics [ gprs-service srvc_name ] [ verbose ] [ | { grep grep_options | more } ]
> gprs-service srvc_name
> srvc_name must be a string of 1 to 63 alphanumeric characters that identifies a configured GPRS service.
> verbose
> Causes the system to displays more detailed level of statistics.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display SNDCP traffic statistics. Include the gprs-service keyword to filter the output to statistics for only one GPRS service.
> Example
> Use the following command to display all SNDCP layer traffic statistics:
> show sndcp statistics verbose
> Use the following command to display SNDCP layer traffic statistics for the test1 GPRS service:
> show sndcp statistics gprs-service test1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show snmp
> Displays information on the Simple Network Management Protocol (SNMP) servers and interfaces.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show snmp { accesses | communities | contexts | notifies | server | transports | trap [ history | statistics { verbose } { wide } ] | views } [ | { grep grep_options | more } ]
> accesses
> Displays SNMP server usage statistics.
> communities
> Displays SNMP community strings.
> contexts
> Displays SNMP information per context.
> notifies
> Displays SNMP event trap and notification statistics.
> server
> Displays SNMP server configuration information.
> transports
> Displays trap destination configuration information.
> trap [ history | statistics { verbose } { wide } ]
> history: displays SNMP event trap history. trap history shows up to 5,000 time-stamped trap records stored in a buffer. The buffer may be cleared by entering the clear snmp history command.
> statistics: displays SNMP event trap and notification statistics.
> verbose: displays rows for every defined trap, even if never generated.
> wide: shows trap statistics data in excess of 80 columns.
> views
> Displays SNMP views.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Display SNMP information as part of system verification and troubleshooting.
> Example
> The following commands display the usage statistics, community string information, event trap and notification data, server information, and trap destination configuration, respectively.
> show snmp communities
> show snmp transport
> show snmp server
> show snmp accesses
> show snmp notifies
> show snmp trap history
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show srp
> Displays the Service Redundancy Protocol (SRP) information.
> Product
> All products that support Interchassis Session Recovery (ICSR)
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show srp { call-loss statistics | checkpoint statistics [ active | standby ] [ verbose ] | info | monitor [ all | authentication-probe | bgp | diameter ] | statistics } | [ grep grep_options | more ]
> call-loss statistics
> Displays history of lost calls during switchover.
> checkpoint statistics [ active | standby ] [ verbose ]
> Displays check pointing statistics on session redundancy data (session managers, current call recovery records, etc.).
> active: Displays information for active chassis.
> standby: Displays information for standby chassis.
> verbose: Displays cumulative information for all session managers in tabular output.
> info
> Displays Service Redundancy Protocol information (context, chassis state, peer, connection state, etc.).
> monitor [ all | authentication-probe | bgp | diameter ]
> Displays SRP monitor information.
> all: Displays monitor information for all types (authentication-probe, bgp, and diameter).
> authentication-probe: Displays authentication probe monitor information.
> bgp: Displays BGP monitor information.
> diameter: Displays Diameter monitor information.
> statistics
> Displays SRP statistics (hello messages sent, configuration validation, resource messages, switchovers, etc.).
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> The output of this command may be considered as part of a periodic system auditing program by verifying the Service Redundancy Protocol performance. For more information, refer to the Interchassis Session Recovery chapter of the Cisco ASR 5000 Series System Administration Guide and the Service Redundancy Protocol Configuration Mode chapter of the Command Line Interface Reference.
> Example
> The following commands show Service Redundancy Protocol information:
> show srp call-loss statistics
> show srp checkpoint statistics
> show srp info
> show srp monitor
> show srp statistics
> Important: Output descriptions for commands are available in the Cisco ASR 5000 Series Statistics and Counters Reference.
> show ss7-routing-domain
> This command displays the configuration information for the defined Signalling System #7 (SS7) routing domains. As SS7 routing domains encompass a large number of operational parameters, this command enables you to narrow your displays to specific protocol parameters on a specific link.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show ss7-routing-domain { all | ss7rd_id { m3ua | mtp2 | mtp3 | qsaal | routes [ adjacent ] | sctp asp { all | instance asp_id } | sscf } }
> show ss7-routing-domain ss7rd_id m3ua { statistics { gen | peer-server { all | id peer-server_id peer-server-process { all | instance psp_instance } } } | status { address-translation-table | destination-point-code { all | ss7_dpc } | gen | peer-server peer-server_id [ peer-server-process instance psp_id | verbose ] }
> show ss7-routing-domain 1 sscf { statistics linkset { all | id linkset_id link { all | id link_id } } | status linkset { all | id linkset_id link { all | id link_id [ verbose ] } } }
> ss7-routing-domain { all | ss7rd_id }
> Specifies whether the display will output information for all SS7 routing domains or only for a specific SS7 routing domain.
> ss7rd_id must be an integer value from 1 through 12.
> m3ua
> Provides access to statistics or status information for the SS7 MTP3 User Adaptation Layer (M3UA) in the specified SS7 routing domain.
> mtp2
> Provides access to statistics or status information for the SS7 Message Transfer Part-2 (MTP2) in the specified SS7 routing domain.
> mtp3
> Provides access to statistics or status information for the SS7 Message Transfer Part-3 (MTP3) in the specified SS7 routing domain.
> qsaal
> Provides access to statistics or status information for the Service Specific Connection-Oriented Protocol (SSCOP) sub-layer of the Quasi Signaling Application Adaptation Layer (QSAAL) in the specified SS7 routing domain.
> routes [ adjacent ]
> Displays the destination point code (DPC) routing table.
> adjacent - If this keyword is used with the routes keyword, access is provided to the statistics and status information for configured adjacent point codes.
> sctp asp { all | instance asp_id }
> Provides access to the status or statistics for the Stream Control Transmission Protocol (SCTP) application server processes (ASP) in the specified SS7 routing domain for all or a specified SCTP ASP instance.

> • | all: This keyword displays the information for all SCTP application server process instances for a specific SS7 routing domain.

> • | instance asp_id : Indicates the specific SCTP application server process instance where instance_id must be an integer from 1 through 4.

> sscf
> Provides access to the statistics or status information for the Service Specific Coordination Function (SSCF (q.2140)) in the specified SS7 routing domain.
> peer-server [ all | id peer-server_id ]
> This keyword filters the information for the specific protocol in the SS7 routing domain for all or a specific peer server ID.

> • | all: This keyword displays the information for all peer servers fora specific protocol.

> • | id peer-server_id : Indicates the specific linkset identifier where peer-server_id must be an integer from 1 through 49.

> peer-server-process [ all | instance instance_id ]
> This keyword filters the information for the specific protocol in the SS7 routing domain for all or a specific instance of peer-server process.

> • | all: This keyword displays the information for all peer server process instances for a specific protocol.

> • | instance instance_id : Indicates the specific peer server process instance where instance_id must be an integer from 1 through 4.

> destination-point-code [ all | dest_point_code]
> This keyword filters the information for the specific protocol in the SS7 routing domain for all or a specific DPC.

> • | all: This keyword displays the information for all DPCs in the SS7 routing domain.

> • | dest_point_code: Indicates the specific DPC in the SS7 routing domain.

> gen
> This keyword displays the general information for the specific protocol in the specified SS7 routing domain.
> verbose
> This keyword enables the display of maximum information for a protocol.
> linkset [ all | id linkset_id ]
> This keyword filters the information for the specific protocol in SS7 routing domain for all or a specific link set.

> • | all: This keyword displays the information for all linksets for a specific protocol.

> • | id linkset_id : Indicates the specific linkset identifier where linkset_id must be an integer from 1 through 49.

> link [ all | id link_id ]
> This keyword filters the information for a specified protocol in the SS7 routing domain for all or a specific link set.

> • | all: This keyword displays the information for all links for a specific protocol.

> • | id link_id : Indicates the specific linkset identifier where link_id must be an integer from 1 through 16.

> Usage
> Use this command to display the SS7 routing domain and different layer protocol information for SGSN service.
> Example
> The following command displays the information/statistics for all SCTP application server processes of peer server ID 17 and peer server process instance 1 in SS7 routing domain 12:
> show ss7-routing-domain 12 sctp asp all status peer-server id 17 peer-server-process instance 1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ssh key
> Displays the secure shell (SSH) public key information.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ssh key [ type { v1-rsa | v2-rsa | v2-dsa } ] [ | { grep grep_options | more } ]
> [ type { v1-rsa | v2-rsa | v2-dsa } ]
> Specifies the type of SSH key information to display. If type is not specified, information for all types is displayed.
> v1-rsa: SSH v1 RSA host key only
> v2-rsa: SSH v2 DSA host key only
> v2-dsa: SSH v2 RSA host key only
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Show the secure shell key information for all types to verify installed keys.
> Example
> The following command shows information for all SSH V1 and SSH V2 keys:
> show ssh key
> The following command shows information for only SSH V2 RSA host keys:
> show ssh key type v2-rsa
> show ssl cipher-suite
> Displays information related to Secure Sockets Layer (SSL) cipher suites since the last restart or clear command. A cipher suite contains the cryptographic algorithms supported by the client.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show ssl cipher-suite [ name name ] [ | { grep grep_options | more } ]
> name name
> Displays information related to the specified SSL cipher suite.
> name must be from 1 to 127 alphanumeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display information related to SSL cipher suites.
> Example
> The following command displays information for the SSL cipher suite ssl_cipher_suite_1:
> show ssl cipher-suite name ssl_cipher_suite_1
> show ssl connection
> Displays information pertaining to Secure Sockets Layer (SSL) connections on the Proxy Call Session Control Function (P-CSCF).
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show ssl connection [ list | summary [ service-name name ] ] [ name name ] [ | { grep grep_options | more } ]
> list
> Lists the SSL connections on the P-CSCF.
> summary
> Displays state and statistical information for the SSL connections on the P-CSCF.
> service-name name
> Lists the SSL connections on the P-CSCF for the specified P-CSCF service, or displays state and statistical information for the SSL connections on the P-CSCF for the specified P-CSCF service.
> name must be from 1 to 63 alphanumeric characters.
> name name
> Displays state and statistical information for the specified SSL connection.
> name must be from 1 to 127 alphanumeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command in Exec Mode to display information and statistics pertaining to SSL connections.
> If the summary keyword is not used, detailed information is displayed.
> Example
> The following command displays SSL connection information for the P-CSCF service pcscf_tls_1:
> show ssl connection list service-name pcscf_tls_1
> show ssl map
> Displays information related to configured Secure Sockets Layer (SSL) maps/templates since the last restart or clear command.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show ssl map [ map-type ssl-subscriber-template ] [ name name ] [ | { grep grep_options | more } ]
> map-type ssl-subscriber-template
> Displays information related to configured SSL maps/templates for the SSL map/template type ssl-subscriber-template.
> name name
> Displays information related to configured SSL maps/templates for the specified map/template name.
> name must be from 1 to 127 alphanumeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display information related to configured SSL maps/templates.
> Example
> The following command displays information related to configured SSL maps/templates for the SSL map/template ssl_template_1:
> show ssl map name ssl_template_1
> show ssl statistics
> Displays statistics for Secure Sockets Layer (SSL) since the last restart or clear command.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show ssl statistics [ service-name name ] [ | { grep grep_options | more } ]
> service-name name
> Displays SSL statistics for the specified Proxy Call Session Control Function (P-CSCF) service.
> name must be from 1 to 127 alphanumeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display SSL statistics.
> Example
> The following command displays SSL statistics for all P-CSCF services:
> show ssl statistics
> show subscribers
> Shows information for subscriber sessions defined by the specified keywords. Keywords described under Command Keywords below are base commands that display distinctive type of data. Keywords described under Filter Keywords are filters that modify or filter the output of the base commands. Not all filter keywords are available for all command keywords. Each command keyword lists the filter keywords that it accepts.
> Product
> All
> Privilege
> Security Administrator, Administrator, Inspector, Operator
> Syntax
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> command_keyword
> The following keywords are base commands that each have a distinct display output. Only one Command Keyword can entered on the command line.
> aaa-configuration
> Displays Authentication Authorization and Accounting (AAA) configuration information for subscriber sessions defined by the specified filter keywords. The following filter keywords are valid with this command:
> active, all, apn, callid, card-num, configured-idle-timeout, connected-time, dhcp-server, dormant, fa, fa-service, ggsn-service, ha, ha-service, idle-time, imsi, ip-address, ip-pool, lac, lac-service, lns, lns-service, long-duration-time-left, msid, network-requested, network-type, pcf, pdsn-service, plmn-type, rx-data, session-time-left, sgsn-address, sgsn-service, tx-data, username, verbose, grep, more
> access-flows { accounting | dynamic | pre-provisioned | static }
> Shows the ip-flows for the subscribers defined by the specified filter keywords.
> accounting: Use this keyword to display the accounting type of access flows for a subscriber.
> dynamic: Use this keyword to display the dynamic type of access flows for a subscriber.
> pre-provisioned: Use this keyword to display the pre-provisioned type of access flows for a WiMAX subscriber.
> static: Use this keyword to display the static type of access flows for a subscriber.
> The following filter keywords are valid with this command:
> active, active-charging-service, all, asngw-service, asnpc-service, asn-peer-address, apn, callid, card-num, ccoa-only, configured-idle-timeout, connected-time, dhcp-server, dormant, fa, fa-service, flow-type, ggsn-service, gsm-traffic-class, hnbgw-only, ha, ha-ipsec-only, ha-service, idle-time, imsi, ip-address, ip-pool, ipv6-address, ipv6-prefix, l3-tunnel-local-address, l3-tunnel-remote-address, lac, lac-service, lns, lns-service, long-duration-time-left, mip-udp-tunnel-only, msid, msiddn, network-requested, network-type, pcf, pdsn-service, plmn-type, rulebase, rx-data, session-time-left, sgsn-address, sgsn-service, tpo, tx-data, username, verbose, grep, more
> activity
> Display subscribers link activity percentage. When no Filter Keywords are specified, the output is a summary of all subscriber activity. When Filter Keywords are specified, the link activity percentage is displayed as graphs in which one is displayed using a high sampling rate, a 10-second interval between samples, and a low sampling rate, a 15-minute interval between samples
> The following filter keywords are valid with this command:
> active, all, asngw-service, asnpc-service, asn-peer-address, apn, callid, card-num, configured-idle-timeout, connected-time, dhcp-server, dormant, fa, fa-service, ggsn-service, ha, ha-service, idle-time, imsi, ip-address, ip-pool, lac, lac-service, lns, lns-service, long-duration-time-left, msid, network-requested, pcf, pdsn-service, plmn-type, rx-data, session-time-left, sgsn-address, sgsn-service, tpo, tx-data, username, grep, more
> asn-peer-address ip_address
> Displays information for subscribers on an ASN-GW trusted peer.
> ip_address is the IP address of the ASN-GW peer server expressed in IPv4 dotted-decimal notation.
> The following filter keywords are valid with this command:
> all, counters all, asngw-service, full, summary, grep, more
> asngw-service service_name
> Displays counters for subscribers accessing the ASN-GW service.
> service_name must be an existing service and be from 1 to 63 alphanumeric characters.
> The following filter keywords are valid with this command:
> all, counters all, full, summary, grep, more
> asnpc-service service_name
> Displays counters for subscribers accessing the ASN Paging Controller and Location Registry service.
> service_name must be an existing Access Service Network Paging Controller (ASN PC) service and be from 1 to 63 alphanumeric characters.
> The following filter keywords are valid with this command:
> all, counters all, full, summary, grep, more
> bearer-establishment { direct-tunnel | normal | pending }
> Selects Bearer Establishment type defined by the specified filter keywords.
> direct-tunnel: Select subscribers having direct tunnel establshed with the Radio Network Controller (RNC).
> normal: Select subscribers having bearer established with SGSN.
> pending: Select subscribers for whom bearer is not fully established.
> configuration
> Display current configuration for all subscribers or a specified subscriber. The following filter keywords are valid with this command:
> all, username, grep, more
> counters
> Show the counters associated with the subscriber. The following filter keywords are valid with this command:
> active, all, asngw-service, asnpc-service, asn-peer-address, apn, callid, card-num, configured-idle-timeout, connected-time, dhcp-server, dormant, fa, fa-service, ggsn-service, ha, ha-service, idle-time, imsi, ip-address, ip-pool, lac, lac-service, lns, lns-service, long-duration-time-left, msid, network-requested, network-type, pcf, pdsn-service, plmn-type, rx-data, session-time-left, sgsn-address, sgsn-service, tpo, tx-data, username, grep, more
> cscf-only
> Displays information for Call Session Control Function (CSCF) subscribers only.
> The following filter keywords are valid with this command:
> aaa-configuration, access-flows, active, activity, all, bearer-establishment, callid, card-num, configured-idle-timeout, connected-time, counters, cscf-service, data-rate, dormant, fa, full, gtp-version, ha, idle-time, ims-auth-service, imsi, ip-address, ip-alloc-method, ip-pool ipv6-address, ipv6-prefix, l3-tunnel-local-addr, l3-tunnel-remote-addr, long-duration-time-left, mipv6ha-service, msid, network-type, policy, rx-data, session-time-left, smgr-instance, subscription, summary, tft, tx-data, username, wf1
> cscf-service service_name
> Displays information for subscribers accessing the specified CSCF service.
> service_name must be an existing service and be from 1 to 63 alphanumeric characters.
> The following filter keywords are valid with this command:
> bearer-establishment, callid, card-num, configured-idle-timeout, connected-time, cscf-service, fa, gtp-version, ha, idle-time, ims-auth-service, imsi, ip-address, ip-alloc-method, ip-pool, ipv6-address, ipv6-prefix, l3-tunnel-local-addr, l3-tunnel-remote-addr, long-duration-time-left, mipv6ha-service, msid, network-type, rx-data, session-time-left, smgr-instance, subscription, tx-data, username
> css-delivery-sequence
> Important: This is a restricted keyword. In StarOS 9.0 and later, this keyword is obsoleted.
> css-service csssvc_name
> Important: This is a restricted keyword. In StarOS 9.0 and later releases, this keyword is obsolete.
> data-rate [ summary | full ] [ verbose | graph { high | low } ] [ high | low ]
> Indicates how to display subscriber throughput data.
> Important: This keyword is best used for individual subscriber output.
> summary: Combine statistics for the matching subscriber and show a summary in text form.
> full: Display a separate output for each matching subscriber separately in tabular form.
> verbose: Display cumulative information for all matching subscribers in tabular output.
> graph { high | low }: Display the throughput data as a graph using either a high sampling rate of every 30 seconds or a low sampling rate of every 15 minutes. The graph contains data points over the last 24 hours, if available. The command displays a graph each for the transmit and receive peak, average, and sustained throughput for a total of six graphs.
> high: Display the raw data collected for the throughput analysis using a high sampling rate (smaller interval). The data displayed uses a sampling interval of 30 seconds and includes the data collected over the last 24 hours, if available.
> low: Display the raw data collected for the throughput analysis using a low sampling rate (larger interval). The data displayed uses a sampling interval of 15 minutes and includes the data collected over the last 24 hours, if available.
> The following filter keywords are valid with this command:
> active, all, asngw-service, asnpc-service, asn-peer-address, apn, callid, card-num, configured-idle-timeout, connected-time, dhcp-server, dormant, fa, fa-service, ggsn-service, ha, ha-service, hnbgw-service,hsgw-only, hsgw-service, idle-time, imsi, ip-address, ip-pool, lac, lac-service, lma-service, lns, lns-service, long-duration-time-left, mag-service, mme-address, mme-service, msid, network-requested, pcf, pdsn-service, plmn-type, rx-data, session-time-left, sgsn-address, sgsn-service, tpo, tx-data, username, grep, more
> debug-info { callid id | msid id | username name }
> Displays internal call troubleshooting information for subscriber sessions defined by the specified keywords.
> callid id: Displays subscriber information for the call specified by id. The call ID must be specified as an 8-digit hexadecimal number.
> msid id: Displays information for the mobile user identified by id. id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
> username name: Displays information for connections for the subscriber identified by name. The user must have ben previously configured. name must be a sequence of characters and/or wildcard characters ('$' and '*') from 1 to 127 characters. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as wildcard enclose them in single quotes ( ‘). For example; ‘$’.
> ebi number
> Displays subscribers based on an EPS bearer identity. number specifies the EBI number and must be an integer value from 5 to 15.
> enodeb-address ip_address
> Displays subscribers based on the eNodeB to which they are attached. ip_address must be a valid IPv4 or IPv6 address of an existing eNodeB and be specified in dotted-decimal notation (IPv4) or colon-separated notation (IPv6).
> fng-only
> Displays Femto Network Gateway (FNG) context information for the session.
> fng-service service_name
> Displays information for subscribers accessing the specified FNG service.
> service_name must be an existing service and be from 1 to 63 alphanumeric characters.
> full
> Shows all available subscriber information. The following filter keywords are valid with this command:
> active, all, asngw-service, asnpc-service, asn-peer-address, apn, callid, card-num, configured-idle-timeout, connected-time, dhcp-server, dormant, fa, fa-service, ggsn-service, ha, ha-service, idle-time, imsi, ip-address, ip-pool, lac, lac-service, lns, lns-service, long-duration-time-left, msid, network-requested, network-type, pcf, pdsn-service, plmn-type, rx-data, session-time-left, sgsn-address, sgsn-service, tpo, tx-data, username, grep, more
> ggsn-only
> Displays only GGSN-specific subscriber context information.
> gprs-only
> This keyword is specific to the SGSN and only displays 2G SGSN subscriber information.
> The following filter keywords are valid with this keyword :
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> gprs-service srvc_name
> Enter the name of the configured 2G GPRS se rvice to display subscriber information specific to the named GPRS service for the SGSN.
> srvc_name must be a string of 1 to 63 alphanumeric characters that identifies a configured GPRS service.
> The following filter keywords are valid with this command:
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> gtp-version { 0 | 1 }
> Displays the specific GTP version number. Must be followed by one of the supported GTP versions (0 or 1).
> The following filter keywords are valid with this command:
> active-charging-service, apn,bearer-establishment, callid, dhcp-server, fa, fa-service, ggsn-service, gprs-service, gsm-traffic-class, msid, msisdn, plmn-type, sgsn-address, sgsn-service, smgr-instance, tx-data, username, grep, more.
> hnbgw-only
> Displays HNB-GW subscriber session information.
> The following filters/keywords are valid with this command:
> all, full, summary
> hnbgw-service svc_name: Displays subscriber information based on the HNB-GW service name. svc_name must be an existing HNB-GW service and be from 1 to 63 alphanumeric characters.
> hsgw-only
> Displays HSGW subscriber session information.
> The following filters/keywords are valid with this command:
> all, full, summary
> hsgw-service svc_name: Displays subscriber information based on the HSGW service name. svc_name must be an existing HSGW service and be from 1 to 63 alphanumeric characters.
> hsgw-service svc_name
> Displays subscriber information based on the HSGW service name. svc_name must be an existing HSGW service and be from 1 to 63 alphanumeric characters.
> imsi imsi
> Display information specific to one subscriber or group of subscribers. Enter 1 to 15 digits to identify a specific subscriber’s IMSI (International Mobile Subscriber Identity).
> The following filter keywords are valid with this command:
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> ip-alloc-method {aaa-assigned | dhcp [ relay-agent | proxy-client ] | dynamic-pool | l2tp-lns-assigned | mip-ha-assigned | ms-provided-static | not-ms-provided-static | static pool }
> Displays the specific IP Allocation Method. Must be followed by one of the IP Allocation Methods:
> aaa-assigned: Selects subscribers whose IP addresses were assigned by AAA.
> dhcp: Selects subscribers whose IP addresses were assigned by DHCP.

> • | relay-agent: Selects subscribers whose IP addresses were assigned by the DHCP Relay Agent

> • | proxy-client: Selects subscribers whose IP addresses were assigned by the DHCP Proxy Client

> dynamic-pool: Selects subscribers whose IP addresses were assigned from a dynamic IP address pool.
> l2tp-lns-assigned: Selects subscribers whose IP addresses were assigned by the Layer 2 Tunneling Protocol (LT2P) Network Server.
> mip-ha-assigned: Selects subscribers whose IP addresses were assigned by the Mobile IP Home Agent.
> ms-provided-static: Selects subscribers whose IP addresses were provided by the Mobile Station.
> not-ms-provided-static: Selects subscribers whose IP addresses were not provided by the Mobile Station.
> static-pool: Selects subscribers whose IP addresses were assigned from a static IP address pool.
> ipsg-only
> Displays IPSG subscriber session information.
> lma-service svc_name
> Displays subscriber information based on the Local Mobility Anchor (LMA) service name. svc_name must be an existing LMA service and be from 1 to 63 alphanumeric characters.
> mag-only
> Displays MAG subscriber session information.
> The following filters/keywords are valid with this command:
> all, full, summary
> mag-service svc_name: Displays subscriber information based on the Mobile Access Gateway (MAG) service name. svc_name must be an existing MAG service and be from 1 to 63 alphanumeric characters.
> mag-service svc_name
> Displays subscriber information based on the MAG service name. svc_name must be an existing MAG service and be from 1 to 63 alphanumeric characters.
> mme-address
> Displays subscriber information based on the MME IP address. ip_address must be an existing MME IP address and be entered in IPv4 dotted-decimal notation.
> mme-only
> Displays MME subscriber session information.
> The following filter keywords are valid with this command:
> all, full, summary
> mme-service svc_name: Displays subscriber information based on the MME service name. svc_name must be an existing MME service and be from 1 to 63 alphanumeric characters.
> mme-address ip_address: Displays subscriber information based on the MMM IP address. ip_address must be an existing MME IP address and be entered in IPv4 dotted decimal notation.
> msid msid
> For this SGSN-specific keyword, enter the MSID (Mobile Dtation IDentifier) to display information specific to one subscriber’s equipment by entering the MSID.
> The following filter keywords are valid with this command:
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> msisdn msisdn
> For this SGSN-specific keyword, enter the MSISDN (Mobile Station ISDN number - unique SIM phone number) to display information specific to one subscriber’s equipment by entering the MSISDN.
> The following filter keywords are valid with this command:
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> pdg-only
> Displays a summary of PDG subscriber statistics.
> pdg-service name
> Displays statistics for users associated with a specific PDG service name.
> pdif-only
> Displays a summary of Packet Data Interworking Function (PDIF) subscriber statistics.
> pdif-service name
> Displays connection statistics for users associated with a specific PDIF service name.
> pgw-only
> Displays PDN-Gateway (P-GW) subscriber session information.
> The following filters/keywords are valid with this command:
> all, full, summary
> pgw-service svc_name: Displays subscriber information based on the P-GW service name. svc_name must be an existing P-GW service and be from 1 to 63 alphanumeric characters.
> sgw-address ip_address: Displays subscriber information based on the S-GW IP address. ip_address must be an existing S-GW IP address in IPv4 dotted-decimal notation.
> qci number
> Displays subscriber session information based on the QoS Class Identifier (QCI) value assigned to the subscriber. number must be an integer value from 0 to 9.
> s1u-state { active | idle | idle-active }
> Displays session information based on the subscriber’s S1-U state. The S1-U interface is the interface from the eNodeB to the S-GW.
> active: Displays session information for subscribers with an S1-U state set to active.
> idle: Displays session information for subscribers with an S1-U state set to idle.
> idle-active: Displays session information for subscribers with an S1-U state set to idle-active.
> s5-proto { gtp | pmip }
> Displays subscriber session information based on the S5 interface protocol used. Choose either GPRS Tunneling Protocol (GTP) or Proxy Mobile IPv6 (PMIP).
> sgsn-only
> This SGSN-only keyword displays only 3G SGSN-specific subscriber context information.
> The following filter keywords are valid with this command:
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> sgsn-service service_name
> For this SGSN-only keyword, enter the name of the configured 3G SGSN service to display subscriber information specific to the named SGSN service.
> The following filter keywords are valid with this command:
> apn, callid, card-num, connected-time, idle-time, gprs-service, gsm-traffic-class, gtp-version, imsi, msid, msisdn, nri, nsei, sgsn-service, smgr-instance
> sgw-only
> Displays S-GW subscriber session information.
> The following filters/keywords are valid with this command:
> all, full, summary
> sgw-service svc_name: Displays subscriber information based on the S-GW service name. svc_name must be an existing S-GW service and be from 1 to 63 alphanumeric characters.
> pgw-address ip_address: Displays subscriber information based on the P-GW IP address. ip_address must be an existing P-GW IP address in IPv4 dotted-decimal notation.
> sgw-service svc_name
> Displays subscriber information based on the S-GW service name. svc_name must be an existing S-GW service and be from 1 to 63 alphanumeric characters.
> subscription { aor address | callid id | full }
> Displays subscription information for defined subscribers, based on defined parameters.
> aor address: Clear session(s) by Address of Record.
> callid id: Specific Call Identification Number.
> full: Displays all available information.
> summary
> Displays only a summary of the subscriber information. The following filter keywords are valid with this command:
> active, active-charging-service, activity, all, asngw-service, asnpc-service, asn-peer-address, apn, bandwidth-policy, bearer-establishment, callid, card-num, cbb-policy, configured-idle-timeout, connected-time, dhcp-server, dormant, enodeb-address, fa, fa-service, firewall, fw-and-nat, ggsn-service, gprs-service, gsm-traffic-class, gtp-version, ha, ha-service, idle-time, ims-auth-service, imsi, ip-address, ip-alloc-method, ip-pool, ipv6-address, ipv6-prefix, lac, lac-service, lns, lns-service, long-duration-time-left, msid, msisdn, nat, network-requested pcf, pdsn-service,plmn-type, profile-id, qci, rulebase, rx-data, session-time-left, sgsn-address, tpo, tx-data, username, grep, more
> tft
> Displays the current Traffic Flow Template (TFT) associated with the subscriber session.
> tx-data
> Bytes transmitted by the subscriber.
> wf1
> Displays subscriber information in wide format number 1. Wide format number 1 includes the following information for each listed subscriber session:

> • | Access Type

> • | Access Technology

> • | Call State

> • | Link Status

> • | Network Type

> • | Call ID

> • | MSID

> • | Username

> • | IP Address

> • | Time-Idle

> • | Access Peer Address

> • | Service Address

> • | Network Peer Address

> • | Connect Time

> filter_keywords
> The following keywords are filters that modify or filter the output of the Command Keywords. Not all filters are available for all Command Keywords. Multiple Filter Keywords can be entered on a command line.
> When multiple Filter Keywords are specified, the output conforms to all of the Filter Keywords specifications.
> For example; if you enter the following command:
> show subscribers counters ip-pool pool1 card-num 1
> Counters for all subscriber sessions that were assigned an IP address from the IP pool named pool1 and also are being processed by the processing card in slot 1 is displayed. Information for all other subscribers is not displayed.
> active
> Only display information for those subscribers who currently have active sessions.
> active-charging-service acs_service
> Displays information for subscribers under active charging service processing.
> acs_service must be a string of 1 through 15 characters.
> all
> If no keywords are specified before all, information for all subscribers is displayed. If keywords are specified before all, all information is displayed with no further options being allowed.
> apn name
> Displays subscribers currently facilitated by the access point name (APN) configured on the SGSN or GGSN.
> name : enter an alphanumeric string to identify the configured APN.
> asngw-only
> Displays counters for subscribers accessing the ASN-GW service only.
> asnpc-only
> Displays counters for subscribers accessing the ASN Paging Controller and Location Registry service only.
> hnbgw-only
> Displays counters for subscribers accessing the HNB-GW service only.
> callid id
> Displays subscriber information for the call specified by id. The call ID must be specified as an 8-byte hexadecimal number.
> card-num card_num
> The slot number of the processing card by which the subscriber session is processed. pac_num is a slot number from 1 through 7 or 10 through 16.
> ccoa-only
> Displays the subscribers that registered a MIP with CoA directly with the HA.
> This option is only valid when a MIPHA session license is enabled.
> configured-idle-timeout [ < | > | greater-than | less-than ] value
> Shows the idle timeout that is configured for the specified subscriber. A value of 0 (zero) indicates that the subscribers idle timeout is disabled.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 4294967295.
> connected-time [ < | > | greater-than | less-than ] value
> Shows how long the subscriber has been connected. <: Filters output so that only information less than the specified value is displayed.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 4294967295.
> cscf-only
> Displays information for Call Session Control Function (CSCF) subscribers only.
> cscf-service service_name
> Displays information for subscribers accessing the specified CSCF service.
> service_name must be an existing service and be from 1 to 63 alphanumeric characters.
> dhcp-server address
> Displays subscribers currently accessing the system that have been provided an IP address by the DHCP server specified by address. This command is for GGSN only.
> dormant
> Shows information for subscriber sessions that are dormant (not transmitting or receiving data).
> enodeb-address IPv4_ddress
> Displays information for Evolved Packet System (EPS) subscribers connected to the eNodeB specified by IPv4_address. The address must be specified using IPv4 dotted-decimal notation.
> fa address
> Displays information for subscribers connected to the foreign agent specified by address. The address must be specified using IPv4 dotted-decimal notation.
> fa-only
> Only display FA-specific context information.
> fa-service name
> Displays information for subscribers connected to the foreign agent (FA) service specified by name. The foreign agent service name must have been previously defined.
> firewall { not-required | required }
> Displays information for the specified subscribers:
> not-required: Subscribers for whom firewall processing is not required.
> required: Subscribers for whom firewall processing is required.
> firewall-policy fw_policy_name
> This keyword is obsolete.
> fw-and-nat policy fw_nat_policy
> Important: This option is customer-specific and is only available in StarOS 8.1.
> Displays information for subscribers using the specified Firewall-and-NAT policy.
> fw_nat_policy specifies the Firewall-and-NAT policy name, and must be an alphanumeric string of 1 through 15 characters.
> ggsn-address ip_address
> Displays information for subscribers connected to the GGSN with specific IP address specified by ip_address. The GGSN IP address ip_address must have been previously defined.
> ip_address: must use IPv4 dotted-decimal notation.
> This keyword is for SGSN only.
> ggsn-preservation-mode
> Displays information for subscribers connected to the GGSN service with preservation mode enabled. This filter keyword is for GGSN only.
> ggsn-service name
> Displays information for subscribers connected to the GGSN service specified by name. The GGSN service name must have been previously defined. This keyword is for GGSN only.
> gprs-only
> Displays only 2G SGSN subscribers content. SGSN only.
> gprs-service srvc_name
> Enter the name of the configured 2G GPRS service to display subscriber information specific to the named GPRS service. SGSN only.
> gsm-traffic-class { background | conversational | interactive | streaming }
> Displays information for subscriber traffic that matches the specified 3GPP traffic class.

> • | background: 3GPP QoS background class.

> • | conversational: 3GPP QoS conversational class.

> • | interactive: 3GPP QoS interactive class. Must be followed by a traffic priority.

> • | streaming: 3GPP QoS streaming class.

> ha address
> Displays information for subscribers connected to the home agent specified by address. The address must be specified using IPv4 dotted-decimal notation.
> ha-ipsec-only
> Only display information for subscriber sessions that are using IP-Security (IPSec).
> ha-only
> Only display HA-specific context information.
> ha-service name
> Displays information for subscribers connected to the home agent service specified by name. The home agent service name must have been previously defined.
> idle-time [ < | > | greater-than | less-than ] value
> Displays how long the subscriber session has been idle or display subscriber sessions that meet the idle time criteria specified.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 4294967295.
> ims-auth-service service_name
> Displays information for subscribers with specified IMS Authorization Service. service_name must have been previously defined.
> imsi id
> Shows the subscriber with the specified id. The IMSI (International Mobile Subscriber Identity) ID is a 15-character field which identifies the subscriber’s home country and carrier. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
> ip-address [ < | > | greater-than | less-than ] address
> Displays information for subscribers connected to the specified address.
> <: Filters output so that only information for subscribers with an IP address lower than the specified address is displayed.
> >: Filters output so that only information for subscribers with an IP address higher than the specified address is displayed.
> greater-than: Filters output so that only information for subscribers with an IP address higher than the specified address is displayed.
> less-than: Filters output so that only information for subscribers with an IP address lower than the specified address is displayed.
> address: The address must be specified using IPv4 dotted-decimal notation. Used in conjunction with <, >, greater-than, less-than. If the IP address is specified without a qualifier, only subscribers with the specified IP address have their information displayed.
> ip-pool name
> Displays information for subscribers assigned addresses from the IP address pool name. name must be the name of an existing IP pool or IP pool group.
> IP pool name will be either IPv4 dotted-decimal or IPv6 colon-separated notation based on the call line setup for the specified pool name.
> ipv4
> Displays information for subscribers with an IPv4 Firewall enabled/disabled.
> ipv6
> Displays information for subscribers with an IPv6 Firewall enabled/disabled.
> ipv6-address address
> Displays information for subscribers connected to the specified address.
> ipv6-prefix prefix
> Displays information for subscribers connected to the specified address and prefix.
> lac address
> Displays information for calls to the peer L2TP Access Concentrator (LAC) specified by address.
> lac-only
> Show LAC specific information only.
> lac-service name [ local-tunnel-id id | remote-tunnel-id id ]
> Displays information for calls associated with the LAC service named name. This is a string of 1 to 63 characters.
> local-tunnel-id id : Specifies a specific local tunnel from which to clear calls. id must be in the range of 1 to 65535.
> remote-tunnel-id id : Specifies a specific remote tunnel from which to clear calls. id must be in the range of 1 to 65535.
> l3-tunnel-local-addr ip_address
> A layer 3 tunneling interface specified by ip_address. The address must be specified using IPv4 dotted-decimal notation.
> l3-tunnel-remote-addr ip_address
> A layer 3 tunneling peer specified by ip_address. The address must be specified using IPv4 dotted-decimal notation.
> lns address
> Displays information for calls to the peer L2TP Network Server (LNS) specified by address.
> lns-only
> Show LNS specific information only.
> lns-service name [ local-tunnel-id id | remote-tunnel-id id ]
> Displays information for calls associated with the LNS service named name. This is a string of 1 to 63 characters.
> local-tunnel-id id : Indicates a specific local tunnel from which to clear calls. id must be in the range of 1 to 65535.
> remote-tunnel-id id : Indicates a specific remote tunnel from which to clear calls. id must be in the range of 1 to 65535.
> long-duration-time-left [ < | > | greater-than | less-than ] value
> Shows how much time is left for the maximum duration of a specified subscriber session.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 4294967295.
> mip-udp-tunnel-only
> Displays the subscribers that negotiated MIP-UDP tunneling with the HA.
> This option is only valid when MIP NAT Traversal license is enabled.
> mipv6ha-only
> Shows MIPV6HA-specific context information for the session.
> mipv6ha-service service_name
> Displays specific configured MIPV6 Home Agent service. service_name must have been previously defined.
> msid id
> Displays information for the mobile user identified by id. id must be from 7 to 16 hexadecimal digits specified as an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example: ‘$’.
> In case of enforce imsi-min equivalence is enabled on the chasis and MIN or IMSI numbers supplied, this filter will show subscribers with a corresponding MSID (MIN or IMSI) whose lower 10 digits matches to lower 10 digits of the supplied MSID.
> show subscribers msid ABCD0123456789 or
> show subscribers msid 0123456789
> will show any subscriber with a MSID that match the lower 10 digits of MSID supplid, for example, 0123456789.
> msisdn msisdn
> Displays information for the mobile user identified by the Mobile Subscriber ISDN Number (MSISDN).
> msisdn must be 7 to 16 digits; specified as an IMSI, MIN, or RMI.
> nat { not-required | required [ nat-ip nat_ip_address | nat-realm nat_realm ] }
> Displays information for the specified subscribers.
> not-required: Subscribers for whom Network Address Translation (NAT) processing is not required.
> required: Subscribers for whom NAT processing is required.
> Important: The nat-ip keyword is only available in StarOS 8.3 and later releases.
> nat-ip nat_ip_address: Subscribers for whom NAT processing is enabled and are using the specified NAT IP address. nat_ip_address specifies the NAT IP address and must be in IPv4 dotted-decimal notation.
> nat-realm nat_realm: Subscribers for whom NAT processing is enabled and are using the specified NAT realm. nat_realm specifies the NAT realm name and must be a string from 1 through 63 characters.
> network-requested
> Display information for currently active subscribers whose sessions were initiated by the GGSN network requested create PDP context procedure.
> network-type { gre | ipip | ipsec | ipv4 | ipv6 | l2tp | mobile-ip | proxy-mobile-ip }
> Displays network type information for the subscriber session. The following network types can be selected:

> • | gre : Generic Routing Encapsulation (GRE) per RFC 2784

> • | ipip : IP-in-IP encapsulation per RFC 2003

> • | ipsec : IPSec

> • | ipv4: Internet Protocol version 4 (IPv4)

> • | ipv6: Internet Protocol version 6 (IPv6)

> • | l2tp: Layer 2 Tunneling Protocol (L2TP) encryption per RFC 2661

> • | mobile-ip : Mobile IP

> • | proxy-mobile-ip : Proxy Mobile IPv6

> nri nri_value
> This SGSN-specific filter uses the configured network resource identifier (NRI) to identify a specific SGSN in a pool to finetune the subscriber information to be displayed.
> nri_value: enter an integer from 0 to 63
> This filter can be used in combination with further refining filters.
> partial qos { negotiated | requested }
> This filter is specific to the SGSN.
> Is limits the display of information to requested or negotiated QoS information for the subscriber.
> This filter can be used in combination with further defining filters: active, active-charging-service, all, apn, callid, card-num, configured-idle-timeout, connected-time, ggsn-address, gprs-service, gsm-traffic-class, idle-time, imsi, msid, msisdn, negotiated, plmn-type, requested, rx-data, session-time-left, tx-data
> pcf [ < | > | less-than | greater-than] ipv4_address [[ < | > | less-than | greater-than ] ipv4_address ]
> Displays information for subscribers connected via the packet control function with a specific or range of IP addresses ipv4_ddress. The address must be specified using IPv4 dotted-decimal notation.

> • | <: Filters output so that only information less than the specified IPv4 address value is displayed.

> • | >: Filters output so that only information greater than the specified IPv4 address value is displayed.

> • | less-than:Filters output so that only information less than the specified IPv4 address value is displayed.

> • | greater-than:Filters output so that only information greater than the specified IPv4 address value is displayed.

> Note: It is possible to define a limited range of IP addresses by using the less-than and greater-than options to define minimum and maximum values.
> pdsn-only
> Show PDSN specific information only.
> pdsn-service name
> Displays information for subscribers connected to the packet data service name. The packet data service must have been previously configured.
> plmn-type
> Displays subscriber type (HOME, VISITING, or ROAMING).
> This keyword is for the GGSN or the SGSN only.
> policy
> Displays the current policies associated with the subscriber session.
> rnc id rnc_id mcc mcc_num mnc mnc_num
> Displays information for subscribers connected to the SGSN via a specific RNC (radio network controller) identified by the RNC ID, the MCC (mobile country code), and the MNC (mobile network code).
> This keyword is for SGSN only.
> rx-data [ < | > | greater-than | less-than ] value
> The number of bytes received by the specified subscriber.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 18446744073709551615.
> session-time-left [ < | > | greather-than | less ] value
> How much session time is left for the specified subscriber.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 4294967295.
> smgr-instance number
> Specific sessmgr instance. number must be in the range of 1 to 4294967295.
> sgsn-address address
> Shows information for subscribers whose PDP contexts are currently being facilitated by the SGSN specified by address. This command is for GGSN only.
> sgsn-service srvc_name
> Shows subscriber information for a specified 3G SGSN service.
> srvc_name must be a string of 1 to 63 alphanumeric characters that identifies a configured SGSN service.
> This command is for SGSN only.
> tpo { not-required | required }
> Displays information for specified subscribers.

> • | not-required: Subscribers for whom Traffic Performance Optimizer (TPO) processing is not enabled.

> • | required: Subscribers for whom TPO processing is enabled.

> tx-data [ < | > | greater-than | less-than ] value
> The number of bytes transmitted by the specified subscriber.
> <: Filters output so that only information less than the specified value is displayed.
> >: Filters output so that only information greater than the specified value is displayed.
> greater-than: Filters output so that only information greater than the specified value is displayed.
> less-than: Filters output so that only information less than the specified value is displayed.
> value: Used in conjunction with <, >, greater-than, less-than, If no other filtering options are specified only output matching value is displayed. If value is not specified all data is displayed. value must be an integer from 0 through 18446744073709551615.
> username name
> Displays information for connections for the subscriber identified by name. The user must have been previously configured. name must be a sequence of characters and/or wildcard characters ('$' and '*') from 1 to 127 characters. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘). For example; ‘$’.
> verbose
> Display detailed information.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to view information about subscriber sessions.
> The output of this command may be considered for part of a periodic system auditing program by verifying active and dormant subscribers.
> The Command Keywords may be used standalone to display detailed information or you may use one or more of the various Filter Keywords to reduce the amount of information displayed.
> Caution: Executing this command may negatively impact performance if multiple instances are executed while the system is under heavy load and simultaneously facilitating multiple CLI sessions.
> Example
> The following command displays information for all subscriber sessions:
> show subscribers all
> The following command displays information for all ggsn-only subscriber sessions:
> show subscribers ggsn-only all
> The following command displays information for all subscriber sessions in wide format 1:
> show subscribers wf1 all
> show subscribers aaa-configuration
> show subscribers counters username isp1user1
> The following command displays information for subscriber in GGSN service:
> show subscribers ggsn-only allshow subscribers ggsn-only full
> The following command displays information for all subscriber with SGSN session having partial QoS requests:
> show subscribers sgsn-only partial qos requested
> The following command displays information for all subscriber with MME session connected to MME service having IP address as 1.1.1.1:
> show subscribers mme-only mme-address 1.1.1.1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show super-charger
> Lists subscribers with valid super-charger configuration. When super-charger is enabled for a subscriber, the SGSN handles 2G or 3G connections controlled by an operator policy and changes hand-off and location update procedures to reduce signaling traffic management (3GPP, TS.23.116).
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show super-charger { imsi imsi | all }
> imsi
> Defines a specific subscriber’s international mobile subscriber identity (IMSI) number.
> imsi - up to 15 digits that include the MCC (mobile country code), the MNC (mobile network code) and the MSIN (mobile station identification number),
> all
> Instructs the SGSN to display super charger subscription information for all subscribers.
> Usage
> Use this command to determine if a single subscriber, identified by the IMSI, has a super charger configuration. Also, this command can display the list of all subscribers with a super charger configuration. If a subscriber has super charger as part of the configuration, subscriber data is backed up (using the IMSI Manager) after the subscriber detaches and the purge timer expires.
> Example
> The following command displays the super charger configuration information for the subscriber identified by the IMSI 90121882144672.
> show super-charger imsi 90121882144672
> show support details
> This command outputs a comprehensive list of system information that is useful for troubleshooting purposes. In most cases, the output of this command is requested by the Technical Assistance Center (TAC).
> Product
> All
> Privilege
> All
> Syntax
> show support details [ to file url [ compress ] ]
> to file urlurl
> Specifies the location where a tar file with the support detail information should be created. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [ file: ] { /flash | /pcmcia1 | /hd } [ /directory ] /file_name [ compress ]

> • | tftp:// { host [ :port# ] } [ /directory ] /file_name

> • | [ ftp: | sftp: ] // [ username[ :password ] @ ] { host } [ :port# ] [ /directory ] /file_name

> directory is the directory name.
> filename is the actual file of interest.
> username is the user to be authenticated.
> password is the password to use for authentication.
> host is the IP address or host name of the server.
> port# is the logical port number that the communication protocol is to use.
> If the filename is not specified with a .tar extension, it is automatically appended to the filename when the file is created and a message is generated.
> The content of the tar file is:

> • | support_summary - An ASCII text file that contains the support detail information.

> • | information.minicores.tar - A tar file that contains any minicore files found on the system. Minicore files contain memory core dumps that are captured during some events. These core dumps provide specific memory locations and other information about the event. This information is useful to the technical support team in identifying where and when an event occurred along with its probably cause.

> compress
> Including the compress keyword instructs the system to generate a compressed .tar.gz file for the output of the command.
> Usage
> Use this command to obtain extensive system information for use in troubleshooting. This command does the work of over 30 separate commands, which saves time and ensures that all of the information needed is collected and displayed in the same order every time.
> In addition to the information provided, the show support details command includes information that is not otherwise accessible to users but that is helpful in the swift resolution of issues.
> Example
> The following command displays the system information on your console.
> show support details
> The following command displays the information on your console and also writes it to the local device (pcmcia1 in this case) and includes the mini core dumps, using the filename r-p_problem.tar:
> show support details to file /pcmcia1/r-p_problem.tar
> The following command displays the information on your console and also writes it to an FTP server (named host), placing the file in the dir directory and includes the mini core dumps, using the filename re_problem.tar:
> show support details to file ftp://host/dir/re_problem.tar
> show system uptime
> Shows the amount of time the system has been operational since its last down time (maintenance or otherwise).
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show system uptime [ | { grep grep_options | more } ]
> uptime
> Indicates only the system up time is to be displayed.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Display the system up time to check for the possibility of anomalous behavior related to longer up times.
> Example
> The following command displays basic system basic information and up time.
> show system uptime

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883