> Replacing Upper or Lower Fan Tray
> The upper fan tray draws air up through the chassis for cooling and ventilation. It then exhausts the heated air through the vents at the upper-rear of the chassis.
> The lower fan tray draws air from the front and sides and pushes it through the chassis for cooling and ventilation.
> Caution: Do not operate the chassis without the fan tray(s) installed. Doing so even for short periods of time may cause the system to overheat and result in component damage.
> This chapter provides instructions for the removal and replacement of the upper and lower fan tray assemblies should there be a partial or complete failure of either one.
> ESD Caution: During installation, maintenance, and/or removal, wear a grounding wrist strap to avoid ESD damage to the components. Failure to do so could result in damage to sensitive electronic components and potentially void your warranty.
> Determining Whether a Fan Tray Needs Replacing
> The system has several ways to indicate a fan tray failure. The first indicator is that the Status LED on the System Resource Card (SRC) turns red to indicate the failure of a chassis component.
> If you see a red Status LED on the SRC, you can determine whether it is a fan tray failure via the CLI or by checking the Simple Network Management Protocol (SNMP) traps.
> Using the CLI
> To monitor chassis temperature and fan speed, issue the following CLI command in the Exec mode:
> show fans
> The following is a sample output for this command:
> Upper Fan Controller: State=All Running Speed=Normal Temp=20 (C)
> Lower Fan Controller: State=All Running Speed=Normal Temp=20 (C)
> Using SNMP Traps and MIB Objects
> The system supports SNMP traps that are triggered for conditions that may indicate the need to change the fan tray. The system provides the following traps:

> SNMP Trap | Description
> starFanFailed | One or more fans have failed on the indicated fan controller.
> starFanRemoved | A fan tray has been removed.
> starFanLocation | The physical location of the fan controller, upper or lower.
> starFanFailures | The type of failure experienced:
> 0: There are no errors. This is the normal operating condition.
> 2: Multiple fans on the fan tray have failed.
> 4: A single fan on the fan tray has failed.
> 8: The redundant fan controller on the fan tray did not respond to the heartbeat signal.
> 10: An error has occurred on the primary fan controller bus for the fan tray.
> 20: An error has occurred on the redundant fan controller bus for the fan tray.
> 40: An inter-bus communication error was experienced between the primary and redundant fan controllers on the fan tray.
> 80: The fan tray is not present.
> starFanSpeed | The speed of the fans controlled by this fan controller. The value normal(1) represents the normal operating speed of the fans. The value high(2) represents that the fans are running at a higher rate of speed.

> ‌
> Removing an Upper Fan Tray
> Follow the instructions below to remove an upper fan tray from the chassis.

> Step 1 | Remove the plastic bezel from the upper-front of the chassis by placing your fingers in the notches on the sides of the bezel and pulling it toward you.

> Step 2 | Use a Phillips #1 screwdriver to loosen the four screws securing the fan tray.

> Step 3 | Grasp the two bezel mounts on the front of the fan tray and pull toward you. The fan tray should easily slide out of the chassis.

> Warning: The upper fan tray assembly contains multiple fans that are spinning at a high rate of speed when the system is powered on. If system is powered on, do not touch moving fans. To minimize the risk of personal injury and potential damage to equipment, follow these instructions.

> 1. | Pull the fan tray towards you until the fan tray extends out of the chassis approximately two inches (5 cm).

> 2. | Wait 30 seconds to allow fans to stop spinning.

> 3. | Fully remove fan tray.

> Warning: Die obere Lüfter Schublade enthaelt mehrere Lüfter. Verletzungsgefahr bei Beruehrung der Lüfter. Hohe Umdrehungszahl der Lüfter unter Stromanschluss. Vorsicht nicht beruehren. Um persoenliche Verletzungen und Geraeteschaden zu verhueten bitte Anleitungen beachten.

> 1. | Schublade ca. 5cm herausziehen.

> 2. | 30 Sekunden warten bis die Luefter zum stehen kommen.

> 3. | Schublade erst jetzt komplett herausziehen.

> Step 4 | Proceed to the Installing a Replacement Upper Fan Tray section that follows.

> Installing an Upper Fan Tray
> Follow the instructions below to install an upper fan tray.

> Step 1 | Hold the front of the fan tray by its sides and align it with the upper fan tray bay of the chassis.

> Step 2 | Slowly slide the fan tray into the chassis along the guides until its face plate is flush against the chassis.

> Step 3 | Use a Phillips #1 screwdriver to tighten the four screws on the face plate to secure the fan.

> Step 4 | Replace the plastic bezel by aligning it over the bezel mounts that protrude from the fan tray and snapping the bezel in place.

> Removing a Lower Fan Tray Assembly
> Follow the instructions below to remove a lower fan tray assembly from the chassis.

> Step 1 | Remove the plastic bezel from the lower-front of the chassis by placing your fingers in the notches on its sides and pulling it toward you.

> Step 2 | Use a Phillips #1 screwdriver to remove the fan tray cover by loosening the four screws securing it in place.

> Step 3 | Pull the fan tray toward you with the handle cut-out on the front of the fan tray assembly. The fan tray assembly should easily slide out of the chassis.

> Warning: The upper fan tray assembly contains multiple fans that are spinning at a high rate of speed when the system is powered on. If system is powered on, do not touch moving fans. To minimize the risk of personal injury and potential damage to equipment, follow these instructions.

> 1. | Pull the fan tray towards you until the fan tray extends out of the chassis approximately two inches (5 cm).

> 2. | Wait 30 seconds to allow fans to stop spinning.

> 3. | Fully remove fan tray.

> Warning: Die obere Lüfter Schublade enthaelt mehrere Lüfter. Verletzungsgefahr bei Beruehrung der Lüfter. Hohe Umdrehungszahl der Lüfter unter Stromanschluss. Vorsicht nicht beruehren. Um persoenliche Verletzungen und Geraeteschaden zu verhueten bitte Anleitungen beachten.

> 1. | Schublade ca. 5cm herausziehen.

> 2. | 30 Sekunden warten bis die Luefter zum stehen kommen.

> 3. | Schublade erst jetzt komplett herausziehen.

> Step 4 | Proceed to the Installing a Replacement Lower Fan Tray Assembly section that follows.

> Installing a Lower Fan Tray Assembly
> Follow the instructions below to install a lower fan tray.

> Step 1 | Hold the front of the fan tray by its handle with one hand and use your other hand to align it with the lower fan tray bay of the chassis. The lower fan tray bay is located at the bottom front of the chassis.

> Step 2 | Slowly slide the fan tray into the chassis along the guides until it is seated firmly in the chassis and can go no further.

> Step 3 | Verify that the particulate filter is securely in place. Its front should be flush with the front of the fan tray assembly and its tab should be lowered to keep it in place.

> Step 4 | Use a Phillips #1 screwdriver to replace the fan tray bay cover and tighten each of the four screws to secure it.

> Important: The fan tray bay cover is keyed and can only be installed in one direction.

> Step 5 | Replace the lower plastic bezel by aligning it over the bezel mounts that protrude from the fan tray bay cover and snapping the it in place.

> What to do with the Failed Fan Tray
> If the failed fan tray is still under warranty, return it to the vendor for repair.
> If the failed fan tray is out of warranty, contact the vendor to determine if it can be sent in for repair at an additional cost.
> Important: Disposal of this product should be performed in accordance with all national laws and regulations.
> For new customers: Refer to the support area of http://www.cisco.com for up-to-date product documentation pertaining to installation, configuration, and maintenance. A valid username and password are required to use this site. Please contact your local sales or service representative for additional information.
> For existing customers with support contracts through Starent Networks: Refer to the support area of http://www.starentnetworks.com for up-to-date product documentation pertaining to installation, configuration, and maintenance. A valid username and password are required to use this site. Please contact your local sales or service representative for additional information.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883