> Peer-Server Configuration Mode Commands
> The Peer-Server configuration mode provides the commands to define and manage the peer server configuration part of the SS7 routing on an SGSN.
> In this mode, the prompt line usually appears similar to:
> [local]hostname(config-ss7-rd-<ss7rd_id>-ps-id-<ps_id>)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> mode
> Configures the operational mode of the peer-server.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> mode ( loadshare | standby )
> loadshare
> Sets the peer-server to load share. This is the default.
> standby
> Sets the peer-server to be in standby mode.
> Usage
> Configure the operational mode of the peer-server.
> Example
> Configure the peer-server for standby mode.
> mode standby
> name
> Defines the unique identification - the name - of the peer-server in the SS7 routing domain.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> name name
> no name
> no
> Removes the peer server’s name from this configuration instance.
> name
> name: Must be a string of 1 to 64 alphanumeric characters to define a unique identification for the peer-server within the specific SS7 routing domain. Double quotes must be used to create a name that includes spaces.
> Usage
> Create peer server names that are easy to remember and uniquely identify the PSP.
> Example
> Use this command to create an easily remembered alphanumeric name for the peer-server:
> name “Berlin West”
> psp
> Creates the peer-server-process (PSP) instance and enters the PSP configuration mode. See the PSP Configuration Mode chapter in this guide for information on the configuration commands.
> Important: This command configures a mandatory parameter in the configuration of the peer server.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] psp instance id
> no
> Removes the PSP instance from the peer server configuration.
> id
> id Uniquely identifies the specific peer-server-process configuration. The Id must be an integer from 1 to 4.
> Usage
> Use this command to define the peer-server-process (PSP) instance ID number for the SGSN configuration.
> Example
> Use this command to create instance #3 for the PSP configuration:
> psp instance 3
> routing-context
> Defines the ID of the routing context for the peer-server to use.
> Important: This command configures a mandatory parameter in the configuration of the peer server.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> routing-context id
> no routing-context
> id
> id Uniquely identifies a specific routing context for the peer-server-process to use. The Id must be an integer from 1 to 65535.
> no
> Removes the routing-context definition from the peer server configuration.
> Usage
> Use this command to define routing contexts for the peer server.
> Example
> Define routing-context instance 15:
> routing-context 15
> self-point-code
> This command defines the point-code to identify the SGSN as a peer server.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> self-point-code point-code
> no self-point-code
> point-code
> Point-code is an SS7-type address for an element in the SS7 network. Point-codes must be defined in dotted-decimal format in a string of 1 to 11 digits. Options include:

> • | 0.0.1 to 7.255.7 for point-code in the ITU range.

> • | 0.0.1 to 255.255.255 for point-code in the ANSI range.

> • | 0.0.1 to 15.31.255 for point-code in the TTC Range.

> • | a string of 1 to 11 digits in dotted-decimal to represent a point-code in a different range.

> no
> Removes the self-point-code configuration for this linkset in the peer server.
> Important: Removing the self-point-code will result in the termination of all traffic on this link.
> Usage
> Use this command to define the point-code to identify the SGSN.
> Example
> Use the following command to remove the self-point-code definition from the peer-server configuration:
> no self-point-code

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883