> show congestion-control
> This chapter includes the show congestion-control command output tables.
> show congestion-control statistics a11mgr instance
> show congestion-control statistics a11mgr instance Command Output Descriptions

> Field | Description
> Current congestion status | The current congestion control state as “Cleared” or “Applied”.
> Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
> Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. Refer to the congestion-control threshold command in the Global Configuration Mode chapter of this reference.

> ‌
> show congestion-control statistics asngwmgr instance
> show congestion-control statistics asngwmgr instance Command Output Descriptions

> Field | Description
> Current congestion status | The current congestion control state as “Cleared” or “Applied”.
> Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
> Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. Refer to the congestion-control threshold command in the Global Configuration Mode chapter of this reference.
> system cpu use exceeded | Indicates the number of time the ASNGW Manager exceeded the system CPU usage limit.
> service cpu use exceeded | Indicates the number of time the ASNGW Manager exceeded the CPU usage limit specified for this service.
> system memory use exceeded | Indicates the number of time the ASNGW Manager exceeded the allocated system memory usage limit.
> port rx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Rx port usage limit.
> port tx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Tx port usage limit.
> port specific rx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Rx port usage limit for a specific port number.
> port specific tx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Tx port usage limit for a specific port number.
> max sess use exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum session usage limit for a service.
> license use exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum license usage limit.
> msg queue size use exceeded | Indicates the number of time the ASNGW Manager exceeded the message queue size usage.
> msg queue wait time exceeded | Indicates the number of time the ASNGW Manager exceeded the message queue wait time.
> license threshold exceeded | Indicates the number of time the ASNGW Manager exceeded the license threshold limit.
> max sess threshold exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum session threshold limit.
> Sessions disconnected due to overload disconnect | Indicates the total number of sessions disconnected due to overload.

> ‌
> show congestion-control statistics asnpcmgr instance
> show congestion-control statistics asnpcmgr instance Command Output Descriptions

> Field | Description
> Current congestion status | The current congestion control state as “Cleared” or “Applied”.
> Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
> Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. Refer to the congestion-control threshold command in the Global Configuration Mode chapter of this reference.
> system cpu use exceeded | Indicates the number of time the ASNPC Manager exceeded the system CPU usage limit.
> service cpu use exceeded | Indicates the number of time the ASNPC Manager exceeded the CPU usage limit specified for this service.
> system memory use exceeded | Indicates the number of time the ASNPC Manager exceeded the allocated system memory usage limit.
> port rx use exceeded | Indicates the number of time the ASNPC Manager exceeded the Rx port usage limit.
> port tx use exceeded | Indicates the number of time the ASNPC Manager exceeded the Tx port usage limit.
> port specific rx use exceeded | Indicates the number of time the ASNPC Manager exceeded the Rx port usage limit for a specific port number.
> port specific tx use exceeded | Indicates the number of time the ASNPC Manager exceeded the Tx port usage limit for a specific port number.
> max sess use exceeded | Indicates the number of time the ASNPC Manager exceeded the maximum session usage limit for a service.
> license use exceeded | Indicates the number of time the ASNPC Manager exceeded the maximum license usage limit.
> msg queue size use exceeded | Indicates the number of time the ASNPC Manager exceeded the message queue size usage.
> msg queue wait time exceeded | Indicates the number of time the ASNPC Manager exceeded the message queue wait time.
> license threshold exceeded | Indicates the number of time the ASNPC Manager exceeded the license threshold limit.
> max sess threshold exceeded | Indicates the number of time the ASNPC Manager exceeded the maximum session threshold limit.
> Sessions disconnected due to overload disconnect | Indicates the total number of sessions disconnected due to overload.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883