> Sample Personal Stateful Firewall Configuration
> The following is a sample Personal Stateful Firewall configuration.
> configure
> license key "\
> VER=1|C1M=SanDiskSDJNJKL742749406|C1S=14J3KJI20|DOI=108|DOE=12\
> SIG=MC4CFQCf9f7bAibGKJWqMd5XowxVwIVALIVgTVDsVAAogKe7fUHAEUTokw"
> aaa default-domain subscriber radius
> aaa last-resort context subscriber radius
> gtpp single-source
> system hostname ABCCH4
> autoconfirm
> clock timezone asia-calcutta
> crash enable encrypted url 123abc456def789ghi
> card 1
> mode active psc
> exit
> card 2
> mode active psc
> exit
> card 4
> mode active psc
> exit
> require session recovery
> require active-charging
> context local
> interface SPIO1
> ip address 1.2.3.4 255.255.255.0
> exit
> server ftpd
> exit
> ssh key 123abc456def789ghi123abc456def789ghi len 461
> server sshd
> subsystem sftp
> exit
> server telnetd
> exit
> subscriber default
> exit
> administrator staradmin encrypted password 123abc456def789ghi ftp
> aaa group default
> exit
> gtpp group default
> exit
> ip route 0.0.0.0 0.0.0.0 2.3.4.5 SPIO1
> exit
> port ethernet 24/1
> no shutdown
> bind interface SPIO1 local
> exit
> ntp
> enable
> server 10.6.1.1
> exit
> snmp engine-id local 77777e66666a55555
> active-charging service service_1
> nat allocation-failure send-icmp-dest-unreachable
> host-pool host1
> ip range 1.2.3.4 to 2.3.4.5
> exit
> host-pool host2
> ip range 3.4.5.6 to 4.5.6.7
> exit
> host-pool host3
> ip range 5.6.7.8 to 6.7.8.9
> exit
> ruledef ip_any
> ip any-match = TRUE
> exit
> ruledef rt_ftp
> tcp either-port = 21
> rule-application routing
> exit
> ruledef rt_ftp_data
> tcp either-port = 20
> rule-application routing
> exit
> ruledef rt_http
> tcp either-port = 80
> rule-application routing
> vexit
> ruledef rt_rtp
> rtp any-match = TRUE
> rule-application routing
> exit
> ruledef rt_rtsp
> tcp either-port = 554
> rule-application routing
> exit
> access-ruledef fw_icmp
> icmp any-match = TRUE
> exit
> access-ruledef fw_tcp
> tcp any-match = TRUE
> exit
> access-ruledef fw_udp
> udp any-match = TRUE
> exit
> edr-format nbr_format1
> attribute sn-start-time format MM/DD/YYYY-HH:MM:SS priority 5
> attribute sn-end-time format MM/DD/YYYY-HH:MM:SS priority 10
> attribute radius-nas-ip-address priority 15
> attribute sn-correlation-id priority 20
> rule-variable ip subscriber-ip-address priority 25
> rule-variable ip server-ip-address priority 30
> attribute sn-subscriber-port priority 35
> attribute sn-server-port priority 40
> attribute sn-flow-id priority 45
> attribute sn-volume-amt ip bytes uplink priority 50
> attribute sn-volume-amt ip bytes downlink priority 55
> attribute sn-volume-amt ip pkts uplink priority 60
> attribute sn-volume-amt ip pkts downlink priority 65
> attribute sn-volume-amt tcp pkts downlink priority 66
> attribute sn-volume-amt tcp pkts uplink priority 67
> attribute sn-volume-amt tcp bytes downlink priority 68
> attribute sn-volume-amt tcp bytes uplink priority 69
> rule-variable ip protocol priority 70
> attribute sn-app-protocol priority 75
> attribute radius-user-name priority 80
> attribute radius-calling-station-id priority 85
> attribute sn-direction priority 90
> attribute sn-volume-dropped-amt ip bytes uplink priority 100
> attribute sn-volume-dropped-amt ip bytes downlink priority 110
> attribute sn-volume-dropped-amt ip packts uplink priority 115
> attribute sn-volume-dropped-amt ip packts downlink priority 120
> attribute sn-volume-dropped-amt tcp bytes uplink priority 130
> attribute sn-volume-dropped-amt tcp bytes downlink priority 140
> attribute sn-volume-dropped-amt tcp packts uplink priority 155
> attribute sn-volume-dropped-amt tcp packts downlink priority 160
> exit
> udr-format udr_format
> attribute sn-start-time format MM/DD/YYYY-HH:MM:SS localtime priority 1
> attribute sn-end-time format MM/DD/YYYY-HH:MM:SS localtime priority 2
> attribute sn-correlation-id priority 4
> attribute sn-content-vol bytes uplink priority 6
> attribute sn-content-vol bytes downlink priority 7
> attribute sn-fa-correlation-id priority 8
> attribute radius-fa-nas-ip-address priority 9
> attribute radius-fa-nas-identifier priority 10
> attribute radius-user-name priority 11
> attribute sn-content-vol pkts uplink priority 12
> attribute sn-content-vol pkts downlink priority 13
> attribute sn-group-id priority 14
> attribute sn-content-id priority 15
> exit
> xheader-format header
> insert Stpid-1 variable bearer sn-rulebase
> insert Stpid-2 variable bearer subscriber-ip-address
> exit
> charging-action ca_nothing
> content-id 20
> exit
> bandwidth-policy bw1
> exit
> bandwidth-policy bw2
> exit
> rulebase base_1
> tcp packets-out-of-order timeout 30000
> tcp packets-out-of-order transmit after-reordering
> billing-records udr udr-format udr_format
> action priority 1 ruledef ip_any charging-action ca_nothing
> route priority 1 ruledef rt_ftp analyzer ftp-control
> route priority 10 ruledef rt_ftp_data analyzer ftp-data
> route priority 20 ruledef rt_rtsp analyzer rtsp
> route priority 30 ruledef rt_rtp analyzer rtp
> route priority 40 ruledef rt_http analyzer http
> route priority 50 ruledef rt_pptp analyzer pptp
> route priority 60 ruledef rt_tftp analyzer tftp
> rtp dynamic-flow-detection
> bandwidth default-policy bw1
> fw-and-nat default-policy base_1
> exit
> rulebase base_2
> action priority 1 ruledef ip_any charging-action ca_nothing
> route priority 1 ruledef rt_ftp analyzer ftp-control
> route priority 10 ruledef rt_ftp_data analyzer ftp-data
> route priority 40 ruledef rt_http analyzer http
> route priority 50 ruledef rt_pptp analyzer pptp
> route priority 60 ruledef rt_tftp analyzer tftp
> bandwidth default-policy bw2
> fw-and-nat default-policy base_2
> exit
> rulebase default
> exit
> fw-and-nat policy base_1
> access-rule priority 1 access-ruledef fw_tcp permit
> access-rule priority 2 access-ruledef fw_udp permit
> firewall dos-protection source-router
> firewall dos-protection winnuke
> firewall dos-protection mime-flood
> firewall dos-protection ftp-bounce
> firewall dos-protection ip-unaligned-timestamp
> firewall dos-protection tcp-window-containment
> firewall dos-protection teardrop
> firewall dos-protection flooding udp
> firewall dos-protection flooding icmp
> firewall dos-protection flooding tcp-syn
> firewall dos-protection port-scan
> firewall dos-protection ipv6-dst-options invalid-options
> firewall dos-protection ipv6-extension-hdrs limit 2
> firewall dos-protection ipv6-hop-by-hop jumbo-payload
> firewall dos-protection ipv6-hop-by-hop router-alert
> firewall tcp-first-packet-non-syn reset
> firewall policy ipv4-and-ipv6
> exit
> fw-and-nat policy base_2
> access-rule priority 5 access-ruledef fw_tcp_port_3000 permit trigger open-port 5000 direction reverse
> access-rule priority 10 access-ruledef fw_tcp permit
> access-rule priority 20 access-ruledef fw_udp permit
> access-rule priority 30 access-ruledef fw_icmp deny
> firewall policy ipv4-and-ipv6
> exit
> nat tcp-2msl-timeout 120
> exit
> context pdsn
> interface pdsn
> ip address 11.22.33.44 255.255.255.0
> ip address 22.33.44.55 255.255.255.0 secondary
> exit
> ssh key 123abc456def789ghi123abc456def789ghi len 461
> server sshd
> subsystem sftp
> exit
> subscriber default
> ip access-group css-1 in
> ip access-group css-1 out
> ip context-name isp
> mobile-ip send accounting-correlation-info
> active-charging rulebase base_1
> exit
> aaa group default
> exit
> gtpp group default
> exit
> pdsn-service pdsn
> spi remote-address 1.1.1.1 spi-number 256 encrypted secret 5c4a38dc2ff61f72 timestamp-tolerance 0
> spi remote-address 2.2.2.2 spi-number 256 encrypted secret 5c4a38dc2ff61f72 timestamp-tolerance 0
> spi remote-address 3.3.3.3 spi-number 9999 encrypted secret 5c4a38dc2ff61f72 timestamp-tolerance 0
> authentication pap 1 chap 2 allow-noauth
> bind address 4.4.4.4
> exit
> edr-module active-charging-service
> file name NBR_nat current-prefix Record rotation time 45 headers edr-format-name
> exit
> exit
> context isp
> ip access-list css
> redirect css service service_1 ip any any
> exit
> ip pool pool1 5.5.5.5 255.255.0.0 public 0
> interface isp
> ip address 6.6.6.6 255.255.255.0
> exit
> subscriber default
> exit
> aaa group default
> exit
> gtpp group default
> exit
> ip route 0.0.0.0 0.0.0.0 7.7.7.7 isp
> exit
> context radius
> interface radius
> ip address 8.8.8.8 255.255.255.0
> exit
> subscriber default
> exit
> subscriber name ABC7-sub
> ip access-group css in
> ip access-group css out
> ip context-name isp
> active-charging rulebase base_1
> exit
> subscriber name ABC9-sub
> ip access-group css in
> ip access-group css out
> ip context-name isp1
> active-charging rulebase base_2
> exit
> domain ABC7.com default subscriber ABC7-sub
> domain ABC9.com default subscriber ABC9-sub
> radius change-authorize-nas-ip 77.77.77.77 encrypted key 123abc456def789ghi port 4000
> aaa group default
> radius attribute nas-ip-address address 99.99.99.99
> radius dictionary custom9
> radius server 9.9.9.9 encrypted key 123abc456def789gh port 1645
> radius accounting server 8.8.8.8 encrypted key 123abc port 1646
> exit
> gtpp group default
> exit
> diameter endpoint acs-fire.star.com
> origin host acs-fire.star.com address 44.44.44.44
> peer minid realm star.com address 55.55.55.55
> exit
> exit
> bulkstats collection
> bulkstats mode
> sample-interval 1
> transfer-interval 15
> file 1
> remotefile format /localdisk/ABCCH4.bulkstat
> receiver 66.66.66.66 primary mechanism ftp login root encrypted password 123abc456def789ghi
> context schema sfw-dir format "sfw-dir\nsfw-dnlnk-droppkts:%sfw-dnlnk-droppkts%\nsfw-dnlnk-dropbytes:%sfw-dnlnk-dropbytes%\nsfw-uplnk-droppkts:%sfw-uplnk-droppkts%\nsfw-uplnk-dropbytes:%sfw-uplnk-dropbytes%\nsfw-ip-discardpackets:%sfw-ip-discardpackets%\nsfw-ip-malpackets:%sfw-ip-malpackets%\nsfw-icmp-discardpackets:%sfw-icmp-discardpackets%\nsfw-icmp-malpackets:%sfw-icmp-malpackets%\nsfw-tcp-discardpackets:%sfw-tcp-discardpackets%\nsfw-tcp-malpackets:%sfw-tcp-malpackets%\nsfw-udp-discardpackets:%sfw-udp-discardpackets%\nsfw-udp-malpackets:%sfw-udp-malpackets%\n---------------------\n"
> context schema sfw-total format "sfw-total\nvpnname:%vpnname%\nvpnid:%vpnid%\nsfw-total-rxpackets:%sfw-total-rxpackets%\nsfw-total-rxbytes:%sfw-total-rxbytes%\nsfw-total-txpackets:%sfw-total-txpackets%\nsfw-total-txbytes:%sfw-total-txbytes%\nsfw-total-injectedpkts:%sfw-total-injectedpkts%\nsfw-total-injectedbytes:%sfw-total-injectedbytes%sfw-total-malpackets:%sfw-total-malpackets%\nsfw-total-dosattacks:%sfw-total-dosattacks%\nsfw-total-flows:%sfw-total-flows%\n---------------------\n"
> exit
> exit
> port ethernet 17/1
> no shutdown
> bind interface pdsn pdsn
> exit
> port ethernet 17/2
> no shutdown
> bind interface isp isp
> exit
> port ethernet 17/3
> no shutdown
> bind interface radius radius
> exit
> port ethernet 17/4
> no shutdown
> exit
> port ethernet 17/5
> no shutdown
> exit
> end

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883