> show pcc-service
> This chapter describes the output of the show pcc-service command.
> show pcc-service all
> show pcc-service all Command Output Description

> Field | Description
> Service name | Indicates the name of the PCC service for which counters are displayed.
> Context name | Indicates the name of the context in which the PCC service is configured and running.
> Charging-Method | Indicates the charging methods communicated to PCEF at command level for this PCC service. Possible methods are:
> • | None
> • | Offline
> • | Online
> • | Offline and Online
> By default “None” is the enabled option.
> Online Charging-Server(s) | This group displays information of online charging servers (primary and secondary) configured and used in this PCC service.
> Primary | Indicates the name of the primary online charging server configured and used in this PCC service.
> Secondary | Indicates the name of the secondary online charging server configured and used in this PCC service.
> Offline Charging-Server(s) | This group displays information of offline charging servers (primary and secondary) configured and used in this PCC service.
> Primary | Indicates the name of the primary offline charging server configured and used in this PCC service.
> Secondary | Indicates the name of the secondary offline charging server configured and used in this PCC service.
> Subscriber-Profile Refresh Interval (sec) | Indicates the interval duration in seconds after which Subscriber profile is refreshed from SSC/SPR in a PCC service.
> Multiple PCEF Per Subscriber | Indicates status of support for more than one Gx-session for single subscriber session coming from multiple PCEF in this PCC service instance. By default this feature is supported.
> Setup Timeout | Indicates IPCF setup timeout duration set on a system for setup timer. Possible range of duration is 1 to 120 in seconds. Special value of 0 indicates that timer is disabled.
> Idle Timeout | Indicates the idle session timeout duration set for a subscriber session timer. Possible range of duration is 1 to 4294967295 in seconds. Special value of 0 indicates that timer is disabled. It also displays the action configured for initiation when idle timer expires. Possible actions are:
> • | None
> • | Reauthorization of session.
> • | Disconnection of session if reauthorization of session fails.
> Long-duration Timeout | Indicates the long duration idle session timeout set for a subscriber session timer. Possible range of duration is 1 to 4294967295 in seconds. Special value of 0 indicates that timer is disabled. It also displays the action configured for initiation when long duration timeout timer expires. Possible actions are:
> • | None
> • | Detection of idle session and sending of SNMP traps or CORBA notification.
> • | Detection of idle session and then disconnect the session after sending of SNMP traps or CORBA notification

> ‌
> show pcc-service session all
> show pcc-service session all Command Output Descriptions

> Field | Description
> vvvv | Displays service and session state information. This column provides a code consisting of four characters. From left-to-right, the first character represents the Session State that the subscriber is using. The possible call types are:
> • | c: Closed
> • | C: Connected
> • | D: Disconnected
> • | o: Open
> • | S: Waiting on SPR
> • | r: Waiting on DREG
> • | s: Waiting on STR
> • | e: Waiting on deallocate
> • | t: Waiting on CCR-T
> • | A: Waiting on ASR
> • | R: Waiting on RAR
> From left-to-right, the second character represents the Gx Session Count. It indicates the total number of Gx sessions between PCEF and IPCF active in this session. From left-to-right, the third character represents the Gy Session Count. It indicates the total number of Gy sessions active in this session. From left-to-right, the second character represents the Gxa Session Count. It indicates the total number of Gx sessions between PCEF (eHRPD) and IPCF active in this session.
> CALLID | Indicates the IP-CAN session subscriber’s call identification number.
> IMSI/MSID | Indicates the IP-CAN session subscriber’s IMSI/MSID number used in this session in bindmux.
> User Name | Indicates the user name used in IP-CAN session to identify the subscriber in this session in bindmux. This is typically used in IP-CAN session between PDSN and IPCF/PCRF over Gx interface.
> Total number of PCC sessions | The total number of PCC sessions on chassis including all modes.

> ‌
> show pcc-service session full
> show pcc-service session full Command Output Descriptions

> Field | Description
> CALLID | Indicates the IP-CAN session subscriber’s call identification number.
> IMSI/MSID | Indicates the IP-CAN session subscriber’s IMSI/MSID number used in this session in bindmux.
> User Name | Indicates the user name used in IP-CAN session to identify the subscriber in this session in bindmux. This is typically used in IP-CAN session between PDSN and IPCF/PCRF over Gx interface.
> Profile Name | Indicates the name of the subscriber used in IP-CAN session to provide QoS parameters.
> Default-EPS-Bearer | Indicates whether default EPS bearer is provisioned for subscriber in IP-CAN session for which information is displayed
> APN-AMBR | Indicates whether an Aggregate Maximum Bit Rate (AMBR) associated with APN is provisioned for subscriber in IP-CAN session for which information is displayed.
> Authorized QCIs | This group displays the parameters for authorized Quality Class Identifiers (QCIs) used in IP-CAN session for which information is displayed.
> QCI | Indicates the Quality Class Identifier (QCI) authorized and used in IP-CAN session for which information is displayed.
> Uplink | Indicates the uplink bit rate provisioned in authorized QCI for IP-CAN session for which information is displayed.
> Downlink | Indicates the downlink bit rate provisioned in authorized QCI for IP-CAN session for which information is displayed.
> Total Predefined Rules | Indicates the total predefined Rules applicable for IP-CAN session for which information is displayed.
> Predefined Rules | Indicates the name of the predefined Rules, if applicable, for IP-CAN session for which information is displayed.
> Rule Status | Indicates the status of the predefined Rules, if applicable, for IP-CAN session for which information is displayed. Possible status are:
> • | Active
> • | Inactive
> • | Temporarily Active
> Rule Failure Code | Indicates the predefined Rule failure codes, if applicable, for IP-CAN session for which information is displayed. Possible failure codes are:
> • | Out-of-credit
> • | Reallocation-of-credit
> • | Unknown rule name
> • | Invalid Rating Group
> • | Invalid Service Identifier
> • | GW/PCEF Malfunction
> • | Limited Resources
> • | Max No. of Bearers Reached
> • | Unknown Bearer Id
> • | Missing Bearer Id
> • | Missing Flow Description
> • | Resource Allocation Failure
> • | QoS Validation Failure
> Rule Activation Time | Indicates the time configured to activate predefined Rule for IP-CAN session for which information is displayed.
> Rule deactivation Time | Indicates the time configured to deactivate predefined Rule for IP-CAN session for which information is displayed.
> Total Dynamic Rules | Indicates the total dynamic Rules applicable for IP-CAN session for which information is displayed.
> Dynamic Rules | Indicates the name of the dynamic Rules, if applicable, for IP-CAN session for which information is displayed.
> Rating-Group | Indicates the rating group configured to the dynamic Rules, if applicable, for IP-CAN session for which information is displayed.
> Precedence | Indicates the precedence configured to the dynamic Rules, if applicable, for IP-CAN session for which information is displayed.
> Gate Status | Indicates the status of the Gate configured to the dynamic Rules, if applicable, for IP-CAN session for which information is displayed.
> QoS Profile | Indicates the QoS profile configured to the dynamic Rules, if applicable, for IP-CAN session for which information is displayed.
> Flow | Indicates the total number of flows applicable for IP-CAN session for which information is displayed.
> AF Information | Indicates the Application Function information for dynamic Rules, if applicable, for IP-CAN session for which information is displayed.
> Rule Status | Indicates the status of the predefined Rules, if applicable, for IP-CAN session for which information is displayed. Possible status are:
> • | Active
> • | Inactive
> • | Temporarily Active
> Rule Failure Code | Indicates the predefined Rule failure codes, if applicable, for IP-CAN session for which information is displayed. Possible failure codes are:
> • | Out-of-credit
> • | Reallocation-of-credit
> • | Unknown rule name
> • | Invalid Rating Group
> • | Invalid Service Identifier
> • | GW/PCEF Malfunction
> • | Limited Resources
> • | Max No. of Bearers Reached
> • | Unknown Bearer Id
> • | Missing Bearer Id
> • | Missing Flow Description
> • | Resource Allocation Failure
> • | QoS Validation Failure
> Rule Activation Time | Indicates the time configured to activate dynamic Rule for IP-CAN session for which information is displayed.
> Rule deactivation Time | Indicates the time configured to deactivate dynamic Rule for IP-CAN session for which information is displayed.
> Quota Information | This group displays the Quota related information applicable for IP-CAN session for which information is displayed.
> Usage Monitor Information | Indicates the Usage Monitor status applicable for IP-CAN session for which information is displayed.
> Total number of PCC sessions | The total number of PCC sessions on chassis including all modes.

> ‌
> show pcc-service statistics
> show pcc-service statistics Command Output Description

> Field | Description
> Service name | Indicates the name of the PCC service for which counters are displayed.
> Total Gx req processed | Indicates the total number of Gx request messages from PCEF processed by PCC-service node.
> Total Gy req processed | Indicates the total number of Gy request messages from OCS processed by PCC-service node.
> Total SSC req processed | Indicates the total number of request messages from SSC/SPR processed by PCC-service node.
> Total Unknown requests | Indicates the total number of unknown type of request messages from network nodes received by PCC-service node.
> PUR Updates | Indicates the total number of Profile-Update-Request update messages from network nodes received at PCC-service node.
> SNR Updates | Indicates the total number of Subscribe-Notifications-Request update messages from network nodes received at PCC-service node.
> PNR Updates | Indicates the total number of Push-Notifications-Request update messages from network nodes received at PCC-service node.
> Total Profile Hits | Indicates the total number of Subscribe profiles accessed by PCC-service node.
> Total Profile Miss | Indicates the total number of Subscribe profiles missed by PCC-service node.
> Total Quota Reports | Indicates the total number of quota reports processed by PCC-service node.
> Total Unknown rating-groups | Indicates the total number of unknown type of rating groups received by PCC-service node.
> Total Rules Activated | Indicates the total number of Rules at PCEF activated by PCC-service node.
> Total Rules Deactivated | Indicates the total number of Rules at PCEF deactivated by PCC-service node.
> Total Rulebases Activated | Indicates the total number of Rulebases at PCEF activated by PCC-service node.
> Total Rulebases Deactivated | Indicates the total number of Rulebases at PCEF deactivated by PCC-service node.
> Total Rules Installed | Indicates the total number of Rules installed at PCEF by PCC-service node.
> Total Rules Uninstalled | Indicates the total number of Rules installed at PCEF by PCC-service node.
> Profile Name | Indicates the name of the subscriber profiles accessed by PCC-service node.
> Profile Hits | Indicates the total number of hits received by specific subscriber profile at PCC-service node.
> Eval-Priority Hits | This group displays the statistics of Evaluation Priority hits at PCC-service node.
> Action Statistics | This group displays the statistics of actions triggered at PCC-service node.
> Default EPS Bearer Auth | Indicates the total number of authorization action processed for the default EPS bearer authorization on PCC-service node.
> APN AMBR Auth | Indicates the total number of authorization action processed for the APN associated Aggregate Maximum Bit Rate (AMBR) on PCC-service node.
> QCI Auth | Indicates the total number of authorization action processed for the Quality Class Indicator (QCI) on PCC-service node.
> Event-trigger Statistics | This group displays the statistics of event triggers at PCC-service node.
> SGSN Change | Indicates the total number of “SGSN change” events triggered on PCC-service node.
> QoS Change | Indicates the total number of “QoS change” events triggered on PCC-service node.
> RAT Change | Indicates the total number of “RAT (Radio Access Technology) change” events triggered on PCC-service node.
> TFT Change | Indicates the total number of “TFT (traffic flow template) change” events triggered on PCC-service node.
> PLMN Change | Indicates the total number of “PLMN change” events triggered on PCC-service node.
> Loss of flow | Indicates the total number of “Loss of Flow” events triggered on PCC-service node.
> Recovery of flow | Indicates the total number of “Recovery of Flow” events triggered on PCC-service node.
> IP-CAN Change | Indicates the total number of “IP-CAN Change” events triggered on PCC-service node.
> Qos Change Exceeding Auth | Indicates the total number of QoS change event triggers exceeded from authorized limit on PCC-service node.
> RAI Change | Indicates the total number of “RAI (Routing Area Indicator) Change” events triggered on PCC-service node.
> User Location Change | Indicates the total number of “User Location Change” events triggered on PCC-service node.
> Out Of Credit | Indicates the total number of “Out of Credit” events triggered on PCC-service node.
> Reallocation of Credit | Indicates the total number of “Reallocation of Credit” events triggered on PCC-service node.
> Revalidation timeout | Indicates the total number of timeout events triggered for “Revalidation” on PCC-service node.
> IP Address Allocation | Indicates the total number of “IP Address Allocation” events triggered on PCC-service node.
> IP Address Release | Indicates the total number of “IP Address Release” events triggered on PCC-service node.
> Def EPS Bearer QoS Change | Indicates the total number of QoS change events triggered for Default EPS bearer on PCC-service node.
> AN-GW Change | Indicates the total number of “AN-GW (Access Network Gateway)” events triggered on PCC-service node.
> Successful Resource Alloc | Indicates the total number of “Successful Resource Allocation” events triggered on PCC-service node.
> Resource Modification Req | Indicates the total number of resource modification request messages received by PCC-service node.
> PGW Trace Control | Indicates the status of subscriber session trace control reported on PCC-service node for P-GW.
> UE Timezone Change | Indicates the total number of “UE Timezone Change” events triggered on PCC-service node.
> Usage Report | Indicates the total number of Usage Reports processed on PCC-service node.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883