> LTE Policy Configuration Mode Commands
> The LTE Policy Configuration Mode is used to create and manage the LTE policies for LTE/SAE networks.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> ho-restrict-list
> Creates a handover (HO) restriction list or specifies an existing HO restriction list and enters the Handover Restriction List Configuration Mode.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] ho-restrict-list list_name [ -noconfirm ]
> no
> Removes the specified restriction list from the system.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> list_name
> Specifies the name of the HO restriction list. If list_name does not refer to an existing list, a new list is created. list_name must be from 1 to 64 alphanumeric characters.
> Usage
> Use this command to enter the Handover Restriction List Configuration Mode for an existing list or for a newly defined list. This command is also used to remove an existing list.
> Entering this command results in the following prompt:
> [context_name]hostname(ho-restrict-list)#
> Handover Restriction List Configuration Mode commands are defined in the LTE Handover Restriction List Configuration Mode Commands chapter.
> Example
> The following command enters the Handover Restriction List Configuration Mode for a new or existing list named ho_restricit_list1:
> ho-restrict-list ho_restrict_list1
> subscriber-map
> Creates a subscriber map or specifies an existing subscriber map and enters the Subscriber Map Configuration Mode.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] subscriber-map map_name [ -noconfirm ]
> no
> Removes the specified subscriber map from the system.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> map_name
> Specifies the name of the subscriber map. If map_name does not refer to an existing map, a new map is created. map_name must be from 1 to 64 alphanumeric characters.
> Usage
> Enter the Subscriber Map Configuration Mode for an existing or newly defined map. This command is also used to remove an existing map.
> Entering this command results in the following prompt:
> [context_name]hostname(subscriber-map)#
> Subscriber Map Configuration Mode commands are defined in the Subscriber Map Configuration Mode Commands chapter.
> Example
> The following command enters the existing Subscriber Map Configuration Mode (or creates it if it does not already exist) for the map named map1:
> subscriber-map map1
> tai-mgmt-db
> Creates a Tracking Area Identifier (TAI) Management Database or specifies an existing database and enters the TAI Management Database Configuration Mode.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] tai-mgmt-db db_name [ -noconfirm ]
> no
> Removes the specified management database from the system.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> db_name
> Specifies the name of the management database. If db_name does not refer to an existing database, a new database is created. db_name must be from 1 to 64 alphanumeric characters.
> Usage
> Enter the TAI Management Database Configuration Mode for an existing or newly defined database. This command is also used to remove an existing database.
> Entering this command results in the following prompt:
> [context_name]hostname(tai-mgmt-db)#
> TAI Management Database Configuration Mode commands are defined in the TAI Management Database Configuration Mode Commands chapter.
> Example
> The following command enters the existing TAI Management Database configuration mode (or creates it if it does not already exist) for the database named tai_db1:
> tai-mgmt-db tai_db1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883