> System Schema Statistics
> The System schema provides operational statistics that can be used for monitoring and troubleshooting the following products: All
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the System-Level Schema

> Variables | Description | Data Type
> sess-ttlarrived | The total number of calls for all Session Managers for which registration requests were received. | Int32
> sess-ttlrejected | The total number of calls for all Session Managers that were rejected. | Int32
> sess-ttlconnected | The total number of calls for all Session Managers that are connected (including active, dormant, being set up, and being torn down). | Int32
> sess-ttlfailed | The total number of calls for all Session Managers that failed. | Int32
> sess-ttldisconn | The total number of calls disconnected for all Session Managers. | Int32
> sess-ttlhandoff | The total number of handoffs for all Session Managers. | Int64
> sess-ttlrenewal | The total number of renewals for all Session Managers. | Int64
> sess-ttlcallop | The total number of call operations for all Session Managers. The number of call operations is calculated as the total number of calls that arrived, were rejected, were disconnected, handed-off, and renewed. | Int64
> sess-ttlauthsucc | The total number of successful authentications for calls for all Session Managers. | Int32
> sess-ttlauthfail | The total number of failed authentications for calls for all Session Managers. | Int32
> sess-curaaaactive | Description: Indicates the number of current active AAA sessions for all Session Managers. Trigger: Increments whenever a new AAA session is established Decrements when the session is disconnected Availability: Per Session Manager instance Type: Gauge | Int32
> sess-curaaadeleting | Description: Indicates the number of current AAA sessions being deleted for all Session Managers. Trigger: Increments when a AAA session is disconnected and the final accounting message is still pending to be delivered to an external server Decrements when the final accounting message is delivered to the server Availability: Per Session Manager instance Type: Gauge | Int32
> sess-curaaaacctpending | Description: Indicates the number of current AAA sessions with accounting pending for all Session Managers. Trigger: Increments for every occurrence of AAA sessions with accounting message pending for all Session Managers Decrements when the accounting message is delivered to the external server Availability: Per Session Manager instance Type: Gauge | Int32
> sess-curaaaacctitemsused | Description: Indicates the number of current AAA accounting items used by all Session Manager instances. Trigger: Increments whenever the current AAA accounting request is generated and used by all Session Manager instances. Availability: Per Session Manager instance Type: Gauge | Int32
> sess-curaaaacctitemsmax | Description: Indicates the number of current AAA accounting items allowed by all Session Manager instances. Trigger: Increments whenever the current AAA accounting request is allowed by all Session Manager instances. Availability: Per Session Manager instance Type: Gauge | Int32
> sess-curaaabuffused | Description: Indicates the number of current AAA buffer space in megabytes used by all Session Manager instances. Trigger: Increments whenever the current AAA buffer is allocated and used by all Session Manager instances Decrements whenever the current AAA buffer is freed for use Availability: Per Session Manager instance Type: Gauge | Int32
> sess-curaaabuffmax | Description: Indicates the current maximum AAA buffer space allowed in megabytes used by all Session Manager instances. Trigger: Increments whenever the current AAA buffer space is allowed and used by all Session Manager instances Availability: Per Session Manager instance Type: Gauge | Int32
> sess-ttlaaacancauth | Description: The total number of AAA authentication requests cancelled by all Session Manager instances. The cancellation can be due to various reasons like administrative clear or access side call clear, etc. Trigger: Increments when a Session Manager cancels an outstanding authentication request which is waiting for a response from authentication server. Availability: Per Session Manager instance | Int32
> sess-ttlaaaacctpurged | Description: The total number of AAA accounting requests received by this Session Manager instance, that have to be purged for all Session Managers because the storage limit of pending accounting requests has exceeded. Trigger: Increments whenever a AAA accounting request has to be purged for all Session Managers Availability: Per Session Manager instance | Int32
> sess-ttlradacctpurged | Description: The total number of RADIUS accounting requests received by this Session Manager instance, that have to be purged for all Session Managers because the storage limit of pending accounting requests has exceeded. Trigger: Increments whenever a RADIUS accounting request has to be purged for all Session Managers Availability: Per Session Manager instance | Int32
> sess-ttllcpup | The total number of calls for all Session Managers that have completed the Link Control Protocol (LCP) phase of the registration process. | Int32
> sess-ttlipcpup | The total number of calls for all Session Managers that have completed the Internet Protocol Control Protocol (IPCP) phase of the registration process. | Int32
> sess-ttlsrcviol | The total number of source violations experienced for all calls for all Session Managers. | Int32
> sess-ttlkeepfail | The total number of keep-alive failures experienced for all calls for all Session Managers. | Int32
> sess-ttlemptyfwd | The total number of empty forwarded packet sessions. | Int32
> sess-ttlemptyrev | The total number of empty reverse packet sessions. | Int32
> sess-ttlproxydns-redirect | The total number of sessions redirected by Proxy-DNS. | Int32
> sess-ttlproxydns-passthru | The total number of sessions passed through by Proxy-DNS. | Int32
> sess-ttlproxydns-drop | The total number of sessions dropped by Proxy-DNS. | Int32
> sess-curttlcalls | The number of calls for all Session Managers that are currently in progress (active, dormant, being set up, or being torn down). | Int32
> sess-curnonanchorconn | Total number of non-anchor session connections on ASN-GW. | Int32
> sess-cursipconn | The total number of Simple IP data sessions that are currently being supported for all Session Managers. | Int32
> sess-curmipconn | The total number of Mobile IP data sessions that are currently being supported for all Session Managers. | Int32
> sess-curpmipconn | The total number of Proxy Mobile IP data sessions that are currently being supported for all Session Managers. | Int32
> sess-curhaipsecconn | The total number of sessions that are in progress in the HA-IPSEC connected state | Int32
> sess-curl2tplacconn | The number of L2TP LAC sessions that are currently being supported for all Session Managers. Type: Gauge | Int32
> sess-curpdptypeipconn | The number of sessions that are currently in progress in the PDP-TYPE-IP Connected State Type: Gauge | Int32
> sess-curpdptypepppconn | The number of sessions that are currently in progress in the PDP-TYPE-PPP Connected State Type: Gauge | Int32
> sess-curbcmcsconn | The number of sessions that are currently in progress in the BCMCS Connected State. Type: Gauge | Int32
> sess-curactcall | The number of sessions currently active for all Session Managers. Type: Gauge | Int32
> sess-curdormcall | The number of sessions currently dormant for all Session Managers. Type: Gauge | Int32
> sess-curalwayson | The number of always-on calls that are currently in progress. Type: Gauge | Int32
> sess-curarrived | The number of sessions that are currently at the onset of the registration process for all Session Managers. Type: Gauge | Int32
> sess-curlcpnegot | The number of sessions for all Session Managers that are currently in the Link Control Protocol (LCP) negotiation phase of the registration process. Type: Gauge | Int32
> sess-curlcpup | The number of sessions for all Session Managers that have just completed the Link Control Protocol (LCP) negotiation phase of the registration process. Type: Gauge | Int32
> sess-curauth | The number of sessions for all Session Managers that are currently in the process of being authenticated. Type: Gauge | Int32
> sess-curbcmcsauth | The number of sessions currently in progress that are at the BCMCS Service Authenticating state. Type: Gauge | Int32
> sess-curauthed | The number of sessions for all Session Managers that have just completed the authentication phase of the registration process. Type: Gauge | Int32
> sess-curdhcppending | The number of sessions for all Session Managers that are pending for DHCP. Type: Gauge | Int32
> sess-curl2tplacconnecting | The number of sessions currently in progress that are at the L2TP-LAC Connecting state. Type: Gauge | Int32
> sess-curipcpup | The number of sessions for all Session Managers that have just completed the Internet Protocol Control Protocol (IPCP) phase of the registration process. Type: Gauge | Int32
> sess-curimsauthorizing | The number of sessions for all Session Managers that are currently in the process of being authorized for IMS. Type: Gauge | Int32
> sess-curimsauthorized | The number of sessions for all Session Managers that are currently being authorized for IMS. Type: Gauge | Int32
> sess-curmmeattached | The total number of MME sessions that are currently attached with this MME. Type: Gauge | Int32
> sess-curdisc | The number of sessions for all Session Managers that are currently in the process of disconnecting. Type: Gauge | Int32
> sess-ttlprepaid | The total number of pre-paid sessions processed by all Session Managers. | Int32
> sess-curprepaid | The number of pre-paid sessions currently being processed by all Session Managers. Type: Gauge | Int32
> sess-ttlonlineauthreq | The total number of 3gpp2 online authentication requests for all Session Managers. | Int32
> sess-ttlonlineauthsucc | The total number of successful authentications for Online Access Requests for all Session Managers. | Int32
> sess-ttlonlineauthfail | The total number of failed authentications for Online Access Requests for all Session Managers. | Int32
> sess-ttlonlineprepaiderr | The total number of 3gpp2 online prepaid errors. | Int32
> sess-ttlprepaidinitautherr | The total number of 3gpp2 prepaid initial authorization errors. | Int32
> sess-ttlcrprpattempt | The total number of Closed RP-RP handoff attempted. | Int32
> sess-ttlcrprpsuccess | The total number of Closed RP-RP handoff succeeded. | Int32
> sess-ttlrpcrpattempt | The total number of RP-Closed RP handoff attempted. | Int32
> sess-ttlrpcrpsuccess | The total number of RP-Closed RP handoff succeeded. | Int32
> sess-ttlinterasngwattempt | The total number of sessions attempted for inter-ASN-GW handover. | Int32
> sess-ttlinterasngwsuccess | The total number of sessions attempts successful for inter-ASN-GW handover. | Int32
> sess-ttlintraasngwattempt | The total number of sessions attempted for intra-ASN-GW handover. | Int32
> sess-ttlintraasngwsuccess | The total number of sessions attempts successful for intra-ASN-GW handover. | Int32
> sess-rxpkt-16 | The total number of uplink packets (sent from the UE) of less than 17 bytes in length received by all Session Managers. | Int64
> sess-txpkt-16 | The total number of downlink packets (sent to the UE) of less than 17 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-64 | The total number of uplink packets (sent from the UE) between 17 and 64 bytes in length received by all Session Managers. | Int64
> sess-txpkt-64 | The total number of downlink packets (sent to the UE) between 17 and 64 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-127 | The total number of uplink packets (sent from the UE) between 65 and 127 bytes in length received by all Session Managers. | Int64
> sess-txpkt-127 | The total number of downlink packets (sent to the UE) between 65 and 127 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-255 | The total number of uplink packets (sent from the UE) between 128 and 255 bytes in length received by all Session Managers. | Int64
> sess-txpkt-255 | The total number of downlink packets (sent to the UE) between 128 and 255 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-511 | The total number of uplink packets (sent from the UE) between 256 and 511 bytes in length received by all Session Managers. | Int64
> sess-txpkt-511 | The total number of downlink packets (sent to the UE) between 256 and 511 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-1023 | The total number of uplink packets (sent from the UE) between 512 and 1023 bytes in length received by all Session Managers. | Int64
> sess-txpkt-1023 | The total number of downlink packets (sent to the UE) between 512 and 1023 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-2047 | The total number of uplink packets (sent from the UE) between 1024 and 2047 bytes in length received by all Session Managers. | Int64
> sess-txpkt-2047 | The total number of downlink packets (sent to the UE) between 1024 and 2047 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-4095 | The total number of uplink packets (sent from the UE) between 2048 and 4095 bytes in length received by all Session Managers. | Int64
> sess-txpkt-4095 | The total number of downlink packets (sent to the UE) between 2048 and 4095 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-4500 | The total number of uplink packets (sent from the UE) between 4096 and 4500 bytes in length received by all Session Managers. | Int64
> sess-txpkt-4500 | The total number of downlink packets (sent to the UE) between 4096 and 4500 bytes in length transmitted by all Session Managers. | Int64
> sess-rxpkt-over4500 | The total number of uplink packets (sent from the UE) greater than 4500 bytes in length received by all Session Managers. | Int64
> sess-txpkt-over4500 | The total number of downlink packets (sent to the UE) greater than 4500 bytes transmitted by all Session Managers. | Int64
> sess-txbytes | The number of downlink bytes (sent to the UE) transmitted by all Session Managers. | Int64
> sess-rxbytes | The number of uplink bytes (sent from the UE) received by all Session Managers. | Int64
> sess-txpackets | The number of downlink packets (sent to the UE) transmitted by all Session Managers. | Int64
> sess-rxpackets | The number of uplink packets (sent from the UE) received by all Session Managers. | Int64
> sess-ttlconnected-1xrtt | The total number of sessions connected with 1xrtt. | Int32
> sess-txbytes-1xrtt | The number to bytes transmitted via 1rxtt. | Int64
> sess-rxbytes-1xrtt | The number to bytes received via 1rxtt. | Int64
> sess-txpackets-1xrtt | The number to packets transmitted via 1rxtt. | Int64
> sess-rxpackets-1xrtt | The number to packets received via 1rxtt. | Int64
> sess-ttlconnected-evdorev0 | The total number of sessions connected with EvDO Rev 0. | Int32
> sess-txbytes-evdorev0 | The number to bytes transmitted via EvDO Rev 0. | Int64
> sess-rxbytes-evdorev0 | The number to bytes received via EvDO Rev 0. | Int64
> sess-txpackets-evdorev0 | The number to packets transmitted via EvDO Rev 0. | Int64
> sess-rxpackets-evdorev0 | The number to packets received via EvDO Rev 0. | Int64
> sess-ttlconnected-evdoreva | The total number of sessions connected with EvDO Rev A. | Int32
> sess-txbytes-evdoreva | The number to bytes transmitted via EvDO Rev A. | Int64
> sess-rxbytes-evdoreva | The number to bytes received via EvDO Rev A. | Int64
> sess-txpackets-evdoreva | The number to packets transmitted via EvDO Rev A. | Int64
> sess-rxpackets-evdoreva | The number to packets received via EvDO Rev A. | Int64
> sess-siptxbytes | The number of bytes transmitted for Simple IP-type sessions. | Int64
> sess-siprxbytes | The number of bytes received for Simple IP-type sessions. | Int64
> sess-miptxbytes | The number of bytes transmitted for Mobile IP-type sessions. | Int64
> sess-miprxbytes | The number of bytes received for Mobile IP-type sessions. | Int64
> sess-calldur-1min | The total number of sessions for all Session Managers that lasted less than 1 minute. | Int32
> sess-calldur-2min | The total number of sessions for all Session Managers that lasted less than 2 minutes but were greater than or equal to 1 minute. | Int32
> sess-calldur-5min | The total number of sessions for all Session Managers that lasted less than 5 minutes but were greater than or equal to 2 minutes. | Int32
> sess-calldur-15min | The total number of sessions for all Session Managers that lasted less than 15 minutes but were greater than or equal to 5 minutes. | Int32
> sess-calldur-1hour | The total number of sessions for all Session Managers that lasted less than 1 hour but greater than or equal to 15 minutes. | Int32
> sess-calldur-4hour | The total number of sessions for all Session Managers that lasted less than 4 hours but were greater than or equal to 1 hour. | Int32
> sess-calldur-12hour | The total number of sessions for all Session Managers that lasted less than 12 hours but were greater than or equal to 4 hours. | Int32
> sess-calldur-24hour | The total number of sessions for all Session Managers that lasted less than 24 hours but were greater than or equal to 12 hours. | Int32
> sess-calldur-over24hour | The total number of sessions for all Session Managers that lasted 24 hours or longer. | Int32
> sess-setuptime-100ms | The total number of sessions for all Session Managers that were setup in less than 100 milliseconds. | Int32
> sess-setuptime-200ms | The total number of sessions for all Session Managers for which the setup time was less than 200 milliseconds but greater than or equal to 100 milliseconds. | Int32
> sess-setuptime-300ms | The total number of sessions for all Session Managers for which the setup time was less than 300 milliseconds but greater than or equal to 200 milliseconds. | Int32
> sess-setuptime-400ms | The total number of sessions for all Session Managers for which the setup time was less than 400 milliseconds but greater than or equal to 300 milliseconds. | Int32
> sess-setuptime-500ms | The total number of sessions for all Session Managers for which the setup time was less than 500 milliseconds but greater than or equal to 400 milliseconds. | Int32
> sess-setuptime-600ms | The total number of sessions for all Session Managers for which the setup time was less than 600 milliseconds but greater than or equal to 500 milliseconds. | Int32
> sess-setuptime-700ms | The total number of sessions for all Session Managers for which the setup time was less than 700 milliseconds but greater than or equal to 600 milliseconds. | Int32
> sess-setuptime-800ms | The total number of sessions for all Session Managers for which the setup time was less than 800 milliseconds but greater than or equal to 700 milliseconds. | Int32
> sess-setuptime-900ms | The total number of sessions for all Session Managers for which the setup time was less than 900 milliseconds but greater than or equal to 800 milliseconds. | Int32
> sess-setuptime-1sec | The total number of sessions for all Session Managers for which the setup time was less than 1 second but greater than or equal to 200 milliseconds. | Int32
> sess-setuptime-2sec | The total number of sessions for all Session Managers for which the setup time was less than 2 seconds but greater than or equal to 1 second. | Int32
> sess-setuptime-3sec | The total number of sessions for all Session Managers for which the setup time was less than 3 seconds but greater than or equal to 2 seconds. | Int32
> sess-setuptime-4sec | The total number of sessions for all Session Managers for which the setup time was less than 4 seconds but greater than or equal to 3 seconds. | Int32
> sess-setuptime-6sec | The total number of sessions for all Session Managers for which the setup time was less than 6 seconds but greater than or equal to 4 seconds. | Int32
> sess-setuptime-8sec | The total number of sessions for all Session Managers for which the setup time was less than 8 seconds but greater than or equal to 6 seconds. | Int32
> sess-setuptime-10sec | The total number of sessions for all Session Managers for which the setup time was less than 10 seconds but greater than or equal to 8 seconds. | Int32
> sess-setuptime-12sec | The total number of sessions for all Session Managers for which the setup time was less than 12 seconds but greater than or equal to 10 seconds. | Int32
> sess-setuptime-14sec | The total number of sessions for all Session Managers for which the setup time was less than 14 seconds but greater than or equal to 12 seconds. | Int32
> sess-setuptime-16sec | The total number of sessions for all Session Managers for which the setup time was less than 16 seconds but greater than or equal to 14 seconds. | Int32
> sess-setuptime-over16sec | The total number of sessions for all Session Managers for which the setup time was 16 seconds or more. | Int32
> sess-setuptime-18sec | Proprietary counter indicates the total number of sessions for all Session Managers for which the setup time was more than 16 seconds but less than or equal to 18 seconds. Triggers: changes every time when a new session takes setup time of more that 16 seconds but less than or equal to 18 seconds. Availability: Across the System. | Int32
> sess-setuptime-over18sec | Proprietary counter indicates the total number of sessions for all Session Managers for which the setup time was more than 18seconds. Triggers: changes every time when a new session takes more than 18 seconds to setup. Availability: Across the System. | Int32
> ggsn-ttlsgsnconn | Total number of connections registered between GGSN and SGSN on this system. | Int32
> ggsn-cursgsnact | Total number of SGSNs active with GGSN on this system. | Int32
> flow-ttlestab | The total number of flows that were established by the session manager. | Int32
> flow-ttldisconn | The total number of flows that were disconnected by the session manager. | Int32
> flow-curdynamic | The current number of dynamic flows. | Int32
> aaa-ttlreq | Description: The total number of AAA requests. Trigger: Increments when a AAA request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curreq | Description: The number of active AAA requests. Trigger: Increments when an active AAA request is sent to the server Decrements when a response is received from the server for the active AAA request Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlauthreq | Description: The total number of AAA authentication requests. Trigger: Increments when a AAA authentication request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curauthreq | Description:The number of active AAA authentication requests. Trigger: Increments when an active AAA authentication request is sent to the server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlauthprobe | Description: The total number of AAA authentication probes. Trigger: Increments when a AAA authentication probe request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curauthprobe | Description: The number of active AAA authentication probes. Trigger: Increments when an active AAA authentication probe request is sent to the server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlauthkeepalive | Description: The total number of AAA authentication keepalive requests sent. Trigger: Increments when a AAA authentication keepalive request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curauthkeepalive | Description: The number of current AAA authentication keepalive requests being processed. Trigger: Increments when an active AAA authentication keepalive request is sent to the server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlacctreq | Description: The total number of AAA accounting requests. Trigger: Increments when a AAA accounting request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curacctreq | Description: The number of active AAA accounting requests. Trigger: Increments when an active AAA accounting request is sent to the server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlacctkeepalive | Description: The total number of AAA accounting keepalive requests sent. Trigger: Increments when a AAA accounting keepalive request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curacctkeepalive | Description: The number of current AAA accounting keepalive requests being processed. Trigger: Increments when an active AAA accounting keepalive request is sent to the server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlauthsucc | Description: The total number of successful AAA authentication. Trigger: Increments whenever the AAA authentication is successful Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthfail | Description: The total number of AAA authentication failed. Trigger: Increments whenever the AAA authentication fails Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthpurged | Description: The total number of AAA authentication purged. Trigger: Increments whenever a AAA authentication request is purged Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthcancelled | Description: The total number of AAA authentication requests cancelled. Trigger: Increments whenever a AAA authentication request is cancelled Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthkeepalivesuccess | Description: The total number of AAA authentication keepalive successes. Trigger: Increments whenever a AAA keepalive authentication is successful Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthkeepalivefailure | Description: The total number of AAA authentication keepalive failures. Trigger: Increments whenever a AAA keepalive authentication fails Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthkeepalivepurged | Description: The total number of AAA authentication keepalive purges. Trigger: Increments whenever a AAA authentication keepalive request is purged Availability: Per AAA Manager Instance | Int32
> aaa-ttlauthdmuchal | Description: The total number of AAA authentication DMU challenged. Trigger: Increments whenever a AAA authentication request is challenged for Dynamic Mobile Keying update. Availability: Per AAA Manager Instance | Int32
> aaa-curallocreq | Description: The number of current allocation requests being processed. Trigger: Increments when a currently allocated request has been processed Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-curmaxreq | Description: The number of current maximum requests being processed. Trigger: Increments when a current maximum request has been processed Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttldiamauthreq | Description: The total number of Diameter authentication requests. Trigger: Increments when a Diameter authentication request is sent to the Diameter server Availability: Per AAA Manager Instance | Int32
> aaa-curdiamauthreq | Description: The total number of current Diameter authentication requests. Trigger: Increments when a Diameter authentication request is sent to the Diameter server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttldiamauthreqretried | Description: The total number of Diameter authentication requests retried. Trigger: Increments when a Diameter authentication request is retried Availability: Per AAA Manager Instance | Int32
> aaa-ttldiamauthreqdrop | Description: The total number of Diameter authentication requests dropped. Trigger: Increments when a Diameter authentication request is dropped or ignored Availability: Per AAA Manager Instance | Int32
> aaa-ttlradauthreq | Description: The total number of AAA authentication requests on RADIUS server. Trigger: Increments when a AAA authentication request is sent to the RADIUS server Availability: Per AAA Manager Instance | Int32
> aaa-curradauthreq | Description: The number of active AAA authentication requests on RADIUS server. Trigger: Increments when an active AAA authentication request is sent to the RADIUS server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlradauthreqretried | Description: The total number of AAA authentication requests retried on RADIUS server. Trigger: Increments when a AAA authentication request is retried on to the RADIUS server Availability: Per AAA Manager Instance | Int32
> aaa-ttlradauthrspdrop | Description: The total number of RADIUS authentication requests dropped. Trigger: Increments when a RADIUS authentication request is dropped or ignored Availability: Per AAA Manager Instance | Int32
> aaa-ttllclauthreq | Description: The total number of AAA authentication requests on local server. Trigger: Increments when a AAA authentication request is sent to the local server Availability: Per AAA Manager Instance | Int32
> aaa-curlclauthreq | Description: The number of active local authentication requests. Trigger: Increments when an active AAA authentication request is sent to the local server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlpseudoauthreq | Description: The total number of pseudo AAA authentication requests. Trigger: Increments when a pseudo AAA authentication request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-curpseudoauthreq | Description: The number of active pseudo AAA authentication requests. Trigger: Increments when an active pseudo AAA authentication request is sent to the server Availability: Per AAA Manager Instance Type: Gauge | Int32
> aaa-ttlauthnulluser | Description: The total number of unattempted AAA authentication requests. Trigger: Increments when an unattempted AAA authentication request is sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-ttlacctsucc | Description: The total number of AAA accounting requests succeeded. Trigger: Increments when a AAA accounting request is successfully sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-ttlacctpurged | Description: The total number of AAA accounting requests purged. Trigger: Increments when a AAA accounting request is purged Availability: Per AAA Manager Instance | Int32
> aaa-ttlacctcancelled | Description: The total number of AAA accounting requests cancelled. Trigger: Increments when a AAA accounting request is cancelled Availability: Per AAA Manager Instance | Int32
> aaa-ttlacctkeepalivesuccess | Description: The total number of AAA accounting keepalive successes. Trigger: Increments when a AAA accounting keepalive request is successfully sent to the server Availability: Per AAA Manager Instance | Int32
> aaa-ttlacctkeepalivetimeout | Description: The total number of AAA accounting keepalive timeouts Trigger: Increments when a AAA accounting keepalive request is timed out Availability: Per AAA Manager Instance | Int32
> aaa-ttlacctkeepalivepurged | Description: The total number of AAA accounting keepalive purges. Trigger: Increments when a AAA accounting keepalive request is purged Availability: Per AAA Manager Instance | Int32
> aaa-ttlradacctreq | Description: The total number of RADIUS accounting requests. Trigger: Increments when a RADIUS accounting request is sent to the RADIUS server Availability: Per AAA Manager Instance | Int32
> aaa-ttlradacctcancelled | Description: The total number of RADIUS accounting requests cancelled. Trigger: Increments when a RADIUS accounting request is cancelled Availability: Per AAA Manager Instance | Int32
> aaa-ttlradacctpurged | Description: The total number of RADIUS accounting requests purged. Trigger: Increments when a RADIUS accounting request is purged Availability: Per AAA Manager Instance | Int32
> aaa-ttlradacctreqretried | Description: The total number of AAA accounting requests retried on RADIUS server. Trigger: Increments when a AAA accounting request is retried on to the RADIUS server Availability: Per AAA Manager Instance | Int32
> aaa-ttlradacctrspdropped | Description: The total number of RADIUS accounting requests dropped. Trigger: Increments when a RADIUS accounting request is dropped or ignored Availability: Per AAA Manager Instance | Int32
> aaa-ttlmgrpurgedrequests | Description: The total number of AAAMgr purged requests. Trigger: Increments for every occurrence of AAA Manager purged requests Availability: Per AAA Manager Instance | Int32
> diamauth-msg-mareq | Description: Diameter Authentication Message Stats - The total number of Multimedia-Auth-Request messages sent. Triggers: Increments when an MAR is sent Availability: Per AAA Manager instance. | Int32
> diamauth-msg-maans | Description: Diameter Authentication Message Stats - The total number of Multimedia-Auth-Answer messages received. Triggers: Increments when an MAA is received Availability: Per AAA Manager instance. | Int32
> diamauth-msg-marretry | Description: Diameter Authentication Message Stats - Total number of retries for Multimedia-Auth-Request messages. Triggers: Increments when an MAR is retried Availability: Per AAA Manager instance. | Int32
> diamauth-msg-maatimeout | Description: Diameter Authentication Message Stats - The total number of timeouts of Multimedia-Auth-Answer messages. Triggers: Increments when an MAA is timed out Availability: Per AAA Manager instance. | Int32
> diamauth-msg-maadropped | Description: Diameter Authentication Message Stats - The total number of Multimedia-Auth-Answer messages dropped. Triggers: Increments when an MAA is dropped Availability: Per AAA Manager instance. | Int32
> diamauth-msg-sareq | Description: Diameter Authentication Message Stats - The total number of Server-Assignment-Request messages sent. Triggers: Increments when an SAR is sent Availability: Per AAA Manager instance. | Int32
> diamauth-msg-saans | Description: Diameter Authentication Message Stats - The total number of Server-Assignment-Answer messages received. Triggers: Increments when an SAA is received Availability: Per AAA Manager instance. | Int32
> diamauth-msg-sarretry | Description: Diameter Authentication Message Stats - The total number of retries for Server-Assignment-Request Messages. Triggers: Increments when an SAR is retried Availability: Per AAA Manager instance. | Int32
> diamauth-msg-saatimeout | Description: Diameter Authentication Message Stats - The total number of timeouts of Server-Assignment-Answer messages. Triggers: Increments when an SAA is timed out Availability: Per AAA Manager instance. | Int32
> diamauth-msg-saadropped | Description: Diameter Authentication Message Stats - The total number of Server-Assignment-Answer messages dropped. Triggers: Increments when an SAA is dropped Availability: Per AAA Manager instance. | Int32
> diamauth-msg-uareq | Description: Diameter Authentication Message Stats - The total number of User-Authorization-Request messages sent. Triggers: Increments when a UAR is sent Availability: Per AAA Manager instance. | Int32
> diamauth-msg-uaans | Description: Diameter Authentication Message Stats - The total number of User-Authorization-Answer messages received. Triggers: Increments when a UAA is received Availability: Per AAA Manager instance. | Int32
> diamauth-msg-uarretry | Description: Diameter Authentication Message Stats - The total number of retries for User-Authorization-Request messages. Triggers: Increments when a UAR is retried Availability: Per AAA Manager instance. | Int32
> diamauth-msg-uaatimeout | Description: Diameter Authentication Message Stats - The total number of timeouts of User-Authorization-Answer messages. Triggers: Increments when a UAA is timed out Availability: Per AAA Manager instance. | Int32
> diamauth-msg-uaadropped | Description: Diameter Authentication Message Stats - The total number of User-Authorization-Answer messages dropped. Triggers: Increments when a UAA is dropped Availability: Per AAA Manager instance. | Int32
> diamauth-msg-lireq | Description: Diameter Authentication Message Stats - The total number of Location-Info-Request messages sent. Triggers: Increments when an LIR is sent Availability: Per AAA Manager instance. | Int32
> diamauth-msg-lians | Description: Diameter Authentication Message Stats - The total number of Location-Info-Answer messages received. Triggers: Increments when an LIA is received Availability: Per AAA Manager instance. | Int32
> diamauth-msg-lirretry | Description: Diameter Authentication Message Stats - The total number of retries for Location-Info-Request messages. Triggers: Increments when an LIR is retried Availability: Per AAA Manager instance. | Int32
> diamauth-msg-liatimeout | Description: Diameter Authentication Message Stats - The total number of timeouts of Location-Info-Answer messages. Triggers: Increments when an LIA is timed out Availability: Per AAA Manager instance. | Int32
> diamauth-msg-liadropped | Description: Diameter Authentication Message Stats - The total number of Location-Info-Answer messages dropped. Triggers: Increments when an LIA is dropped Availability: Per AAA Manager instance. | Int32
> diamauth-msg-rtreq | Description: Diameter Authentication Message Stats - The total number of Registration-Termination-Request messages received. Triggers: Increments when an RTR is received Availability: Per AAA Manager instance. | Int32
> diamauth-msg-rtans | Description: Diameter Authentication Message Stats - The total number of Registration-Termination-Answer messages sent. Triggers: Increments when an RTA is sent Availability: Per AAA Manager instance. | Int32
> diamauth-msg-rtrreject | Description: Diameter Authentication Message Stats - The total number of Registration-Termination-Request messages rejected. Triggers: Increments when an RTR is rejected. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-ppreq | Description: Diameter Authentication Message Stats - The total number of Push-Profile-Request messages received. Triggers: Increments when a PPR is received. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-ppans | Description: Diameter Authentication Message Stats - The total number of Push-Profile-Answer Messages Request messages sent. Triggers: Increments when a PPR is sent. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-pprreject | Description: Diameter Authentication Message Stats - The total number of Push-Profile-Request messages rejected. Triggers: Increments when a PPR is rejected. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-dereq | Description: Diameter Authentication Message Stats - The total number of Diameter-EAP-Request messages sent. Triggers: Increments when a DER is sent. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-deans | Description: Diameter Authentication Message Stats - The total number of Diameter-EAP-Answer messages received. Triggers: Increments when a DEA is received. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-deaaccept | Description: Diameter Authentication Message Stats - The total number of Diameter-EAP-Answer messages accepted. Triggers: Increments when a DEA is received with Result-Code value as 2001. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-deareject | Description: Diameter Authentication Message Stats - The total number of Diameter-EAP-Answer messages rejected. Triggers: Increments when a DEA is rejected. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-derretry | Description: Diameter Authentication Message Stats - The total number of retries for Diameter-EAP-Request messages. Triggers: Increments when a DER is retried. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-deatimeout | Description: Diameter Authentication Message Stats - The total number of timeouts of Diameter-EAP-Answer messages. Triggers: Increments when a DEA is timed out. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-deadropped | Description: Diameter Authentication Message Stats - The total number of Diameter-EAP-Answer messages dropped. Triggers: Increments when a DEA is dropped. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-asr | Description: Diameter Authentication Message Stats - The total number of Abort-Session-Request messages received. Triggers: Increments when an ASR is received. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-asa | Description: Diameter Authentication Message Stats - The total number of Abort-Session-Answer messages sent. Triggers: Increments when an ASA is sent. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-rar | Description: Diameter Authentication Message Stats - The total number of Re-Auth-Request messages received. Triggers: Increments when an RAR is received. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-raa | Description: Diameter Authentication Message Stats - The total number of Re-Auth-Answer messages sent. Triggers: Increments when an RAA is sent. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-str | Description: Diameter Authentication Message Stats - The total number of Session-Termination-Request messages sent. Triggers: Increments when an STR is sent. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-sta | Description: Diameter Authentication Message Stats - The total number of Session-Termination-Answer messages received. Triggers: Increments when an STA is received. Availability: Per AAA Manager instance. | Int32
> diamauth-msg-strretry | Description: Diameter Authentication Message Stats - The total number of retries for Session-Termination-Request Messages. Triggers: Increments when an STR is retried Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-proto | Description: Diameter Authentication DE Message Error Stats - The total number of error messages received with error Diameter Protocol Errors. Triggers: Increments when a DEA is received with 3xxx result-code. Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-badans | Description: Diameter Authentication DE Message Error Stats - The total number of error messages received with error Bad-Answer. Triggers: Increments when a DEA is received with malformed or wrong AVPs. Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-unksessreq | Description: Diameter Authentication DE Message Error Stats - The total number of error messages received with error Session-Id or unknown session values. Triggers: Increments when a DEA is received with unknown session-id. Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-unkcmd | This variable is obsolete. | Int32
> diamauth-demsgerr-badreq | Description: Diameter Authentication DE Message Error Stats - The total number of error messages received with bad request command code value. Triggers: Increments when a DEA is received with wrong command-code value. Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-reqtmo | Description: Diameter Authentication DE Message Error Stats - The total number of Request Timeout happened for DER message. Triggers: Increments when a DER is timed out. Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-parse | Description: Diameter Authentication DE Message Error Stats - The total number of parse failures happened for DEA message. Triggers: Increments when parse failure happens for DEA. Availability: Per AAA Manager instance. | Int32
> diamauth-demsgerr-reqretry | Description: Diameter Authentication DE Message Error Stats - The total number of request retries happened for DER message. Triggers: Increments when a DER is retried Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-logout | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Diameter-Logout. Triggers: Increments when an STR is sent with Termination-Cause as Diameter-Logout. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-noserv | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Service-Not-Provided. Triggers: Increments when an STR is sent with Termination-Cause as Service-Not-Provided. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-badans | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Bad-Answer. Triggers: Increments when an STR is sent with Termination-Cause as Bad-Answer. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-admin | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Administrative. Triggers: Increments when an STR is sent with Termination-Cause as Administrative. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-linkbroken | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Link-Broken Triggers: Increments when an STR is sent with Termination-Cause as Link-Broken. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-authexp | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Auth-Expired. Triggers: Increments when an STR is sent with Termination-Cause as Auth-Expired. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-usermoved | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause User-Moved. Triggers: Increments when an STR is sent with Termination-Cause as User-Moved. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-sesstmo | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Session-Timeout. Triggers: Increments when an STR is sent with Termination-Cause as Session-Timeout. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-userreq | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause User-Request. Triggers: Increments when an STR is sent with Termination-Cause as User-Request. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-lostcarrier | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Lost Carrier. Triggers: Increments when an STR is sent with Termination-Cause as Lost-Carrier. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-lostsvc | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Lost Service. Triggers: Increments when an STR is sent with Termination-Cause as Lost-Service. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-idletmo | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Idle-Timeout. Triggers: Increments when an STR is sent with Termination-Cause as Idle-Timeout. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-nastmo | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause NAS Related Session-Timeout. Triggers: Increments when an STR is sent with Termination-Cause as NAS-Related-Session-Timeout. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-adminreset | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Admin-Reset. Triggers: Increments when an STR is sent with Termination-Cause as Admin-Reset. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-adminreboot | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Admin Reboot. Triggers: Increments when an STR is sent with Termination-Cause as Admin-Reboot. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-port | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Port Error Triggers: Increments when an STR is sent with Termination-Cause as Port-Error. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-naserr | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause NAS Error. Triggers: Increments when an STR is sent with Termination-Cause as NAS-Error. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-nasreq | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause NAS Request. Triggers: Increments when an STR is sent with Termination-Cause as NAS-Request. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-nasreboot | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause NAS Reboot. Triggers: Increments when an STR is sent with Termination-Cause as NAS-Reboot. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-portunneed | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Port Unneeded. Triggers: Increments when an STR is sent with Termination-Cause as Port-Unneeded. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-portpreempt | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Port Preempted. Triggers: Increments when an STR is sent with Termination-Cause as Port-Preempted. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-portsusp | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Port Suspended. Triggers: Increments when an STR is sent with Termination-Cause as Port-Suspended. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-svcunavail | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Service Unavailable. Triggers: Increments when an STR is sent with Termination-Cause as Service-Unavailable. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-cback | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Callback. Triggers: Increments when an STR is sent with Termination-Cause as Callback. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-user | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause User-Error. Triggers: Increments when an STR is sent with Termination-Cause as User-Error. Availability: Per AAA Manager instance. | Int32
> diamauth-strterm-hostreq | Description: Diameter Authentication STR Termination Cause Stats - The total number of Session-Termination-Request messages with termination cause Host-Request. Triggers: Increments when an STR is sent with Termination-Cause as Host-Request. Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acreq | Description: Diameter Accounting Message Stats - The total number of Accounting-Request messages sent. Triggers: Increments when an ACR is sent Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acans | Description: Diameter Accounting Message Stats - The total number of Accounting-Answer messages received. Triggers: Increments when an ACA is received Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrstart | Description: Diameter Accounting Message Stats - The total number of Accounting-Request Start messages sent. Triggers: Increments when an ACR-START is sent Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acastart | Description: Diameter Accounting Message Stats - The total number of Accounting-Answer Start messages received. Triggers: Increments when an ACA-START is received Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrstartretry | Description: Diameter Accounting Message Stats - The total number of retries for Accounting-Request Start messages. Triggers: Increments when an ACR-START is retried Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acastarttmo | Description: Diameter Accounting Message Stats - The total number of timeouts of Accounting-Answer Start messages. Triggers: Increments when an ACA-START is timed out Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrinterim | Description: Diameter Accounting Message Stats - The total number of Accounting-Request Interim messages sent. Triggers: Increments when an ACR-INTERIM is sent Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acainterim | Description: Diameter Accounting Message Stats - The total number of Accounting-Answer Interim messages received. Triggers: Increments when an ACA-INTERIM is received Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrinterimretry | Description: Diameter Accounting Message Stats - The total number of retries for Accounting-Request Interim messages. Triggers: Increments when an ACR-INTERIM is retried Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acainterimtmo | Description: Diameter Accounting Message Stats - The total number of timeouts of Accounting-Answer Interim messages. Triggers: Increments when an ACA-INTERIM is timed out Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrevent | Description: Diameter Accounting Message Stats - The total number of Accounting-Request Event messages sent. Triggers: Increments when an ACR-EVENT is sent Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acaevent | Description: Diameter Accounting Message Stats - The total number of Accounting-Answer Event messages received. Triggers: Increments when an ACA-EVENT is received Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrstop | Description: Diameter Accounting Message Stats - The total number of Accounting-Request Stop messages sent. Triggers: Increments when an ACR-STOP is sent. Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acastop | Description: Diameter Accounting Message Stats - The total number of Accounting-Answer Stop messages received. Triggers: Increments when an ACR-STOP is received. Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acrstopretry | Description: Diameter Accounting Message Stats - The total number of retries for Accounting-Request Stop messages. Triggers: Increments when an ACR-STOP is retried. Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acastoptmo | Description: Diameter Accounting Message Stats - The total number of timeouts of Accounting-Answer Stop messages. Triggers: Increments when an ACA-STOP is timed out Availability: Per AAA Manager instance. | Int32
> diamacct-msg-acadropped | Description: Diameter Accounting Message Stats - The total number of Accounting-Answer messages dropped. Triggers: Increments when an ACA is dropped. Availability: Per AAA Manager instance. | Int32
> diamacct-acmsgerr-proto | Description: Diameter Accounting Message Error Stats - The total number of error messages received with error Diameter Protocol Errors. Triggers: Increments when an ACA is received with Result-Code value as 3xxx. Availability: Per AAA Manager instance. | Int32
> diamacct-acmsgerr-badans | Description: Diameter Accounting Message Error Stats - The total number of error messages received with error Bad-Answer. Triggers: Increments when an ACA is received with malformed or wrong AVPs. Availability: Per AAA Manager instance. | Int32
> diamacct-acmsgerr-unksessreq | Description: Diameter Accounting Message Error Stats - The total number of error messages received with error Session-Id or unknown session values. Triggers: Increments when an ACA is received with unknown session-id Availability: Per AAA Manager instance. | Int32
> diamacct-acmsgerr-unkcmdcode | This variable is obsolete. | Int32
> diamacct-acmsgerr-reqtmo | Description: Diameter Accounting Message Error Stats - The total number of ACRs that are timed out. Triggers: Increments when an ACR is timed out. Availability: Per AAA Manager instance. | Int32
> diamacct-acmsgerr-parse | Description: Diameter Accounting Message Error Stats - The total number of parse failures happened for ACR mesage. Triggers: Increments when parse failure happens for ACR. Availability: Per AAA Manager instance. | Int32
> diamacct-acmsgerr-reqretry | Description: Diameter Accounting Message Error Stats - The total number of request retries happened for ACR message. Triggers: Increments when an ACR is retried. Availability: Per AAA Manager instance. | Int32
> a11-ttlarrived | The total number of sessions for all A11 Managers that were received. | Int32
> a11-ttlrejected | The total number of sessions for all A11 Managers that were rejected. | Int32
> a11-ttldemult | The total number of sessions that were successfully setup for all A11 Managers. | Int32
> a11-ttldereg | The total number of sessions for all A11 Managers that were successfully de-registered, or disconnected. | Int32
> a11-curactive | The number of active sessions currently being facilitated by all A11 Managers. Type: Gauge | Int32
> fa-ttlarrived | The total number of sessions for all FA Managers that were received. | Int32
> fa-ttlrejected | The total number of sessions for all FA Managers that were rejected. | Int32
> fa-ttldemult | The total number of sessions for all FA Managers that were successfully setup. | Int32
> fa-ttldereg | The total number of sessions for all FA Managers that were successfully de-registered, or disconnected. | Int32
> fa-curactive | The number of active sessions currently being facilitated by all FA Managers. Type: Gauge | Int32
> ha-ttlarrived | The total number of sessions for all HA Managers that were received. | Int32
> ha-ttlrejected | The total number of sessions for all HA Managers that were rejected. | Int32
> ha-ttldemult | The total number of sessions for all HA Managers that were successfully setup. | Int32
> ha-ttldereg | The total number of sessions for all HA Managers that were successfully de-registered, or disconnected. | Int32
> ha-curactive | The number of active sessions currently being facilitated by all HA Managers. Type: Gauge | Int32
> pdif-cursess | The number of Credit Control Application (CCA) sessions currently active. Type: Gauge | Int32
> pdif-curactive | The number of active sessions currently being facilitated by PDIF. Type: Gauge | Int32
> pdif-curdormant | The number of dormant sessions currently being facilitated by PDIF. Type: Gauge | Int32
> pdif-ttlsetup | The total number of pdif sessions on a system. | Int32
> pdif-curchildsa | The number of current child SAs Type: Gauge | Int32
> sess-15peak-curactcall | The number of current calls (active only). Peak values represent the highest sample seen over the last 15 minutes. Type: Gauge | Int32
> sess-15peak-curttlcall | The number of current calls. Peak values represent the highest sample seen over the last 15 minutes. Type: Gauge | Int32
> sess-cursipactive | The number of SImple IP sessions currently active. Type: Gauge | Int32
> sess-15peak-cursipactive | The number of Simple IP sessions currently active. Peak values represent the highest sample seen over the last 15 minutes. Type: Gauge | Int32
> sess-curmipactive | The number of Mobile IP sessions currently active. Type: Gauge | Int32
> sess-15peak-curmipactive | The number of currently active Mobile IP sessions Peak values represent the highest sample seen over the last 15 minutes. Type: Gauge | Int32
> a11-15peak-curactive | Peak active A11 sessions (a11-curactive) over last 15 minutes. Type: Gauge | Int32
> crp-curactive | Current number of active ClosedRP calls. Type: Gauge | Int32
> crp-15peak-curactive | Peak active ClosedRP calls (crp-curactive) over last 15 minutes. Type: Gauge | Int32
> fa-15peak-curactive | The number of FA sessions currently active. Peak values represent the highest sample seen over the last 15 minutes. Type: Gauge | Int32
> ha-15peak-curactive | The number of HA sessions currently active. Peak values represent the highest sample seen over the last 15 minutes. Type: Gauge | Int32
> flow-15peak-curdynamic | Peak flows (flow-curdynamic) over last 15 minutes. Type: Gauge | Int32
> sess-15min-usageactive | Total minute usage by all the active sessions over last 15 minutes. Type: Gauge | Int32
> sess-15min-usageall | Total minute usage by all flows over last 15 minutes. Type: Gauge | Int32
> pdp-ctx-15peak-active | The number of peak active simultaneous PDP contexts over last 15 minutes. This is sum of both SGSN & GGSN service session on a system. Type: Gauge | Int32
> pdp-ctx-5peak-active | The number of peak active simultaneous PDP contexts over last 5 minutes. This is sum of both SGSN & GGSN service session on a system. Type: Gauge | Int32
> cc-cursess | Description: The total number of Credit Control Application (CCA) sessions currently active. Trigger: Increments when a Gy session is successfully created Decrements when the Gy session is terminated Availability: Per Credit-Control group Type: Gauge | Int64
> cc-ttlecsadd | Description: The total number of ECS sessions added to CCA. Trigger: Increments when a new CC session is being created by ECS. Availability: Per Credit-Control group | Int64
> cc-ttlstart | Description: The total number of CCA sessions started. Trigger: Increments when CCR-I is successfully sent. Availability: Per Credit-Control group | Int64
> cc-ttlsessupd | Description: The total number of CCA sessions updated. Trigger: Increments when a CC session update is sent by ECS to DCCA module Availability: Per Credit-Control group | Int64
> cc-ttlterm | Description: The total number of CCA sessions terminated. Trigger: Increments when a CC session terminate is sent by ECS to DCCA module Availability: Per Credit-Control group | Int64
> cc-sessfailover | Description: The total number of CCA sessions failed. Trigger: Increments when a CC session message is retried on a secondary server due to session failover Availability: Per Credit-Control group | Int64
> cc-msg-recv | Description: The total number of CCA messages received. Trigger: Increments when a CCA message is successfully received Availability: Per Credit-Control group | Int64
> cc-msg-sent | Description: The total number of CCA messages sent. Trigger: Increments when a CCA message is successfully sent to the server Availability: Per Credit-Control group | Int64
> cc-msg-request | Description: The total number of CCR (Credit Control Request) messages that are sent out from the system to the Diameter Server. The CCR can be Initial/Update or Terminate. Trigger: Increments when CCR (Credit Control Request) message is sent out from system to the Diameter Server Availability: Per Credit-Control group | Int64
> cc-msg-answer | Description: The total number of CCA (Credit Control Answer) messages that are received by the system from the Diameter Server. Trigger: Increments when CCA message is received Availability: Per Credit-Control group | Int64
> cc-msg-ccrinit | Description: The total number of CCR-Initial (Initial Credit Control Request) messages that are sent out from the system to the Diameter Server. Trigger: Increments when CCR-I message is successfully sent Availability: Per Credit-Control group | Int64
> cc-msg-ccainit | Description: The total number of CCA-Initial (Initial Credit Control Answer) messages that are received by the system from the Diameter Server. Trigger: Increments when CCA-I message is successfully received Availability: Per Credit-Control group | Int64
> cc-msg-ccainitaccept | Description: The total number of CCA-Initial (Initial Credit Control Answer) messages that are sent from Diameter Server and accepted by the system Trigger: Increments when a CCA-Initial message from Diameter Server is accepted by the system Availability: Per Credit-Control group | Int64
> cc-msg-ccainitreject | Description: The total number of CCA-Initial (Initial Credit Control Answer sent) messages that are sent from Diameter Server and rejected by the system Trigger: Increments when a CCA-Initial (Initial Credit Control Answer sent) message from Diameter Server is rejected by system Availability: Per Credit-Control group | Int64
> cc-msg-ccainittimeout | Description: The total number of CCA-Initial-Timeouts (CCR-I sent but did not receive CCA till the timer expired) messages that are sent to the system from Diameter Server. Trigger: Increments when CCR-I is sent but CCA-I is not received till Tx timer expiry. Availability: Per Credit-Control group | Int64
> cc-msg-ccrupdate | Description: The total number of CCR-Updates (Credit Control Request with Update) messages that are sent out from the system to the Diameter Server. Trigger: Increments whenever a CCR-Update request is successfully sent from the system. Availability: Per Credit-Control group | Int64
> cc-msg-ccaupdate | Description: The total number of CCA-Update (Credit Control Answer for update) messages that are received by the system from the Diameter Server. Trigger: Increments whenever an update answer message is received from the server. Availability: Per Credit-Control group | Int64
> cc-msg-ccaupdatetimeout | Description: The total number of CCA-Update Timeouts (CCR-U sent but did not receive CCA till the timer expired) messages that are sent to the system from Diameter Server. Trigger: Increments when CCR-U is sent but an answer for this request is not received till Tx timer expiry. Availability: Per Credit-Control group | Int64
> cc-msg-ccrfinal | Description: The total number of CCR-Final (Credit Control Request with Final) messages that are sent out from the system to the Diameter Server. Trigger: Increments whenever a CCR-Terminate request for a session is successfully sent from the system Availability: Per Credit-Control group | Int64
> cc-msg-ccafinal | Description: The total number of CCA-Final (Credit Control Answer for final update sent) messages that are received by the system from Diameter Server. Trigger: Increments when the system receives answer message (CCA-T) for Terminate request that was sent Availability: Per Credit-Control group | Int64
> cc-msg-ccafinaltimeout | Description: The total number of CCA-Final Timeouts (CCR-T sent but did not receive CCA till the timer expired) messages that are received by the system from Diameter Server. Trigger: Increments when CCR-T is sent but an answer for this request is not received till Tx timer expiry. Availability: Per Credit-Control group | Int64
> cc-msg-asr | Description: The total number of Abort Session Request messages that are sent from the Diameter Server to the system. Trigger: Increments when the system receives answer message (CCA-T) for Terminate request that was sent Availability: Per Credit-Control group | Int64
> cc-msg-asa | Description: The total number of Abort Session Answer messages sent from the system to the Diameter server. This message will be followed by a CCR-Terminate to terminate the session. Trigger: Increments when the system replies with an Abort Session Answer message for the Abort Session Request message sent from Diameter Server Availability: Per Credit-Control group | Int64
> cc-msg-rar | Description: The total number of ReAuth Request messages that are sent from the Diameter Server to the system. Trigger: Increments when a Re-Authorization Request message is sent from Diameter Server Availability: Per Credit-Control group | Int64
> cc-msg-raa | Description: The total number of ReAuth Answer messages sent from the system to the Diameter server. This message is followed by a CCR-Update to update the Diameter server about the session. Trigger: Increments when the system replies with a Re-auth Answer message for the Re-Auth Request sent from Diameter Server Availability: Per Credit-Control group | Int64
> cc-msg-ccadropped | Description: The total number of CCA (Credit Control Answer) messages dropped by the system. Trigger: Increments when the system drops/ignores a CCA message received from the server Availability: Per Credit-Control group | Int64
> cc-msgerr-proto | Description: The total message errors due to Diameter protocol. Trigger: Increments whenever a message with result-codes 3xxx- errors due to diameter protocol is received from the server Availability: Per Credit-Control group | Int64
> cc-msgerr-badanswer | Description: The total message errors due to invalid response - CCA Parse error. Trigger: Increments when the system receives an undefined mandatory AVP from the server Availability: Per Credit-Control group | Int64
> cc-msgerr-unknownsess | Description: The total message errors due to invalid session requests. Trigger: Increments for every occurrence of invalid session request message Availability: Per Credit-Control group | Int64
> cc-msgerr-unknowncomm | Description: The total message errors due to invalid/unknown command code (CCA, ASR, RAR). Trigger: Increments whenever a response is received for a valid request with corrupted Command Code. Availability: Per Credit-Control group | Int64
> cc-msgerr-reqtimeout | Description: The total message errors due to request timeout. Trigger: Increments whenever a request message is timed-out Availability: Per Credit-Control group | Int64
> cc-msgerr-parse | Description: The total message errors due to parsing errors. Trigger: Increments whenever a message is received with parsing errors Availability: Per Credit-Control group | Int64
> cc-msgerr-unkratinggrp | Description: The total message errors due to invalid/unknown Rating Groups. Rating group is used to identify a particular type of traffic. Trigger: Increments when Unknown Rating-Group is preemptively received from server or a preemptive MSCC is received after session abortion Availability: Per Credit-Control group | Int64
> cc-msgerr-unkrulebase | Description: The total message errors due to invalid/unknown Rulebase applied. Trigger: Increments when rulebase change is attempted and the system is not able to switch to this because the plan indicated might be unknown/invalid. Availability: Per Credit-Control group | Int64
> cc-msgerr-unkfailure | Description: The total number of unknown server -provided session failover actions. This counts the number of unknown server-provided session failover actions. Trigger: Increments when an unknown CCFH action is received from the server (terminate/continue/retry and terminate are considered to be valid CCFH values) Availability: Per Credit-Control group | Int64
> cc-upd-threshold | Description: For each Rating group, the Diameter server sends a threshold (this is also configurable in the system) after which an update needs to be sent. For example, a subscriber quota of 1000 bytes with 900 as a threshold is sent to CCA. When 900 bytes have been used by the system, an update message is sent for quota. This counter gives the number of updates sent because of the threshold. Trigger: Increments whenever threshold value for a quota-type allocated to any rating-group is reached and an update request is sent to the server to report the usage. Availability: Per Credit-Control group | Int64
> cc-upd-qht | Description: The total number of updates sent due to expiry of Quota Hold Timer (QHT). Trigger: Increments when updates are sent due to QHT expiry Availability: Per Credit-Control group | Int64
> cc-upd-final | Description: The total number of updates sent due to exhaustion/invalidation/service denial. Trigger: Increments when updates are sent due to quota exhaustion/invalidation/service denial. Availability: Per Credit-Control group | Int64
> cc-upd-quotaexhaust | Description: The total number of updates sent due to exhaustion of subscriber quota. Trigger: Increments when updates are sent because the quota for a particular rating-group is exhausted Availability: Per Credit-Control group | Int64
> cc-upd-validitytime | Description: The total number of updates sent due to expiry of the session validity time. Trigger: Increments when updates are sent due to validity time expiry for a rating-group. Availability: Per Credit-Control group | Int64
> cc-upd-otherquota | Description: The total number of updates sent to report the usage of one quota type, while the other quota reached a trigger condition. Trigger: Increments when updates are sent to report the usage of one quota type, while the other quota reached a trigger condition Availability: Per Credit-Control group | Int64
> cc-upd-ratingchange | Description: The total number of updates sent due to change in RAT/QOS/SGSN/CELLID/LAC. Trigger: Increments when updates are sent due to change in RAT/QOS/SGSN/CELLID/LAC Availability: Per Credit-Control group | Int64
> cc-upd-forcedreauth | Description: The total number of updates sent because of RAR. Trigger: Increments when the server asks for forced-reauthorization of the subscriber and sends the update request Availability: Per Credit-Control group | Int64
> cc-term-diamlogout | Description: The total number of CCA sessions terminated due to subscriber logout. Trigger: Increments when a subscriber initiates termination of a Diameter session Availability: Per Credit-Control group | Int64
> cc-term-servnotprov | Description: The total number of CCA sessions terminated due to unavailability of service. Trigger: Increments when a session is terminated due to unavailability of Diameter service Availability: Per Credit-Control group | Int64
> cc-term-badanswer | Description: The total number of CCA sessions terminated due to invalid/unknown response received. Trigger: Increments when a session is terminated due to invalid/unknown/unsuccessful response received Availability: Per Credit-Control group | Int64
> cc-term-admin | Description: The total number of CCA sessions terminated by an administrative user. Trigger: Increments when a session termination is done by the system - administrative decision taken by our system in relevant scenarios Availability: Per Credit-Control group | Int64
> cc-term-linkbroken | Description: The total number of CCA sessions terminated due to broken uplink/downlink (connection between peers). Trigger: Increments when a session is terminated because the connection between peers is lost - diameter link is broken Availability: Per Credit-Control group | Int64
> cc-term-authexpired | Description: The total number of CCA sessions terminated due to expiry of subscriber authorization. Trigger: Increments when an update is sent to check for the expiry of lifetime authorization of the subscriber and if the server indicates expiry of authorization, the session will be terminated Availability: Per Credit-Control group | Int64
> cc-term-usermoved | Description: The total number of CCA sessions terminated as subscriber moved out of the service area. Trigger: Increments when session termination happens because the subscriber has moved out of the service area Availability: Per Credit-Control group | Int64
> cc-term-sesstimeout | Description: The total number of CCA sessions terminated due to timeout. Trigger: Increments when a session terminates because the session manager has indicated a session-timeout Availability: Per Credit-Control group | Int64
> cc-badans-auth-appid | Description: The absence or unexpected value in Auth-Application-Id AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to absence or unexpected value of Auth-Application-Id AVP Availability: Per Credit-Control group | Int64
> cc-badans-sessid | Description: The absence or unexpected value in Session-Id AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to absence or unexpected value of Session-id AVP Availability: Per Credit-Control group | Int64
> cc-badans-cc-req-num | Description: The absence or unexpected value in CC-Request-Number AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to absence or unexpected value of CC-Request-Number AVP Availability: Per Credit-Control group | Int64
> cc-badans-cc-req-type | Description: The absence or unexpected value in CC-Request-Type AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to absence or unexpected value of CC-Request-Type AVP Availability: Per Credit-Control group | Int64
> cc-badans-origin-host | Description: The absence of Origin-Host AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to absence or unexpected value of Origin-Host AVP Availability: Per Credit-Control group | Int64
> cc-badans-origin-realm | Description: The absence of Origin-Realm AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to absence or unexpected value of Origin-Realm AVP Availability: Per Credit-Control group | Int64
> cc-badans-parsemsg-err | Description: The number of parse errors in the message. Trigger: Increments when session is terminated because of Diameter bad answer due to parsing errors in the message Availability: Per Credit-Control group | Int64
> cc-badans-parsemscc-err | Description: The number of parse errors in MSCC AVP. Trigger: Increments when a session is terminated because of Diameter bad answer due to parsing errors detected while processing the Multiple-Services-Credit-Control AVP in the message Availability: Per Credit-Control group | Int64
> cc-badans-misc-err | Description: The number of other miscellaneous errors. Trigger: Increments when a session is terminated because of Diameter bad answer due to miscellaneous reasons like failure installing the rulebase change/bandwith/firewall policy, etc. Availability: Per Credit-Control group | Int64
> cc-traf-catcreate | Description: The total traffic categories (MSCC) created. Trigger: Increments when a new MSCC is created Availability: Per Credit-Control group | Int64
> cc-traf-catdelete | Description: The total traffic categories (MSCC) deleted. Trigger: Increments whenever an MSCC is deleted in an ongoing session Availability: Per Credit-Control group | Int64
> cc-traf-catlookup | Description: The total traffic categories/MSCC lookups failed. Trigger: Increments when a lookup operation is performed in the list of MSCCs Availability: Per Credit-Control group | Int64
> cc-traf-hits | Description: The total traffic categories/MSCC lookups successful. Trigger: Increments when a lookup of MSCC is successful Availability: Per Credit-Control group | Int64
> cc-traf-misses | Description: The total traffic categories triggered/MSCC lookups failed. Trigger: Increments when a lookup operation for a particular MSCC fails. Availability: Per Credit-Control group | Int64
> cc-traf-triggerevent | Description: The total triggers for traffic categories/MSCCs. Trigger: Increments whenever there is a change in certain trigger parameters like change in RAT, SGSN-IP-ADDRESS, QOS, CELLID, etc. Availability: Per Credit-Control group | Int64
> cc-traf-finalunit | Description: The total final-units-actions taken on MSCCs. Trigger: Increments whenever FUI action is imposed on a particular rating group. Availability: Per Credit-Control group | Int64
> cc-traf-catsuccess | Description: The total number of successful allocation of credits for traffic category/MSCC (result-code 2001). Trigger: Increments when the server responds with result-code 2001 indicating successful allocation of credits for traffic category Availability: Per Credit-Control group | Int64
> cc-traf-ratingfail | Description: The total number of quota retries because of rating failure due to category not recognized (result-code 5031). Trigger: Increments when the server responds with result-code 5031 indicating rating failure due to category not recognized Availability: Per Credit-Control group | Int64
> cc-traf-servdenied | Description: The total number of quota retries due to denial of end user service (result-code 4010). Trigger: Increments when the server responds with result-code 4010 indicating end user service denial. Availability: Per Credit-Control group | Int64
> cc-traf-limitreached | Description: The total number of retries due to credit limit reached (result-code 4012). Trigger: Increments when the server responds with result-code 4012 indicating that the credit limit has reached Availability: Per Credit-Control group | Int64
> cc-traf-authreject | Description: The total number of retries due to authorization rejected (result-code 5003). Trigger: Increments when the server responds with result-code 5003 indicating authorization rejection. Availability: Per Credit-Control group | Int64
> cc-traf-othererror | Description: The total number of miscellaneous/unknown errors not specified by the system (Diameter_unable_to_comply (5012)). Trigger: Increments when the server responds with result-code 5012 indicating miscellaneous/unknown errors not specified by the system Availability: Per Credit-Control group | Int64
> url-blacklisting-hits | Description: Total number of blacklisted URL hits of all the configured billing plans. Triggers: Increments when a URL is found in the BL DB (stored as BL cache at ACSMgr). Availability: Per Active Charging Service. | Int64
> url-blacklisting-misses | Description: Total number of blacklisted URL misses of all the configured billing plans. Triggers: Increments when a URL is not found in the BL DB (stored as BL cache at ACSMgr). Availability: Per Active Charging Service. | Int64
> cf-static-ratereq | Description: The total number of static rating requests. Triggers: Increments when a request arrives at any SRDB for static rating. Availability: Per Active Charging Service. | Int64
> cf-static-ratesucc | Description: The total number of “successful” response for static rating requests. Triggers: Increments when a "successful" response is sent for static rating requests from SRDBs. Availability: Per Active Charging Service. | Int64
> cf-static-rateblock | Description: The total number of “blocked” response for static rating requests. Triggers: Increments when a "blocked" response is sent for static rating requests from SRDBs. Availability: Per Active Charging Service. | Int64
> cf-static-ratefail | Description: The total number of “failed” response for static rating requests. Triggers: Increments when an SRDB fails to send a response for static rating requests. Availability: Per Active Charging Service. | Int64
> cf-static-ratefail-nr | Description: The total number of “failed” response for static requests due to no rating in database. Triggers: Increments when an SRDB fails to send a response for static rating requests, due to no rating in database. Availability: Per Active Charging Service. | Int64
> cf-static-ratefail-notindb | Description: The total number of “failed” response for static requests due to no listing in database. Triggers: Increments when an SRDB fails to send a response for static rating requests, due to no listing in database. Availability: Per Active Charging Service. | Int64
> cf-dyn-ratereq | Description: The total number of dynamic rating requests. Triggers: Increments when a request arrives at any SRDB for dynamic rating. Availability: Per Active Charging Service. | Int64
> cf-dyn-ratesucc | Description: The total number of “successful” response for dynamic rating requests. Triggers: Increments when a "successful" response is sent for dynamic rating requests from SRDBs. Availability: Per Active Charging Service. | Int64
> cf-dyn-rateblock | Description: The total number of "blocked" response for dynamic rating requests. This variable is obsolete in 8.1 and later releases. | Int64
> cf-dyn-ratefail | Description: The total number of “failed” response for dynamic rating requests. Triggers: Increments when an SRDB fails to send a response for dynamic rating requests. Availability: Per Active Charging Service. | Int64
> cf-cache-hits | Description: The total number of URLs that get a hit (found) in the CF cache. Triggers: Increments when a URL is found in the CF cache. Availability: Per Active Charging Service. | Int64
> cf-cache-misses | Description: The total number of URLs that get a miss (not found) in the CF cache. Triggers: Increments when a URL is not found in the CF cache. Availability: Per Active Charging Service. | Int64
> cf-cache-has-path-hits | Description: The total number of URLs whose domain_name entries are found in the CF cache based, and haspath bit was not set in the domain_name entry. I.e., no extended URLs are present in the SRDB for those domain_name URLs, so there is no need to go for rating. Triggers: Increments when a URL, whose domain_name entries is found in the CF cache based, and haspath bit was not set in the domain_name entry. That is, no extended URLs are present in the SRDB for that domain_name URL, so there is no need to go for rating, is found in the CF cache. Availability: Per Active Charging Service. | Int64
> cf-cache-flushes | Description: The total number of URLs that are flushed from the CF cache. Triggers: Increments when a URL is flushed from the CF cache. Availability: Per Active Charging Service. | Int64
> cf-ratereq | Description: The total number of rating requests including dynamic and static. Triggers: Increments when a static or dynamic request is sent to SRDB for rating. Availability: Per Active Charging Service. | Int64
> cf-ratesucc | Description: The total number of “successful” response against all rating requests including dynamic and rating. Triggers: Increments when a "successful" response is sent for static or dynamic rating requests from SRDBs. Availability: Per Active Charging Service. | Int64
> cf-rateblock | Description: The total number of "blocked" response against all rating requests including dynamic and rating. Triggers: Increments when a "blocked" response is sent for static rating requests from SRDBs. Availability: Per Active Charging Service. | Int64
> cf-ratefail | Description: The total number of “failed” response against all rating requests including dynamic and rating. Triggers: Increments when an SRDB fails to send a response for static or dynamic rating requests. Availability: Per Active Charging Service. | Int64
> cf-ttlsub | Description: The total number of CF subscribers. Triggers: Increments when a subscriber enables CF policy. Availability: Per Active Charging Service. | Int32
> cf-cursub | Description: The current number of CF subscribers. Triggers: Increments when a subscriber enables CF policy. Decrements when a call is aborted. Availability: Per Active Charging Service. Type: Gauge | Int32
> cf-cat-abor-pkts-hit | Description: Total number of packets from sites with CF category “abortion” accessed. Triggers: Increments whenever a packet from sites with CF category "abortion" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-abor-pkts-block | Description: Total number of packets from sites with CF category “abortion” blocked. Triggers: Increments whenever a packet from sites with CF category "abortion" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-adult-pkts-hit | Description: Total number of packets from sites with CF category “adult” accessed. Triggers: Increments whenever a packet from sites with CF category "adult" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-adult-pkts-block | Description: Total number of packets from sites with CF category “adult” blocked. Triggers: Increments whenever a packet from sites with CF category "adult" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-adv-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-adv-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-advert-pkts-hit | Description: Total number of packets from sites with CF category “advertising site” accessed. Triggers: Increments whenever a packet from sites with CF category "advertising site" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-advert-pkts-block | Description: Total number of packets from sites with CF category “advertising site” blocked. Triggers: Increments whenever a packet from sites with CF category "advertising site" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-anon-pkts-hit | Description: Total number of packets from sites with CF category “anonymous” accessed. Triggers: Increments whenever a packet from sites with CF category "anonymous" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-anon-pkts-block | Description: Total number of packets from sites with CF category “anonymous” blocked. Triggers: Increments whenever a packet from sites with CF category "anonymous" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-art-pkts-hit | Description: Total number of packets from sites with CF category “art” accessed. Triggers: Increments whenever a packet from sites with CF category "art" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-art-pkts-block | Description: Total number of packets from sites with CF category “art” blocked. Triggers: Increments whenever a packet from sites with CF category "art" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-auct-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-auct-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-auto-pkts-hit | Description: Total number of packets from sites with CF category “auto” accessed. Triggers: Increments whenever a packet from sites with CF category "auto" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-auto-pkts-block | Description: Total number of packets from sites with CF category “auto” blocked. Triggers: Increments whenever a packet from sites with CF category "auto" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-backup-pkts-hit | Description: Total number of packets from sites with CF category “backup” accessed. Triggers: Increments whenever a packet from sites with CF category "backup" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-backup-pkts-block | Description: Total number of packets from sites with CF category “backup” blocked. Triggers: Increments whenever a packet from sites with CF category "backup" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-black-pkts-hit | Description: Total number of packets from sites with CF category “black” accessed. Triggers: Increments whenever a packet from sites with CF category "black" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-black-pkts-block | Description: Total number of packets from sites with CF category “black” blocked. Triggers: Increments whenever a packet from sites with CF category "black" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-blog-pkts-hit | Description: Total number of packets from sites with CF category “blog” accessed. Triggers: Increments whenever a packet from sites with CF category "blog" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-blog-pkts-block | Description: Total number of packets from sites with CF category “blog” blocked. Triggers: Increments whenever a packet from sites with CF category "blog" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-busi-pkts-hit | Description: Total number of packets from sites with CF category “business” accessed. Triggers: Increments whenever a packet from sites with CF category "business" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-busi-pkts-block | Description: Total number of packets from sites with CF category “business” blocked. Triggers: Increments whenever a packet from sites with CF category "business" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-car-pkts-hit | Description: Total number of packets from sites with CF category “career” accessed. Triggers: Increments whenever a packet from sites with CF category "career" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-car-pkts-block | Description: Total number of packets from sites with CF category “career” blocked. Triggers: Increments whenever a packet from sites with CF category "career" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-cdn-pkts-hit | Description: Total number of packets from sites with CF category “cdn” accessed. Triggers: Increments whenever a packet from sites with CF category "cdn" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-cdn-pkts-block | Description: Total number of packets from sites with CF category “cdn” blocked. Triggers: Increments whenever a packet from sites with CF category "cdn" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-chat-pkts-hit | Description: Total number of packets from sites with CF category “chat” accessed. Triggers: Increments whenever a packet from sites with CF category "chat" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-chat-pkts-block | Description: Total number of packets from sites with CF category “chat” blocked. Triggers: Increments whenever a packet from sites with CF category "chat" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-clean-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-clean-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-cmc-pkts-hit | Description: Total number of packets with CF category “virtual community” accessed. Triggers: Increments whenever a packet from sites with CF category "virtual community" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-cmc-pkts-block | Description: Total number of packets with CF category “virtual community” blocked. Triggers: Increments whenever a packet from sites with CF category "virtual community" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-cporn-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-cporn-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-crime-pkts-hit | Description: Total number of packets from sites with CF category “crime” accessed. Triggers: Increments whenever a packet from sites with CF category "crime" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-crime-pkts-block | Description: Total number of packets from sites with CF category “crime” blocked. Triggers: Increments whenever a packet from sites with CF category "crime" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-cult-pkts-hit | Description: Total number of packets from sites with CF category “cult” accessed. Triggers: Increments whenever a packet from sites with CF category "cult" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-cult-pkts-block | Description: Total number of packets from sites with CF category “cult” blocked. Triggers: Increments whenever a packet from sites with CF category "cult" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-drug-pkts-hit | Description: Total number of packets from sites with CF category “drug” accessed. Triggers: Increments whenever a packet from sites with CF category "drug" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-drug-pkts-block | Description: Total number of packets from sites with CF category “drug” blocked. Triggers: Increments whenever a packet from sites with CF category "drug" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-dynam-pkts-hit | Description: Total number of packets from sites with CF category “dynamic content” accessed. Triggers: Increments whenever a packet from sites with CF category "dynamic content" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-dynam-pkts-block | Description: Total number of packets from sites with CF category “dynamic content” blocked. Triggers: Increments whenever a packet from sites with CF category "dynamic content" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-edu-pkts-hit | Description: Total number of packets from sites with CF category “education” accessed. Triggers: Increments whenever a packet from sites with CF category "education" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-edu-pkts-block | Description: Total number of packets from sites with CF category “education” blocked. Triggers: Increments whenever a packet from sites with CF category "education" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-energy-pkts-hit | Description: Total number of packets from sites with CF category “energy” accessed. Triggers: Increments whenever a packet from sites with CF category "energy" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-energy-pkts-block | Description: Total number of packets from sites with CF category “energy” blocked. Triggers: Increments whenever a packet from sites with CF category "energy" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-ent-pkts-hit | Description: Total number of packets from sites with CF category “entertainment” accessed. Triggers: Increments whenever a packet from sites with CF category "entertainment" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-ent-pkts-block | Description: Total number of packets from sites with CF category “entertainment” blocked. Triggers: Increments whenever a packet from sites with CF category "entertainment" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-esrb-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-esrb-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-fin-pkts-hit | Description: Total number of packets from sites with CF category “finance” accessed. Triggers: Increments whenever a packet from sites with CF category "finance" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-fin-pkts-block | Description: Total number of packets from sites with CF category “finance” blocked. Triggers: Increments whenever a packet from sites with CF category "finance" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-forum-pkts-hit | Description: Total number of packets from sites with CF category “forum” accessed. Triggers: Increments whenever a packet from sites with CF category "forum" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-forum-pkts-block | Description: Total number of packets from sites with CF category “forum” blocked. Triggers: Increments whenever a packet from sites with CF category "forum" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-gamb-pkts-hit | Description: Total number of packets from sites with CF category “gambling” accessed. Triggers: Increments whenever a packet from sites with CF category "gambling" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-gamb-pkts-block | Description: Total number of packets from sites with CF category “gambling” blocked. Triggers: Increments whenever a packet from sites with CF category "gambling" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-game-pkts-hit | Description: Total number of packets from sites with CF category “game” accessed. Triggers: Increments whenever a packet from sites with CF category "game" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-game-pkts-block | Description: Total number of packets from sites with CF category “game” blocked. Triggers: Increments whenever a packet from sites with CF category "game" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-glam-pkts-hit | Description: Total number of packets from sites with CF category “glamour” accessed. Triggers: Increments whenever a packet from sites with CF category "glamour" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-glam-pkts-block | Description: Total number of packets from sites with CF category “glamour” blocked. Triggers: Increments whenever a packet from sites with CF category "glamour" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-govern-pkts-hit | Description: Total number of packets from sites with CF category “government” accessed. Triggers: Increments whenever a packet from sites with CF category "government" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-govern-pkts-block | Description: Total number of packets from sites with CF category “government” blocked. Triggers: Increments whenever a packet from sites with CF category "government" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-hack-pkts-hit | Description: Total number of packets from sites with CF category “hacker” accessed. Triggers: Increments whenever a packet from sites with CF category "hacker" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-hack-pkts-block | Description: Total number of packets from sites with CF category “hacker” blocked. Triggers: Increments whenever a packet from sites with CF category "hacker" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-hate-pkts-hit | Description: Total number of packets from sites with CF category “hate” accessed. Triggers: Increments whenever a packet from sites with CF category "hate" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-hate-pkts-block | Description: Total number of packets from sites with CF category “hate” blocked. Triggers: Increments whenever a packet from sites with CF category "hate" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-health-pkts-hit | Description: Total number of packets from sites with CF category “health” accessed. Triggers: Increments whenever a packet from sites with CF category "health" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-health-pkts-block | Description: Total number of packets from sites with CF category “health” blocked. Triggers: Increments whenever a packet from sites with CF category "health" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-hobby-pkts-hit | Description: Total number of packets from sites with CF category “hobby” accessed. Triggers: Increments whenever a packet from sites with CF category "hobby" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-hobby-pkts-block | Description: Total number of packets from sites with CF category “hobby” blocked. Triggers: Increments whenever a packet from sites with CF category "hobby" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-hosts-pkts-hit | Description: Total number of packets from sites with CF category “host” accessed. Triggers: Increments whenever a packet from sites with CF category "host" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-hosts-pkts-block | Description: Total number of packets from sites with CF category “host” blocked. Triggers: Increments whenever a packet from sites with CF category "host" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-kids-pkts-hit | Description: Total number of packets from sites with CF category “kids” accessed. Triggers: Increments whenever a packet from sites with CF category "kids" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-kids-pkts-block | Description: Total number of packets from sites with CF category “kids” blocked. Triggers: Increments whenever a packet from sites with CF category "kids" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-legal-pkts-hit | Description: Total number of packets from sites with CF category “legal” accessed. Triggers: Increments whenever a packet from sites with CF category "legal" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-legal-pkts-block | Description: Total number of packets from sites with CF category “legal” blocked. Triggers: Increments whenever a packet from sites with CF category "legal" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-lifes-pkts-hit | Description: Total number of packets from sites with CF category “lifes” accessed. Triggers: Increments whenever a packet from sites with CF category "life" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-lifes-pkts-block | Description: Total number of packets from sites with CF category “lifes” blocked. Triggers: Increments whenever a packet from sites with CF category "life" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-mail-pkts-hit | Description: Total number of packets from sites with CF category “mail” accessed. Triggers: Increments whenever a packet from sites with CF category "mail" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-mail-pkts-block | Description: Total number of packets from sites with CF category “mail” blocked. Triggers: Increments whenever a packet from sites with CF category "mail" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-mil-pkts-hit | Description: Total number of packets from sites with CF category “military” accessed. Triggers: Increments whenever a packet from sites with CF category "military" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-mil-pkts-block | Description: Total number of packets from sites with CF category “military” blocked. Triggers: Increments whenever a packet from sites with CF category "military" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-news-pkts-hit | Description: Total number of packets from sites with CF category “news” accessed. Triggers: Increments whenever a packet from sites with CF category "news" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-news-pkts-block | Description: Total number of packets from sites with CF category “news” blocked. Triggers: Increments whenever a packet from sites with CF category "news" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-occult-pkts-hit | Description: Total number of packets from sites with CF category “occult” accessed. Triggers: Increments whenever a packet from sites with CF category "occult" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-occult-pkts-block | Description: Total number of packets from sites with CF category “occult” blocked. Triggers: Increments whenever a packet from sites with CF category "occult" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-p2p-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-p2p-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-peer-pkts-hit | Description: Total number of packets from sites with CF category “peer” accessed. Triggers: Increments whenever a packet from sites with CF category "peer" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-peer-pkts-block | Description: Total number of packets from sites with CF category “peer” blocked. Triggers: Increments whenever a packet from sites with CF category "peer" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-pers-pkts-hit | Description: Total number of packets from sites with CF category “pers” accessed. Triggers: Increments whenever a packet from sites with CF category "pers" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-pers-pkts-block | Description: Total number of packets from sites with CF category “pers” blocked. Triggers: Increments whenever a packet from sites with CF category "pers" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-phish-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-phish-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-photo-pkts-hit | Description: Total number of packets from sites with CF category “photo” accessed. Triggers: Increments whenever a packet from sites with CF category "photo" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-photo-pkts-block | Description: Total number of packets from sites with CF category “photo” blocked. Triggers: Increments whenever a packet from sites with CF category "photo" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-plag-pkts-hit | Description: Total number of packets from sites with CF category “plag” accessed. Triggers: Increments whenever a packet from sites with CF category "plag" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-plag-pkts-block | Description: Total number of packets from sites with CF category “plag” blocked. Triggers: Increments whenever a packet from sites with CF category "plag" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-poltic-pkts-hit | Description: Total number of packets from sites with CF category “poltic” accessed. Triggers: Increments whenever a packet from sites with CF category "poltic" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-poltic-pkts-block | Description: Total number of packets from sites with CF category “poltic” blocked. Triggers: Increments whenever a packet from sites with CF category "poltic" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-porn-pkts-hit | Description: Total number of packets from sites with CF category “porn” accessed. Triggers: Increments whenever a packet from sites with CF category "porn" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-porn-pkts-block | Description: Total number of packets from sites with CF category “porn” blocked. Triggers: Increments whenever a packet from sites with CF category "porn" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-portal-pkts-hit | Description: Total number of packets from sites with CF category “portal” accessed. Triggers: Increments whenever a packet from sites with CF category "portal" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-portal-pkts-block | Description: Total number of packets from sites with CF category “portal” blocked. Triggers: Increments whenever a packet from sites with CF category "portal" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-proxy-pkts-hit | Description: Total number of packets from sites with CF category “proxy” accessed. Triggers: Increments whenever a packet from sites with CF category "proxy" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-proxy-pkts-block | Description: Total number of packets from sites with CF category “proxy” blocked. Triggers: Increments whenever a packet from sites with CF category "proxy" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-radio-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-radio-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-ref-pkts-hit | Description: Total number of packets from sites with CF category “ref” accessed. Triggers: Increments whenever a packet from sites with CF category "ref" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-ref-pkts-block | Description: Total number of packets from sites with CF category “ref” blocked. Triggers: Increments whenever a packet from sites with CF category "ref" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-rel-pkts-hit | Description: Total number of packets from sites with CF category “rel” accessed. Triggers: Increments whenever a packet from sites with CF category "rel" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-rel-pkts-block | Description: Total number of packets from sites with CF category “rel” blocked. Triggers: Increments whenever a packet from sites with CF category "rel" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-sci-pkts-hit | Description: Total number of packets from sites with CF category “sci” accessed. Triggers: Increments whenever a packet from sites with CF category "sci" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-sci-pkts-block | Description: Total number of packets from sites with CF category “sci” blocked. Triggers: Increments whenever a packet from sites with CF category "sci" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-search-pkts-hit | Description: Total number of packets from sites with CF category “search” accessed. Triggers: Increments whenever a packet from sites with CF category "search" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-search-pkts-block | Description: Total number of packets from sites with CF category “search” blocked. Triggers: Increments whenever a packet from sites with CF category "search" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-sftwre-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-sftwre-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-shop-pkts-hit | Description: Total number of packets from sites with CF category “shop” accessed. Triggers: Increments whenever a packet from sites with CF category "shop" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-shop-pkts-block | Description: Total number of packets from sites with CF category “shop” blocked. Triggers: Increments whenever a packet from sites with CF category "shop" is blocked Availability: Per Active Charging Service. | Int32
> cf-cat-sport-pkts-hit | Description: Total number of packets from sites with CF category “sport” accessed. Triggers: Increments whenever a packet from sites with CF category "sport" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-sport-pkts-block | Description: Total number of packets from sites with CF category “sport” blocked. Triggers: Increments whenever a packet from sites with CF category "sport" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-stream-pkts-hit | Description: Total number of packets from sites with CF category “stream” accessed. Triggers: Increments whenever a packet from sites with CF category "stream" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-stream-pkts-block | Description: Total number of packets from sites with CF category “stream” blocked. Triggers: Increments whenever a packet from sites with CF category "stream" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-spywre-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-spywre-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-suic-pkts-hit | Description: Total number of packets from sites with CF category “suic” accessed. Triggers: Increments whenever a packet from sites with CF category "suic" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-suic-pkts-block | Description: Total number of packets from sites with CF category “suic” blocked. Triggers: Increments whenever a packet from sites with CF category "suic" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-susp-pkts-hit | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-susp-pkts-block | Important: This variable is obsolete in 8.1 and later releases. | Int32
> cf-cat-sxed-pkts-hit | Description: Total number of packets from sites with CF category “sxed” accessed. Triggers: Increments whenever a packet from sites with CF category "sxed" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-sxed-pkts-block | Description: Total number of packets from sites with CF category “sxed” blocked. Triggers: Increments whenever a packet from sites with CF category "sxed" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-tech-pkts-hit | Description: Total number of packets from sites with CF category “tech” accessed. Triggers: Increments whenever a packet from sites with CF category "tech" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-tech-pkts-block | Description: Total number of packets from sites with CF category “tech” blocked. Triggers: Increments whenever a packet from sites with CF category "tech" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-trav-pkts-hit | Description: Total number of packets from sites with CF category “trav” accessed. Triggers: Increments whenever a packet from sites with CF category "trav" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-trav-pkts-block | Description: Total number of packets from sites with CF category “trav” blocked. Triggers: Increments whenever a packet from sites with CF category "trav" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-viol-pkts-hit | Description: Total number of packets from sites with CF category “viol” accessed. Triggers: Increments whenever a packet from sites with CF category "viol" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-viol-pkts-block | Description: Total number of packets from sites with CF category “viol” blocked. Triggers: Increments whenever a packet from sites with CF category "viol" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-voip-pkts-hit | Description: Total number of packets from sites with CF category “voip” accessed. Triggers: Increments whenever a packet from sites with CF category "voip" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-voip-pkts-block | Description: Total number of packets from sites with CF category “voip” blocked. Triggers: Increments whenever a packet from sites with CF category "voip" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-weap-pkts-hit | Description: Total number of packets from sites with CF category “weap” accessed. Triggers: Increments whenever a packet from sites with CF category "weap" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-weap-pkts-block | Description: Total number of packets from sites with CF category “weap” blocked. Triggers: Increments whenever a packet from sites with CF category "weap" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-white-pkts-hit | Description: Total number of packets from sites with CF category “white” accessed. Triggers: Increments whenever a packet from sites with CF category "white" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-white-pkts-block | Description: Total number of packets from sites with CF category “white” blocked. Triggers: Increments whenever a packet from sites with CF category "white" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-unknow-pkts-hit | Description: Total number of packets from sites with CF category “unknow” accessed. Triggers: Increments whenever a packet from sites with CF category "unknow" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-unknow-pkts-block | Description: Total number of packets from sites with CF category “unknow” blocked. Triggers: Increments whenever a packet from sites with CF category "unknow" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-xcategory-pkts-hit | Description: Total number of packets from sites with CF category “xcategory” accessed. Triggers: Increments whenever a packet from sites with CF category "xcategory" is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-xcategory-pkts-block | Description: Total number of packets from sites with CF category “xcategory” blocked. Triggers: Increments whenever a packet from sites with CF category "xcategory" is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-all-pkts-hit | Description: Total number of URLs categorized by default action. Triggers: Increments whenever a packet categorized by default action is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-all-pkts-block | Description: Total number of URLs blocked by default action. Triggers: Increments whenever a packet categorized by default action is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-timer-pkts-hit | Description: Total number of URLs categorized by timeout action. Triggers: Increments whenever a packet categorized by timeout action is accessed. Availability: Per Active Charging Service. | Int32
> cf-cat-timer-pkts-block | Description: Total number of URLs blocked by timeout action. Triggers: Increments whenever a packet categorized by timeout action is blocked. Availability: Per Active Charging Service. | Int32
> cf-cat-pkts-hit-summary | Description: Summary of total packets with CF category accessed. Triggers: Increments whenever a packet of any of the above categories is accessed. Availability: Per Active Charging Service. | String
> cf-cat-pkts-block-summary | Description: Summary of total packets with CF category blocked. Triggers: Increments whenever a packet of any of the above categories is blocked. Availability: Per Active Charging Service. | String
> ipsg-total-call-arrived | The total number of IPSG calls arrived on this system. Triggers: Increments when a new IPSG call arrives. Availability: Per system. | Int32
> ipsg-total-call-rejected | The total number of IPSG calls rejected by this system. Triggers: Increments when an IPSG call is rejected. Availability: Per system. | Int32
> ipsg-total-call-demult | The total number of IPSG calls de-multiplexed by this system. Triggers: Increments when an IPSG is de-multiplexed. Availability: Per system. | Int32
> ipsg-total-dereg-rep-sent | The total number of IPSG call de-registered by this system. Triggers: Increments when an IPSG call is de-registered. Availability: Per system. | Int32
> ipsg-cur-active-call | The number of IPSG calls currently active on this system. Triggers: Increments when an IPSG call comes up. Decrements when an IPSG call ends. Availability: Per system. Type: Gauge | Int32
> ipsg-total-active-serv | The total number of active IPSG services on this system. Triggers: Increments when an IPSG service is configured on the system. Availability: Per system. | Int32
> dpca-cursess | Description: The total number of active DPCA sessions currently running on the node. Triggers: Increments when a DPCA session is created. Decrements when a DPCA session is terminated. Availability: Per IMS authorization service Type: Gauge | Int32
> dcca-cursess | Description: The total number of active DCCA sessions currently running on the node. Triggers: Increments when an online Diameter session is created Decrements when an online session is terminated, or when an online session is converted to offline Type: Gauge | Int32
> asngw-cur-active-call | The total number of active ASN-GW session on a system. Type: Gauge | Int32
> asngw-total-sess-setup | The total number of ASN-GW sessions setup on a system. | Int32
> asngw-retriesexhaust | Total number of retries for R6 connection setup for ASN-GW service on a system. | Int32
> asngw-sfs | Total number of ASN-GW service flows. | Int32
> asngw-tidfail | The total number of ASN-GW Transaction id (tid) failures on a system. | Int32
> asngw-handoffattempt | The total number of intra-ASN Gateway and inter-ASN Gateway hand-offs attempted on a system. | Int32
> asngw-handoffdenied | The total number of intra-ASN Gateway and inter-ASN Gateway hand-offs denied/failed on a system. | Int32
> asngw-handoffcomp | The total number of successful intra-ASN Gateway and inter-ASN Gateway hand-offs attempted on a system. | Int32
> asngw-authsucc | The total number of successful EAP authorization on a system for ASN-GW service. | Int32
> asngw-authfailures | The total number of failed EAP authorization on a system for ASN-GW service. | Int32
> phsgw-cursess | Not supported in this release. Type: Gauge | Int32
> phsgw-cur-active-call | Not supported in this release. Type: Gauge | Int32
> phsgw-total-sess-setup | Not supported in this release. | Int32
> phsgw-retriesexhaust | Not supported in this release. | Int32
> phsgw-uplink-sfs | Not supported in this release. | Int32
> phsgw-downlink-sfs | Not supported in this release. | Int32
> phsgw-tidfail | Not supported in this release. | Int32
> phsgw-handoffattempt | Not supported in this release. | Int32
> phsgw-handoffdenied | Not supported in this release. | Int32
> phsgw-handoffcomp | Not supported in this release. | Int32
> phsgw-authsucc | Not supported in this release. | Int32
> phsgw-authfailures | Not supported in this release. | Int32
> phsgw-3partyauthsucc | Not supported in this release. | Int32
> phsgw-3partyauthfailures | Not supported in this release. | Int32
> phspc-cursess | Not supported in this release. Type: Gauge | Int32
> phspc-total-sess-setup | Not supported in this release. | Int32
> phspc-retriesexhaust | Not supported in this release. | Int32
> phspc-tidfail | Not supported in this release. | Int32
> phspc-locupdate-attempt | Not supported in this release. | Int32
> phspc-locupdate-denied | Not supported in this release. | Int32
> phspc-locupdate-comp | Not supported in this release. | Int32
> phspc-paging-attempt | Not supported in this release. | Int32
> ikev2-cursa | Total number of current security associations with Internet Key Exchange v2 (IKEv2). Type: Gauge | Int32
> ikev2-cursainit | Total number of current security associations in initialization state with Internet Key Exchange v2 (IKEv2). Type: Gauge | Int32
> ikev2-cursaresp | Total number of response for active security associations with Internet Key Exchange v2 (IKEv2) Type: Gauge | Int32
> ikev2-ttlsa | Total number of security associations with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-ttlsainit | Total number of security associations in initialization state with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-ttlsaresp | Total number of response for security associations with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-attempt | Total number of attempts for security association tunnel with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-attemptinit | Total number of attempts to initialize the security association tunnel with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-attemptresp | Total number of response against attempts to initialize the security association tunnel with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-rxpacket | Total number of packets received with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-txpacket | Total number of packets transmitted with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-rxoctet | Total number of octets received with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-txoctet | Total number of octets transmitted with Internet Key Exchange v2 (IKEv2) | Int32
> ikev2-initfail | Total number of security association initialization failed | Int32
> ikev2-initfail-noresp | Total number of security association initialization failed without any response | Int32
> ikev2-initfail-resp | Total number of security association initialization failed with response | Int32
> ikev2-invcookie | Total number of cookies with session invitation for IKEv2 security association | Int32
> ikev2-congrej | Total number of packets rejected due to congestion. | Int32
> ikev2-congdrop | Total number of packets dropped due to congestion. | Int32
> ikev2-unkxchgspi | Total number of unknown exchange security parameter indexes. | Int32
> ikev2-nattkeepalive-recv | Total number of NAT-T Keep-Alive messages received with IKEv2 | Int32
> ikev2-nattkeepalive-send | Total number of NAT-Keep-Alive messages sent with IKEv2 | Int32
> ikev2-dpd-recv | Total number of Dead-Peer-Detection (DPD) messages received with IKEv2 | Int32
> ikev2-dpd-send | Total number of Dead-Peer-Detection (DPD) messages sent with IKEv2 | Int32
> ikev2-dpd-recv-reply | Total number of reply messages for received Dead-Peer-Detection (DPD) messages | Int32
> ikev2-dpd-send-reply | Total number of reply messages for sent Dead-Peer-Detection (DPD) messages | Int32
> ikev2-dpd-timeout | Total number of Dead-Peer-Detection (DPD) timed-out | Int32
> ikev2-dpd-disconnect | Total number of Dead-Peer-Detection (DPD) disconnected | Int32
> ipsec-dpd-p1rekey | Total number of Dead-Peer-Detection (DPD) messages to wait for phase 1 rekey period. | Int32
> ikev2-ikesadel | Total number of IKEv2 Security Association Delete Packets sent and received. | Int32
> ikev2-ikesadelreq-sent | Total number of IKEv2 Security Association Delete Requests sent. | Int32
> ikev2-ikesadelreq-recv | Total number of IKEv2 Security Association Delete Requests received. | Int32
> ikev2-ikesadelrep-sent | Total number of IKEv2 IKE Security Association Delete Responses sent. | Int32
> ikev2-ikesadelrep-recv | Total number of IKEv2 Security Association Delete Responses received. | Int32
> ikev2-curikev2sa | Total number of current IKEv2 Security Associations. Type: Gauge | Int32
> ikev2-curhalfsa | Total number of currently half-open IKEv2 Security Associations. Type: Gauge | Int32
> ikev2-curconnsa | Total number of currently connecting IKEv2 Security Associations. Type: Gauge | Int32
> ikev2-curestsa | Total number of currently established IKEv2 Security Associations. Type: Gauge | Int32
> ikev2-curchildsa | Total number of current Child Security Associations. Type: Gauge | Int32
> ikev2-exp-retran | Total number of IKESA retransmission expirations. | Int32
> ikev2-exp-setupnoxchg | Total number of IKESA setup expirations (no exchange). | Int32
> ikev2-exp-setup | Total number of IKESA setup expirations. | Int32
> ikev2-exp-lifesoft | Total number of IKESA lifetime (soft) expirations. | Int32
> ikev2-exp-lifehard | Total number of IKESA lifetime (hard) expirations. | Int32
> ikev2-exp-childsetupnoxchg | Total number of Child Security Association setup expirations (no exchange). | Int32
> ikev2-exp-childlifesoft | Total number of Child Security Association lifetime (soft) expirations. | Int32
> ikev2-exp-childlifehard | Total number of Child Security Association lifetime (hard) expirations. | Int32
> ikev2-csa-createreqsnt | Total number of IKEv2 Create CHILD_SA Exchange Requests sent. | Int32
> ikev2-csa-createreqrcv | Total number of IKEv2 Create CHILD_SA Exchange Requests received. | Int32
> ikev2-csa-createrspsnt | Total number of IKEv2 Create CHILD_SA Exchange Responses sent. | Int32
> ikev2-csa-creatersprcv | Total number of IKEv2 Create CHILD_SA Exchange Responses received. | Int32
> ikev2-csa-createsucc | Total number of IKEv2 Create CHILD_SA Exchange successes. | Int32
> ikev2-csa-createfail | Total number of IKEv2 Create CHILD_SA Exchange failures. | Int32
> ikev2-csa-createsftovrflw | Total number of IKEv2 Create CHILD_SA Exchange soft limit overflow attempts. | Int32
> ikev2-csa-createhrdovrflw | Total number of IKEv2 Create CHILD_SA Exchange hard limit overflow attempts. | Int32
> ikev2-csa-sngldelpldsnt | Total number of IKEv2 INFORMATIONAL Exchanges with a single CHILD_SA Delete payload sent. | Int32
> ikev2-csa-sngldelpldrcv | Total number of IKEv2 INFORMATIONAL Exchanges with a single CHILD_SA Delete payload received. | Int32
> ikev2-csa-multdelpldsnt | Total number of IKEv2 INFORMATIONAL Exchanges with multiple CHILD_SA Delete payloads sent. | Int32
> ikev2-csa-multdelpldrcv | Total number of IKEv2 INFORMATIONAL Exchanges with multiple CHILD_SA Delete payloads received. | Int32
> ikev2-csa-delpldsnglspisnt | Total number of IKEv2 INFORMATIONAL Exchanges with a CHILD_SA Delete payload with a single SPI sent. | Int32
> ikev2-csa-delpldsnglspircv | Total number of IKEv2 INFORMATIONAL Exchanges with a CHILD_SA Delete payload with a single SPI received. | Int32
> ikev2-csa-delmultspisnt | Total number of IKEv2 INFORMATIONAL Exchanges with a CHILD_SA Delete payload with multiple SPIs sent. | Int32
> ikev2-csa-delmultspisnt | Total number of IKEv2 INFORMATIONAL Exchanges with a CHILD_SA Delete payload with multiple SPIs received. | Int32
> ikev2-auth-p1succ | Total number of IKEv2 Phase 1 authentication successes. | Int32
> ikev2-auth-p1fail | Total number of IKEv2 Phase 1 authentication failures. | Int32
> ikev2-auth-p1req | Total number of IKEv2 Phase 1 authentication requests sent. | Int32
> ikev2-auth-p1rsp | Total number of IKEv2 Phase 1 authentication responses received. | Int32
> ikev2-auth-p1finalsent | Total number of IKEv2 Phase 1 authentication requests or responses sent in the final exchange of Phase 1 authentication. | Int32
> ikev2-auth-p1finalrcvd | Total number of IKEv2 Phase 1 authentication requests or responses received in the final exchange of Phase 1 authentication. | Int32
> ikev2-auth-p2succ | Total number of IKEv2 Phase 2 authentication successes. | Int32
> ikev2-auth-p2fail | Total number of IKEv2 Phase 2 authentication failures. | Int32
> ikev2-auth-p2req | Total number of IKEv2 Phase 2 authentication requests sent. | Int32
> ikev2-auth-p2rsp | Total number of IKEv2 Phase 2 authentication responses received. | Int32
> ikev2-auth-p2succmd5 | Total number of IKEv2 Phase 2 authentication MD5 successes. | Int32
> ikev2-auth-p2failmd5 | Total number of IKEv2 Phase 2 authentication MD5 failures. | Int32
> ikev2-auth-p2succgtc | Total number of IKEv2 Phase 2 authentication Generic Token Card successes. | Int32
> ikev2-auth-p2failgtc | Total number of IKEv2 Phase 2 authentication Generic Token Card failures. | Int32
> ikev2-auth-p2finalsent | Total number of IKEv2 Phase 2 authentication requests or responses sent in the final exchange of Phase 2 authentication. | Int32
> ikev2-auth-p2finalrcvd | Total number of IKEv2 Phase 2 authentication requests or responses received in the final exchange of Phase 2 authentication. | Int32
> ikev2-auth-failhash | Total number of IKEv2 Phase 2 authentication hash match failures. | Int32
> ikev2-auth-failsign | Total number of IKEv2 Phase 2 authentication signing failures. | Int32
> ikev2-auth-failmskmiss | Total number of IKEv2 Master Session Keys missing at Phase 1 completion. | Int32
> ikev2-auth-failmissanother | Total number of IKEv2 authentication that failed because of missing NOTIFY (ANOTHER_AUTH_FOLLOWS) payload. | Int32
> ikev2-xchg-droprspnoikesa | Total number of IKEv2 exchanges dropped (response packets dropped). No IKE SA. | Int32
> ikev2-xchg-dropinvrsp | Total number of IKEv2 exchanges dropped (invalid responses). | Int32
> ikev2-xchg-dropnoninitnoikesa | Total number of IKEv2 exchanges dropped (non-init exchanges dropped). No IKE SA. | Int32
> ikev2-xchg-dropinvmsgid | Total number of IKEv2 exchanges dropped (invalid message ID). | Int32
> ikev2-xchg-dropinvmajver | Total number of IKEv2 exchanges dropped (invalid major version). | Int32
> ikev2-xchg-dropikesaerr | Total number of IKEv2 exchanges dropped (IKE SA error). | Int32
> ikev2-xchg-dropunkcrit | Total number of IKEv2 exchanges dropped (unknown critical payload). | Int32
> ikev2-xchg-dropretransdisc | Total number of IKEv2 exchanges dropped (retransmitted request). | Int32
> ikev2-notif-cooksent | Total number of IKEv2 Cookie Notify messages sent. | Int32
> ikev2-notif-cookrecv | Total number of IKEv2 Cookie Notify messages received. | Int32
> ikev2-notif-cookmatch | Total number of IKEv2 Cookie Notify messages matched. | Int32
> ikev2-notif-cooknotmatch | Total number of IKEv2 Cookie Notify messages not matched. | Int32
> ikev2-notif-multauthsupp | Total number of IKEv2 multiple authentications supported. | Int32
> ikev2-notif-anothauth | Total number of NOTIFY (ANOTHER_AUTH_FOLLOWS) payloads received. | Int32
> ikev2-rekey-ikesareqsent | Total IKEv2 IKE SA rekey requests sent. | Int32
> ikev2-rekey-ikesareqrcvd | Total IKEv2 IKE SA rekey requests received. | Int32
> ikev2-rekey-ikesarspsent | Total IKEv2 IKE SA rekey responses sent. | Int32
> ikev2-rekey-ikesarsprcvd | Total IKEv2 IKE SA rekey responses received. | Int32
> ikev2-rekey-ikesaignored | Total IKEv2 IKE SA rekeys ignored. | Int32
> ikev2-rekey-childsareqsent | Total IKEv2 Child SA rekey requests sent. | Int32
> ikev2-rekey-childsareqrecv | Total IKEv2 Child SA rekey requests received. | Int32
> ikev2-rekey-childsarspsent | Total IKEv2 Child SA rekey responses sent. | Int32
> ikev2-rekey-childsarsprecv | Total IKEv2 Child SA rekey responses received. | Int32
> ikev2-rekey-childsaignored | Total IKEv2 Child SA rekeys ignored. | Int32
> ikev2-mobike-sent | Total IKEv2 MOBIKE Notify messages sent. | Int32
> ikev2-mobike-recv | Total IKEv2 MOBIKE Notify messages received. | Int32
> ikev2-mobike-ignored | Total IKEv2 MOBIKE Notify messages ignored. | Int32
> ikev2-misc-ikesacrefail | Total IKEv2 SA create failures. | Int32
> ikev2-misc-saflowopfail | Total IKEv2 SA flow operation failures. | Int32
> ikev2-notifpaysent-invke | Total IKEv2 Notify payloads sent (invalid KE payload). | Int32
> ikev2-notifpaysent-invmajver | Total IKEv2 Notify payloads sent (invalid major version). | Int32
> ikev2-notifpaysent-invmsgid | Total IKEv2 Notify payloads sent (invalid message ID). | Int32
> ikev2-notifpaysent-invsyn | Total IKEv2 Notify payloads sent (invalid syntax). | Int32
> ikev2-notifpaysent-noaddsa | Total IKEv2 Notify payloads sent (no additional SAs). | Int32
> ikev2-notifpaysent-noprop | Total IKEv2 Notify payloads sent (no proposal chosen). | Int32
> ikev2-notifpaysent-tsunaccept | Total IKEv2 Notify payloads sent (TS unacceptable). | Int32
> ikev2-notifpaysent-unsuppcrit | Total IKEv2 Notify payloads sent (unsupported critical payload). | Int32
> ikev2-notifpaysent-intfail | Total IKEv2 Notify payloads received (internal failure sent). | Int32
> ikev2-notifpayrecv-invke | Total IKEv2 Notify payloads received (invalid KE payload). | Int32
> ikev2-notifpayrecv-invmajver | Total IKEv2 Notify payloads received (invalid major version). | Int32
> ikev2-notifpayrecv-invmsgid | Total IKEv2 Notify payloads received (invalid message ID). | Int32
> ikev2-notifpayrecv-invsyn | Total IKEv2 Notify payloads received (invalid syntax). | Int32
> ikev2-notifpayrecv-noaddsa | Total IKEv2 Notify payloads received (no additional SAs). | Int32
> ikev2-notifpayrecv-noprop | Total IKEv2 Notify payloads received (no proposal chosen). | Int32
> ikev2-notifpayrecv-tsunaccept | Total IKEv2 Notify payloads received (TS unacceptable). | Int32
> ikev2-notifpayrecv-unsuppcrit | Total IKEv2 Notify payloads received (unsupported critical payload). | Int32
> ikev2-decfail-pktfail | Total IKEv2 exchange decode failures (packet errors). | Int32
> ikev2-decfail-interr | Total IKEv2 exchange decode failures (internal errors). | Int32
> ikev2-decfail-iphdr | Total IKEv2 exchange decode failures (invalid IP header). | Int32
> ikev2-decfail-udphdr | Total IKEv2 exchange decode failures (invalid UDP header). | Int32
> ikev2-decfail-ikehdr | Total IKEv2 exchange decode failures (invalid IKE header). | Int32
> ikev2-decfail-ikehdrpay | Total IKEv2 exchange decode failures (invalid IKE header payload). | Int32
> ikev2-decfail-ikehdrinitspi | Total IKEv2 exchange decode failures (invalid IKE header init Security Parameter Index). | Int32
> ikev2-decfail-ikehdrrspspi | Total IKEv2 exchange decode failures (invalid IKE header response Security Parameter Index). | Int32
> ikev2-decfail-ikehdrmajver | Total IKEv2 exchange decode failures (invalid IKE header major version). | Int32
> ikev2-decfail-ikehdrminver | Total IKEv2 exchange decode failures (invalid IKE header minor version). | Int32
> ikev2-decfail-ikehdrxchgtyp | Total IKEv2 exchange decode failures (invalid IKE header exchange type). | Int32
> ikev2-decfail-ikehdrrecvflag | Total IKEv2 exchange decode failures (invalid IKE header received flag). | Int32
> ikev2-decfail-ikehdrlen | Total IKEv2 exchange decode failures (invalid IKE header length). | Int32
> ikev2-decfail-syn | Total IKEv2 exchange decode failures (invalid syntax). | Int32
> ikev2-decfail-paysyn | Total IKEv2 exchange decode failures (invalid payload syntax). | Int32
> ikev2-decfail-paylen | Total IKEv2 exchange decode failures (invalid payload length). | Int32
> ikev2-decfail-unkcritpay | Total IKEv2 exchange decode failures (invalid critical payload). | Int32
> ikev2-decfail-toomanypay | Total IKEv2 exchange decode failures (too many payloads). | Int32
> ikev2-decfail-sapaylen | Total IKEv2 exchange decode failures (invalid SA payload length). | Int32
> ikev2-decfail-saprophdr | Total IKEv2 exchange decode failures (invalid SA proposal header). | Int32
> ikev2-decfail-saprophdrrecv | Total IKEv2 exchange decode failures (invalid SA proposal header received). | Int32
> ikev2-decfail-toomanytrans | Total IKEv2 exchange decode failures (too many transforms). | Int32
> ikev2-decfail-saprophdrlen | Total IKEv2 exchange decode failures (invalid SA proposal header length). | Int32
> ikev2-decfail-toomanyprop | Total IKEv2 exchange decode failures (too many proposals). | Int32
> ikev2-decfail-1stsapropnum | Total IKEv2 exchange decode failures (invalid first SA proposal). | Int32
> ikev2-decfail-saprotid | Total IKEv2 exchange decode failures (invalid first SA proposal). | Int32
> ikev2-decfail-sapropnum | Total IKEv2 exchange decode failures (invalid SA proposal number). | Int32
> ikev2-decfail-translen | Total IKEv2 exchange decode failures (invalid transform length). | Int32
> ikev2-decfail-transhdr | Total IKEv2 exchange decode failures (invalid transform header). | Int32
> ikev2-decfail-transhdrrecv | Total IKEv2 exchange decode failures (invalid transform header received). | Int32
> ikev2-decfail-transtype | Total IKEv2 exchange decode failures (invalid transform type). | Int32
> ikev2-decfail-transid | Total IKEv2 exchange decode failures (invalid transform ID). | Int32
> ikev2-decfail-kepaylen | Total IKEv2 exchange decode failures (invalid KE payload length). | Int32
> ikev2-decfail-kedhgrp | Total IKEv2 exchange decode failures (invalid KE DH group). | Int32
> ikev2-decfail-kedhgrplen | Total IKEv2 exchange decode failures (invalid KE DH group length). | Int32
> ikev2-decfail-idpaylen | Total IKEv2 exchange decode failures (invalid ID payload length). | Int32
> ikev2-decfail-idpaytype | Total IKEv2 exchange decode failures (invalid ID payload type). | Int32
> ikev2-decfail-authpaylen | Total IKEv2 exchange decode failures (invalid authentication payload length). | Int32
> ikev2-decfail-noncepaylen | Total IKEv2 exchange decode failures (invalid nonce payload length). | Int32
> ikev2-decfail-notifpaylen | Total IKEv2 exchange decode failures (invalid Notify payload length). | Int32
> ikev2-decfail-notifpayspilen | Total IKEv2 exchange decode failures (invalid Notify payload Security Parameter Index length). | Int32
> ikev2-decfail-notifpaynat | Total IKEv2 exchange decode failures (invalid Notify payload NAT). | Int32
> ikev2-decfail-notifpayprotid | Total IKEv2 exchange decode failures (invalid Notify payload protocol ID). | Int32
> ikev2-decfail-eappaylen | Total IKEv2 exchange decode failures (invalid EAP payload length). | Int32
> ikev2-decfail-notifpayrekey | Total IKEv2 exchange decode failures (invalid Notify payload rekey). | Int32
> ikev2-decfail-cppaylen | Total IKEv2 exchange decode failures (invalid CP payload length). | Int32
> ikev2-decfail-notifpaycook | Total IKEv2 exchange decode failures (invalid Notify payload cookie). | Int32
> ikev2-decfail-tspaylen | Total IKEv2 exchange decode failures (invalid TS payload length). | Int32
> ikev2-decfail-cppayattrlen | Total IKEv2 exchange decode failures (invalid CP payload attribute length). | Int32
> ikev2-decfail-tspayrecv | Total IKEv2 exchange decode failures (invalid TS payload received). | Int32
> ikev2-decfail-encrpaylen | Total IKEv2 exchange decode failures (invalid encrypted payload length). | Int32
> ikev2-decfail-tspaytstype | Total IKEv2 exchange decode failures (invalid TS payload TS type). | Int32
> ikev2-decfail-unsuppcritpay | Total IKEv2 exchange decode failures (unsupported critical payload). | Int32
> ikev2-decfail-unsuppcertpay | Total IKEv2 exchange decode failures (unsupported certificate payload). | Int32
> ikev2-decfail-unsuppnotifprotah | Total IKEv2 exchange decode failures (unsupported Notify protocol authentication header). | Int32
> ikev2-decfail-unsuppauthmeth | Total IKEv2 exchange decode failures (unsupported Notify protocol authentication header). | Int32
> ikev2-decfail-unsupppaycritvid | Total IKEv2 exchange decode failures (unsupported payload critical VID). | Int32
> ikev2-decfail-unsuppmeth | Total IKEv2 exchange decode failures (unsupported method). | Int32
> ikev2-decfail-unkerr | Total IKEv2 exchange decode failures (unknown error). | Int32
> ikev2-decfail-unsuppsapayprotah | Total IKEv2 exchange decode failures (unsupported SA payload protocol authentication header). | Int32
> ikev2-decfail-unsupptspaytsnum | Total IKEv2 exchange decode failures (unsupported TS payload TS number). | Int32
> ikev2-decfail-unsupptspaytstype | Total IKEv2 exchange decode failures (unsupported TS payload TS type). | Int32
> ikev2-decfail-unsupptspaytsprot | Total IKEv2 exchange decode failures (unsupported TS payload TS protocol). | Int32
> ikev2-decfail-cppaynoipaddr | Total IKEv2 exchange decode failures (invalid CP payload—-no IP address). | Int32
> ikev2-decfail-cppayunkattr | Total IKEv2 exchange decode failures (invalid CP payload—-unknown attribute). | Int32
> ikev2-decryptfail | Total IKEv2 decryption failures (packets failure). | Int32
> ikev2-decryptfail-hmac | Total IKEv2 decryption failures (HMAC mismatch). | Int32
> ikev2-decryptfail-pad | Total IKEv2 decryption failures (PAD length error). | Int32
> ikev2-xchg-badmsgid | Total IKEv2 exchange statistics (bad message ID). | Int32
> ikev2-xchg-badresp | Total IKEv2 exchange statistics (bad response). | Int32
> ikev2-xchg-stalemsgid | Total IKEv2 exchange statistics (stale message ID). | Int32
> ikev2-xchg-unkerr | Total IKEv2 exchange statistics (unknown error). | Int32
> ikev2-xchg-statelookfail | Total IKEv2 exchange statistics (state lookup failure). | Int32
> ikev2-notifrecv-unsuppcritpay | Total IKEv2 Notify message receive statistics (unsupported critical payload). | Int32
> ikev2-notifrecv-invikespi | Total IKEv2 Notify message receive statistics (invalid IKE Security Parameter Index). | Int32
> ikev2-notifrecv-invmajver | Total IKEv2 Notify message receive statistics (invalid major version). | Int32
> ikev2-notifrecv-invsyn | Total IKEv2 Notify message receive statistics (invalid syntax). | Int32
> ikev2-notifrecv-invmsgid | Total IKEv2 Notify message receive statistics (invalid message ID). | Int32
> ikev2-notifrecv-invspi | Total IKEv2 Notify message receive statistics (invalid Security Parameter Index). | Int32
> ikev2-notifrecv-nopropchosen | Total IKEv2 Notify message receive statistics (no proposal chosen). | Int32
> ikev2-notifrecv-invkepay | Total IKEv2 Notify message receive statistics (invalid KE payload). | Int32
> ikev2-notifrecv-authfail | Total IKEv2 Notify message receive statistics (authentication failure). | Int32
> ikev2-notifrecv-singpairreq | Total IKEv2 Notify message receive statistics (single pair required). | Int32
> ikev2-notifrecv-noaddsa | Total IKEv2 Notify message receive statistics (no additional SAs). | Int32
> ikev2-notifrecv-intaddrfail | Total IKEv2 Notify message receive statistics (internal address failure). | Int32
> ikev2-notifrecv-failcpreq | Total IKEv2 Notify message receive statistics (failed CP required). | Int32
> ikev2-notifrecv-tsunaccept | Total IKEv2 Notify message receive statistics (TS unacceptable). | Int32
> ikev2-notifrecv-invsel | Total IKEv2 Notify message receive statistics (invalid selectors). | Int32
> ikev2-notifrecv-unacceptaddr | Total IKEv2 Notify message receive statistics (unacceptable addresses). | Int32
> ikev2-notifrecv-multiauthsupp | Total IKEv2 Notify message receive statistics (multiple authentication supported). | Int32
> ikev2-notifrecv-anothauthfoll | Total IKEv2 Notify message receive statistics (another authentication follows). | Int32
> ikev2-notifrecv-unexpectnat | Total IKEv2 Notify message receive statistics (unexpected NAT detected). | Int32
> ikev2-notifrecv-macauthfail | Total IKEv2 Notify message receive statistics (MAC address authentication failed). | Int32
> ikev2-notifrecv-hsserrusrunk | Total IKEv2 Notify message receive statistics (HSS error—user unknown). | Int32
> ikev2-notifrecv-initcont | Total IKEv2 Notify message receive statistics (initial contact). | Int32
> ikev2-notifrecv-windsiz | Total IKEv2 Notify message receive statistics (set window size). | Int32
> ikev2-notifrecv-addtsposs | Total IKEv2 Notify message receive statistics (additional TS possible). | Int32
> ikev2-notifrecv-ipcompsupp | Total IKEv2 Notify message receive statistics (IPCOMP supported). | Int32
> ikev2-notifrecv-natdetsrcip | Total IKEv2 Notify message receive statistics (NAT detection—source IP). | Int32
> ikev2-notifrecv-natdetdstip | Total IKEv2 Notify message receive statistics (NAT detection—destination IP). | Int32
> ikev2-notifrecv-cookie | Total IKEv2 Notify message receive statistics (cookie). | Int32
> ikev2-notifrecv-usetransmode | Total IKEv2 Notify message receive statistics (use transport mode). | Int32
> ikev2-notifrecv-httpcertsupp | Total IKEv2 Notify message receive statistics (HTTP certificate lookup supported). | Int32
> ikev2-notifrecv-rekeysa | Total IKEv2 Notify message receive statistics (rekey SA). | Int32
> ikev2-notifrecv-nonfirstfragalso | Total IKEv2 Notify message receive statistics (non-first fragment also). | Int32
> ikev2-notifrecv-mobikesupp | Total IKEv2 Notify message receive statistics (MOBIKE supported). | Int32
> ikev2-notifrecv-addip4addr | Total IKEv2 Notify message receive statistics (additional IPv4 address). | Int32
> ikev2-notifrecv-addip6addr | Total IKEv2 Notify message receive statistics (additional IPv6 address). | Int32
> ikev2-notifrecv-noaddaddr | Total IKEv2 Notify message receive statistics (no additional address). | Int32
> ikev2-notifrecv-updsaaddr | Total IKEv2 Notify message receive statistics (update SA addresses). | Int32
> ikev2-notifrecv-cookie2 | Total IKEv2 Notify message receive statistics (cookie 2). | Int32
> ikev2-notifrecv-nonatallow | Total IKEv2 Notify message receive statistics (no NAT allowed). | Int32
> ikev2-notifrecv-other | Total IKEv2 Notify message receive statistics (others or unknown). | Int32
> ikev2-notifrecv-sipfallbnotallow | Total IKEv2 Notify message receive statistics (SIP fallback not allowed). | Int32
> ikev2-notifrecv-esptfcpadnotsupp | Total IKEv2 Notify message receive statistics (ESP TFC padding not supported). | Int32
> ikev2-notifrecv-congrejrecv | Total IKEv2 Notify message receive statistics (congestion rejections received). | Int32
> ikev2-cert-reqsent | Total IKEv2 certification statistics (certificate requests sent). | Int32
> ikev2-cert-reqrecv | Total IKEv2 certification statistics (certificate requests received). | Int32
> ikev2-cert-sent | Total IKEv2 certification statistics (certificates sent). | Int32
> ikev2-cert-recv | Total IKEv2 certification statistics (certificates received). | Int32
> ike-udpflows | IKE statistics (current UDP flows). Type: Gauge | Int32
> ike-cookieflows | IKE statistics (current cookie flows). Type: Gauge | Int32
> ike-txpackets | Total IKE Transmit statistics (IKE packets transmitted). | Int32
> ike-rxpackets | Total IKE Receive statistics (IKE packets received). | Int32
> ike-reqrecv | Total IKE Receive statistics (new IKE requests). | Int32
> ike-udpflowpackets | Total IKE Receive statistics (UDP flow packets). | Int32
> ike-cookieflowpackets | Total IKE Receive statistics (cookie flow packets). | Int32
> crypto-txesppacket | Total Transmit statistics (ESP encoded packets). | Int64
> crypto-txespoctet | Total Transmit statistics (ESP encoded bytes). | Int64
> crypto-txahpacket | Total Transmit statistics (Authentication Header encoded packets). | Int64
> crypto-txahoctet | Total Transmit statistics (Authentication Header encoded bytes). | Int64
> crypto-rxesppacket | Total Receive statistics (ESP decoded packets). | Int64
> crypto-rxespoctet | Total Receive statistics (ESP decoded bytes). | Int64
> crypto-rxahpacket | Total Receive statistics (Authentication Header encoded packets). | Int64
> crypto-rxahoctet | Total Receive statistics (Authentication Header encoded bytes). | Int64
> crypto-errauthpacket | Total Receive statistics (error counter—authentication packets). | Int64
> crypto-errauthoctet | Total Receive statistics (error counter—authentication packets). | Int64
> crypto-errbadrecpacket | Total Receive statistics (error counter—authentication bytes). | Int64
> crypto-errbadrecoctet | Total Receive statistics (error counter—bad record packets). | Int64
> crypto-errdiscpacket | Total Receive statistics (error counter—discarded packets). | Int64
> crypto-errdiscoctet | Total Receive statistics (error counter—discarded bytes). | Int64
> crypto-errignpacket | Total Receive statistics (error counter—ignored packets). | Int64
> crypto-errignoctet | Total Receive statistics (error counter—ignored bytes). | Int64
> crypto-errunderrunpacket | Total Receive statistics (error counter—input under-run packets). | Int64
> crypto-errunderrunoctet | Total Receive statistics (error counter—input under-run bytes). | Int64
> crypto-errinvpacket | Total Receive statistics (error counter—invalid packets). | Int64
> crypto-errinvoctet | Total Receive statistics (error counter—invalid bytes). | Int64
> crypto-errreplaypacket | Total Receive statistics (error counter—replay packets). | Int64
> crypto-errreplayoctet | Total Receive statistics (error counter—replay bytes). | Int64
> ipsecctrl-lte-template-reqs | IPSec Controller - LTE - The total number of service template request messages. | Int32
> ipsecctrl-lte-template-unreg-reqs | IPSec Controller - LTE - The total number of service template unregister request messages. | Int32
> ipsecctrl-lte-map-reqs | IPSec Controller - LTE - The total number of crypto map request messages. | Int32
> ipsecctrl-lte-map-est | IPSec Controller - LTE - The total number of crypto map established messages. | Int32
> ipsecctrl-lte-map-del-reqs | IPSec Controller - LTE - The total number of crypto map delete request messages. | Int32
> ipsecctrl-lte-map-failed | IPSec Controller - LTE - The total number of crypto map failed messages. | Int32
> ipsecctrl-lte-map-state-notif | IPSec Controller - LTE - The total number of crypto map state change notifications sent by this system. | Int32
> ipsecctrl-lte-ipsecmgr-death-notif | IPSec Controller - LTE - The total number of ipsecmgr death notification messages sent to the registered facilites. | Int32
> ipsecctrl-lte-qos-maps | IPSec Controller - LTE - The total number of crypto maps with QoS. | Int32
> ssl-cursess | This proprietary gauge indicates the total number of SSL sessions currently running on the system. Type: Gauge | Int64
> ssl-curconninit | This proprietary gauge indicates the total number of current SSL connections that have been initiated. Type: Gauge | Int64
> ssl-curconnresp | This proprietary gauge indicates the total number of current SSL connections that have been responded to. Type: Gauge | Int64
> ssl-curconnected | This proprietary gauge indicates the total number of current SSL connections that are connected. Type: Gauge | Int64
> ssl-curconnfail | This proprietary gauge indicates the total number of current SSL connections that have failed. Type: Gauge | Int64
> ssl-curconnecting | This proprietary gauge indicates the total number of current SSL connections that are connecting. Type: Gauge | Int64
> ssl-conclosesent | This proprietary counter tracks the total number of SSL connection close messages sent. | Int64
> ssl-conclosercvd | This proprietary counter tracks the total number of SSL connection close messages received. | Int64
> ssl-cachehits | This proprietary counter tracks the total number of hits for the SSL session cache. | Int64
> ssl-cachemiss | This proprietary counter tracks the total number of misses for the SSL session cache. | Int64
> ssl-cachetimeout | This proprietary counter tracks the total number of timeouts for the SSL session cache. | Int64
> ssl-cachefull | This proprietary counter tracks the total number of times the SSL session cache has been full. | Int64
> ssl-cachetotalsess | This proprietary counter tracks the total number of current sessions for the SSL session cache. | Int64
> ssl-txrecord | This proprietary counter tracks the total number of SSL records transmitted. | Int64
> ssl-txmsg | This proprietary counter tracks the total number of SSL messages transmitted. | Int64
> ssl-txbyte | This proprietary counter tracks the total number of SSL bytes transmitted. | Int64
> ssl-rxrecord | This proprietary counter tracks the total number of SSL records received. | Int64
> ssl-rxmsg | This proprietary counter tracks the total number of SSL messages transmit received. | Int64
> ssl-rxbyte | This proprietary counter tracks the total number of SSL bytes received. | Int64
> ssl-encerr | This proprietary counter tracks the total number of SSL encryption errors. | Int64
> ssl-decerr | This proprietary counter tracks the total number of SSL decode errors. | Int64
> ssl-decryerr | This proprietary counter tracks the total number of SSL decryption errors. | Int64
> ssl-autherr | This proprietary counter tracks the total number of SSL authentication errors. | Int64
> ssl-failinithserr | This proprietary counter tracks the total number of SSL initiated handshakes failed with errors. | Int64
> ssl-failtimeouthserr | This proprietary counter tracks the total number of SSL handshakes failed with timeouts. | Int64
> ssl-failresphserr | This proprietary counter tracks the total number of SSL responded handshakes failed with errors. | Int64
> ssl-alertrecv | This proprietary counter tracks the total number of SSL alerts received. | Int64
> ssl-alertrecv-unexpmsg | This proprietary counter tracks the total number of SSL alerts received for unexpected message. | Int64
> ssl-alertrecv-badrecmac | This proprietary counter tracks the total number of SSL alerts received for bad MAC record. | Int64
> ssl-alertrecv-decryfail | This proprietary counter tracks the total number of SSL alerts received for decryption failure. | Int64
> ssl-alertrecv-compfail | This proprietary counter tracks the total number of SSL alerts received for decompression failure. | Int64
> ssl-alertrecv-recoflow | This proprietary counter tracks the total number of SSL alerts received for record overflow. | Int64
> ssl-alertrecv-handshake | This proprietary counter tracks the total number of SSL alerts received for handshake failure. | Int64
> ssl-alertrecv-illparm | This proprietary counter tracks the total number of SSL alerts received for illegal parameters. | Int64
> ssl-alertrecv-certunsupp | This proprietary counter tracks the total number of SSL alerts received for unsupported certificates. | Int64
> ssl-alertrecv-certbad | This proprietary counter tracks the total number of SSL alerts received for bad certificate. | Int64
> ssl-alertrecv-certexpir | This proprietary counter tracks the total number of SSL alerts received - certificate expired. | Int64
> ssl-alertrecv-certrevok | Number of SSL alerts received for certificate revoked. | Int64
> ssl-alertrecv-certunk | This proprietary counter tracks the total number of SSL alerts received for certificate unknown. | Int64
> ssl-alertrecv-accdeny | This proprietary counter tracks the total number of SSL alerts received for access denied. | Int64
> ssl-alertrecv-decode | This proprietary counter tracks the total number of SSL alerts received for decode errors. | Int64
> ssl-alertrecv-decryerr | Number of SSL alerts received - decryption error. | Int64
> ssl-alertrecv-export | This proprietary counter tracks the total number of SSL alerts received for export restricted. | Int64
> ssl-alertrecv-protover | This proprietary counter tracks the total number of SSL alerts received for protocol version. | Int64
> ssl-alertrecv-interr | This proprietary counter tracks the total number of SSL alerts received for internal errors. | Int64
> ssl-alertrecv-insuffsec | This proprietary counter tracks the total number of SSL alerts received for insufficient security. | Int64
> ssl-alertrecv-usercanc | This proprietary counter tracks the total number of SSL alerts received for user cancellation. | Int64
> ssl-alertrecv-noreneg | This proprietary counter tracks the total number of SSL alerts received for no renegotiation. | Int64
> ssl-alertrecv-unknownca | This proprietary counter tracks the total number of SSL alerts received for unknown certificate authority. | Int64
> ssl-alertsent | This proprietary counter tracks the total number of SSL alerts sent. | Int64
> ssl-alertsent-unexpmsg | This proprietary counter tracks the total number of SSL alerts sent for unexpected messages. | Int64
> ssl-alertsent-badrecmac | This proprietary counter tracks the total number of SSL alerts sent for bad MAC records. | Int64
> ssl-alertsent-decryfailed | This proprietary counter tracks the total number of SSL alerts sent for decryption failed. | Int64
> ssl-alertsent-recoflow | This proprietary counter tracks the total number of SSL alerts sent for record overflow. | Int64
> ssl-alertsent-handshake | This proprietary counter tracks the total number of SSL alerts sent for handshake failure. | Int64
> ssl-alertsent-illparam | This proprietary counter tracks the total number of SSL alerts sent for illegal parameters. | Int64
> ssl-alertsent-accdenied | This proprietary counter tracks the total number of SSL alerts sent for access denied. | Int64
> ssl-alertsent-decodeerror | This proprietary counter tracks the total number of SSL alerts sent for decode error. | Int64
> ssl-alertsent-decrypterror | This proprietary counter tracks the total number of SSL alerts sent for decryption error. | Int64
> ssl-alertsent-export | This proprietary counter tracks the total number of SSL alerts sent for export restriction. | Int64
> ssl-alertsent-protover | This proprietary counter tracks the total number of SSL alerts sent for protocol version. | Int64
> ssl-alertsent-interr | This proprietary counter tracks the total number of SSL alerts sent for internal error. | Int64
> ssl-alertsent-noregen | This proprietary counter tracks the total number of SSL alerts sent for no renegotiation. | Int64
> ssl-alertsent-unknown | This proprietary counter tracks the total number of SSL alerts sent for unknown reason. | Int64
> hamipv6-totsubscriber | Current number of system-wide HAMIPv6 subscribers. Type: Gauge | Int32
> disc-reason-0 through disc-reason-xxx | Refer to the separate table for disconnect reasons System-level Schema Statistics for Disconnect Reasons | Int64
> enddate | The date at which data ceased to be gathered in YYYYMMDD format where YYYY represents the year, MM represents the month and DD represents the day. Type: Information | String
> endtime | The time at which data ceased to be gathered in HHMMSS format where HH represents the hours, MM represents the minutes, and SS represents the seconds. Type: Information | String
> localenddate | The date (adjusted for the local timezone) at which data ceased to be gathered in YYYYMMDD format where YYYY represents the year, MM represents the month and DD represents the day. Type: Information | String
> localendtime | The time (adjusted for the local timezone) at which data ceased to be gathered in HHMMSS format where HH represents the hours, MM represents the minutes, and SS represents the seconds. Type: Information | String
> incremental | This variable is obsolete. | Int32
> swversion | The system software version in a string of the form "5.0" Type: Information | String
> peak-cpuusage | The system level maximum value of CPU usage. Type: Gauge | Float
> peak-memusage | The system level maximum value of memory usage. Type: Gauge | Float
> uptimestr | The system uptime as a string that shows days, hours, and minutes. Type: Information | String
> sess-max-lastreset-time | The timestamp the last reset for the maximum number of sessions. Type: Information | String
> sess-maxpdsn | The maximum number of PDSN sessions. Type: Gauge | Int32
> sess-maxpdsn-time | The timestamp for max PDSN sessions. Type: Information | String
> sess-maxha | The maximum number of HA sessions. Type: Gauge | Int32
> sess-maxha-time | The timestamp for max HA sessions. Type: Information | String
> sess-maxl2tplns | The maximum number of L2TP LNS sessions. Type: Gauge | Int32
> sess-maxl2tplns-time | The timestamp for max L2TP sessions. Type: Information | String
> sess-maxecsv2 | The maximum number of ECSv2 sessions. Type: Gauge | Int32
> sess-maxecsv2-time | The timestamp for max ECSv2 sessions. Type: Information | String
> sess-maxevdoreva-pdsn | The maximum number of EVDO Rev A sessions. Type: Gauge | Int32
> sess-maxevdoreva-pdsn-time | The timestamp for max EVDO Rev A Sessions. Type: Information | String
> sess-maxipsg | The maximum number of IPSG sessions. Type: Gauge | Int32
> sess-maxipsg-time | The timestamp for max IPSG sessions. Type: Information | String
> sess-maxasngw | The maximum number of ASNGW sessions. Type: Gauge | Int32
> sess-maxasngw-time | The timestamp for max ASNGW sessions. Type: Information | String
> sess-maxasnlr | The maximum number of ASNLR sessions. Type: Gauge | Int32
> sess-maxasnlr-time | The timestamp for max ASNLR sessions. Type: Information | String
> lic-pdsn | The number of licensed PDSN sessions supported by the system. Type: Information | Int32
> lic-ha | The number of licensed HA sessions supported by the system. Type: Information | Int32
> lic-ggsn | The number of licensed GGSN sessions supported by the system. Type: Information | Int32
> lic-l2tplns | The number of licensed L2TP LNS sessions supported by the system. Type: Information | Int32
> lic-combo-phone | The number of licensed combo phone sessions supported by the system Type: Information | Int32
> lic-ecsv2 | The number of licensed Enhanced Charging Service version 2 sessions supported by the system. Type: Information | Int32
> lic-ipservices-gateway | The number of licensed IP Services Gateway sessions supported by the system. Type: Information | Int32
> lic-evdoreva-pdsn | The number of licensed EVDO rev. A PDSN sessions supported by the system. Type: Information | Int32
> lic-scm-proxyregistrar-ietfrfc3261 | The number of licensed SCM proxy server IETF RFC3261 sessions supported by the system. Type: Information | Int32
> lic-scm-proxypcscf | The number of licensed SCM proxy Call Service Control Function (CSCF) sessions supported by the system Type: Information | Int32
> lic-scm-servingscscf | The number of licensed SCM serving CSCF sessions supported by the system. Type: Information | Int32
> lic-scm-interrogatingicscf | The number of licensed SCM interrogating CSCF sessions supported by the system. Type: Information | Int32
> lic-asngw | The number of licensed Access Service Network (ASN) Gateway sessions supported by the system. Type: Information | Int32
> lic-asnlr | The number of ASN Location Register sessions supported by the system. Type: Information | Int32
> lic-ipsg | The number of IPSG Location Register sessions supported by the system. Type: Information | Int32
> lic-combo-3g4g-gw | The number of licensed sessions supported for generic 3G and 4G combined subscribers by the system. Type: Information | Int32
> sess-total-curr | Total number of sessions currently registered with system. Type: Gauge | Int32
> curr-proxy | Total number of current DHCP proxy sessions. Type: Gauge | Int32
> curr-relay-agent | Total number of current DHCP relay agent sessions. Type: Gauge | Int32
> dhcp-curservsess | Total number of DHCP service sessions active on this system. Available across the system. Changes every time when the new DHCP server is started or existing session is terminated. Type: Gauge | Int32
> sess-total-setup | Total number of DHCP setup sessions. | Int32
> setup-proxy | Total number of setup DHCP proxy sessions. | Int32
> setup-relay-agent | Total number of DHCP setup relay agent sessions. | Int32
> dhcp-ttlservsess | Total number of DHCP service sessions registered on this system. Available across the system. Changes every time when the new DHCP session started. | Int32
> total-released | Total number of DHCP sessions released. | Int32
> proxy-bearer-call-term | Total number of DHCP proxy session calls terminated by bearer. | Int32
> proxy-lease-exp-policy | Total number of DHCP proxy session released due to lease expiry policy. | Int32
> proxy-lease-renew-failure | Total number of DHCP proxy session released due to lease renew failure. | Int32
> proxy-ip-mis-match | Total number of DHCP proxy session released due to IP address mis-match. | Int32
> proxy-lease-time-mis-match | Total number of DHCP proxy session released due to lease time mis-match. | Int32
> proxy-other-reasons | Total number of DHCP proxy session released due reasons not mentioned in this table. | Int32
> relay-admin-releases | Total number of DHCP relay session released due administrative reasons. | Int32
> relay-bearer-call-term | Total number of DHCP relay session calls terminated by bearer. | Int32
> relay-lease-time-out | Total number of DHCP relay session released due to lease timeout. | Int32
> relay-other-reasons | Total number of DHCP relay session released due reasons not mentioned in this table. | Int32
> dhcp-servdisc-admin | Total number of DHCP servers disconnected due administrative reasons. Available across the system. Changes every time when the DHCP session is disconnected due to admin intervention. | Int32
> dhcp-servdisc-callterm | Total number of DHCP session calls terminated by bearer. Available across the system. Changes every time when the DHCP call is cleared due to arrival of DHCP Release. | Int32
> dhcp-servdisc-leasetmo | Total number of DHCP session released due to lease timeout. Available across the system. Changes every time when the DHCP session is released due to lease expiry. | Int32
> dhcp-servdisc-other | Total number of DHCP server sessions disconnected due to reasons other than those in this table. | Int32
> dhcp-msg-discover-tx | Total number of DHCP discover messages transmitted. | Int32
> dhcp-msg-discover-retransmitted | Total number of DHCP discover messages retransmitted. | Int32
> dhcp-msg-discover-rx | Total number of DHCP discover messages received. | Int32
> dhcp-msg-discover-retried-rx | Total number of DHCP discover messages received after retry. | Int32
> dhcp-msg-discover-relayed | Total number of DHCP discover messages relayed. | Int32
> dhcp-msg-discoverd-retried-relayed | Total number of DHCP discover messages retried and relayed. | Int32
> dhcp-msg-offer-rx | Total number of DHCP offer messages received. | Int32
> dhcp-msg-offer-discarded | Total number of DHCP offer messages received and discarded. | Int32
> dhcp-msg-offer-tx | Total number of DHCP offer messages transmitted. | Int32
> dhcp-msg-offer-relayed | Total number of DHCP offer messages relayed. | Int32
> dhcp-msg-request-tx | Total number of DHCP request messages transmitted. | Int32
> dhcp-msg-request-retransmitted | Total number of DHCP request messages retransmitted. | Int32
> dhcp-msg-request-rx | Total number of DHCP request messages received. | Int32
> dhcp-msg-request-renewal-rx | Total number of DHCP request messages received for renewal. | Int32
> dhcp-msg-request-requesting-relayed | Total number of DHCP request messages relayed while requesting. | Int32
> dhcp-msg-request-renewing-relayed | Total number of DHCP request messages relayed while renewing. | Int32
> dhcp-msg-ack-rx | Total number of DHCP Ack messages received. | Int32
> dhcp-msg-ack-for-inform | Total number of DHCP Ack messages received for information. | Int32
> dhcp-msg-ack-renewing-rx | Total number of DHCP Ack messages for renewing received. | Int32
> dhcp-msg-ack-tx | Total number of DHCP Ack messages transmitted. | Int32
> dhcp-msg-ack-renewing-tx | Total number of DHCP Ack messages for renewing transmitted. | Int32
> dhcp-msg-ack-relayed | Total number of DHCP Ack messages relayed. | Int32
> dhcp-msg-ack-renewing-relayed | Total number of DHCP Ack messages for renewing relayed. | Int32
> dhcp-msg-nak-rx | Total number of DHCP NAck messages received. | Int32
> dhcp-msg-nak-for-inform | Total number of DHCP NAck messages received for information. | Int32
> dhcp-msg-nak-tx | Total number of DHCP NAck messages transmitted. | Int32
> dhcp-msg-nak-relayed | Total number of DHCP NAck messages relayed. | Int32
> dhcp-msg-decline-tx | Total number of DHCP decline messages transmitted. | Int32
> dhcp-msg-decline-rx | Total number of DHCP decline messages received. | Int32
> dhcp-msg-decline-relayed | Total number of DHCP decline messages relayed. | Int32
> dhcp-msg-release-tx | Total number of DHCP release messages transmitted. | Int32
> dhcp-msg-release-rx | Total number of DHCP release messages received. | Int32
> dhcp-msg-release-relayed | Total number of DHCP release messages relayed. | Int32
> dhcp-msg-release-for-relay-call | Total number of DHCP release messages for relay calls. | Int32
> dhcp-msg-inform-tx | Total number of DHCP inform messages transmitted. | Int32
> dhcp-msg-inform-retransmitted | Total number of DHCP inform messages retransmitted. | Int32
> dhcp-msg-inform-rx | Total number of DHCP inform messages received. | Int32
> dhcp-msg-inform-relayed | Total number of DHCP inform messages relayed. | Int32
> offer-dis-parse-err | Total number of DHCP offer messages discarded due to parse error. | Int32
> offer-dis-lease-less-than-min | Total number of DHCP offer messages discarded due to lease time was less than the minimum duration. | Int32
> offer-dis-lease-greater-than-max | Total number of DHCP offer messages discarded due to lease time was greater than the maximum duration. | Int32
> offer-dis-ip-val-failed | Total number of DHCP offer messages discarded due to IP validation failed. | Int32
> offer-dis-xid-mis-match | Total number of DHCP offer messages discarded due to exchange id mismatch. | Int32
> ack-dis-parse-err | Total number of DHCP Ack messages discarded due to parse error. | Int32
> ack-dis-xid-mis-match | Total number of DHCP Ack messages discarded due to exchange id mismatch. | Int32
> decline-dis-ip-mis-match | Total number of DHCP decline messages discarded due to IP address mismatch. | Int32
> ip-lease-renewal | Total number of DHCP IP lease renewals. | Int32
> failed-ip-lease-renew | Total number of DHCP IP lease renewals failed. | Int32
> no-rly-from-server | Total number of replies from DHCP server. | Int32
> server-nak | Total number of NAck replies from DHCP server. | Int32
> ip-addr-mis-match | Total number of IP address mis-match in DHCP session. | Int32
> lease-mis-match | Total number of lease time mis-match in DHCP session. | Int32
> discover-dis-parse-err | Total number of discover messages discarded due to a parsing error. | Int32
> request-dis-parse-err | Total number of request messages discarded due to a parsing error. | Int32
> release-dis-parse-err | Total number of release messages discarded due to a parsing error. | Int32
> storage-name | Name of the Harddisk Storage available on SMC card on system. This statistic is available with St40 only. Type: Information | String
> storage-curavail | Total storage space currently remained (in bytes) on HDD available on SMC card on system. This statistic is available with St40 only. Type: Gauge | Int64
> storage-ttlavail | Total storage capacity (in bytes) of HDD available on SMC card on system. This statistic is available with St40 only. Type: Information | Int64
> fng-cursess | The total number of current FNG sessions. Type: Gauge | Int32
> fng-curactive | The total number of active sessions currently being facilitated by all Session Managers. Type: Gauge | Int32
> fng-curdormant | The total number of dormant sessions currently being facilitated by the FNG. Type: Gauge | Int32
> fng-ttlsetup | The total number of FNG sessions setup on a system. | Int32
> fng-curchildsa | The total number of current Child Security Associations. Type: Gauge | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌
> Another bulk-stats for “Disconnect Reasons” under system-level schema is available to export system wide counts for disconnect reasons.
> In the following table, the indicator number at the end of the statistic name will vary depending upon the software build in which the show command is issued. To ensure that you have the correct reason, issue the show session disconnect-reasons verbose command.
> A special field “disc-reason-summary” contains all of the disconnect reason counters at once in following semi-colon separated format:
> code = count; code = count; code = count; ........ code = count
> The following variables are supported:
> System-level Schema Statistics for Disconnect Reasons

> Statistic | Description | Data Type
> disc-reason-0 | The total number of sessions disconnected due to unknown reason. | Int64
> disc-reason-1 | The total number of sessions disconnected Administratively. | Int64
> disc-reason-2 | The total number of sessions disconnected by remote system | Int64
> disc-reason-3 | The total number of sessions disconnected by local system. | Int64
> disc-reason-4 | The total number of sessions disconnected due to non-availability of resources. | Int64
> disc-reason-5 | The total number of sessions disconnected due to exceed in service limit. | Int64
> disc-reason-6 | The total number of sessions disconnected due to LCP negotiation failed. | Int64
> disc-reason-7 | The total number of sessions disconnected due to no response in PPP-LCP session. | Int64
> disc-reason-8 | The total number of sessions disconnected due to loop back detected in PPP-LCP. | Int64
> disc-reason-9 | The total number of sessions disconnected due to maximum retries in PPP-LCP session. | Int64
> disc-reason-10 | The total number of sessions disconnected due to PPP-LCP echo not received. | Int64
> disc-reason-11 | The total number of sessions disconnected due to authorization failed in PPP. | Int64
> disc-reason-12 | The total number of sessions disconnected due to authorization failed by no response on AAA server. | Int64
> disc-reason-13 | The total number of sessions disconnected due to PPP authorization failed on no peer response. | Int64
> disc-reason-14 | The total number of sessions disconnected due to PPP authorization failed and reaching maximum retries limit. | Int64
> disc-reason-15 | The total number of sessions disconnected due to invalid AAA attributes in authorization response. | Int64
> disc-reason-16 | The total number of sessions disconnected due to inability in applying subscriber's Access Control List (ACL). | Int64
> disc-reason-17 | The total number of sessions disconnected due to service is not available. | Int64
> disc-reason-18 | The total number of sessions disconnected due to return IP address from AAA server is invalid. | Int64
> disc-reason-19 | The total number of sessions disconnected due to IP address in pool is invalid. | Int64
> disc-reason-20 | The total number of sessions disconnected due to PPP-IPCP negotiation failed. | Int64
> disc-reason-21 | The total number of sessions disconnected due to no response in PPP-IPCP. | Int64
> disc-reason-22 | The total number of sessions disconnected due to maximum retries in PPP-IPCP session. | Int64
> disc-reason-23 | The total number of sessions disconnected due to no IPv4 address are available for subscriber. | Int64
> disc-reason-24 | The total number of sessions disconnected due to system time out limit for silence (ideal) reached. | Int64
> disc-reason-25 | The total number of sessions disconnected due to timeout in complete session. | Int64
> disc-reason-26 | The total number of sessions disconnected due to maximum data limit exceeded. | Int64
> disc-reason-27 | The total number of sessions disconnected due to invalid IPv4 address of subscriber. | Int64
> disc-reason-28 | The total number of sessions disconnected due to MSID authentication failed. | Int64
> disc-reason-29 | The total number of sessions disconnected due to MSID authentication failed and/or no response from AAA server. | Int64
> disc-reason-30 | The total number of sessions disconnected due to maximum limit for retries reached for A11 interface. | Int64
> disc-reason-31 | The total number of sessions disconnected due to A11 interface lifetime expired. | Int64
> disc-reason-32 | The total number of sessions disconnected due to failure in message integrity in A11 interface. | Int64
> disc-reason-33 | The total number of sessions disconnected due to PPP-LCP remote disconnect. | Int64
> disc-reason-34 | The total number of sessions disconnected due to timeout in setting up of session. | Int64
> disc-reason-35 | The total number of sessions disconnected due to PPP keepalive attribute failure. | Int64
> disc-reason-36 | The total number of sessions disconnected due to fail in adding flow to session. | Int64
> disc-reason-37 | The total number of sessions disconnected due to failure in call type detection. | Int64
> disc-reason-38 | The total number of sessions disconnected due to IPCP parameters are wrong. | Int64
> disc-reason-39 | The total number of sessions disconnected due to de-registration of Mobile IP on remote system. | Int64
> disc-reason-40 | The total number of sessions disconnected due to expiry of Mobile IP life time. | Int64
> disc-reason-41 | The total number of sessions disconnected due to protocol error in Mobile IP. | Int64
> disc-reason-42 | The total number of sessions disconnected due to Mobile IP authentication failure. | Int64
> disc-reason-43 | The total number of sessions disconnected due to registration request timeout. | Int64
> disc-reason-44 | The total number of sessions disconnected due to invalid destination context. | Int64
> disc-reason-45 | The total number of sessions disconnected due to source context is removed from system. | Int64
> disc-reason-46 | The total number of sessions disconnected due to destination context is removed from system. | Int64
> disc-reason-47 | The total number of sessions disconnected due to unavailability of required service address. | Int64
> disc-reason-48 | The total number of sessions disconnected due to failure in demux-mgr. | Int64
> disc-reason-49 | The total number of sessions disconnected due to some internal system error. | Int64
> disc-reason-50 | The total number of sessions disconnected due to AAA context is removed from system. | Int64
> disc-reason-51 | The total number of sessions disconnected due to invalid service type. | Int64
> disc-reason-52 | The total number of sessions disconnected due to failure in Mobile IP relay request. | Int64
> disc-reason-53 | The total number of sessions disconnected due to failure in Mobile IP received. | Int64
> disc-reason-54 | The total number of sessions disconnected due to restart in inter PDSN handoff. | Int64
> disc-reason-55 | The total number of sessions disconnected due to mismatch in Generic Routing Encapsulation (GRE) key. | Int64
> disc-reason-56 | The total number of sessions disconnected due to invalid Tunnel context. | Int64
> disc-reason-57 | The total number of sessions disconnected due to no peer LNS address | Int64
> disc-reason-58 | The total number of sessions disconnected due to failure in Tunnel connect. | Int64
> disc-reason-59 | The total number of sessions disconnected due to tunnel disconnected by remote system. | Int64
> disc-reason-60 | The total number of sessions disconnected due to tunnel timeout. | Int64
> disc-reason-61 | The total number of sessions disconnected due to protocol error on remote system. | Int64
> disc-reason-62 | The total number of sessions disconnected due to protocol error on local system. | Int64
> disc-reason-63 | The total number of sessions disconnected due to authorization failed on remote system. | Int64
> disc-reason-64 | The total number of sessions disconnected due to authorization failed on local system | Int64
> disc-reason-65 | The total number of sessions disconnected due to remote system tried for another LNS. | Int64
> disc-reason-66 | The total number of sessions disconnected due to non-availability of resource on local system. | Int64
> disc-reason-67 | The total number of sessions disconnected due to non-availability of resource on remote system. | Int64
> disc-reason-68 | The total number of sessions disconnected due to tunnel disconnected on local system. | Int64
> disc-reason-69 | The total number of sessions disconnected by administrator on remote system. | Int64
> disc-reason-70 | The total number of sessions disconnected due to L2TP Manager logging facility reached to maximum logging capacity. | Int64
> disc-reason-71 | The total number of sessions disconnected due to a failure in Mobile IP registration revocation. | Int64
> disc-reason-72 | The total number of sessions disconnected due to path failure in connecting session. | Int64
> disc-reason-73 | The total number of sessions disconnected due to a failure with the validation of the IP addresses with DHCP relay method. | Int64
> disc-reason-74 | The total number of sessions disconnected due to unknown PDP address or PDP type. | Int64
> disc-reason-75 | The total number of sessions disconnected due to all dynamic PDP addresses are occupied and no PDP address is available to allocate. | Int64
> disc-reason-76 | The total number of sessions disconnected due to out of memory problem. | Int64
> disc-reason-77 | The total number of sessions disconnected due to the mobile requesting the use of a static IP address when static IP address requests are not allowed. | Int64
> disc-reason-78 | The total number of sessions disconnected as no IP address is allocated on DHCP Server. | Int64
> disc-reason-79 | The total number of sessions disconnected due to time expired for IP address allocation on DHCP Server. | Int64
> disc-reason-80 | The total number of sessions disconnected due to a failure with the validation of the IP address. This occurs because the IP address returned by DHCP Server is not present in the static pool in the destination context. | Int64
> disc-reason-81 | The total number of sessions disconnected due to a failure with IP address in the static pool on destination context is not allowed by DHCP Server. | Int64
> disc-reason-82 | The total number of sessions disconnected due to non availability of IP address on DHCP Server. | Int64
> disc-reason-83 | The total number of sessions disconnected due to expiration of IP address lease time. | Int64
> disc-reason-84 | The total number of sessions disconnected due to validation failure of IP address in IP pool. | Int64
> disc-reason-85 | The total number of sessions disconnected due to specified static IP address is not allowed in IP pool. | Int64
> disc-reason-86 | The total number of sessions disconnected due to a failure in validation of static IP address on remote system. | Int64
> disc-reason-87 | The total number of sessions disconnected due to allocated static address is removed or not available. | Int64
> disc-reason-88 | The total number of sessions disconnected due to prohibition of defined static IP address. | Int64
> disc-reason-89 | The total number of sessions disconnected due to a failure in IP address validation on RADIUS. | Int64
> disc-reason-90 | The total number of sessions disconnected due to IP address is not provided by RADIUS. | Int64
> disc-reason-91 | The total number of sessions disconnected due to invalid IP address received from SGSN. | Int64
> disc-reason-92 | The total number of sessions disconnected due to sessions cleared in AAA. | Int64
> disc-reason-93 | The total number of sessions disconnected due to authentication request failure between GGSN and AAA server. | Int64
> disc-reason-94 | The total number of sessions disconnected due to conflict in IP address assignment. | Int64
> disc-reason-95 | The total number of sessions disconnected due to APN removed during session. | Int64
> disc-reason-96 | The total number of sessions disconnected due to exceeding the incoming data/bytes credit. | Int64
> disc-reason-97 | The total number of sessions disconnected due to exceeding the outgoing data/bytes credit. | Int64
> disc-reason-98 | The total number of sessions disconnected due to exceeding the total data/bytes credit. | Int64
> disc-reason-99 | The total number of sessions disconnected due to a failure in processing prepaid account information. | Int64
> disc-reason-100 | The total number of sessions disconnected due to the IPSec tunnel being failed to connect. | Int64
> disc-reason-101 | The total number of sessions disconnected due to the IPSec tunnel being disconnected. | Int64
> disc-reason-102 | The total number of sessions disconnected due to in active security association (sa) of IPSec for specific Mobile IP address. | Int64
> disc-reason-103 | The total number of sessions disconnected due to the expiration of the configured long-duration timer. | Int64
> disc-reason-104 | The total number of Proxy Mobile IP sessions disconnected due to Registration failures. | Int64
> disc-reason-105 | The total number of Proxy Mobile IP sessions disconnected due to errors occurring during binding updates. | Int64
> disc-reason-106 | The total number of Proxy Mobile IP sessions disconnected due to the mobile not providing the IP address it was assigned during IPCP negotiations resulting from inter-PDSN handoffs. | Int64
> disc-reason-107 | The total number of Proxy Mobile IP sessions disconnected due to the mobile providing an IP address other than what it was assigned during IPCP negotiations resulting from inter-PDSN handoffs. | Int64
> disc-reason-108 | The total number of sessions disconnected due to a locally-initiated purge. | Int64
> disc-reason-109 | The total number of sessions disconnected due to failure in update handoff. | Int64
> disc-reason-110 | The total number of sessions disconnected due to handoff completed. | Int64
> disc-reason-111 | The total number of sessions disconnected due to duplicate session. | Int64
> disc-reason-112 | The total number of sessions disconnected due to hand off session not found. | Int64
> disc-reason-113 | The total number of sessions disconnected due to handoff failed for session. | Int64
> disc-reason-114 | The total number of sessions disconnected due to the expiration of the configured max-inactivity timer indicating that the PCF was unavailable. | Int64
> disc-reason-115 | The total number of sessions disconnected due to call rejected internally. | Int64
> disc-reason-116 | The total number of sessions disconnected due to call restarted on unknown reason. | Int64
> disc-reason-117 | The total number of sessions disconnected due to failure in authentication between Mobile node and Home Agent (HA). | Int64
> disc-reason-118 | The total number of sessions disconnected as A11 interface is formed badly. | Int64
> disc-reason-119 | The total number of sessions disconnected due to t-bit is not set in interface. | Int64
> disc-reason-120 | The total number of sessions disconnected due to unsupported vendor Id in interface. | Int64
> disc-reason-121 | The total number of sessions disconnected due to mismatched Id in A11 interface. | Int64
> disc-reason-122 | The total number of sessions disconnected due to duplicate home address request on HA. | Int64
> disc-reason-123 | The total number of sessions disconnected due to duplicate IMSI in session on HA. | Int64
> disc-reason-124 | The total number of sessions disconnected due to unreachable HA. | Int64
> disc-reason-125 | The total number of sessions disconnected due to IP Pool Sharing Protocol address is in use/not free on HA. | Int64
> disc-reason-126 | The total number of sessions disconnected due to duplicate home address request on FA. | Int64
> disc-reason-127 | The total number of sessions disconnected due to IP pool busyout. | Int64
> disc-reason-128 | The total number of sessions disconnected due to inter-PDSN handoff failure. | Int64
> disc-reason-129 | The total number of sessions disconnected due to system enters to dormant state from active state. Note: Sessions facilitated through PDSN Closed R-P services are always displayed as "Active" due to the fact that PDSN Closed R-P services do not receive dormancy information from the PCF. | Int64
> disc-reason-130 | The total number of sessions disconnected due to failure/conflict in PPP renegotiation. | Int64
> disc-reason-131 | The total number of sessions disconnected due to change in start parameters. | Int64
> disc-reason-132 | The total number of sessions disconnected due to the closure of an accounting record based configured tariff time. | Int64
> disc-reason-133 | The total number of sessions disconnected due to A11 interface is not active or stopped. | Int64
> disc-reason-134 | The total number of sessions disconnected due to failure in network reachability and request rejected. | Int64
> disc-reason-135 | The total number of sessions disconnected due to failure in network reachability and request redirected. | Int64
> disc-reason-136 | The total number of sessions disconnected due to the closure of an accounting record based on the configured maximum number of container changes being exceeded. | Int64
> disc-reason-137 | The total number of sessions disconnected due to static IP address is not allowed in APN. | Int64
> disc-reason-138 | The total number of sessions disconnected due to static IP address required by RADIUS. | Int64
> disc-reason-139 | The total number of sessions disconnected due to static IP address is not allowed by RADIUS. | Int64
> disc-reason-140 | The total number of sessions disconnected due to registration dropped for Mobile IP address. | Int64
> disc-reason-141 | The total number of sessions disconnected due to counter rollover. | Int64
> disc-reason-142 | The total number of sessions disconnected due to authentication failure in subscriber’s Network Access Identifier (NAI). | Int64
> disc-reason-143 | The total number of sessions disconnected due to disabled inter-PDSN service optimization handoff. | Int64
> disc-reason-144 | The total number of sessions disconnected due to collision in Generic Routing Encapsulation (GRE) key. | Int64
> disc-reason-145 | The total number of sessions disconnected when inter PDSN service optimization handoff triggered. | Int64
> disc-reason-146 | The total number of sessions disconnected when intra-PDSN service optimization handoff triggered. | Int64
> disc-reason-147 | The total number of sessions disconnected due to abort timer duration expired. | Int64
> disc-reason-148 | The total number of sessions disconnected as AAA server disconnected Administratively. | Int64
> disc-reason-149 | The total number of sessions disconnected due to AAA handoff disconnected Administratively. | Int64
> disc-reason-150 | The total number of sessions disconnected due to IPv6CP negotiation failed. | Int64
> disc-reason-151 | The total number of sessions disconnected due to no response during IPv6CP negotiation. | Int64
> disc-reason-152 | The total number of sessions disconnected due to maximum retries failed on IPv6CP negotiation. | Int64
> disc-reason-153 | The total number of sessions disconnected due to PPP restarted by invalid Pv4 address of source. | Int64
> disc-reason-154 | The total number of sessions disconnected due to handoff in A11 interface is not active or stopped. | Int64
> disc-reason-155 | The total number of sessions disconnected due to call restarted during inter PDSN handoff. | Int64
> disc-reason-156 | The total number of sessions disconnected due to call restarted on PPP termination. | Int64
> disc-reason-157 | The total number of sessions disconnected due to resource conflict on FA. | Int64
> disc-reason-158 | The total number of sessions disconnected due to authentication failure in charging services. | Int64
> disc-reason-159 | The total number of sessions disconnected due to clearing of duplicate IMSI in session on HA. | Int64
> disc-reason-160 | The total number of sessions disconnected due to revival of pending new calls. | Int64
> disc-reason-161 | The total number of sessions disconnected due to allocated data quota volume reached. | Int64
> disc-reason-162 | The total number of sessions disconnected due to time-out reached. | Int64
> disc-reason-163 | The total number of sessions disconnected due to a failure in user/subscriber authentication. | Int64
> disc-reason-164 | The total number of sessions disconnected due to termination of an MIP Session for a Revocation being received from the HA and the PDSN is not configured to send a LCP Terminate Request. | Int64
> disc-reason-165 | The total number of sessions disconnected due to no reverse tunnel for MIP. | Int64
> disc-reason-166 | The total number of sessions disconnected due to invalid Prepaid attribute in authentication response. | Int64
> disc-reason-167 | The total number of MIP HA sessions disconnected due to receiving MIP registration with a home address of 0.0.0.0. | Int64
> disc-reason-168 | The total number of RP sessions disconnected due to the PCF not removing flow control for a specified amount of time if GRE flow control for RP sessions is enabled. | Int64
> disc-reason-169 | The total number of sessions that were disconnected because the binding cache was not found. | Int64
> disc-reason-170 | The total number of MIP HA sessions that were disconnected because a dynamic IP address was not available. | Int64
> disc-reason-171 | The total number of sessions disconnected due to a mismatched ID in the A11 interface during a handoff. | Int64
> disc-reason-172 | The total number of sessions disconnected because the A11 interface is formed badly during a handoff. | Int64
> disc-reason-173 | The total number of sessions disconnected due to unsupported vendor Id in the A11 interface during a handoff. | Int64
> disc-reason-174 | The total number of sessions disconnected due to t-bit is not set in the A11 interface during a handoff. | Int64
> disc-reason-175 | The total number of Mobile IP sessions disconnected at the PDSN/FA due to Revocation received from HA (with I bit set). | Int64
> disc-reason-176 | The total number of sessions disconnected due to failures in processing A11-Registration-Request despite retries of the message by the PCF. | Int64
> disc-reason-177 | The total number of sessions disconnected because they entered the dormant state during session setup. Note: Sessions facilitated through PDSN Closed R-P services are always displayed as "Active" due to the fact that PDSN Closed R-P services do not receive dormancy information from the PCF. | Int64
> disc-reason-178 | The total number of PPP sessions disconnected because they were renegotiated by the remote side by sending LCP Conf-req/nak/ack and the “always” option was used for the remote-renegotiation disconnect command/attribute. | Int64
> disc-reason-179 | The total number of PPP sessions disconnected because they were renegotiated by the remote side by sending LCP Conf-req/nak/ack and the “nai-prefix-msid-mismatch” option was used for the remote-renegotiation disconnect command/attribute. | Int64
> disc-reason-180 | The total number of subscribers disconnected because the IPSec tunnel facilitating their sessions went down. | Int64
> disc-reason-181 | The total number of subscribers disconnected because an IPSec tunnel failed to be established. | Int64
> disc-reason-182 | The total number of subscribers disconnected because the IPSec Manager software task facilitating their sessions crashed. | Int64
> disc-reason-183 | The total number of sessions disconnected because their respective flow was deactivated. | Int64
> disc-reason-184 | The total number of sessions disconnected because the licensed session capacity for the Enhanced Charging Service feature has been exceeded. | Int64
> disc-reason-185 | The total number of sessions disconnected because IPSG authentication failed. | Int64
> disc-reason-186 | The total number of sessions disconnected due to driver initiation. | Int64
> disc-reason-187 | The total number of sessions disconnected because of IMS authorization failures. | Int64
> disc-reason-188 | The total number of sessions disconnected because they were released by the service instances facilitating them. | Int64
> disc-reason-189 | The total number of sessions disconnected because their respective flows were released. | Int64
> disc-reason-190 | The total number of sessions disconnect because no HA address was supplied during PPP renegotiation. | Int64
> disc-reason-191 | The total number of sessions disconnected during an intra-PDSN service handoff. | Int64
> disc-reason-192 | The total number of sessions disconnected because the configured overload-disconnect threshold has been exceeded. | Int64
> disc-reason-193 | The total number of sessions because the CSS service specified for handling the session was not found. | Int64
> disc-reason-194 | This is not supported at this time. | Int64
> disc-reason-195 | The total number of sessions disconnected because the DHCP client sent a release. | Int64
> disc-reason-196 | The total number of sessions disconnected because the DHCP client sent a negative acknowledge message. | Int64
> disc-reason-197 | The total number of sessions disconnected because the DHCP Client Hardware (MAC) Address (CHADDR) does not match with MSID of the ASN-GW session. | Int64
> disc-reason-198 | The total number of sessions disconnected because the link between the SGSN and the GGSN is broken resulting in the termination of ongoing Diameter Credit-Control sessions with the DIAMETER_LINK_BROKEN termination-cause. | Int64
> disc-reason-199 | The total number of sessions disconnected because the allowed BCMCS program limit time expires. | Int64
> disc-reason-200 | The total number of sessions disconnected because the PDSN failed to update QoS for them. | Int64
> disc-reason-201 | The total number of sessions disconnected because the session-audit between the ACS Manager task and Session Manager disconnects any dangling sessions in the Session Manager. | Int64
> disc-reason-202 | The total number of sessions disconnected due to GTP context replacement. | Int64
> disc-reason-203 | The total number of sessions disconnected due to PDIF authentication process unable to set up a secure IPSec tunnel to subscriber. | Int64
> disc-reason-204 | The total number of sessions disconnected due to unknown APN in L2TP message. | Int64
> disc-reason-205 | The total number of sessions disconnected due unexpected network reentry by MS in Wimax network. | Int64
> disc-reason-206 | The total number of sessions disconnected due invalid NAI in R6 message in WiMAX network. | Int64
> disc-reason-207 | The total number of sessions disconnected due maximum retry limit for EAP authentication exhausted in Wimax network. | Int64
> disc-reason-208 | vbm-hoa-session-disconnected | Int64
> disc-reason-209 | vbm-voa-session-disconnected | Int64
> disc-reason-210 | in-acl-disconnect-on-violation | Int64
> disc-reason-211 | The total number of sessions disconnected due to EAP Master Session Key lifetime expiry in Wimax network. | Int64
> disc-reason-212 | The total number of sessions disconnected due to EAP Master Session Key lifetime is too less to allow session. | Int64
> disc-reason-213 | The total number of sessions disconnected due to inter-service handoff in Wimax network. | Int64
> disc-reason-214 | The total number of sessions disconnected due to maximum retry limit for R6 message exhausted in Wimax network. | Int64
> disc-reason-215 | The total number of sessions disconnected due to network exit message received on R6 interface in Wimax network. | Int64
> disc-reason-216 | The total number of sessions disconnected due to de-registration message received on R6 interface in Wimax network. | Int64
> disc-reason-217 | The total number of sessions disconnected due to remote peer failure on R6 interface in Wimax network. | Int64
> disc-reason-218 | The total number of sessions disconnected due to protocol error on R6 and/or R4 interface in Wimax network. | Int64
> disc-reason-219 | The total number of sessions disconnected due to invalid AAA attributes for QoS to a subscriber in Wimax network. | Int64
> disc-reason-220 | The total number of sessions disconnected due to requested NPU GRE flow is not available for a subscriber in Wimax network. | Int64
> disc-reason-221 | The total number of sessions disconnected due to maximum retry limit for R4 message exhausted in Wimax network. | Int64
> disc-reason-222 | The total number of sessions disconnected due to network exit message received on R4 interface in Wimax network. | Int64
> disc-reason-223 | The total number of sessions disconnected due to de-registration message received on R4 interface in Wimax network. | Int64
> disc-reason-224 | The total number of sessions disconnected due to remote peer failure on R4 interface in Wimax network. | Int64
> disc-reason-225 | The total number of sessions disconnected due to IMS authorization revoked. | Int64
> disc-reason-226 | The total number of sessions disconnected due to IMS authorization released. | Int64
> disc-reason-227 | The total number of sessions disconnected due to invalid IMS authorization decision. | Int64
> disc-reason-228 | The total number of sessions disconnected due to MAC address validation failure in WiMAX network. | Int64
> disc-reason-229 | The total number of sessions disconnected due to excessive packet data flows configured in WiMAX network. | Int64
> disc-reason-230 | The total number of sessions disconnected due to request for location substitution withdrawn was cancelled. | Int64
> disc-reason-231 | The total number of sessions disconnected because the location update was cancelled. | Int64
> disc-reason-232 | The total number of sessions disconnected due to manager expiry. | Int64
> disc-reason-233 | The total number of sessions disconnected due to identity check failure. | Int64
> disc-reason-234 | The total number of sessions disconnected due to security verification failure. | Int64
> disc-reason-235 | The total number of sessions disconnected due to authentication failure. | Int64
> disc-reason-236 | The total number of sessions disconnected due to GLU failure. | Int64
> disc-reason-237 | The total number of sessions disconnected due to an implicit detach. | Int64
> disc-reason-238 | The total number of sessions disconnected due to subscriber moving to a different SMGR instance. | Int64
> disc-reason-239 | The total number of sessions disconnected due to subscriber moving to a peer SGSN. | Int64
> disc-reason-240 | The total number of sessions disconnected due to DNS failure during Inter-RAU. | Int64
> disc-reason-241 | The total number of sessions disconnected due to context response failure. | Int64
> disc-reason-242 | The total number of sessions disconnected due to HLR not found for particular IMSI. | Int64
> disc-reason-243 | The total number of sessions disconnected due to MS initiated detach. | Int64
> disc-reason-244 | The total number of sessions disconnected because MS was not allowed to roam. | Int64
> disc-reason-245 | The total number of sessions disconnected due to duplicate context. | Int64
> disc-reason-246 | The total number of sessions disconnected due to failure of profile update. | Int64
> disc-reason-247 | The total number of sessions disconnected where session is inactive and no PDP context is activated from this session. | Int64
> disc-reason-248 | The total number of sessions disconnected due to configured idle mode timeout duration is exhausted for ASN paging controller in WiMAX network. | Int64
> disc-reason-249 | The total number of sessions disconnected due to idle mode exit message for ASN paging controller in WiMAX network. | Int64
> disc-reason-250 | The total number of sessions disconnected due to authentication failure during idle mode entry for ASN paging controller in WiMAX network. | Int64
> disc-reason-251 | The total number of sessions disconnected due to invalid QoS configuration for subscriber in WiMAX network. | Int64
> disc-reason-252 | The total number of sessions disconnected due to receipt of Delete Subscriber Data (DSD) message including the IE “all GPRS subscriptions withdrawn”. | Int64
> disc-reason-253 | The total number of sessions disconnected due to primary master key change failure on R6 interface in WiMAX network. | Int64
> disc-reason-254 | The total number of sessions disconnected because the ME was illegal. | Int64
> disc-reason-255 | The total number of sessions disconnected due to failure monitored through BS monitor keep-alive probe. | Int64
> disc-reason-256 | The total number of sessions disconnected due to error in SGSN attachment in registration state. | Int64
> disc-reason-257 | The total number of sessions disconnected due to error in SGSN inbound SRNS in registration state. | Int64
> disc-reason-258 | The total number of sessions disconnected due to error in Update PDP Context Response message for direct tunnel functionality. Direct tunnel functionality at GGSN was expecting some fields which were not received in the Update PDP Context Response message. Hence, GGSN was not able to establish tunnel appropriately with SGSN or RNC. | Int64
> disc-reason-259 | The total number of sessions disconnected at SGSN due to unknown PDP context. | Int64
> disc-reason-260 | The total number of sessions disconnected at SGSN due to PDP authentication failed. | Int64
> disc-reason-261 | The total number of sessions disconnected at SGSN due to duplicate PDP context | Int64
> disc-reason-262 | The total number of sessions disconnected at SGSN due to no response from GGSN. | Int64
> disc-reason-263 | The total number of sessions disconnected at SGSN due to failed response from GGSN. | Int64
> disc-reason-264 | The total number of sessions disconnected at SGSN due to unknown APN. | Int64
> disc-reason-265 | The total number of sessions disconnected at SGSN due to service request initiated deactivation. | Int64
> disc-reason-266 | The total number of sessions disconnected at SGSN due to attachment procedure initiated abort. | Int64
> disc-reason-267 | The total number of sessions disconnected at SGSN due to ISRAU initiated abort procedure. | Int64
> disc-reason-268 | The total number of sessions disconnected at SGSN due to unknown APN. | Int64
> disc-reason-269 | The total number of sessions disconnected at SGSN due to MM context cleanup initiated abort procedure. | Int64
> disc-reason-270 | The total number of sessions disconnected at SGSN due to unknown abort procedure. | Int64
> disc-reason-271 | The total number of sessions disconnected at SGSN due to abort procedure started by guard timeout. | Int64
> disc-reason-272 | The total number of sessions disconnected at SGSN due to abort procedure initiated on DHCP IP validate request. | Int64
> disc-reason-273 | The total number of sessions disconnected due to id mismatch in MIPv6 session. | Int64
> disc-reason-274 | The total number of sessions disconnected as AAA session id not-found | Int64
> disc-reason-275 | The total number of sessions disconnected due to security associate rekeying failure. | Int64
> disc-reason-276 | The total number of sessions disconnected due to failure in relocation in ASN-PC service. | Int64
> disc-reason-277 | The total number of sessions disconnected due to failure in paging controller relocation in ASN PC service. | Int64
> disc-reason-278 | The total number of sessions disconnected due to mismatch in authentication policy. | Int64
> disc-reason-279 | The total number of sessions disconnected as DELETE MS ENTRY message received by the ASN Paging Controller. | Int64
> disc-reason-280 | The total number of sessions disconnected due to non-anchor ASN GW being prohibited. | Int64
> disc-reason-281 | The total number of sessions disconnected due to unknown reason. | Int64
> disc-reason-282 | The total number of sessions disconnected Administratively. | Int64
> disc-reason-283 | The total number of sessions disconnected by remote system | Int64
> disc-reason-284 | The total number of sessions disconnected by local system. | Int64
> disc-reason-285 | The total number of sessions disconnected due to non-availability of resources. | Int64
> disc-reason-286 | The total number of sessions disconnected due to exceed in service limit. | Int64
> disc-reason-287 | The total number of sessions disconnected due to LCP negotiation failed. | Int64
> disc-reason-288 | The total number of sessions disconnected due to no response in PPP-LCP session. | Int64
> disc-reason-289 | The total number of sessions disconnected due to loop back detected in PPP-LCP. | Int64
> disc-reason-290 | The total number of sessions disconnected due to maximum retries in PPP-LCP session. | Int64
> disc-reason-291 | The total number of SGSN sessions disconnected due to an error in the SGSN attachment during the registration state. | Int64
> disc-reason-292 | The total number of SGSN sessions disconnected due to an error in the SGSN inbound SRNS in a registration state. | Int64
> disc-reason-293 | The total number of SGSN sessions disconnected due to error in Update PDP Context Response message for direct tunnel functionality. Direct tunnel functionality at GGSN was expecting some fields which were not received in the Update PDP Context Response message. Hence, the GGSN was not able to establish a tunnel appropriately with the SGSN or the RNC. | Int64
> disc-reason-294 | The total number of SGSN sessions disconnected due to an unknown PDP context. | Int64
> disc-reason-295 | The total number of SGSN sessions disconnected because the PDP authentication failed. | Int64
> disc-reason-296 | The total number of SGSN sessions disconnected because the PDP authentication failed. | Int64
> disc-reason-297 | The total number of SGSN sessions disconnected because the SGSN does note receive a response from the GGSN. | Int64
> disc-reason-298 | The total number of SGSN sessions disconnected due to failed response from the GGSN. | Int64
> disc-reason-299 | The total number of SGSN sessions disconnected due to an unknown APN. | Int64
> disc-reason-300 | The total number of SGSN sessions disconnected due to deactivation initiated by a service request. | Int64
> disc-reason-301 | The total number of SGSN sessions disconnected due to an attachment procedure-initiated abort. | Int64
> disc-reason-302 | The total number of SGSN sessions disconnected due to an ISRAU-initiated abort procedure. | Int64
> disc-reason-303 | The total number of SGSN sessions disconnected because the SessMgr initiates an abort. | Int64
> disc-reason-304 | The total number of SGSN sessions disconnected due to the MM context cleanup-initiated abort procedure. | Int64
> disc-reason-305 | The total number of SGSN sessions disconnected due to an unknown abort procedure. | Int64
> disc-reason-306 | The total number of SGSN sessions disconnected because the abort procedure was started by the guard timer timeout. | Int64
> disc-reason-307 | The total number of SGSN sessions disconnected because the abort procedure was initiated upon receiving a DHCP IP validate request. | Int64
> disc-reason-308 | The total number of sessions disconnected due to id mismatch in MIPv6 session. | Int64
> disc-reason-309 | The total number of sessions disconnected as AAA session id not-found | Int64
> disc-reason-310 | The total number of sessions disconnected due to security associate rekeying failure. | Int64
> disc-reason-311 | The total number of sessions disconnected due to failure in relocation in ASN-PC service. | Int64
> disc-reason-312 | The total number of sessions disconnected due to failure in paging controller relocation in ASN PC service. | Int64
> disc-reason-313 | The total number of sessions disconnected due to mismatch in authentication policy. | Int64
> disc-reason-314 | The total number of sessions disconnected as DELETE MS ENTRY message received by the ASN Paging Controller. | Int64
> disc-reason-315 | The total number of sessions disconnected because the ASNGW TID entry was not found. | Int64
> disc-reason-316 | The total number of sessions disconnected due to network exit message received on X2 interface in PHS network. | Int64
> disc-reason-317 | The total number of sessions disconnected due to deregistration request received on X2 interface in PHS network. | Int64
> disc-reason-318 | The total number of sessions disconnected by remote system due to failure on X2 interface in PHS network. | Int64
> disc-reason-319 | The total number of sessions disconnected due to primary master key change failure on X1 interface in PHS network. | Int64
> disc-reason-320 | The total number of sessions disconnected because of an IKE SA rekeying failure. | Int64
> disc-reason-321 | The total number of sessions disconnected due to session sleep mode entry timeout on PHS GW. | Int64
> disc-reason-322 | The total number of sessions disconnected due to non-anchor PHS GW being prohibited. | Int64
> disc-reason-323 | The total number of sessions disconnected due to failure in paging controller relocation in ASN PC service. | Int64
> disc-reason-324 | The total number of sessions disconnected due to paging controller relocation in ASN PC service. | Int64
> disc-reason-325 | The total number of sessions disconnected due to authorization policy mismatch. | Int64
> disc-reason-326 | The total number of sessions disconnected due to IKE/IPsec security associate lifetime timer expiration. | Int64
> disc-reason-327 | The total number of sessions disconnected as DELETE MS ENTRY message received by the ASN Paging Controller. | Int64
> disc-reason-328 | The total number of sessions disconnected due to sleep mode timeout by the PHS Paging Controller. | Int64
> disc-reason-329 | The total number of sessions disconnected due to sleep mode exit by the PHS Paging Controller. | Int64
> disc-reason-330 | The total number of sessions disconnected due to failed sleep mode entry authorization by the PHS Paging Controller. | Int64
> disc-reason-331 | The total number of sessions disconnected due to ms power down network exit message received by the PHS Paging Controller. | Int64
> disc-reason-332 | The total number of PHS Paging Controller sessions disconnected due to network exit message received from X2 interface in PHS network. | Int64
> disc-reason-333 | The total number of sessions disconnected due to the following reasons: 1. When SessMgr and ACSMgr are running in non-optimized mode. 2. When an undefined NAT pool is configured for subscriber. NAT must be disabled if ACS is not running in optimized mode. | Int64
> disc-reason-334 | The total number of sessions disconnected because the ASNGW TID entry was not found. | Int64
> disc-reason-335 | The total number of sessions disconnected due to NAT IP address being unavailable during call setup for allocation to a subscriber. | Int64
> disc-reason-336 | The total number of sessions disconnected due to configuration of excessive PHS pd flows. | Int64
> disc-reason-337 | The total number of sessions disconnected due to invalid QoS configuration for subscriber in PHS network. | Int64
> disc-reason-338 | The total number of sessions disconnected due to Interim Update. | Int64
> disc-reason-339 | The total number of SGSN sessions disconnected because the inbound attach requests aborted due to poor radio status or lost radio connections. | Int64
> disc-reason-340 | The total number of SGSN sessions disconnected due to inbound IRAU requests aborting as the radio status was poor or the radio connection lost. | Int64
> disc-reason-341 | The total number of sessions disconnected due to IKE keepalive failure. | Int64
> disc-reason-342 | The total number of SGSN sessions disconnected due to attach requests aborting because MS was in suspend mode. | Int64
> disc-reason-343 | The total number of SGSN sessions disconnected due to IRAU requests aborted when MS was in suspend mode. | Int64
> disc-reason-344 | The total number of sessions disconnected due to detection of duplicate sessions for the same session id. | Int64
> disc-reason-345 | The total number of SGSN sessions disconnected due to XID response failure. | Int64
> disc-reason-346 | The total number of SGSN sessions disconnected due to record cleanup or reset on the network service entity (NSE). | Int64
> disc-reason-347 | The total number of SGSN sessions disconnected due to failure of the GTPP request. | Int64
> disc-reason-348 | The total number of SGSN sessions disconnected due to mismatches of the IMSIs. | Int64
> disc-reason-349 | The total number of SGSN sessions disconnected because the BSSGP Virtual Connection (BVC) was blocked. | Int64
> disc-reason-350 | The total number of SGSN sessions disconnected as the session was attached on inbound IRAU requests. | Int64
> disc-reason-351 | The total number of SGSN sessions disconnected while the session was attached on outbound IRAU requests. | Int64
> disc-reason-352 | The total number of SGSN sessions disconnected due to incorrect state of network elements. | Int64
> disc-reason-353 | The total number of SGSN sessions disconnected due to expiry of the T-3350 timer. | Int64
> disc-reason-354 | The total number of SGSN sessions disconnected due to expiry of the paging timer. | Int64
> disc-reason-355 | The total number of SGSN sessions disconnected due to local purging of PDP contexts. | Int64
> disc-reason-356 | The total number of sessions disconnected as DELETE MS ENTRY message received by the PHS Paging Controller. | Int64
> disc-reason-357 | The total number of SGSN sessions disconnected due to local purging of PDP contexts. The field indicator number will vary depending upon the build of the software | Int64
> disc-reason-358 | The total number of sessions disconnected due to invalid NAI in PHS network. | Int64
> disc-reason-359 | The total number of sessions disconnected due to sleep mode exit timeout for PHS paging controller in PHS network. | Int64
> disc-reason-360 | With Iu/Gb flex enabled, this is the total number of SGSN sessions disconnected when the subscriber has been forcefully cleared via phase2 offloading from one SGSN to another SGSN within the SGSN pool. | Int64
> disc-reason-361 | The total number of sessions disconnected due to third party authorization failure in PHS network. | Int64
> disc-reason-362 | The total number of sessions disconnected due to remote error notifications. | Int64
> disc-reason-363 | The total number of sessions disconnected due to no response from any of the network entity. | Int64
> disc-reason-364 | The total number of sessions disconnected due re-authorization failure at any stage. | Int64
> disc-reason-365 | The total number of sessions disconnected because of a MME and s1AP send failure. | Int64
> disc-reason-366 | The total number of sessions disconnected because of a MME-eGTPC connection failure. | Int64
> disc-reason-367 | The total number of sessions disconnected because of the MME-eGTPC create session failed. | Int64
> disc-reason-368 | The total number of sessions disconnected because of a MME authentication failure. | Int64
> disc-reason-369 | The total number of sessions disconnected because of MME and UE detach. | Int64
> disc-reason-370 | The total number of sessions disconnected because of MME to MME detach. | Int64
> disc-reason-371 | The total number of sessions disconnected because of a MME HSS detach. | Int64
> disc-reason-372 | The total number of sessions disconnected because of a MME and P-GW detach. | Int64
> disc-reason-373 | The total number of sessions disconnected because of a MME sub validation failure. | Int64
> disc-reason-374 | The total number of sessions disconnected because of a MME HSS connection failure. | Int64
> disc-reason-375 | The total number of sessions disconnected because the MME HSS user is unknown. | Int64
> disc-reason-376 | The total number of sessions disconnected due to mismatch in DHCP lease time mismatch. | Int64
> disc-reason-377 | The total number of disconnected sessions due to the NEMO link layer being down. | Int64
> disc-reason-378 | The total number of sessions disconnected because of eapol-max-retry-reached. | Int64
> disc-reason-379 | With Iu/Gb flex enabled, this is the total number of SGSN sessions disconnected when the subscriber has been forcefully cleared via phase3 offloading from one SGSN to another SGSN within the SGSN pool. | Int64
> disc-reason-380 | The total number of sessions disconnected due to disconnect in MBMS bearer service. | Int64
> disc-reason-381 | The total number of sessions disconnected due to violation on Operator Determined Barring (ODB) of services. | Int64
> disc-reason-382 | The total number of sessions disconnected due to violation on Operator Determined Barring (ODB) of Free-of-Charge service (FOCS). | Int64
> disc-reason-383 | The total number of CSCF sessions disconnected through CLI registration clearing by administrator. | Int64
> disc-reason-384 | The total number of CSCF sessions disconnected by UE with an explicit deregister message. | Int64
> disc-reason-385 | The total number of CSCF sessions disconnected due to registration expiry. | Int64
> disc-reason-386 | The total number of CSCF sessions disconnected due to network-initiated deregistration. | Int64
> disc-reason-387 | The total number of CSCF sessions disconnected through CLI call clearing by administrator. | Int64
> disc-reason-388 | The total number of CSCF sessions disconnected by UE using BYE message. | Int64
> disc-reason-389 | The total number of CSCF sessions disconnected locally due to some processing failure, task death, recovery failure, etc. | Int64
> disc-reason-390 | The total number of CSCF sessions disconnected because locally due to congestion caused by max calline/flow usage from high cpu/memory utilization in sessmgr. | Int64
> disc-reason-391 | The total number of CSCF sessions disconnected due to response timeout (SIP response code 408). | Int64
> disc-reason-392 | The total number of CSCF sessions disconnected due to session timer timeout | Int64
> disc-reason-393 | The total number of CSCF sessions disconnected due to media authorization failure. | Int64
> disc-reason-394 | The total number of CSCF sessions disconnected because register message is rejected due to congestion caused by max calline/flow usage from high cpu/memory utilization in sessmgr. | Int64
> disc-reason-395 | The total number of disconnects due to ms-unexpected-idle-mode-entry. | Int64
> disc-reason-396 | The total number of disconnects due to Re-Auth-failed. | Int64
> disc-reason-397 | The total number of SGSN sessions disconnected because the NSE configured in the GPRS service is removed and there are PDP contexts associated with the subscribers attached in this NSE. | Int64
> disc-reason-398 | The total number of SGSN sessions disconnected because an SGTP service could not be assigned to an MM context. The field indicator number will vary depending upon the build of the software | Int64
> disc-reason-399 | The total number of disconnects due to an unknown-apn. | Int64
> disc-reason-400 | The total number of disconnects due to a gtpc-path-failure. | Int64
> disc-reason-401 | The total number of disconnects due to a gtpi-path-failure. | Int64
> disc-reason-402 | The total number of disconnects due to a actv-rejected-by-ggsn. | Int64
> disc-reason-403 | The total number of PDP activation failures due to release from CAMEL. | Int64
> disc-reason-404 | The total number of of Attaches / RAUs rejected due to failure in the IMEI checking (i.e. due either to black listing or to grey listing and an SGSN operator policy is configured with deny-grey-list). This counter is available in releases 9.0 and higher. | Int64
> disc-reason-405 | The total number of PDP contexts deactivated upon receiving a cleanup indication from the SNDCP layer. The field indicator number may vary depending upon the build of the software. | Int64
> disc-reason-406 | The total number of subscribers detached or PDP context(s) deactivated due to subscriber inactivity during a configured (in the SGSN operator policy) time. The field indicator number may vary depending upon the build of the software. | Int64
> disc-reason-407 | The total number of NAT-enabled sessions dropped due to Firewall-and-NAT policy updates in mid session. | Int64
> disc-reason-408 | The total number of FNG sessions disconnected due to authorization failures based on mismatched Femtocell Access Point (FAP) credentials. | Int64
> disc-reason-409 | The total number of disconnects due to an ha-stale-key. | Int64
> disc-reason-410 | The total number of disconnects due to No-IPv6-address-for-subscriber. | Int64
> disc-reason-411 | The total number of disconnects due to prefix-registration-failure. | Int64
> disc-reason-412 | disconnect-from-policy-server | Int64
> disc-reason-413 | The total number of subscriber sessions disconnected due to failure of authentication over S6b interface with HSS. This support is added for interoperability of GGSN with P-GW and HA. | Int64
> disc-reason-414 | The total number of sessions disconnected due to a GTP control plane error indication message. | Int64
> disc-reason-415 | The total number of sessions disconnected due to a GTP user plane error indication message. | Int64
> disc-reason-416 | The total number of sessions disconnected due to an invalid PDN-type error. | Int64
> disc-reason-417 | The total number of subscriber sessions disconnected due to a AAA authentication request failure. | Int64
> disc-reason-418 | The total number of subscriber sessions disconnected due to denial of APN as requested APN was not subscribed to subscriber. | Int64
> disc-reason-419 | The total number of sessions disconnected due to an S-GW context replacement. | Int64
> disc-reason-420 | The total number of subscriber sessions disconnected due to new session request received with duplicate IP address at GGSN. This support is added for interoperability of GGSN with P-GW and HA. | Int64
> disc-reason-421 | The total number of subscriber sessions disconnected due to violation of level of restriction to ensure controlled co-existence of the Primary PDP Contexts in APN. | Int64
> disc-reason-422 | invalid-wapn | Int64
> disc-reason-423 | ttg-nsapi-allocation-failed | Int64
> disc-reason-424 | mandatory-gtp-ie-missing | Int64
> disc-reason-425 | The total number of disconnected sessions due to RADIUS server not reachable. For mobile-IP calls, aaa-unreachable cause code is set when re-authentication failure happens. RADIUS generates this only for a mobile IP call and RADIUS server is down during authentication. | Int64
> disc-reason-426 | asngw-service-flow-deletion | Int64
> disc-reason-427 | CT-PMIP-RRQ-NVSE-Value-Change | Int64
> disc-reason-428 | The total number of disconnected sessions due to a TCP read failure. | Int64
> disc-reason-429 | The total number of disconnected sessions due to a TCP write failure. | Int64
> disc-reason-430 | The total number of disconnected SSL ssessions due to a handshake failure. | Int64
> disc-reason-431 | The total number of disconnected SSL ssessions due to a renegotiation failure. | Int64
> disc-reason-432 | The total number of disconnected SSL ssessions due to corrupted messages. | Int64
> disc-reason-433 | The total number of disconnected SSL ssessions due to an alert. | Int64
> disc-reason-434 | The total number of SSL disconnections. | Int64
> disc-reason-435 | The total number of SSL migrations. | Int64
> disc-reason-436 | The total number of session disconnects due to ARD (access restriction data) subscription restriction received from the HLR. | Int64
> disc-reason-437 | The total number of session disconnects experienced by the SGSN due to Detach/Attach Rejects due to explicit “Release GPRS” received from CAMEL component GSM-SCF or due to failures during CAMEL handling. | Int64
> disc-reason-438 | The total number of session disconnects occurring when the S4-SGSN was not able to establish a PDP context, due to GTPv2 (EGTP) module failure, when trying to connect to a given SGW. | Int64
> disc-reason-439 | The total number of session disconnects occurring when the S4-SGSN is not able to establish a PDP context when the SGW returned a failure cause in "Create Session Response". The SGW did not respond at all to "Create Session Request". | Int64
> disc-reason-440 | The total number of session disconnects resulting from subscriptions being removed from the HSS; subscription removal initiates a detach. | Int64
> disc-reason-441 | The total number of session disconnects resulting from failed connections to the HSS; connection failure initiates a detach. | Int64
> disc-reason-442 | This is a place holder for functionality that is still in development. | Int64
> disc-reason-443 | The total number of session disconnects resulting from the S4-SGSN’s inability to establish a PDP context for an APN because the APN was not served by a P-GW. | Int64
> disc-reason-444 | The total number of session disconnects resulting from the S4-SGSN initiating a “Deactivate PDP” as RABs are released for a non-GBR PDP context (conversational or streaming). [TS 23.060 v8.10.0 says the S4-SGSN should deactivate a PDP context if RAB or Iu Release occurs for either a conversational or streaming PDP context.] | Int64
> disc-reason-445 | The total number of session disconnects resulting from the S4-SGSN’s inability to establish a PDP context when the S-GW selection for the given RAI fails. [There may be no S-GW configured at the DNS for the given RAI.] | Int64
> disc-reason-446 | The total number of session disconnects resulting from the S4-SGSN’s inability to establish a PDP context for the given APN when neither a P-GW or a GGSN is configured for the APN. | Int64
> disc-reason-447 | wimax-hotlining-status-change | Int64
> disc-reason-448 | The total number of sessions disconnected on GGSN node due to no response received from SGSN for a request. | Int64
> disc-reason-449 | The total number of sessions disconnected on IPCF node due to an error in Diameter protocol (i.e. CCR-I parse failure). | Int64
> disc-reason-450 | The total number of sessions disconnected on IPCF node due to Diameter (RAR/ASR) request timeout on IPCF node. | Int64
> disc-reason-451 | The total number of session disconnected on IPCF node due to parameters configured by operator for PCC policy. | Int64
> disc-reason-452 | The total number of sessions disconnected on IPCF node due to an error in connection between SSC and IPCF node or non-availability of SSC. | Int64
> disc-reason-453 | mipha-dup-wimax-session | Int64
> disc-reason-455 | The total number of session disconnects experienced by the SGSN due to verification failure during the zone-code checking procedure. | Int64
> disc-reason-456 | The total number of session disconnects resulting from the receipt of invalid QoS class identifiers (QCIs). This error is returned if an invalid QCI is used in certain operations such as create bearer, which expects a QCI. A QCI is deemed invalid if it is not a standard QCI (1-9) or the QCI is not defined in the QCI table associated with the service. | Int64
> disc-reason-summary | Contain all of the disconnect reason counters at once in following format: code = count; code = count; ..... ;code = count all non-zero disconnect counters will be exported in a semi-colon separated format. If no disconnect stats are available, the value of this statistics will be a zero-length string. | String
> Important: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883