> CSCF Peer Server Monitoring Configuration Mode Commands
> The CSCF Peer Server Monitoring Configuration Mode is used to configure an individual peer server’s monitoring parameters and operational mode. It also associates a network session template with the server.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> ims-capable
> Indicates whether the peer server belongs to a 3GPP/IMS network or a non-IMS network such as the Internet. This command is used to determine at the S-CSCF whether SIP signaling inter-working is needed when the calls are forwarded to external networks.
> Product
> SCM (S-CSCF)
> Privilege
> Administrator
> Syntax
> [ no ] ims-capable
> no
> Removes the identification of “IMS capable” from the selected peer server.
> Usage
> Use this command to identify a peer server as IMS capable allowing the S-CSCF to use SIP signalling inter-working when forwarding calls to non-IMS capable networks.
> lro-selection-profile
> Binds a CSCF last route profile with the peer server.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> lro-selection-profile name profile_name
> no lro-selection-profile
> lro-selection-profile name profile_name
> profile_name must be an existing CSCF last route profile and be from 1 to 79 alpha and/or numeric characters.
> no lro-selection-profile
> Removes CSCF last route profile from the peer server group.
> Usage
> Use this command to identify a CSCF last route profile to use for finding the correct Public Safety Answering Point (PSAP) during emergency calls.
> Example
> The following command assigns a CSCF last route profile named lro1 to the peer server group:
> lro-selection-profile name lro1
> The following command removes a CSCF last route profile from the peer server group:
> no lro-selection-profile
> mode
> Sets the peer server mode to either active or standby. By default, peer servers are in active mode.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> mode { active | standby }
> active
> Defines the mode of the CSCF peer server as active.
> standby
> Defines the mode of the CSCF peer server as standby.
> Usage
> Use this command to set the peer server mode to either active or standby.
> Example
> The following command sets the peer server’s mode to standby:
> mode standby
> monitor-status
> Sets parameters for monitoring the status of peer servers.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> monitor-status [ monitor-interval seconds ] [ monitor-message options ] [ monitor-response-timer seconds ]
> no monitor-status
> monitor-interval seconds
> Default: 30
> Specifies the interval that peer server monitoring will occur.
> seconds must be an integer from 1 to 65535.
> monitor-message options
> Specifies that SIP message (OPTIONS) are to be sent periodically after each monitoring interval.
> monitor-response-timer seconds
> Default: 180
> Specifies the interval that the CSCF will wait for responses from the peer server.
> seconds must be an integer from 1 to 65535.
> no
> Disables peering server status monitoring.
> Usage
> Use this command to set parameters for monitoring the status of a peer server.
> Example
> The following command sets the monitoring interval to three minutes (180 seconds) and the response timer to six minutes (360 seconds):
> monitor-status monitor-interval 180 monitor-response-timer 360
> nw-session-template
> Specifies a session template for sessions terminating from the peer server group.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> nw-session-template name template-name
> no nw-session-template
> name template-name
> template-name must be an existing session template created in the Session Template Configuration Mode.
> no
> Removes session template from the peer server group.
> Usage
> Use this command to identify a session template to use for sessions terminating from the peer server group.
> Example
> The following command identifies a session template named template-25 to use for sessions terminating from the peer server group:
> nw-session-template template-25

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883