> QCI - RAN ID Mapping Configuration Mode Commands
> The QoS Class Index (QCI) Mapping Configuration Mode is used to map RAN profile IDs to QoS Class Indexes via the HRPD Serving Gateway (HSGW) in an eHRPD network.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> profile-id
> Maps a QCI ID to a RAN profile ID and modifies data flow bit rate ranges.
> Product
> HSGW
> Privilege
> Administrator
> Syntax
> profile-id id qci num [ uplink { gbr rate [ mbr rate ] | mbr rate [ gbr rate ] } downlink { gbr rate [ mbr rate ] | mbr rate [ gbr rate ] ]
> no profile-id id
> no
> Removes the specified profile ID entry from this map.
> id
> Specifies the profile ID to which a QCI ID will be mapped. id must be an integer value from 1 to 65535.
> qci num
> Specifies the QCI number to which the profile ID will be mapped. num must be an integer value from 1 to 255.
> uplink
> Specifies that the guaranteed bit rate (GBR) and/or maximum bite rate (MBR) setting that follow this keyword will be applied to the uplink data flow.
> downlink
> Specifies that the guaranteed bit rate (GBR) and/or maximum bite rate (MBR) settings that follow this keyword will be applied to the downlink data flow.
> gbr rate
> Specifies the guaranteed bit rate for the uplink or downlink data flow. rate must be an integer value from 0 to 4294967295.
> mbr rate
> Specifies the maximum bit rate for the uplink or downlink data flow. rate must be an integer value from 0 to 4294967295.
> Usage
> Use this command to map a QCI ID to a RAN profile ID and, optionally, modify data flow bit rate ranges.
> Example
> The following command maps a QCI ID (1) to a profile ID (10) and sets the uplink guaranteed bite rate to 10000 and the downlink guaranteed bit rate to 20000:
> profile-id 10 qci 1 uplink gbr 10000 downlink gbr 20000

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883