> Crypto Template IKEv2-Dynamic Payload Configuration Mode Commands
> The Crypto Template IKEv2-Dynamic Payload Configuration Mode is used to assign the correct IPSec transform-set from a list of up to four different transform-sets, and to assign Mobile IP addresses. There should be two payloads configured. The first must have a dynamic addressing scheme as this is how the ChildSA gets a TIA address. The second payload supplies the ChildSA with a HoA, which is the default setting for ip-address-allocation.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> default
> Sets or restores the default value for the specified parameter.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> default { ignore-rekeying-requests | ip-address-allocation lifetime | maximum-child-sa | rekey | tsi | tsr }
> ignore-rekeying-requests
> Configures the system to ignore IPSec SA rekey requests.
> ip-address-allocation
> Configures the crypto map payload IP address allocation scheme to be the home address.
> lifetime
> Configures the default lifetime for IPSec Child SAs derived from this crypto template. lifetime: 86400 seconds.
> maximum-child-sa
> Configures the maximum number of IPSec Child SAs to be derived from an IKEv2 IKE SA by default.
> rekey
> Configures the system to disable Child SA rekeying.
> tsi
> Configures the default TSi payload to be that of the mobile endpoint.
> tsr
> Configures the default TSr payload option.
> Usage
> Configures system defaults.
> Example
> Use the following configuration to set the TSi payload start-address to be that of the mobile endpoint:
> default tsi
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec Mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the previous mode.
> ignore-rekeying-requests
> Ignores CHILD SA rekey requests from the PDIF.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> ignore-rekeying-requests
> Usage
> Prevents creation of a CHILD SA based on this crypto template.
> Example
> The following command prevents creation of a CHILD SA based on this crypto template:
> ignore-rekeying-requests
> ip-address-allocation
> Configures IP address allocation for subscribers using this crypto template payload. Configure two payloads per crypto template. The first must have a dynamic address to assign a TIA to the ChildSA. The second payload is configured after a successful MIP initiation and can use the default HoA option.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> ip-address-allocation { dynamic | home-address | static }
> default ip-address-allocation
> dynamic
> Specifies that the IP address for the subscriber is allocated from a dynamic IP pool.
> home-address
> Specifies that the IP address for the subscriber is allocated by the Home Agent. This is the default setting for this command.
> static
> Specifies that the IP address for the subscriber is a static simple IP address.
> Usage
> Use this command to configure how ChildSA payloads are allocated IP addresses for this crypto template.
> Example
> The following command is for the first ChildSA and will ensure that it gets a TIA address from an IP address pool:
> ip-address-allocation dynamic
> The following command is for the second ChildSA and will ensure that it gets a HoA address from the HA:
> default ip-address-allocation
> ipsec
> Configures the IPsec transform set to be used for this crypto template payload.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] ipsec transform-set list name
> no
> Specifies the IPsec transform set to be deleted. This is a space-separated list. From 1 to 4 transform sets can be entered. name must be from 1 to 127 alpha and/or numeric characters.
> list name
> Specifies the context configured IPsec transform set name to be used in the crypto template payload. This is a space-separated list. From 1 to 4 transform sets can be entered. name must be from 1 to 127 alpha and/or numeric characters.
> Usage
> Use this command to list the IPsec transform set(s) to use in this crypto template payload.
> Example
> The following command configures IPsec transform sets named ipset1 and ipset2 to be used in this crypto template payload:
> ipsec transform-set list ipset1 ipset2
> lifetime
> Configures the number of seconds for IPsec Child SAs derived from this crypto template payload to exist.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> lifetime sec
> default lifetime
> sec
> Default: 86400
> Specifies the number of seconds for IPSec Child Security Associations derived from this crypto template payload to exist. sec must be an integer from 60 to 86400.
> default lifetime
> Sets the lifetime to its default value of 86400 seconds.
> Usage
> Use this command to configure the number of seconds for IPsec Child Security Associations derived from this crypto template payload to exist.
> Example
> The following command configures the IPsec child SA lifetime to be 120 seconds:
> lifetime 120
> maximum-child-sa
> Configures the maximum number of IPsec child security associations that can be derived from a single IKEv2 IKE security association.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> maximum-child-sa num
> default maximum-child-sa
> num
> Default: 1
> Specifies the maximum number of IPsec child security associations that can be derived from a single IKEv2 IKE security association. num must be 1.
> default maximum-child-sa
> Sets the maximum number of Child SAs to its default value of 1.
> Usage
> Use this command to configure the maximum number of IPsec child security associations that can be derived from a single IKEv2 IKE security association.
> Example
> The following command configures the maximum number of child SAs to 1:
> maximum-child-sa 1
> rekey
> Configures IPSec Child Security Association rekeying.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] rekey [ keepalive ]
> no
> Disables this feature.
> keepalive
> If specified, a session will be rekeyed even if there has been no data exchanged since the last rekeying operation. By default, rekeying is only performed if there has been data exchanged since the previous rekey.
> Usage
> Use this command to enable or disable the ability to rekey IPSec Child SAs after approximately 90% of the Child SA lifetime has expired. The default, and recommended setting, is not to perform rekeying. No rekeying means the PDIF will not originate rekeying operations and will not process CHILD SA rekeying requests from the UE.
> Example
> The following command disables rekeying:
> no rekey
> tsi
> Configures the IKEv2 Initiator Traffic Selector (TSI) payload address options.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> tsi start-address { any { end-address any } | endpoint { end-address endpoint } }
> any { end-address any }
> Configures the TSi payload to allow all all IP addresses.
> endpoint { end-address endpoint }
> Configures the TSi payload start-address to be that of the Mobile endpoint. This is the default value. endpoint is the mobile endpoint netmask.
> Usage
> On receiving a successful IKE_SA_INIT Response from PDIF, the MS sends an IKE_ AUTH Request for the first EAP-AKA authentication. If the MS is capable of doing multiple-authentication, it includes the MULTI_AUTH_SUPPORTED Notify payload in the IKE_AUTH Request. MS also includes an IDi payload containing the NAI, SA, TSi, TSr, and CP (requesting IP address and DNS address) payloads.
> Example
> Use the following example to configure a TSi payload that allows all addresses:
> tsi start-address any end-address any
> tsr
> Configures the IKEv2 Responder Traffic Selector (TSr) payload address options.
> Product
> PDG/TTG
> Privilege
> Security Administrator, Administrator
> Syntax
> tsr start-address ipv4 address end-address ipv4 address
> start-address ipv4 address
> Configures the TSr payload to include the TSr start IPv4 address of an address range for the Phase 1 multiple traffic selector feature.
> end-address ipv4 address
> Configures the TSr payload start-address to include the TSr end IPv4 address of an address range for the Phase 1 multiple traffic selector feature.
> Usage
> As part of Phase 1 of the Multiple Traffic Selector feature, this command is used to specify an IPv4 address range in the single TSr payload that the PDG/TTG returns in the last IKE_AUTH message. This TSr is Child SA-specific.
> Example
> Use the following example to configure a TSr payload that specifies an IPv4 address range for the payload:
> tsr start-address ipv4 address end-address ipv4 address

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883