> SGSN ASP Configuration Mode Commands
> The ASP (application server process) configuration mode defines the M3UA end-point parameters for a specific SS7 routing domain instance. The ASP instance is generated and accessed via the SS7 routing domain configuration mode commands.
> [local]hostname(config-ss7-rd-<ss7rd_id>-asp-inst-<asp_inst>)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec Mode.
> end-point
> This command defines or deletes the IP address and/or port number to be associated with the local SCTP end-point for this ASP. At least one address needs to be configured before the end-point can be activated.
> When using the bind keyword, this command also activates the end-point once the address has been defined. Once bound, it cannot be reconfigured until it is unbound with the no end-point bind command.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end-point { address ip_address context context_id | bind | port port_number }
> no end-point { address ip_address context context_id | bind }
> address ip_address context context_id:
> Specifies the IP address and the context associated with the address for this end-point.
> ip_address: must be defined using the standard IPv4 dotted decimal notation or the colon notation of IPv6.
> context context_id: a string of 1 to 79 alphanumeric characters to identify the specific context associated with the end-point address.
> bind
> Activates (binds) the end-point.
> Important: Only use bind after you have configured other parameters.
> port port_number
> Identifies the M3UA’s SCTP port associated with this end-point.
> port_number: must be an integer fom 1 to 65535. Default is 2905.
> no
> Removes the end-point configuration or deactivates the end-point.
> Caution: Entering this command will terminate all current subscriber sessions for associated peers.
> Usage
> Use this command to manage the ASP end-point. Once the ASP end-point is bound the end-point configuration can not be changed until it is unbound.
> Example
> Activate the end-point with the following command:
> end-point bind
> Deactivate or unbind the end-point with the following command:
> no end-point bind
> Set the end-point port to default for ASP 1 with the following command:
> default asp instance 1 end-point port
> exit
> Exits the current mode and returns to the previous mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the previous mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883