> BGP Address-Family (VPNv4) Configuration Mode Commands
> The Border Gateway Protocol (BGP) Address-Family (VPNv4) Configuration Mode is used to configure the VPNv4 address family information.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> neighbor
> This command configures VPNv4 address family on BGP routers that interconnect to non-broadcast networks and enables the exchange of routing information with a peer router (neighbor).
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] neighbor ip_address { activate | send-community { both | extended | standard } }
> no
> Delete the specified parameter from the router configuration.
> ip_address
> Specifies the IP address of the peer router (neighbor).
> activate
> Enable the exchange of routing information with this neighbor.
> send-community { both | extended | standard }
> This keyword sends community attributes to a peer router (neighbor).
> both: Sends standard and extended community attributes.
> extended: Sends extended community attributes.
> standard: Sends standard community attributes.
> Usage
> Use this command to enable the exchange of routing information with a peer router. The chassis supports a maximum of 64 peers per context.
> Example
> The following command enables the exchange of routing information with the neighbor at IP address 192.168.100.25:
> neighbor 192.168.100.25 activate

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883