> IPMS Application MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the IPMS application.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1). starentIPMSMIB(102)
> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102). starIPMSMIBObjects(1)
> Object
> starIPMSTimeTicks
> Object ID
> enterprises.8164.1.102.1.1
> Description
> This object indicates the time when this notification was generated.
> Syntax
> TimeStamp
> Access
> Read-Only
> Object
> starIPMSComponentName
> Object ID
> enterprises.8164.1.102.1.2
> Description
> This object indicates the name of the IPMS application component.
> Syntax
> DisplayString
> Access
> Read-Only
> Object
> starIPMSTaskInfo
> Object ID
> enterprises.8164.1.102.1.3
> Description
> This object indicates the IPMS process facility name and instance id of the IPMS application.
> Syntax
> DisplayString
> Access
> Read-Only
> Object
> starIPMSProcessMaxRestartCnt
> Object ID
> enterprises.8164.1.102.1.4
> Description
> This object indicates the maximum restart counts for IPMS processes.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starIPMSProcessRestartWaitTime
> Object ID
> enterprises.8164.1.102.1.5
> Description
> This object indicates the waiting period in seconds to restart IPMS processes.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starIPMSPacketLossCnt
> Object ID
> enterprises.8164.1.102.1.6
> Description
> This object indicates the number of packets detected as lost in the current IPMS process.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starIPMSTotalPacketLossCnt
> Object ID
> enterprises.8164.1.102.1.7
> Description
> This object indicates the total number of packets detected as lost since IPMS process started.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starIPMSDPIFailureReason
> Object ID
> enterprises.8164.1.102.1.8
> Description
> This object indicates the deep packet inspection (DPI) failure reasons with packet monitoring attributes.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> attributenotpresent(1)
> valuenotidentical(2)
> valuefunctionfailed(3)
> Object
> starIPMSDPIDetails
> Object ID
> enterprises.8164.1.102.1.9
> Description
> This object indicates the details of the deep packet inspection information of packets with packet monitoring attributes.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSEventSource
> Object ID
> enterprises.8164.1.102.1.10
> Description
> This object indicates the name of the event source of IPMS processes.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSAttribute
> Object ID
> enterprises.8164.1.102.1.11
> Description
> This object indicates the name of the IPMS attributes.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSResourceType
> Object ID
> enterprises.8164.1.102.1.12
> Description
> This object indicates the type of resource facilitate available/used for IPMS application processes.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> serverhbd(1)
> servmgr(2)
> serverevtlog(3)
> qryproc(4)
> evtproc0(5)
> evtproc1(6)
> evtproc2(7)
> evtproc3(8)
> evtproc4(9)
> queryhbd(10)
> qsmgr(11)
> eventlog(12)
> reqmgr(13)
> ctrlhbd(14)
> ctrlmgr(15)
> ctrlevtlog(16)
> totalcpu(17)
> swapmemory(18)
> export(19)
> log(20)
> data(21)
> crash(22)
> disk(23)
> invalid(24)
> Object
> starIPMSResourceInfoState
> Object ID
> enterprises.8164.1.102.1.13
> Description
> This object indicates the information of resource status for IPMS application processes.
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> available(1)
> notavailable(2)
> unknown(3)
> invalid(4)
> Object
> starIPMSResourceCurrentValue
> Object ID
> enterprises.8164.1.102.1.14
> Description
> This object indicates the current value/status of IPMS process resources like CPU, memory, disk space etc.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSResourceConfThreshold
> Object ID
> enterprises.8164.1.102.1.15
> Description
> This object indicates the configured threshold values of IPMS process resources like CPU, memory, disk space etc. The value is in Float so mapped to string.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSPeerName
> Object ID
> enterprises.8164.1.102.1.16
> Description
> This object indicates the name of the IPMS peer server.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSPeerIP
> Object ID
> enterprises.8164.1.102.1.17
> Description
> This object indicates the IP address of the IPMS peer server.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSPeerPort
> Object ID
> enterprises.8164.1.102.1.18
> Description
> This object indicates the port number of the IPMS server peer.
> Syntax
> DisplayString
> Access
> Read-only
> Object
> starIPMSICMPState
> Object ID
> enterprises.8164.1.102.1.19
> Description
> This object indicates the status of the Internet Control Message Protocol (ICMP) link between IPMS components and AGW. Possible state is either Up (1) or Down (2).
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> icmpstateup(1)
> icmpstatedown(2)
> Object
> starIPMSCORBAState
> Object ID
> enterprises.8164.1.102.1.20
> Description
> This object indicates the status of the Common Object Request Broker Architecture (CORBA) link between IPMS components and AGW. Possible state is either Up (1) or Down (2).
> Syntax
> Integer
> Access
> Read-only
> Enumeration
> corbasateup(1)
> corbastatedown(2)
> starentMIB(8164).starentMIBObjects(1). starentIPMSMIB(102)
> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102). starIPMSMIBTraps(2).
> Object
> starIPMSComponentStart
> Object ID
> enterprises.8164.1.102.2.1
> Description
> This notification generated when an IPMS component started successfully.
> Objects
> starIPMSComponentName
> Object
> starIPMSComponentStop
> Object ID
> enterprises.8164.1.102.2.2
> Description
> This notification generated when an IPMS component stopped or going for shutting down.
> Objects
> starIPMSComponentName
> Object
> starIPMSProcessStart
> Object ID
> enterprises.8164.1.102.2.3
> Description
> This notification generated when an IPMS process started/restarted successfully.
> Objects
> starIPMSTaskInfo
> Object
> starIPMSProcessStartFail
> Object ID
> enterprises.8164.1.102.2.4
> Description
> This notification generated when an IPMS process failed to start/restart.
> Objects
> starIPMSComponentName
> starIPMSProcessMaxRestartCnt
> starIPMSTaskInfo
> starIPMSProcessRestartWaitTime
> Object
> starIPMSPacketLossThreshold
> Object ID
> enterprises.8164.1.102.2.5
> Description
> This notification generated when maximum packet loss count from event source reached the threshold limit.
> Objects
> starIPMSTaskInfo
> starIPMSEventSource
> starIPMSPacketLossCnt
> starIPMSTotalPacketLossCnt
> Object
> starIPMSDPIFail
> Object ID
> enterprises.8164.1.102.2.6
> Description
> This notification generated when deep packet inspection (DPI) has been detected.
> Objects
> starIPMSTaskInfo
> starIPMSEventSource
> starIPMSAttribute
> starIPMSDPIFailureReason
> starIPMSDPIDetails
> Object
> starIPMSThresholdExceed
> Object ID
> enterprises.8164.1.102.2.7
> Description
> This notification generated when system exceeds the configured threshold value for IPMS components, resource, processes.
> Objects
> starIPMSComponentName
> starIPMSResourceType
> starIPMSResourceInfoState
> starIPMSResourceCurrentValue
> starIPMSResourceConfThreshold
> Object
> starIPMSThresholdClear
> Object ID
> enterprises.8164.1.102.2.8
> Description
> This notification generated when system clears the threshold exceed condition for IPMS components, resource, processes.
> Objects
> starIPMSComponentName
> starIPMSResourceType
> starIPMSResourceInfoState
> starIPMSResourceCurrentValue
> starIPMSResourceConfThreshold
> Object
> starIPMSPeerStateChange
> Object ID
> enterprises.8164.1.102.2.9
> Description
> This notification generated when IPMS Server/Query Server peer changes its state.
> Objects
> starIPMSComponentName
> starIPMSPeerName
> starIPMSPeerIP
> starIPMSPeerPort
> starIPMSICMPState
> starIPMSCORBAState
> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102). starIPMSMIBConformances(3).starIPMSMIBCompliances(1)
> Object
> starIPMSMIBCompliance
> Object ID
> enterprises.8164.1.102.3.1.1
> Description
> The compliance statements for entities which implement the STARENT IPMS MIB.
> Objects
> starIPMSObjectGroup
> starIPMSNotifGroup
> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102). starIPMSMIBConformances(3).starIPMSMIBGroups(2)
> Object
> starIPMSObjectGroup
> Object ID
> enterprises.8164.1.102.3.2.1
> Description
> This group is a collection of objects related with notification management on IPMS.
> Objects
> starIPMSTimeTicks
> starIPMSComponentName
> starIPMSTaskInfo
> starIPMSProcessMaxRestartCnt
> starIPMSProcessRestartWaitTime
> starIPMSPacketLossCnt
> starIPMSTotalPacketLossCnt
> starIPMSDPIFailureReason
> starIPMSDPIDetails
> starIPMSEventSource
> starIPMSAttribute
> starIPMSResourceType
> starIPMSResourceInfoState
> starIPMSResourceCurrentValue
> starIPMSResourceConfThreshold
> starIPMSPeerName
> starIPMSPeerIP
> starIPMSPeerPort
> starIPMSICMPState
> starIPMSCORBAState
> Object
> starIPMSNotifGroup
> Object ID
> enterprises.8164.1.102.3.2.2
> Description
> This group is a collection of notifications for IPMS management.
> Objects
> starIPMSComponentStart
> starIPMSComponentStop
> starIPMSProcessStart
> starIPMSProcessStartFail
> starIPMSPacketLossThreshold
> starIPMSDPIFail
> starIPMSThresholdExceed
> starIPMSThresholdClear
> starIPMSPeerStateChange

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883