> HNBGW-RUA Schema Statistics
> The HNBGW-RUA schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HNB-GW.
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the HNBGW-RUA Schema

> Variables | Description | Data Type
> vpnname | Indicates the name of the context in which HNB-GW service is configured. This is a key variable. | String
> vpnid | Indicates the identity number of the context in which HNB-GW service is configured. This is a key variable. | String
> servname | Indicates the name of the HNB-GW service for which statistics are collected or displayed. This is a key variable. | String
> cs-connect-rx | RUA CS Domain: Indicates the total number of Connect message received. Trigger: When RUA CS Domain Connect message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-connect-rx-est-cause-emergency | RUA CS Domain: Indicates the total number of Connect message received with Establishment cause - Emergency Call. Trigger: When RUA CS Domain Connect message is received by HNB-GW with Establishment cause - Emergency Call. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-connect-rx-est-cause-normal | RUA CS Domain: Indicates the total number of Connect message received with Establishment cause - Normal. Trigger: When RUA CS Domain Connect message is received by HNB-GW with Establishment cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-connect-tx | RUA CS Domain: Indicates the total number of Connect message transmitted. Trigger: When RUA CS Domain Connect message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-dir-transfer-rx | RUA CS Domain: Indicates the total number of Direct Transfer message received. Trigger: When RUA CS Domain Direct Transfer message received. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-dir-transfer-tx | RUA CS Domain: Indicates the total number of Direct Transfer message transmitted. Trigger: When RUA CS Domain Direct Transfer message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received. Trigger: When RUA CS Domain Disconnect (with payload) message received. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-normal | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Normal. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-connect-failed | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Connect failed. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-nw-rel | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Network release. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-rnl-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-trans-res-unavailable | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Transport Layer cause - Transport resource unavailable. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-trans-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Transport Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-trans-syn-err | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Transfer syntax error. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-abs-syn-err-rej | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-abs-syn-err-ign-notify | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-msg-not-comp | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-semantic-err | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Semantic error. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-prot-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-falsely-construct-msg | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Abstract syntax error (Falsely constructed message). Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed message). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-processing-overload | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - Processing Overload. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-hw-failure | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - Hardware Failure. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-oam-intervention | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - O&M Intervention. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-rx-misc-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted. Trigger: When RUA CS Domain Disconnect (with payload) message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-normal | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Normal. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-connect-failed | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Connect failed. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-nw-rel | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Network release. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-rnl-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-trans-res-unavailable | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Transport Layer cause - Transport resource unavailable. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-trans-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Transport Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-trans-syn-err | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Transfer syntax error. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-abs-syn-err-rej | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-abs-syn-err-ign-notify | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-msg-not-comp | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-semantic-err | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Semantic error. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-prot-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-falsely-construct-msg | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-processing-overload | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - Processing Overload. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-hw-failure | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - Hardware Failure. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-oam-intervention | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - O&M Intervention. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-payload-tx-misc-unspecified | RUA CS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - Unspecified. Trigger: When RUA CS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received. Trigger: When RUA CS Domain Disconnect (without payload) message received. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-normal | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Normal. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-connect-failed | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Connect failed. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-nw-rel | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Network release. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-rnl-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-trans-res-unavailable | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Transport Layer cause - Transport resource unavailable. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-trans-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Transport Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-trans-syn-err | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Transfer syntax error. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-abs-syn-err-rej | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-abs-syn-err-ign-notify | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-msg-not-comp | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Msg not compatible without receiver state. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Msg not compatible without receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-semantic-err | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Semantic error. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-prot-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-falsely-construct-msg | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-processing-overload | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - Processing Overload. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-hw-failure | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - Hardware Failure. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-oam-intervention | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - O&M Intervention. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-rx-misc-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted. Trigger: When RUA CS Domain Disconnect (without payload) message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-normal | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Normal. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-connect-failed | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Connect failed. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-nw-rel | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Network release. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-rnl-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-trans-res-unavailable | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Transport Layer cause - Transport resource unavailable. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-trans-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Transport Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-trans-syn-err | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Transfer syntax error. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-abs-syn-err-rej | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-abs-syn-err-ign-notify | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-msg-not-comp | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Msg not compatible without receiver state. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Msg not compatible without receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-semantic-err | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Semantic error. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-prot-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-falsely-construct-msg | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-processing-overload | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - Processing Overload. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-hw-failure | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - Hardware Failure. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-oam-intervention | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - O&M Intervention. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-disc-wo-payload-tx-misc-unspecified | RUA CS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - Unspecified. Trigger: When RUA CS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-conn-less-trans-rx | RUA CS Domain: Indicates the total number of Connectionless Transfer message received. Trigger: When RUA CS Domain Connectionless Transfer message received. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-conn-less-trans-tx | RUA CS Domain: Indicates the total number of Connectionless Transfer message transmitted. Trigger: When RUA CS Domain Connectionless Transfer message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx | RUA CS Domain: Indicates the total number of Error Indication message received. Trigger: When RUA CS Domain Error Indication message received. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-normal | RUA CS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Normal. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-connect-failed | RUA CS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Connect failed. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-nw-rel | RUA CS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Network release. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-rnl-unspecified | RUA CS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-trans-res-unavailable | RUA CS Domain: Indicates the total number of Error Indication message received with Transport Layer cause - Transport resource unavailable. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-trans-unspecified | RUA CS Domain: Indicates the total number of Error Indication message received with Transport Layer cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-trans-syn-err | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Transfer syntax error. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-abs-syn-err-rej | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-abs-syn-err-ign-notify | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-msg-not-comp | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-semantic-err | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Semantic error. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-prot-unspecified | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-falsely-construct-msg | RUA CS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-processing-overload | RUA CS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - Processing Overload. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-hw-failure | RUA CS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - Hardware Failure. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-oam-intervention | RUA CS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - O&M Intervention. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-rx-misc-unspecified | RUA CS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx | RUA CS Domain: Indicates the total number of Error Indication message transmitted. Trigger: When RUA CS Domain Error Indication message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-normal | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Normal. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-connect-failed | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Connect failed. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-nw-rel | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Network release. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-rnl-unspecified | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-trans-res-unavailable | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Transport Layer cause - Transport resource unavailable. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-trans-unspecified | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Transport Layer cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-trans-syn-err | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Transfer syntax error. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-abs-syn-err-rej | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-abs-syn-err-ign-notify | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-msg-not-comp | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-semantic-err | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Semantic error. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-prot-unspecified | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-falsely-construct-msg | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-processing-overload | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - Processing Overload. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-hw-failure | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - Hardware Failure. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-oam-intervention | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - O&M Intervention. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-err-ind-tx-misc-unspecified | RUA CS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - Unspecified. Trigger: When RUA CS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-connect-rx | RUA PS Domain: Indicates the total number of Connect message received. Trigger: When RUA PS Domain Connect message received. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-connect-rx-est-cause-emergency | RUA PS Domain: Indicates the total number of Connect message received with Establishment cause - Emergency Call. Trigger: When RUA PS Domain Connect message is received by HNB-GW with Establishment cause - Emergency Call. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-connect-rx-est-cause-normal | RUA PS Domain: Indicates the total number of Connect message received with Establishment cause - Normal. Trigger: When RUA PS Domain Connect message is received by HNB-GW with Establishment cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-connect-tx | RUA PS Domain: Indicates the total number of Connect message transmitted. Trigger: When RUA PS Domain Connect message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-dir-transfer-rx | RUA PS Domain: Indicates the total number of Direct Transfer message received. Trigger: When RUA PS Domain Direct Transfer message received. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-dir-transfer-tx | RUA PS Domain: Indicates the total number of Direct Transfer message transmitted. Trigger: When RUA PS Domain Direct Transfer message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received. Trigger: When RUA PS Domain Disconnect (with payload) message received. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-normal | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Normal. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-connect-failed | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Connect failed. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-nw-rel | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Network release. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-rnl-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Radio Network Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-trans-res-unavailable | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Transport Layer cause - Transport resource unavailable. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-trans-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Transport Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-trans-syn-err | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Transfer syntax error. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-abs-syn-err-rej | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-abs-syn-err-ign-notify | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-msg-not-comp | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-semantic-err | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Semantic error. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-prot-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-falsely-construct-msg | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-processing-overload | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - Processing Overload. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-hw-failure | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - Hardware Failure. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-oam-intervention | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - O&M Intervention. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-rx-misc-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message received with Miscellaneous cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is received by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted. Trigger: When RUA PS Domain Disconnect (with payload) message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-normal | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Normal. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-connect-failed | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Connect failed. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-nw-rel | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Network release. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-rnl-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Radio Network Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-trans-res-unavailable | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Transport Layer cause - Transport resource unavailable. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-trans-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Transport Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-trans-syn-err | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Transfer syntax error. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-abs-syn-err-rej | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-abs-syn-err-ign-notify | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-msg-not-comp | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-semantic-err | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Semantic error. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-prot-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-falsely-construct-msg | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-processing-overload | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - Processing Overload. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-hw-failure | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - Hardware Failure. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-oam-intervention | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - O&M Intervention. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-payload-tx-misc-unspecified | RUA PS Domain: Indicates the total number of Disconnect (with payload) message transmitted with Miscellaneous cause - Unspecified. Trigger: When RUA PS Domain Disconnect (with payload) message is transmitted by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received. Trigger: When RUA PS Domain Disconnect (without payload) message received. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-normal | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Normal. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-connect-failed | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Connect failed. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-nw-rel | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Network release. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-rnl-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Radio Network Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-trans-res-unavailable | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Transport Layer cause - Transport resource unavailable. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-trans-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Transport Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-trans-syn-err | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Transfer syntax error. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-abs-syn-err-rej | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-abs-syn-err-ign-notify | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-msg-not-comp | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Msg not compatible without receiver state. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Msg not compatible without receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-semantic-err | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Semantic error. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-prot-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-falsely-construct-msg | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-processing-overload | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - Processing Overload. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-hw-failure | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - Hardware Failure. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-oam-intervention | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - O&M Intervention. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-rx-misc-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message received with Miscellaneous cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is received by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted. Trigger: When RUA PS Domain Disconnect (without payload) message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-normal | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Normal. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-connect-failed | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Connect failed. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-nw-rel | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Network release. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-rnl-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Radio Network Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-trans-res-unavailable | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Transport Layer cause - Transport resource unavailable. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-trans-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Transport Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-trans-syn-err | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Transfer syntax error. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-abs-syn-err-rej | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-abs-syn-err-ign-notify | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-msg-not-comp | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Msg not compatible without receiver state. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Msg not compatible without receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-semantic-err | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Semantic error. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-prot-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-falsely-construct-msg | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-processing-overload | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - Processing Overload. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-hw-failure | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - Hardware Failure. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-oam-intervention | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - O&M Intervention. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-disc-wo-payload-tx-misc-unspecified | RUA PS Domain: Indicates the total number of Disconnect (without payload) message transmitted with Miscellaneous cause - Unspecified. Trigger: When RUA PS Domain Disconnect (without payload) message is transmitted by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-conn-less-trans-rx | RUA PS Domain: Indicates the total number of Connectionless Transfer message transmitted. Trigger: When RUA PS Domain Connectionless Transfer message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-conn-less-trans-tx | RUA PS Domain: Indicates the total number of Connectionless Transfer message transmitted. Trigger: When RUA PS Domain Connectionless Transfer message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx | RUA PS Domain: Indicates the total number of Error Indication message received. Trigger: When RUA PS Domain Error Indication message received. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-normal | RUA PS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Normal. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-connect-failed | RUA PS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Connect failed. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-nw-rel | RUA PS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Network release. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-rnl-unspecified | RUA PS Domain: Indicates the total number of Error Indication message received with Radio Network Layer cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-trans-res-unavailable | RUA PS Domain: Indicates the total number of Error Indication message received with Transport Layer cause - Transport resource unavailable. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-trans-unspecified | RUA PS Domain: Indicates the total number of Error Indication message received with Transport Layer cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-trans-syn-err | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Transfer syntax error. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-abs-syn-err-rej | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-abs-syn-err-ign-notify | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-msg-not-comp | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-semantic-err | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Semantic error. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-prot-unspecified | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-falsely-construct-msg | RUA PS Domain: Indicates the total number of Error Indication message received with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-processing-overload | RUA PS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - Processing Overload. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-hw-failure | RUA PS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - Hardware Failure. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-oam-intervention | RUA PS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - O&M Intervention. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-rx-misc-unspecified | RUA PS Domain: Indicates the total number of Error Indication message received with Miscellaneous cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is received by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx | RUA PS Domain: Indicates the total number of Error Indication message transmitted. Trigger: When RUA PS Domain Error Indication message transmitted. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-normal | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Normal. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Normal. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-connect-failed | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Connect failed. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Connect failed. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-nw-rel | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Network release. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Network release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-rnl-unspecified | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Radio Network Layer cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Radio Network Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-trans-res-unavailable | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Transport Layer cause - Transport resource unavailable. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Transport Layer cause - Transport resource unavailable. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-trans-unspecified | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Transport Layer cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Transport Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-trans-syn-err | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Transfer syntax error. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-abs-syn-err-rej | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Abstract syntax error (Reject). Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-abs-syn-err-ign-notify | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Ignore and Notify). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-msg-not-comp | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Msg not compatible with receiver state. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-semantic-err | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Semantic error. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-prot-unspecified | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-falsely-construct-msg | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Protocol Layer cause - Abstract syntax error (Falsely constructed msg. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-processing-overload | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - Processing Overload. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - Processing Overload. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-hw-failure | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - Hardware Failure. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - Hardware Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-oam-intervention | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - O&M Intervention. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - O&M Intervention. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-err-ind-tx-misc-unspecified | RUA PS Domain: Indicates the total number of Error Indication message transmitted with Miscellaneous cause - Unspecified. Trigger: When RUA PS Domain Error Indication message is transmitted by HNB-GW with Miscellaneous cause - Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> Important: See Bulk Statistics Overview chapter for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883