> show sgw
> This chapter describes the output of the show sgw command.
> show sgw-service all
> Displays configuration information for all S-GW services configured on the system.
> show sgw-service all Command Output Descriptions

> Field | Description
> Service name | The name of the S-GW service.
> Service-ID | The system generated identification number of the service.
> Context | The context name where the service is located.
> Accounting context | The context where the accounting configuration and or interfaces are configured.
> Status | The status of the service.
> Egress Protocol | The egress protocol, such as “gtp-pmip”
> Ingress EGTP service | The ingress eGTP service configured for this S-GW service.
> Egress context | The egress context configured for this service.
> Egress EGTP service | The egress eGTP service configured for this S-GW service.
> Egress MAG service | The egress Mobile Access Gateway (MAG) service configured for this service.
> IMS auth. service | The IMS authorization (IMSA) service used by this service for IMS subscribers.
> Newcall policy | The newcall policy configured for this service.
> QCI-QOS mapping table | The QoS Class Index to QoS mapping table configured for use with this service.
> S4U-Interface
> S12-Interface
> GTPU Error Indication Handling
> S1U-Interface | local-purge: The S-GW clears the affected bearer (or PDN if the error indication is received on the default bearer) locally without informing the peers. page-ue: The S-GW moves the complete UE state to S1-Idle and starts paging for this UE. This is the default action for GTP-U error indication messages received on the S12 and S1-U interfaces.
> S5U-Interface
> S12-Interface
> S4U-Interface
> PLMN ID List | List of Public Land Mobile Network (PLMN) identifiers associated with the operator policy for this service. A PLMN ID consists of the Mobile Country Code (MCC) + Mobile network Code (MCC).
> Subscriber Map Name | Name of the subscriber map associated with the operator policy for this service.

> ‌
> show sgw-service statistics all verbose
> show sgw-service statistics all Command Output Descriptions

> Field | Description
> Session Level Statistics
> Current
> UE
> Idle | The total number of UE sessions currently idle.
> Active | The total number of UE sessions currently active.
> PDN | The total number of current PDN sessions.
> Home | The total number of current home PDN sessions.
> Roaming | The total number of current roaming PDN sessions.
> Visiting | The total number of current visiting PDN sessions.
> Bearers | The total number of current Bearers.
> Ind-Fwd-Tunnels | Indirect forward tunneling: The total number of current tunnels.
> Ind-Fwd-Bearers | Indirect forward tunneling: The total number of current bearers.
> Setup
> UE | The total number of UE session set up.
> PDN | The total number of PDN sessions set up.
> Bearers | The total number of bearers set up.
> PDNs Setup Per PDN-type
> IPv4 | The total number of PDN sessions set up using IPv4.
> IPv6 | The total number of PDN sessions set up using IPv6.
> IPv4v6 | The total number of PDN sessions set up using IPv4 in IPv6.
> PDNs Setup Per Interface
> S11 | The total number of PDN sessions set up on an S11 interface.
> S4 | The total number of PDN sessions set up on an S4 interface.
> PDNs Setup Per S5 Proto
> GTP | The total number of PDN sessions set up using GTP tunneling.
> PMIP | The total number of PDN sessions set up using PMIP tunneling.
> PDNs Released
> IPv4 | The total number of PDN sessions released using IPv4.
> IPv6 | The total number of PDN sessions released using IPv6.
> IPv4v6 | The total number of PDN sessions released using IPv4 in IPv6.
> PDNs Released Reason
> MME Ini | The total number of PDN sessions released - initiated by the MME.
> PGW Ini | The total number of PDN sessions released - initiated by the P-GW.
> PCRF Ini | The total number of PDN sessions released - initiated by the PCRF.
> Local | The total number of PDN sessions released - initiated locally.
> S1 Error Ind | The total number of PDN sessions released due to an S1 interface error.
> S5 Error Ind | The total number of PDN sessions released due to an S5 interface error.
> Path Failure S11 | The total number of PDN sessions released due to an S11 path failure.
> Path Failure S1-U | The total number of PDN sessions released due to an S1-U path failure.
> Path Failure S5 | The total number of PDN sessions released due to an S5 path failure.
> Path Failure S5-U | The total number of PDN sessions released due to an S5-U path failure.
> Path Failure S4 | The total number of PDN sessions released due to an S4 path failure.
> Path Failure S4-U | The total number of PDN sessions released due to an S4-U path failure.
> Path Failure S12 | The total number of PDN sessions released due to an S12 path failure.
> Other | The total number of PDN sessions released due to other reasons.
> PDNs Rejected
> IPv4 | The total number of PDN sessions rejected using IPv4.
> IPv6 | The total number of PDN sessions rejected using IPv6.
> IPv4v6 | The total number of PDN sessions rejected using IPv4 in IPv6.
> PDNs Rejected Reason
> PGW Ini | The total number of PDN sessions rejected - initiated by the P-GW.
> License | The total number of PDN sessions rejected due to license reasons.
> Newcall | The total number of PDN sessions rejected due to newcall reasons.
> Overload | The total number of PDN sessions rejected due to overload reasons.
> Congestion | The total number of PDN sessions rejected due to congestion reasons.
> Other | The total number of PDN sessions rejected due to other reasons.
> Bearer Level Statistics
> Total EPS Bearers Setup
> QCI 1 - 9 | The total number of EPS bearers set up, with a QoS Class Index.
> Non-Std QCI | The total number of EPS bearers set up, with a non-standard QoS Class Index.
> Total EPS Bearers Released
> QCI 1 - 9 | The total number of EPS bearers released, with a QoS Class Index.
> Non-Std QCI | The total number of EPS bearers released, with a non-standard QoS Class Index.
> Total EPS Bearers Modified |
> QCI 1 - 9 | The total number of EPS bearers modified, with a QoS Class Index.
> Non-Std QCI | The total number of EPS bearers modified, with a non-standard QoS Class Index.
> Dedicated Bearers Released Reason
> PGW Ini | The total number of dedicated bearers released - initiated by the P-GW.
> PCRF Ini | The total number of dedicated bearers released - initiated by the PCRF.
> S1 Error Ind | The total number of dedicated bearers released due to an S1 interface error.
> S5 Error Ind | The total number of dedicated bearers released due to an S5 interface error.
> S4-U Error Ind | The total number of dedicated bearers released due to an S4-U interface error.
> S12 Error Ind | The total number of dedicated bearers released due to an S12 interface error.
> Local | The total number of dedicated bearers released - initiated locally.
> PDN Down | The total number of dedicated bearers released due to an inaccessible PDN.
> Path Failure S1-U | The total number of dedicated bearers released due to an S1-U path failure.
> Path Failure S5-U | The total number of dedicated bearers released due to an S5-U path failure.
> Path Failure S4-U | The total number of dedicated bearers released due to an S4-U path failure.
> Path Failure S12 | The total number of dedicated bearers released due to an S12U path failure.
> Other | The total number of dedicated bearers released due to other reasons.
> S1U Total Data Statistics
> Uplink
> Pkts | The total number of uplink packets over the S1-U interface.
> Bytes | The total number of uplink bytes over the S1-U interface.
> Dropped Pkts | The total number of dropped uplink packets over the S1-U interface.
> Dropped Bytes | The total number of dropped uplink bytes over the S1-U interface.
> Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
> Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
> Downlink
> Pkts | The total number of downlink packets over the S1-U interface.
> Bytes | The total number of downlink bytes over the S1-U interface.
> Dropped Pkts | The total number of dropped downlink packets over the S1-U interface.
> Dropped Bytes | The total number of dropped downlink bytes over the S1-U interface.
> Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
> S4U Total Data Statistics
> Uplink
> Pkts | The total number of uplink packets over the S4-U interface.
> Bytes | The total number of uplink bytes over the S4-U interface.
> Dropped Pkts | The total number of dropped uplink packets over the S4-U interface.
> Dropped Bytes | The total number of dropped uplink bytes over the S4-U interface.
> Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
> Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
> Downlink
> Pkts | The total number of downlink packets over the S4-U interface.
> Bytes | The total number of downlink bytes over the S4-U interface.
> Dropped Pkts | The total number of dropped downlink packets over the S4-U interface.
> Dropped Bytes | The total number of dropped downlink bytes over the S4-U interface.
> Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
> S12 Total Data Statistics
> Uplink
> Pkts | The total number of uplink packets over the S12 interface.
> Bytes | The total number of uplink bytes over the S12 interface.
> Dropped Pkts | The total number of dropped uplink packets over the S12 interface.
> Dropped Bytes | The total number of dropped uplink bytes over the S12 interface.
> Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
> Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
> Downlink
> Pkts | The total number of downlink packets over the S12 interface.
> Bytes | The total number of downlink bytes over the S12 interface.
> Dropped Pkts | The total number of dropped downlink packets over the S12 interface.
> Dropped Bytes | The total number of dropped downlink bytes over the S12 interface.
> Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
> S5 Total Data Statistics
> Uplink
> Pkts | The total number of uplink packets over the S5 interface.
> Bytes | The total number of uplink bytes over the S5 interface.
> Dropped Pkts | The total number of dropped uplink packets over the S5 interface.
> Dropped Bytes | The total number of dropped uplink bytes over the S5 interface.
> Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
> Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
> Downlink
> Pkts | The total number of downlink packets over the S5 interface.
> Bytes | The total number of downlink bytes over the S5 interface.
> Dropped Pkts | The total number of dropped downlink packets over the S5 interface.
> Dropped Bytes | The total number of dropped downlink bytes over the S5 interface.
> Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
> S8 Total Data Statistics
> Uplink
> Pkts | The total number of uplink packets over the S8 interface.
> Bytes | The total number of uplink bytes over the S8 interface.
> Dropped Pkts | The total number of dropped uplink packets over the S8 interface.
> Dropped Bytes | The total number of dropped uplink bytes over the S8 interface.
> Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
> Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
> Downlink
> Pkts | The total number of downlink packets over the S8 interface.
> Bytes | The total number of downlink bytes over the S8 interface.
> Dropped Pkts | The total number of dropped downlink packets over the S8 interface.
> Dropped Bytes | The total number of dropped downlink bytes over the S8 interface.
> Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
> Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
> Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
> Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
> Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
> Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
> Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
> Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
> Inter-SGW Handover Statistics
> PDNs Incoming
> X2 Based | The total number of incoming X2-based PDNs.
> Idle-mode TAU | The total number of incoming PDNs Incoming - Idle-mode TAU
> S1 Based | The total number of incoming S1-based PDNs.
> PDNs Outgoing | The total number of outgoing PDNs.
> Intra-SGW Handover Statistics
> Intra-MME | Intra-MME
> Inter-MME | Inter-MME
> Intra-SGSN | Intra-SGSN
> Inter-SGSN | Inter-SGSN
> MME-to-SGSN | MME-to-SGSN
> SGSN-to-MME | SGSN-to-MME
> Paging Statistics
> Requests | The total number of paging requests.
> Success | The total number of paging successes.
> Rejects | The total number of paging rejects.
> Failures | The total number of paging failures.
> Active-Idle Ue Transitions | The total number of Active-Idle UE transitions
> Idle-Active Ue Transitions | The total number of Idle-Active UE transitions
> Paging Related Data Statistics
> Packets Buffered | The total number of buffered paging packets.
> Bytes Buffered | The total number of buffered paging bytes.
> Packets Discarded | The total number of discarded paging packets.
> Bytes Discarded | The total number of discarded paging bytes.
> Idle Mode ACL Statistics
> Packets Discarded | The total number of discarded paging packets due to ACL idle mode.
> Bytes Discarded | The total number of discarded paging bytes due to ACL idle mode.
> Indirect Forwarding Statistics
> Tunnels Setup | The total number of indirect forwarding tunnels setup.
> Tunnels Failed | The total number of failed indirect forwarding tunnels.
> Tunnels Released | The total number of indirect forwarding tunnels released.
> Bearers Setup | The total number of indirect forwarding bearers setup.
> Bearers Released | The total number of indirect forwarding bearers released.
> DL Packets Forwarded | The total number of indirect forwarding download packets forwarded.
> DL Bytes Forwarded | The total number of indirect forwarding download bytes forwarded.
> Source Violations
> Packets Dropped | The total number of packets dropped due to source violations.
> Bytes Dropped | The total number of bytes dropped due to source violations.
> PDN PLMN Statistics
> Home PDNs
> PDNs active | The total number of home PDNs active.
> PDNs setup | The total number of home PDNs setup.
> PDNs released | The total number of home PDNs released.
> Roaming PDNs
> PDNs active | The total number of roaming PDNs active.
> PDNs setup | The total number of roaming PDNs setup.
> PDNs released | The total number of roaming PDNs released.
> Visiting PDNs
> PDNs active | The total number of visiting PDNs active.
> PDNs setup | The total number of visiting PDNs setup.
> PDNs released | The total number of visiting PDNs released.
> Miscellaneous
> Uplink Data Before MBReq | Uplink data before MBreq
> CBReq Rcvd Before CSRsp | CBReq Rcvd before CSRsp

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883