> show llc statistics
> show llc statistics Command Output Descriptions

> Field | Description
> LLC SAP Statistics
> Data transfer
> Data requests Rx | Total number of LLC data requests received from the MS.
> Data confirms Tx | Total number of LLC data requests confirmation sent to the MS.
> Data indications Tx | Total number of LLC data indications sent to the MS.
> Data-Sent indications Tx | Total number of LLC data sent indications sent to the MS.
> Unit data requests Rx | Total number of LLC unit data requests received from the MS.
> Unit data requests Rx Drop | Description: This proprietary counter indicates the total number of unit data requests received from SNDCP layer and dropped at the LLC layer. Triggers: Increments when LLC receives a downlink packet from SNDCP and the queue in LLC layer is full.
> Unit data indications Tx | Total number of LLC unit data indications sent to the MS.
> Errors reported
> Discarded frames Rx | Total number of LLC discarded frames received from the MS.
> Discarded frames Tx | Total number of LLC discarded frames sent to the MS.
> Error frames Rx | Total number of LLC error frames received from the MS.
> Unrecognised frames Rx | Total number of LLC unrecognized frames received from the MS.
> XID collisions | Total number of LLC exchange identifier (XID) request collisions.
> Ciphering errors | Total number of LLC ciphering errors.
> FCS errors | Total number of LLC frame check sequence errors.
> LLC Frame statistics
> Octets Rx | Total number of bytes of LLC frames received from an MS.
> Octets Tx | Total number of bytes sent from the LLC layer to an MS from the SGSN.
> Unack frames Rx | Total number of unacknowledged UI frames received at the LLC layer from an MS.
> Unack frames Tx | Total number of unacknowledged UI frames sent from the LLC to an MS.
> UI Rx | Total number of LLC frames with unnumbered information received from the MS.
> UI Tx | Total number of LLC frames with unnumbered information sent to the MS.
> UI Ciphered frames Rx | Total number of LLC frames with ciphered unnumbered information received from the MS.
> UI Ciphered frames Tx | Total number of LLC frames with ciphered unnumbered information sent to the MS.
> XID Rx | Total number of XID-reset messages received from the MS.
> XID Tx | Total number of XID-reset messages sent to the MS.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883