> Performance Management
> This chapter identifies new, modified, and obsoleted performance commands available in Releases 12.0 or 12.1.
> Topics covered in this chapter are:

> l | New Commands

> l | Modified Commands

> l | Obsolete Commands

> l | GTPP Storage Server Changes

> l | Web Element Manager Changes

> New Commands
> This section identifies performance management commands that are new in Release 12.0.

> l | Common Commands - New in Release 12.0

> l | Application Detection and Control - New in Release 12.0

> l | Content Filtering Commands - New in Release 12.0

> l | ECS Commands - New in Release 12.0

> l | Firewall Commands - New in Release 12.0

> l | GGSN Commands - New in Release 12.0

> l | HA Commands - New in Release 12.0

> l | Mobility Management Entity Commands - New in Release 12.0

> l | NAT Commands - New in Release 12.0

> l | Packet Data Network Gateway Commands - New in Release 12.0

> l | PDIF Commands - New in Release 12.0

> l | PDSN Commands - New in Release 12.0

> l | Serving Gateway Commands - New in Release 12.0

> l | SGSN Commands - New in Release 12.0

> Common Commands - New in Release 12.0
> The following common commands are new in Release 12.0.
> monitor diameter
> This command enables SRP monitoring of the connection between the specified Diameter server and the primary chassis.
> CLI (Service Redundancy Protocol Configuration Mode)
> [ no ] monitor diameter context context_name endpoint endpoint_name [ fqdn fqdn | peer { IPv4_address | IPv6_address } ] [ port port_number ]
> show tacacs
> Provides TACACS+ configuration and session state information for each active TACACS+ session.
> CLI (Exec Mode)
> show tacacs
> show tacacs client statistics
> Provides system-wide client statistics for all TACACS+ sessions.
> CLI (Exec Mode)
> show tacacs client statistics
> show tacacs session statistics
> Provides system-wide session statistics, including protocol statistics, for active TACACS+ sessions.
> CLI (Exec Mode)
> show tacacs session statistics
> Application Detection and Control - New in Release 12.0
> The following Application Detection and Control commands are new in Release 12.0.
> None for this release.
> Content Filtering Commands - New in Release 12.0
> The following Content Filtering commands are new in Release 12.0.
> None for this release.
> ECS Commands - New in Release 12.0
> The following ECS commands are new in Release 12.0.
> None for this release.
> Firewall Commands - New in Release 12.0
> The following Stateful Firewall commands are new in Release 12.0.
> None for this release.
> GGSN Commands - New in Release 12.0
> The following GGSN commands are new in Release 12.0.
> None for this release.
> HA Commands - New in Release 12.0
> The following HA commands are new in Release 12.0.
> None for this release.
> Mobility Management Entity Commands - New in Release 12.0
> The following Mobility Management Entity (MME) commands are new in Release 12.0.
> show lte-policy
> The show lte-policy command is new in release 12.0 and is a direct replacement for the obsolete command show mme-policy.
> CLI (Exec Mode)
> show lte-policy { ho-restriction-list { name name | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary }} [ | { grep grep_options | more } ]
> show sctp-param-template
> The show sctp-param-template command is new in release 12.0. The output of this command displays configuration information for SCTP parameter templates configured on the system.
> CLI (Exec Mode)
> show sctp-param-template { all | name temlate_name } { | grep grep_options | more } ]
> NAT Commands - New in Release 12.0
> The following NAT commands are new in Release 12.0.
> show active-charging analyzer statistics name h323 verbose
> This command displays active charging protocol analyzer statistics for H323 analyzer. The output of this command includes the following new fields:

> l | H323 Session Stats

> l | Total Uplink Bytes

> l | Total Downlink Bytes

> l | Total Uplink Packets

> l | Total Downlink Packets

> l | Total H323 calls

> l | Total RAS messages

> l | Total Q931 messages

> l | Total H245 messages

> l | RAS messages

> l | GatekeeperRequest

> l | GatekeeperConfirm

> l | GatekeeperReject

> l | RegistrationRequest

> l | RegistrationConfirm

> l | RegistrationReject

> l | UnregistrationRequest

> l | UnregistrationConfirm

> l | AdmissionRequest

> l | UnregistrationReject

> l | AdmissionRequest

> l | AdmissionConfirm

> l | AdmissionReject

> l | LocationRequest

> l | LocationConfirm

> l | LocationReject

> l | DisengageRequest

> l | DisengageConfirm

> l | DisengageReject

> l | InfoRequest

> l | InfoRequestResponse

> l | RequestInProgress

> l | Unclassified

> l | Q931 messages

> l | Alerting

> l | CallProceeding

> l | Setup

> l | Connect

> l | ReleaseComplete

> l | Facility

> l | Progress

> l | Information

> l | Unclassified

> l | H245 messages

> l | OpenLogicalChannel

> l | OpenLogicalChannelAck

> l | OpenLogicalChannelReject

> l | OpenLogicalChannelConfirm

> l | RequestChannelClose

> l | CloseLogicalChannel

> l | CloseLogicalChannelAck

> l | EndSessionCommand

> l | Unclassified

> CLI (Exec Mode)
> show active-charging analyzer statistics name h323 [ verbose ] ] [ | { grep grep_options | more } ]
> Packet Data Network Gateway Commands - New in Release 12.0
> This section provides information on new P-GW commands available in Release 12.0.
> clear local-policy
> Clears local QoS policy service statistics and counters found in show command outputs and bulk statistics associated with all local QoS policy services or a specific service defined by the parameter in this command.
> CLI (Exec Mode)
> clear local-policy statistics [ service service_name ]
> PDIF Commands - New in Release 12.0
> The following PDIF commands are new in Release 12.0.
> None for this release.
> PDSN Commands - New in Release 12.0
> The following PDSN commands are new in Release 12.0.
> show active-charging sessions full all
> The following keyword has been added to the command.

> l | full all

> CLI (Config Mode)
> show active charging sessions full all.
> Serving Gateway Commands - New in Release 12.0
> The following commands are new in Release 12.0.
> show lte-policy
> The show lte-policy command is new in release 12.0 and is a direct replacement for the obsolete command show mme-policy. The S-GW now supports commands in the LTE Policy Configuration Mode.
> CLI (Exec Mode)
> show lte-policy { ho-restriction-list { name name | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary }} [ | { grep grep_options | more } ]
> SGSN Commands - New in Release 12.0
> The following SGSN commands are new in Release 12.0.
> clear sgsn-pool statistics
> The following command clears statistics collected for monitoring the number of subscribers offloaded to a target NRI.
> CLI (Exec Mode)
> clear sgsn-pool statistics { gprs-service <service_name> | sgsn-service <service_name> } { nri-value <0 - 63> | peer-non-broadcast-lac <1 - 65535> rac <0 - 255> | target-offloaded-to-peer [ target-nri <0 - 63> ] }
> show sgsn-pool statistics
> The following command displays statistics collected for monitoring the number of subscribers offloaded to a target NRI.
> CLI (Exec Mode)
> show sgsn-pool statistics { gprs-service <service_name> | sgsn-service <service_name> } { nri-value <0 - 63> | peer-non-broadcast-lac <1 - 65535> rac <0 - 255> | target-load-in-progress [ smgr-instance <1 - 230> | target-nri <0 - 63> ] | target-offloaded-to-peer [ target-nri <0 - 63> ] }
> Modified Commands
> This section identifies performance management commands modified in Release 12.0.

> l | Common Commands - Modified in Release 12.0

> l | Application Detection and Control Commands - Modified in Release 12.0

> l | Content Filtering Commands - Modified in Release 12.0

> l | ECS Commands - Modified in Release 12.0

> l | Firewall Commands - Modified in Release 12.0

> l | GGSN Commands - Modified in Release 12.0

> l | HA Commands - Modified in Release 12.0

> l | HSGW Commands - Modified in Release 12.0

> l | Mobility Management Entity Commands - Modified in Release 12.0

> l | NAT Commands - Modified in Release 12.0

> l | Packet Data Network Gateway Commands - Modified in Release 12.0

> l | PDIF Commands - Modified in Release 12.0

> l | PDSN Commands - Modified in Release 12.0

> l | Session Control Manager Commands - Modified in Release 12.0

> l | SGSN Commands - Modified in Release 12.0

> l | TPO Commands - Modified in Release 12.0

> Common Commands - Modified in Release 12.0
> The following common commands have been modified in Release 12.0.
> clear dns-client
> The clear dns-client command has two new query-type keywords in release 12.0: AAAA and NAPTR. These keywords clear filtered DNS results based on 128-bit domain IPv6 addresses (AAAA resource records) or on Naming Authority Pointer records (NAPTR).
> CLI (Exec Mode)
> clear dns-client name { cache client name [ query-name name | query-type { A | AAAA | NAPTR | SRV } ] | statistics }
> logging filter active facility
> The logging filter active facility command adds the ability to generate logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the logging filter active facility command in release 12.0: event-notif.
> CLI (Exec Mode)
> logging filter active facility facility
> logging filter runtime facility
> The logging filter runtime facility command adds the ability to generate logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the logging filter runtime facility command in release 12.0: event-notif.
> CLI (Global Configuration Mode)
> logging filter runtime facility facility
> monitor protocol
> The monitor protocol command adds the ability to monitor four new protocols in release 12.0: SSCOP, SSCFNNI, PHS (Payload Header Suppression), and PPPOE.
> CLI (Exec Mode)
> monitor protocol
> save logs facility
> The save logs facility command adds the ability to save logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the save logs facility command in release 12.0: event-notif.
> CLI (Exec Mode)
> save logs facility facility
> show aaa group name
> This command is used to view AAA statistics for the current context. The output of this command includes a new field “Fire-and-Forget” to display whether or not the Fire-And-Forget feature is enabled in the AAA Group configuration.
> CLI (Exec Mode)
> show aaa { group { all | name aaa_group_name } | local counters } [ | { grep grep_options | more } ]
> show active-charging analyzer statistics name pptp
> This command displays active charging protocol analyzer statistics for the PPTP analyzer. The output of this command includes the following new fields to display PPTP-GRE traffic statistics:

> l | ACS PPTP-GRE Session Stats

> l | Total Uplink Bytes

> l | Total Downlink Bytes

> l | Total Uplink Pkts

> l | Total Downlink Pkts

> CLI (Exec Mode)
> show active-charging analyzer statistics name sip [ verbose ] ] [ | { grep grep_options | more } ]
> show active-charging flows type p2p
> This command displays active charging protocol analyzer statistics for the PPTP analyzer. The following data transport protocols are added:

> l | (I) - ICMP and ICMPv6

> l | (G) - GREv1

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> show active-charging service all
> This command displays ACS service details. The output of this command includes the following new fields:

> l | Server Unreachable Failure-Handling

> l | Initial-Request

> l | Update-Request

> CLI (Exec Mode)
> show active-charging service { all | name service_name } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays active charging statistics for ACS sessions. The output of the following commands includes the new field “Current PPTP-GRE Sessions”.

> l | show active-charging sessions summary

> l | show active-charging sessions summary type p2p

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full
> This command displays active charging statistics for ACS sessions. The output of this command includes the following new field:

> l | Current PPTP-GRE Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full all
> This command displays ACS session statistics. The output of this command includes the following new fields:

> l | CCR-I Server Unreachable Handling

> l | CCR-U Server Unreachable Handling

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging subsystem all
> This command displays active statistics for ACS sessions. The output of this command includes the following new fields:

> l | Total PPTP-GRE flows

> l | Current PPTP-GRE flows

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> show apn name
> This command is used to display configuration information for either a specific or all configured APNs. The output of this command includes a new field “Radius Secondary Group” to indicate the secondary Accounting group configured in the APN configuration.
> CLI (Exec Mode)
> show apn { all | name apn_name } [ | { grep grep_options | more } ]
> show diameter route table
> This command displays the Diameter routing table. The output of this command has been modified to display the dynamic routes with a flag ‘D’.
> CLI (Exec Mode)
> show diameter route table [ wide ] [ endpoint endpoint_name ] [ | { grep grep_options | more } ]
> show diameter statistics
> This command displays the Diameter peer statistics. The output of this command includes the following new fields.

> l | Dynamic Route statistics

> l | Adds

> l | Add Failures

> l | Removes

> l | Hits

> l | Expires

> CLI (Exec Mode)
> show diameter statistics [ [ proxy ] | endpoint endpoint_name [ peer-host peer_id [ peer-realm realm_id ] ] ] [ | { grep grep_options | more } ]
> show dns-client
> The show dns-client command has two new query-type keywords in release 12.0: AAAA and NAPTR. These keywords filter DNS results based on 128-bit domain IPv6 addresses (AAAA resource records) or on Naming Authority Pointer records (NAPTR).
> CLI (Exec Mode)
> show dns-client { cache client name [ query-name name | query-type { A | AAAA | NAPTR | SRV } ] | statistics client name } [ | { grep grep_options | more } ]
> show ims-authorization policy-control statistics server
> Displays information and statistics specific to the policy control in IP Multimedia Subsystem (IMS) authorization service. This command has been enhanced to display IPv6 address in addition to IPv4 address in Release 12.0.
> CLI (Exec Mode)
> show ims-authorization policy-control statistics [ service ims_auth_svc_name | server { ip-address ip_address [ port port_value ] | name server_name } ] [ | { grep grep_options | more } ]
> show logs facility
> The show logs facility command adds the ability to display logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the show logs facility command in release 12.0: event-notif.
> CLI (Exec Mode)
> show logs facility facility
> show session subsystem facility aaamgr
> Shows information for subscriber sessions defined by the specified keywords. The output of this command includes the following new fields to track the number of secondary accounting requests in the AAAMgr instance.

> l | Total radius sec acct requests

> l | Current radius sec acct requests

> l | Total radius sec acct cancelled

> l | Total radius sec acct purged

> l | Total radius sec acct requests retried

> CLI (Exec Mode)
> show session subsystem facility aaamgr { all | instance | verbose } [ | { grep grep_options | more } ]
> show srp
> This command displays the Service Redundancy Protocol information. The following keywords have been added:

> l | active

> l | standby

> l | diameter

> CLI (Exec Mode)
> show srp { call-loss statistics | checkpoint statistics [ active | standby ] [ verbose ] | info | monitor [ all | authentication-probe | bgp | diameter ] | statistics } | [ grep grep_options | more ]
> show subscribers configuration username
> Shows information for subscriber sessions defined by the specified keywords. The output of this command includes a new field “Radius Secondary Group” to indicate the secondary Accounting group configured in the Subscriber configuration.
> CLI (Exec Mode)
> show subscribers configuration { all | username user_name } [ | { grep grep_options | more } ]
> show subscribers full all
> Shows information for subscriber sessions defined by the specified keywords. The output of this command includes a new field “AAA Radius Secondary group” to indicate the secondary Accounting group configured in the Subscriber configuration.
> CLI (Exec Mode)
> show subscribers full all [ | { grep grep_options | more } ]
> Application Detection and Control Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> clear active-charging analyzer statistics
> This command supports the clearing of protocol analyzer statistics for the following P2P applications:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (Exec Mode)
> clear active-charging charging-action statistics [ name string ] [ | { grep grep_options | more } ]
> show active-charging analyzer statistics name p2p verbose
> This command displays Active Charging protocol analyzer statistics for the P2P protocol analyzer. The output of this command includes the following new fields to display the uplink/downlink bytes and uplink/downlink packets for the following protocols:

> l | Blackberry

> l | Gmail

> l | iTunes

> l | MySpace

> l | TeamViewer

> l | Twitter

> l | Viber

> l | Yahoo-video

> l | Oscar-video

> l | Gtalk-video

> CLI (Exec Mode)
> show active-charging analyzer statistics name p2p [ verbose ] [ | { grep grep_options | more } ]
> show active-charging flows
> This command displays the information for the active charging flows. The P2P protocol type flows now support the following applications:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays statistics for ACS sessions. The P2P protocol type flows now support the following applications:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions summary
> This command displays statistics for specific active charging service sessions. The output of this command includes the following new fields:

> l | Current BLACKBERRY Sessions

> l | Current GMAIL Sessions

> l | Current ITUNES Sessions

> l | Current MYSPACE Sessions

> l | Current TEAMVIEWER Sessions

> l | Current TWITTER Sessions

> l | Current VIBER Sessions

> l | Current YAHOO Video Sessions

> l | Current OSCAR Video Sessions

> l | Current GTALK Video Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions summary type p2p
> This command displays summary information for P2P active charging service sessions. The output of this command includes the following new fields:

> l | Current BLACKBERRY Sessions

> l | Current GMAIL Sessions

> l | Current ITUNES Sessions

> l | Current MYSPACE Sessions

> l | Current TEAMVIEWER Sessions

> l | Current TWITTER Sessions

> l | Current VIBER Sessions

> l | Current YAHOO Video Sessions

> l | Current OSCAR Video Sessions

> l | Current GTALK Video Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> Content Filtering Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> ECS Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> clear active-charging tcp-proxy statistics
> This command clears TCP Proxy related statistics. The socket-migration keyword was added to this command. This enables to clear TCP Proxy Socket Migration related statistics.
> CLI (Exec Mode)
> clear active-charging tcp-proxy statistics [ all | ip-layer | rulebase rulebase_name | socket-migration | tcp-layer ]
> show active-charging flows full
> This command displays active-charging flow information. The output of this command now includes the following TCP Proxy Socket Migration related fields:

> l | Socket Migration Details:

> l | State

> l | Highest ACK Frm Server

> l | Highest Seq Frm Server

> l | Highest ACK Frm MS

> l | Highest Seq Frm MS

> l | Seq Frm MS at Mig

> l | ACK Frm MS at Mig

> l | Seq Frm Server at Mig

> l | ACK Frm Server at Mig

> l | Data To Be Delivered To MS

> l | Data To Be Delivered To Server

> l | Highest Seq Frm MS

> l | Timestamps Enabled

> l | SACK Enabled

> l | Wscale From MS

> l | Wscale From Server

> CLI (Exec Mode)
> show active-charging flows full
> show active-charging tcp-proxy statistics
> This command displays TCP Proxy related statistics. The socket-migration keyword was added to this command. This enables to view TCP Proxy statistics for socket migration.
> CLI (Exec Mode)
> show active-charging tcp-proxy statistics [ all | ip-layer | rulebase rulebase_name | socket-migration | tcp-layer ] [ verbose ] [ | { grep grep_options | more } ]
> Firewall Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> clear active-charging firewall statistics
> This command clears Active Charging Firewall statistics. The following keywords were added to this command:

> l | icmpv6

> l | ipv6

> CLI (Exec Mode)
> clear active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ | { grep grep_options | more } ]
> clear subscribers
> This command disconnects subscribers based on specified criteria.The following keywords were added to this command:

> l | ipv4

> l | ipv6

> CLI (Exec Mode)
> clear subscribers [ keywords ] [ verbose ] [ -noconfirm ]
> show active-charging firewall statistics
> This command displays Active Charging Firewall statistics. The following keywords were added to this command:

> l | icmpv6

> l | ipv6

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics verbose
> This command displays Active Charging Stateful Firewall statistics. The output of this command includes the following new ICMPv6 and IPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> l | IPv6 Stats:

> l | Land Attacks

> l | Jolt Attacks

> l | Teardrop Attacks

> l | Invalid IP Option Length

> l | IPv6 Source-router Attacks

> l | Packets with Short IPv6 Header Length

> l | Packets with Nested Fragmentation Header

> l | Packets with Unspecified IPv6 Address

> l | Packets with invalid Payload Length

> l | Packets with more than threshold Extension Headers

> l | Packets with invalid Hop By Hop Extension Header

> l | Packets with ICMPv4 in IPv6 Header

> l | Packets with invalid Destination Extension Header

> l | Downlink Dropped Bytes on IPv6 Reassembly Failure

> l | Uplink Dropped Bytes on IPv6 Reassembly Failure

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics callid <call_id> verbose
> This command displays Active Charging Stateful Firewall statistics with Call ID. The output of this command includes the following new ICMPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics domainname <domain_name> verbose
> This command displays Active Charging Stateful Firewall statistics with Domain name. The output of this command includes the following new ICMPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics username <user_name> verbose
> This command displays Active Charging Stateful Firewall statistics with Username. The output of this command includes the following new ICMPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics protocol icmpv6 verbose
> This command displays Active Charging Stateful Firewall statistics for ICMPv6 protocol. The output of this command includes the following new ICMPv6 statistics:

> l | Firewall Statistics for Protocol: ICMPv6

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> l | Data Stats:

> l | Total Packets Received

> l | Total Bytes Received

> l | Total Packets Sent

> l | Total Bytes Sent

> l | Total Packets Injected

> l | Total Bytes Injected

> l | Uplink Packets Dropped

> l | Uplink Bytes Dropped

> l | Downlink Packets Dropped

> l | Downlink Bytes Dropped

> l | Total Malformed Packets

> l | Total DOS Attacks

> l | Total Flows Processed by Firewall

> l | Total NAT Flows Processed by Firewall

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics protocol ipv6 verbose
> This command displays Active Charging Stateful Firewall statistics for IPv6 protocol. The output of this command includes the following new IPv6 statistics:

> l | Firewall Statistics for Protocol: IPv6

> l | IPv6 Stats:

> l | Land Attacks

> l | Jolt Attacks

> l | Teardrop Attacks

> l | Invalid IP Option Length

> l | IPv6 Source-router Attacks

> l | Packets with Short IPv6 Header Length

> l | Packets with Nested Fragmentation Header

> l | Packets with Unspecified IPv6 Address

> l | Packets with invalid Payload Length

> l | Packets with more than threshold Extension Headers

> l | Packets with invalid Hop By Hop Extension Header

> l | Packets with ICMPv4 in IPv6 Header

> l | Packets with invalid Destination Extension Header

> l | Downlink Dropped Bytes on IPv6 Reassembly Failure

> l | Uplink Dropped Bytes on IPv6 Reassembly Failure

> l | Data Stats:

> l | Total Packets Received

> l | Total Bytes Received

> l | Total Packets Sent

> l | Total Bytes Sent

> l | Total Packets Injected

> l | Total Bytes Injected

> l | Uplink Packets Dropped

> l | Uplink Bytes Dropped

> l | Downlink Packets Dropped

> l | Downlink Bytes Dropped

> l | Total Malformed Packets

> l | Total DOS Attacks

> l | Total Flows Processed by Firewall

> l | Total NAT Flows Processed by Firewall

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging fw-and-nat policy name
> This command displays Firewall-and-NAT Policy information. The output of this command includes the following new fields:

> l | IPv6 Extension Headers Limit

> l | IPv6 Hop By Hop Options

> l | Hop By Hop Router Alert Option

> l | Hop By Hop Jumbo Payload Option

> l | Invalid Hop By Hop Options

> l | Unknown Hop By Hop Options

> l | IPv6 Destination Options

> l | Invalid Destination Options

> l | Unknown Destination Options

> l | IPv6 Nested Fragmentation

> CLI (Exec Mode)
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy_name } [ service name acs_service_name ] } | { statistics { all | name fw_nat_policy_name } } } [ | { grep grep_options | more } ]
> show active-charging fw-and-nat policy name
> This command displays Firewall-and-NAT Policy information. The output of this command includes the following new fields:

> l | Firewall Status IPv4

> l | Firewall Status IPv6

> CLI (Exec Mode)
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy_name } [ service name acs_service_name ] } | { statistics { all | name fw_nat_policy_name } } } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays statistics for ACS sessions. The following keywords were added to this command:

> l | ipv4

> l | ipv6

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging subsystem all
> This command displays service and configuration counters for the active charging service. The output of this command includes the following new fields:

> l | Firewall IPv4

> l | Firewall IPv6

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> show subscribers
> This command displays all available subscriber information. The following keywords were added to this command:

> l | ipv4

> l | ipv6

> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> show subscribers full
> This command displays all available subscriber information. The output of this command includes the following new fields:

> l | Firewall-and-Nat Policy

> l | Firewall Policy IPv4

> l | Firewall Policy IPv6

> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> GGSN Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> HA Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> accounting [ roaming ]
> <command syntax>
> HSGW Commands - Modified in Release 12.0
> The following HSGW commands have been modified in Release 12.0.
> clear hsgw-service
> The keyword all has been removed from this command.
> CLI (Exec Mode)
> clear hsgw-service statistics [ name service_name ] [ | { grep grep_options | more } ]
> show hsgw-service
> The keywords statistics and pcf-status have been added to this command.
> CLI (Exec Mode)
> show hsgw-service { all | name service_name | statistics { all | name service _name } } [ pcf-status [ address IPv4_address | filter { all | icmp-monitored | no-calls | summary | up } ] [ | { grep grep_options | more } ]
> show mag-service
> The keyword ip-address has been added to this command.
> CLI (Exec Mode)
> show mag-service { all | name service_name | session [ all | callid id | counters | full | ip-address home_ip_address | msid id | summary | username name ] | statistics [ name service_name ] } [ | { grep grep_options | more } ]
> Mobility Management Entity Commands - Modified in Release 12.0
> The following Mobility Management Entity (MME) commands are modified in Release 12.0.
> None for this release.
> NAT Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> show active-charging sessions full
> This command displays statistics for ACS sessions. The output of this command includes the following new field:

> l | Current H323 Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full all
> This command displays statistics for ACS sessions. The output of this command includes the following new field:

> l | Current H323 Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging subsystem all
> This command displays service and configuration counters for the active charging service. The output of this command includes the following new fields:

> l | Total H323 Flows

> l | Current H323 Flows

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> Packet Data Network Gateway Commands - Modified in Release 12.0
> The following P-GW commands have been modified in Release 12.0.
> clear apn statistics
> The keyword smgr-instance has been added to this command.
> CLI (Exec Mode)
> clear apn statistics [ name apn_name | smgr-instance instance ] [ | { grep grep_options | more } ]
> clear pgw-service
> The keyword all has been removed from this command.
> CLI (Exec Mode)
> clear pgw-service statistics [ name service_name ] [ | { grep grep_options | more } ]
> show crypto ipsec security-associations
> The output of this command now includes the Diffie-Hellman group for each IPSec security association.
> CLI (Exec Mode)
> show crypto ipsec security-associations
> show pgw-service
> The keyword verbose has been added to this command.
> CLI (Exec Mode)
> show pgw-service { all | name service_name | statistics { all | name service_name } [ verbose ] } [ | { grep grep_options | more } ]
> PDIF Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> PDSN Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> Session Control Manager Commands - Modified in Release 12.0
> The following SCM commands have been modified in Release 12.0.
> show cscf tcp
> The keywords msrp and sip have been added to this command.
> CLI (Exec Mode)
> show cscf tcp connections service service_name [ facility { cscfmgr | sessmgr } ] [ full ] [ msrp ] [ remote-ip ip_address ] [ remote-port port_number ] [ sip ] [ | { grep grep_options | more } ]
> SGSN Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0 - unless otherwise indicated, the listed fields have been added to the output displays:
> show apn-profile full name <profile_name>

> l | APN Name

> l | Quality of Service Capping

> l | Prefer Type

> l | Traffic Class

> l | SDU delivery order

> l | Delivery Of Erroneous Sdus

> l | Convert Max Bit Rate Uplink From

> l | Convert Max Bit Rate Downlink From

> l | SDU Max Size

> l | DNS Extension with LAC-RAC

> show apn-remap-table full name

> l | Fallback APN to use when Default APN not present in subscription

> show bssgp statistics

> l | packets dropped due to clearing subscriber

> show call-control-profile full all

> l | PTMSI-Signature-Realloc Attach Access-Type

> l | PTMSI-Signature-Realloc Attach Frequency value UMTS

> l | PTMSI-Signature-Realloc Attach Frequency value GPRS

> l | PTMSI-Signature-Realloc Interval Access-Type

> l | PTMSI-Signature-Realloc Interval value UMTS

> l | PTMSI-Signature-Realloc Interval value GPRS

> l | PTMSI-Signature-Realloc Frequency Access-Type

> l | PTMSI-Signature-Realloc Frequency value UMTS

> l | PTMSI-Signature-Realloc Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU(Generic)Access-Type

> l | PTMSI-Signature-Realloc RAU(Generic) Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU(Generic) Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU Periodic Access-Type

> l | PTMSI-Signature-Realloc RAU Periodic Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU Periodic Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU RA Update Access-Type

> l | PTMSI-Signature-Realloc RAU RA Update Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU RA Update Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU Combined Update Access-Type

> l | PTMSI-Signature-Realloc RAU Combined Update Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU Combined Update Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU Imsi Combined Update Access-Type

> l | PTMSI-Signature-Realloc RAU Imsi Combined Update Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU Imsi Combined Update Frequency value GPRS

> l | Authentication SMS

> l | Authentication SMS Access-Type

> l | Authentication SMS Frequency

> l | Authentication SMS (MO-SMS)

> l | Authentication SMS (MO-SMS) Access-Type

> l | Authentication SMS (MO-SMS) Frequency

> l | Authentication SMS (MT-SMS)

> l | Authentication SMS (MT-SMS) Access-Type

> l | Authentication SMS (MT-SMS) Frequency

> show gmm-sm statistics verbose

> l | irat-att-dsd-rcvd-in-2g

> l | irat-att-cl-sub-in-2g

> l | pac-drop-att-rau-ongoing

> l | ActivateContextRequest

> l | Total-Actv-Request

> l | 3G-Actv-Request

> l | 2G-ActvRequest

> l | Primary-Actv-Request

> l | 3G-Primary-Actv-Request

> l | 2G-Primary-Actv-Request

> l | Secondary-Actv-Request

> l | 3G-Secondary-Actv-Request

> l | 2G-Secondary-Actv-Request

> l | Actv-Request-Nrpca

> l | Actv-Request-Mbms

> l | ActivateContextAccept

> l | Total-Actv-Accept

> l | 3G-Actv-Accept

> l | 2G-ActvAccept

> l | Primary-Actv-Accept

> l | 3G-Primary-Actv-Accept

> l | 2G-Primary-Actv-Accept

> l | Secondary-Actv-Accept

> l | 3G-Secondary-Actv-Accept

> l | 2G-Secondary-Actv-Accept

> l | Actv-Mbms-Accept

> l | 3G-Actv-Mbms-Accept

> l | ActivateContextReject

> l | Total-Actv-Reject

> l | 3G-Actv-Reject

> l | 2G-Actv-Reject

> l | Primary-Actv-Reject

> l | 3G-Primary-Actv-Reject

> l | 2G-Primary-Actv-Reject

> l | Secondary-Actv-Reject

> l | 3G-Secondary-Actv-Reject

> l | 2G-Secondary-Actv-Reject

> l | RequestPdpContextActivationReject

> l | Total-Request-Pdp-Ctxt-Reject

> l | 3G-Request-Pdp-Ctxt-Reject

> l | 2G-Request-Pdp-Ctxt-Reject

> show gprsns statistics

> l | Number of ns-block dropped due to invalid nsvc

> l | Number of ns-block-ack dropped due to invalid nsvc

> l | Number of ns-status dropped due to invalid nsvc

> show gprs-service name
> The following field has been removed as it is not configurable:

> l | GMM LLC MAX Retries

> show session disconnect-reasons
> The following SGSN-supported session disconnect reasons are new in this release:

> l | sgsn-ard-failure(436)

> l | sgsn-camel-release(437)

> l | sgsn-zone-code-failure(455)

> The following session disconnect reasons are visible in this release but are in development for a future release:

> l | sgsn-egtpc-connection-failed(438)

> l | sgsn-egtpc-create-session-failed(439)

> l | sgsn-hss-detach(440)

> l | sgsn-hss-connection-failure(441)

> l | sgsn-pgw-detach(442)

> l | sgsn-s5-not-supported-for-apn(443)

> l | sgsn-no-rab-for-gbr-bearer(444)

> l | sgsn-sgw-selection-failure(445)

> l | sgsn-pgw-selection-failure(446)

> show sgtpc statistics verbose

> l | Note Ms Gprs Present Req Denied:

> l | Mandatory IE Incorrect

> l | Mandatory IE Missing

> l | Optional IE Incorrect

> l | Invalid Message Format

> show sgtp-service all

> l | GTP-C IP QOS DSCP value

> l | Gn Delay Monitoring

> l | Response wait time

> l | Delay responses to flag delay

> l | Normal responses to clear delay

> show snmp trap statistics verbose

> l | SGSNGnMsgDelay

> l | SGSNGnMsgDelayClear

> show ss7-routing-domain <ss7rd_id> mtp2 statistics linkset all link all

> l | Number of SIN packets transmitted

> l | Number of SIE packets transmitted

> l | Number of SIOS packets transmitted

> l | Number of SIPO packets transmitted

> l | Number of SIB packets transmitted

> l | Number of SIN packets received

> l | Number of SIE packets received

> l | Number of SIOS packets received

> l | Number of SIPO packets received

> l | Number of SIB packets received

> TPO Commands - Modified in Release 12.0
> The following Traffic Performance Optimizer (TPO) have been modified in release 12.0.
> show active-charging tpo profile statistics
> This command displays TPO profile statistics. The output of this command includes the following new fields:

> l | Number of times TPO is disabled by P2P

> l | Number of times the TPO profile is selected

> CLI (Exec Mode)
> show active-charging tpo profile statistics [ name tpo_profile_name | all ] [ | { grep grep_options | more } ]
> Obsolete Commands
> This section identifies performance management commands obsoleted in Release 12.0.

> l | Common Commands - Obsolete in Release 12.0

> l | Application Detection and Control Commands - Obsolete in Release 12.0

> l | Content Filtering Commands - Obsolete in Release 12.0

> l | ECS Commands - Obsolete in Release 12.0

> l | Firewall Commands - Obsolete in Release 12.0

> l | GGSN Commands - Obsolete in Release 12.0

> l | HA Commands - Obsolete in Release 12.0

> l | NAT Commands - Obsolete in Release 12.0

> l | PDSN Commands - Obsolete in Release 12.0

> l | SGSN Commands - Obsolete in Release 12.0

> Common Commands - Obsolete in Release 12.0
> The following common commands are now obsolete in Release 12.0.
> save logs facility
> CLI (Exec Mode)
> save logs facility facility
> Application Detection and Control Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Content Filtering Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> ECS Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Firewall Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> GGSN Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Mobility Management Entity - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> show mme-policy
> The show mme-policy command is no longer available in release 12.0 It has been replaced with the show lte-policy command.
> CLI (Exec Mode)
> show mme-policy { ho-restriction-list { name name | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary }} [ | { grep grep_options | more } ]
> HA Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> NAT Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> PDSN Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> SGSN Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> GTPP Storage Server Changes
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Web Element Manager Changes
> There were no Web Element Manager changes in Release 12.0.
> There were no Web Element Manager changes in Release 12.1.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883