> PCC-Usage-Monitor Configuration Mode Commands
> The PCC-Usage-Monitor Configuration mode provides a mechanism to set the usage threshold limit in a PCC-Service-Profile to trigger required condition and action set in PCC-Service instance.
> Important: This configuration mode is supported from StarOS Release 12.1 onward.
> usage-limit volume
> This command sets the usage limit in volume for subscriber profile for a PCC-Service-Profile on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> usage-limit volume [downlink dlink_volume | total total_volume | uplink uplink_volume]
> [default] usage-limit volume [downlink | total | uplink]
> default
> Sets the usage limit volume to ‘0’ for downlink, uplink and total bucket in a PCC-Service-Profile in IPCF configuration.
> downlink dlink_volume
> Default: 0
> Specifies the usage volume in KiloBytes in downlink direction (from PCEF to UE) in a PCC-Service-Profile on IPCF node.
> The dlink_volume is volume limit in KiloBytes for downlink traffic and must be an integer from 1 through 4294967296. A ‘zero’ value disables the downlink volume usage limit and sets the usage limit volume to ‘0’.
> total total_volume
> Default: 0
> Specifies the usage volume in KiloBytes in downlink and uplink direction (from PCEF to UE and PCEF to PDN) in a PCC-Service-Profile on IPCF node.
> The total_volume is volume limit in KiloBytes for total traffic and must be an integer from 1 through 4294967296. A ‘zero’ value disables the uplink volume usage limit and sets the usage limit volume to ‘0’.
> uplink uplink_volume
> Default: 0
> Specifies the usage volume in KiloBytes in uplink direction (from PCEF to PDN) in a PCC-Service-Profile on IPCF node.
> The uplink_volume is volume limit in KiloBytes for uplink traffic and must be an integer from 1 through 4294967296. A ‘zero’ value disables the uplink volume usage limit and sets the usage limit volume to ‘0’.
> Usage
> Use this command to set the usage limit in volume for subscriber profile for a PCC-Service-Profile on IPCF node.
> Example
> Following command sets the usage limit volume to 20000 KiloBytes in upload direction with in a PCC-Service-Profile.
> usage-limit volume uplink 20000
> Following command sets the usage limit volume to 400000 KiloBytes in download direction with in a PCC-Service-Profile.
> usage-limit volume downlink 400000

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883