> LTE TAI Management Object Configuration Mode Commands
> The LTE TAI Management Object Configuration Mode is used to create and manage the LTE Tracking Area Identifiers for the TAI database.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> sgw-address
> Configures an S-GW IP address, supported S5/S8 protocol type, and selection weight used in a pool for S-GW selection.
> Product
> MME
> Privilege
> Administrator
> Syntax
> sgw-address ipv4_or_ipv6_address s5-s8-protocol { both | gtp | pmip } weight number
> no sgw-address ipv4_or_ipv6_address s5-s8-protocol { both | gtp | pmip }
> no sgw-address ipv4_or_ipv6_address s5-s8-protocol { both | gtp | pmip }
> Removes the configured S-GW address from this TAI management object.
> ipv4_or_ipv6_address
> Specifies the IP address of the S-GW in the selection pool. ipv4_or_ipv6_address must be entered in dotted decimal notation (for IPv4 addresses) or colon-separated hexidecimal notation (for IPv6 addresses).
> Up to 32 S-GW address can be configured per TAI management object.
> s5-s8-protocol { both | gtp | pmip }
> Specifies the S5/S8 interface type found between the configured S-GW and the P-GW.
> both: Specifies that both the GTP and PMIP protocols are supported over the S5/S8 interface.
> gtp: Specifies that the GTP protocol is supported over the S5/S8 interface.
> pmip: Specifies that the PMIP protocol is supported over the S5/S8 interface.
> weight number
> Specifies the priority or weight of the S-GW address used during weighted round-robin selection within this TAI management object. number must be an integer value from 1 to 100.
> Usage
> Use this command to configure a pool of S-GW addresses used for S-GW selection.
> Example
> The following command configures an S-GW with an IPv4 address of 1.2.3.4, a supported S5/S8 protocol type of GTP, and a selection weight of 3:
> sgw-address 1.2.3.4 s5-s8-protocol gtp weight 3
> tai
> Configures a Tracking Area Identifier (TAI) for this TAI management object.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] tai mcc number mnc number { tac value } +
> no
> Removes a configured TAI from the TAI management object.
> mcc number
> Specifies the mobile country code (MCC) portion of a PLMN‘s identifier. number must be an integer value between 100 and 999.
> mnc number
> Specifies the mobile network code (MNC) portion of a PLMN‘s identifier. number can be configured to any 2 or 3 digit integer value between 00 and 999
> tac value +
> Specifies the Tracking Area Code portion of the TAI. value must be an integer from 1 to 65535. Up to 16 TAC values can be entered on a single line.
> Usage
> Use this command to configure one or more TAIs for this management object. Up to 16 TAIs can be configured per management object.
> Example
> The following command adds a TAI to this management object with an MCC of 111, an MNC of 22, and a TAC value of 1001:
> tai mcc 122 mnc 22 tac 1001

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883