> show asnpc-service
> This chapter includes the show asnpc-service command output tables.
> show asnpc-service all
> show asnpc-service all Command Output Descriptions

> Field | Description
> Service name | The ASN GW service name.
> Context | The context in which the service is configured.
> Anchor PC ID | The anchor paging controller identifier.
> Bind | The bind status.
> Max Subscribers | The maximum number of subscribers.
> IP address | IP address of ASN GW server where this service is located.
> UDP Port | The UDP port number.
> Service Status | Status of this service.
> Maximum number of retransmissions | The maximum number of retransmissions.
> Maximum number of paging-announce retransmissions | The maximum number of paging-announce retransmissions.
> Retransmission timeout | The retransmission timeout duration.
> Setup timeout | The session setup timeout duration.
> Active-relay timeout | Indicates the timeout duration for active relay of R4 or R6 messages.
> Paging-announce timeout | Indicates the paging announce timeout duration in seconds.
> Paging-announce retransmission timeout | Indicates the paging announce retransmission timeout duration in seconds.
> Policy transaction-id-validation | Possible values are:
> • | ALLOW: Enforce tid validation procedure as per NWG specification, section 3.1.
> • | DISALLOW: Do not enforce tid validation procedure as per NWG specification, section 3.1.
> Policy zero-function-type | Possible values are:
> • | ALLOW: If configured, function type is not considered for transaction id generation/validation.
> • | DISALLOW: If configured, function type is considered for transaction id generation/validation.
> Transaction Id. Seed | If configured, initial value of tid is set to this configured value, otherwise, initial value of tid is set to a random number.
> Peer ASNGW address | The list of ASN GW IP addresses with which the PCLR is permitted to interact.
> Number of Paging Groups configured | The total number of paging groups configured for this service.
> Paging Group | The paging group ID associated with this service.
> Paging Offset | The offsets configured for the Paging Group.
> Number of MSIDs | The current total number of MNs assigned/using the offset.

> ‌
> show asnpc-service session all
> show asnpc-service session all Command Output Descriptions

> Field | Description
> CALLID | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> BS/PA Address | IP address of the base-station or paging agent.
> Session Type | Indicates the type of ASN PC session. Possible type of sessions are:
> • | Anchor
> • | Non-anchor
> Total ASNPC Sessions | The total number of ASN PC sessions on chassis including all modes.

> ‌
> show asnpc-service session full
> show asnpc-service session all Command Output Descriptions

> Field | Description
> Username | The subscriber’s user name.
> Callid | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> ASNPC Service Address | IP address of system where ASN PC service is running.
> BS/PA Address | IP address of the base-station or paging agent.
> BS ID | The identifier of base station. Generally it is MAC address of the BS.
> Authenticator Address | IP address of the authenticator ASN GW.
> DPF/ASNGW Address | IP address of the system where data path function/ASN GW service is running.
> Idle-mode timeout | Indicates the total configured timeout duration in seconds for an MS to enter the idle mode from active mode.
> Remaining Idle Mode Timeout | Indicates the remaining timeout duration in seconds for an MS to enter the idle mode from active mode.
> Paging Information
> Paging Cycle | Indicates the number of paging cycles happened in this ASN PC service session.
> Paging Offset | Indicates the paging offset for paging announce.
> Paging Group ID | Indicates the paging group identifier which contains the group of paging agents bounded with this paging controller session.
> Paging Interval | Interval time in seconds between two paging announces.
> MS Information
> Idle Mode Authorization Indication | Indicates the idle mode authorization status.
> SA Descriptor Information | Indicates the Security Association description information. SA descriptor is a compound attribute whose sub-attributes describe the properties of a Security Association (SA). These properties include the SA ID, the SA type, the SA service type, and the cryptographic suite employed within the SA.
> SA ID | Indicates the identifier for the security association.
> SA Type | Indicates the types of security association. Possible values are:
> Cryptographic Suite | Indicates the cryptographic suite employed within the security association. Possible values are:
> • | 0: Primary SA
> • | 1: Static SA
> • | 3: Dynamic SA
> • | 4. Group SA
> • | 5: MBS SA
> SA Service Type | Indicates the service types of the corresponding SA type. Possible values are:
> • | 0: Unicast service
> • | 1: Group multicast service
> • | 2: MBS service
> Note that this shall be defined only when SA type is Static SA or Dynamic SA.
> SA Index | Indicates the index of security association.
> Older/Newer TEK Parameters | Indicates the older or newer Traffic Encryption Key (TEK) parameters involved.
> TEK TLV (in hex) | Indicates the TEK total length value in hexadecimal.
> TEK Sequence Number | Indicates the TEK sequence number.
> TEK Lifetime | Indicates the TEK lifetime in seconds.
> PN Counter | Indicates the packet number counter in downlink direction that are used for encryption and decryption by the Base Station.
> RxPN Counter | Indicates the packet number counter in uplink direction that are used for encryption and decryption by the Base Station.
> Total ASNPC Sessions | The total number of ASN PC sessions on chassis including all modes.

> ‌
> show asnpc-service session counters verbose
> show asnpc-service session counters verbose Command Output Descriptions

> Field | Description
> Username | The subscriber’s user name.
> Callid | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> Message Groups
> R6 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R6 interface.
> R6 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R6 interface.
> R6 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R6 interface.
> R6 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R6 interface.
> R6 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R6 interface.
> R6 Location Update Request Msg | Groups the statistics of the Location Update Request messages on R6 interface.
> R6 Location Update Response Msg | Groups the statistics of the Location Update Response messages on R6 interface.
> R6 Location Update Confirm Msg | Groups the statistics of the Location Update Confirm messages on R6 interface.
> R6 Paging Announce Msg | Groups the statistics of the Paging Announce messages on R6 interface.
> R4 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R4 interface.
> R4 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R4 interface.
> R4 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R4 interface.
> R4 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R4 interface.
> R4 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R4 interface.
> R4 Network Exit MS State Change Request Msg | Groups the statistics of the Network Exit MS State Change Request messages on R4 interface.
> R4 Network Exit MS State Change Response Msg | Groups the statistics of the Network Exit MS State Change Response messages on R4 interface.
> R4 Delete MS Entry Request Msg | Groups the statistics of the Delete MS Entry Request messages on R4 interface.
> R4 Delete MS Entry Response Msg | Groups the statistics of the Delete MS Entry Response messages on R4 interface.
> R4 Initiate Paging Request Msg | Groups the statistics of the Initiate Paging Request messages on R4 interface.
> R4 Initiate Paging Response Msg | Groups the statistics of the Initiate Paging Response messages on R4 interface.
> R4 Anchor PC Ind Msg | Groups the statistics of the Anchor Paging Controller Indicator messages on R4 interface.
> R4 Anchor PC Ack Msg | Groups the statistics of the Anchor Paging Controller Ack messages on R4 interface.
> R4 Context Request Msg | Groups the statistics of the Context Request messages on R4 interface.
> R4 Context Report Msg | Groups the statistics of the Context Report messages on R4 interface.
> R6/R4 Unknown Messages | Groups the statistics of the Unknown type of messages on R6 and/or R4 interface.
> Message Statistics
> Total Sent | The total number of this type of message sent on specific interface.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Retransmissions Sent | The total number of this type of message re-transmitted on specific interface.
> Total Received | The total number of this type of message received on specific interface.
> Total Accepted | The total number of this type of message accepted on specific interface.
> Total Relayed | The total number of this type of message relayed on specific interface.
> Total Denied | The total number of this type of message denied on specific interface.
> Total Discarded | The total number of this type of message discarded on specific interface.
> Badly Formed | The total number of badly formed this type of message on specific interface.
> Decode Error | The total number of this type of message on specific interface with decode error.
> Unspecified Error | The total number of this type of message on specific interface with unspecified error.
> Paging Config Error | The total number of this type of errors messages on specified interface occurred. This error occurs when paging node id (BS id) is not configured in configured paging groups.
> Missing Mandatory TLV | The total number of this type of message on specific interface with missing mandatory TLVs.
> TLV Value Invalid | The total number of this type of message on specific interface with invalid TLV value.
> Unknown TLV | The total number of this type of message on specific interface with unknown TLVs.
> Duplicate TLV Found | The total number of this type of message on specific interface with duplicate TLVs.
> No session Found | The total number of this type of message on specific interface without any session information.
> Transaction Id. Error | The total number of this type of message on specific interface. with transaction id error.
> Data messages
> GRE R6 Receive | The total number of data message received with through GRE tunnel on R6 interface.
> GRE R4 Receive | The total number of data message received through GRE tunnel on R4 interface.
> Packets Received | The total number of data packets received/sent through GRE tunnel on R4/R6 interface.
> Bytes Received | The total number of data bytes received/sent through GRE tunnel on R4/R6 interface.
> Protocol Type Error | The total number of data message received/sent with protocol type error through GRE tunnel on R4/R6 interface.
> GRE Key Absent | The total number of data message received/sent without GRE key through GRE tunnel on R4/R6 interface.
> GRE Checksum Error | The total number of data message received/sent with checksum error through GRE tunnel on R4/R6 interface.
> Invalid Packet Length | The total number of data message received/sent with invalid packet length through GRE tunnel on R4/R6 interface.
> No Session found | The total number of data message received/sent without any session information through GRE tunnel on R4/R6 interface.
> Unspecified Error | The total number of data message received/sent with unknown error through GRE tunnel on R4/R6 interface.
> GRE R6 Send | The total number of data message sent through GRE tunnel on R6 interface.
> GRE R4 Send | The total number of data message sent through GRE tunnel on R4 interface.
> Packets Sent | The total number of data packets sent through GRE tunnel on R4/R6 interface.
> Send Error | The total number of data message sent with error through GRE tunnel on R4/R6 interface.
> Bytes Sent | The total number of data bytes sent through GRE tunnel on R4/R6 interface.

> ‌
> show asnpc-service statistics verbose
> show asnpc-service statistics verbose Command Output Descriptions

> Field | Description
> Message Groups
> R6 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R6 interface.
> R6 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R6 interface.
> R6 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R6 interface.
> R6 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R6 interface.
> R6 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R6 interface.
> R6 Location Update Request Msg | Groups the statistics of the Location Update Request messages on R6 interface.
> R6 Location Update Response Msg | Groups the statistics of the Location Update Response messages on R6 interface.
> R6 Location Update Confirm Msg | Groups the statistics of the Location Update Confirm messages on R6 interface.
> R6 Paging Announce Msg | Groups the statistics of the Paging Announce messages on R6 interface.
> R4 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R4 interface.
> R4 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R4 interface.
> R4 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R4 interface.
> R4 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R4 interface.
> R4 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R4 interface.
> R4 Initiate Paging Request Msg | Groups the statistics of the Initiate Paging Request messages on R4 interface.
> R4 Initiate Paging Response Msg | Groups the statistics of the Initiate Paging Response messages on R4 interface.
> R4 Location Update Request Msg | Groups the statistics of the Location Update Request messages on R4 interface.
> R4 Location Update Response Msg | Groups the statistics of the Location Update Response messages on R4 interface.
> R4 Location Update Confirm Msg | Groups the statistics of the Location Update Confirm messages on R4 interface.
> R4 Network Exit MS State Change Request Msg | Groups the statistics of the Network Exit MS State Change Request messages on R4 interface.
> R4 Network Exit MS State Change Response Msg | Groups the statistics of the Network Exit MS State Change Response messages on R4 interface.
> R4 Delete MS Entry Request Msg | Groups the statistics of the Delete MS Entry Request messages on R4 interface.
> R4 Delete MS Entry Response Msg | Groups the statistics of the Delete MS Entry Response messages on R4 interface.
> R4 Anchor PC Ind Msg | Groups the statistics of the Anchor Paging Controller Indicator messages on R4 interface.
> R4 Anchor PC Ack Msg | Groups the statistics of the Anchor Paging Controller Ack messages on R4 interface.
> R4 PC Relocation Ind Msg | Groups the statistics of the PC Relocation Ind messages on the R4 interface.
> R4 PC Relocation Ack Msg | Groups the statistics of the PC Relocation Ack messages on the R4 interface.
> R4 Context Request Msg | Groups the statistics of the Context Request messages on R4 interface.
> R4 Context Report Msg | Groups the statistics of the Context Report messages on R4 interface.
> R4 CMAC Key Count Update Msg | Groups the statistics of the CMAC Key Count Update messages on the R4 interface.
> R4 CMAC Key Count Ack Msg | Groups the statistics of the CMAC Key Count Ack messages on the R4 interface.
> R6/R4 Unknown Messages | Groups the statistics of the Unknown type of messages on R6 and/or R4 interface.
> Message Statistics
> Total Sent | The total number of this type of message sent on specific interface.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Retransmissions Sent | The total number of this type of message re-transmitted on specific interface.
> Total Received | The total number of this type of message received on specific interface.
> Total Accepted | The total number of this type of message accepted on specific interface.
> Total Relayed | The total number of this type of message relayed on specific interface.
> Total Denied | The total number of this type of message denied on specific interface.
> Total Discarded | The total number of this type of message discarded on specific interface.
> Badly Formed | The total number of badly formed this type of message on specific interface.
> Decode Error | The total number of this type of message on specific interface with decode error.
> Unspecified Error | The total number of this type of message on specific interface with unspecified error.
> Missing Mandatory TLV | The total number of this type of message on specific interface with missing mandatory TLVs.
> TLV Value Invalid | The total number of this type of message on specific interface with invalid TLV value.
> Unknown TLV | The total number of this type of message on specific interface with unknown TLVs.
> Duplicate TLV Found | The total number of this type of message on specific interface with duplicate TLVs.
> No session Found | The total number of this type of message on specific interface without any session information.
> Transaction Id. Error | The total number of this type of message on specific interface. with transaction id error.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883