> GTP-C Schema Statistics
> The GTP-C schema provides operational statistics that can be used for monitoring and troubleshooting the following products: GGSN, P-GW, S-GW.
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the GTP-C Schema

> Variables | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the service. This is a key variable. Type: Information | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the service. This is an internal reference number. This is a key variable. Type: Information | Int32
> servname | The name of the service for which the statistics are displayed. This is a key variable. Type: Information | String
> setup-current | The total number of current sessions setup Type: Gauge | Int32
> current-ip | The total number of current IPv4 Sessions Type: Gauge | Int32
> current-ppp | The total number of current PPP sessions Type: Gauge | Int32
> current-ipv6 | The total number of current IPv6 Sessions Type: Gauge | Int32
> current-ntwkinitd | The total number of current Network initiated Sessions Type: Gauge | Int32
> setup-total | The total number of PDP contexts setup. | Int32
> setup-ip | The total number of IP PDP contexts setup. | Int32
> setup-ppp | The total number of PPP PDP contexts setup. | Int32
> setup-ipv6 | The total number of IPv6 sessions | Int32
> setup-sgsn | The total number of SGSN initiated sessions | Int32
> setup-ggsn | The total number of GGSN initiated sessions | Int32
> released-total | The total number of PDP contexts released. | Int32
> dyn-ipv4-attempt | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were attempted. | Int32
> dyn-ipv6-attempt | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were attempted. | Int32
> dyn-ipv4-success | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. | Int32
> dyn-ipv6-success | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. | Int32
> echo-req-rx | The total number of GTPC echo requests received. | Int32
> echo-req-tx | The total number of GTPC echo requests transmitted. | Int32
> gtpu-echo-req-rx | The total number of GTPU echo requests received. | Int32
> gtpu-echo-req-tx | The total number of GTPU echo requests transmitted. | Int32
> echo-rsp-tx | The total number of GTPC echo responses transmitted. | Int32
> echo-rsp-rx | The total number of GTPC echo responses received. | Int32
> gtpu-echo-rsp-tx | The total number of GTPU echo responses transmitted. | Int32
> gtpu-echo-rsp-rx | The total number of GTPU echo responses received. | Int32
> cpc-total | The total number of Create PDP Context Request messages received. This is the sum of GTPC v0 and GTP v1 messages. | Int32
> cpc-v0 | The total number of Create PDP Context Request messages received that used GTPC version 0. | Int32
> cpc-v1 | The total number of Create PDP Context Request messages received that used GTPC version 1. | Int32
> cpc-sec | The total number of Activate Secondary PDP Context Request received. | Int32
> cpc-retrans | The total number of re-transmitted Create PDP Context Request messages received from the SGSN for either the primary or secondary PDP contexts. | Int32
> cpc-accept | The total number of Create PDP Context Response messages transmitted containing a cause value of 128 (80H, Request accepted). | Int32
> cpc-deny | The total number of “reject” Create PDP Context Response messages transmitted. | Int32
> cpc-discard | The total number of Create PDP Context Request messages received from the SGSN(s) that were discarded. | Int32
> upc-rx | The total number of Update PDP Context Request messages received from the SGSN(s). | Int32
> upc-rx-accept | The total number of Update PDP Context Response messages transmitted to the SGSN(s) containing a cause value of 128 (80H, Request accepted). | Int32
> upc-rx-deny | The total number of “reject” Update PDP Context Response messages transmitted to the SGSN(s). | Int32
> upc-rx-discard | The total number of Update PDP Context Request messages received from SGSN(s) that were discarded | Int32
> upc-tx | The total number of Update PDP Context Request messages transmitted to the SGSN(s). | Int32
> upc-tx-accept | The total number of Update PDP Context Response messages sent to the SGSN(s) containing a cause value of 128 (80H, Request accepted). | Int32
> upc-tx-deny | The total number of “reject” Update PDP Context Response messages sent to the SGSN(s). | Int32
> upc-tx-dt-upd | The total number of Update PDP Context Response messages sent to SGSN(s) for direct tunnel update. | Int32
> dpc-rx | The total number of Delete PDP Context Request messages received from the SGSN(s). | Int32
> dpc-rx-accept | The total number of Delete PDP Context Response messages transmitted containing a cause value of 128 (80H, Request accepted). | Int32
> dpc-rx-deny | The total number of “reject” Delete PDP Context Response messages transmitted. | Int32
> dpc-rx-discard | The total number of Delete PDP Context Request messages received from the SGSN(s) that were discarded | Int32
> dpc-tx | The total number of Delete PDP Context Request messages transmitted to the SGSN(s). | Int32
> dpc-tx-accept | The total number of Delete PDP Context Response messages received from the SGSN(s) containing a cause value of 128 (80H, Request accepted). | Int32
> dpc-tx-deny | The total number of “reject” Delete PDP Context Response messages received from the SGSN(s). | Int32
> cpc-aa | The total number of Create AA (anonymous access) PDP Context Request messages received. | Int32
> cpc-aa-accept | The total number of Create AA PDP Context Response messages transmitted to the SGSN with a cause code of 128 (80H, Request accepted). | Int32
> cpc-aa-deny | The total number of “reject” Create AA PDP Context Response messages transmitted to the SGSN(s). | Int32
> cpc-aa-discard | The total number of Create AA PDP Context Request messages received that were discarded without transmitting a response to the SGSN(s). | Int32
> dpc-aa-rx | The total number of Delete AA PDP Context Request messages received from the SGSN(s). | Int32
> dpc-aa-rx-accept | The total number of Delete AA PDP Context Response messages transmitted containing a cause value of 128 (80H, Request accepted). | Int32
> dpc-aa-rx-deny | The total number of “reject” Delete AA PDP Context Response messages transmitted to the SGSN(s). | Int32
> dpc-aa-rx-discard | The total number of Delete PDP AA Context Request messages received from the SGSN(s) that were discarded | Int32
> dpc-aa-tx | The total number of Delete AA PDP Context Request messages transmitted to the SGSN(s). | Int32
> dpc-aa-tx-accept | The total number of Delete AA PDP Context Response messages received from the SGSN(s) containing a cause value of 128 (80H, Request accepted). | Int32
> dpc-aa-tx-deny | The total number of “reject” Delete AA PDP Context Response messages received from the SGSN(s). | Int32
> err-ind-rx | The total number of error indication messages received from the SGSN(s). | Int32
> err-ind-tx | The total number of error indication messages transmitted to the SGSN(s). | Int32
> err-ind-rx-discard | The total number of error indication messages received and discarded at the SGSN(s). | Int32
> cpc-noresource | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 199 (C7H, No resources available). | Int32
> cpc-addr-occupied | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 211 (D3H, All dynamic PDP addresses are occupied). | Int32
> cpc-nomem | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 212 (D4H, No memory is available). | Int32
> cpc-missing-apn | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 219 (DBH, Missing or unknown APN). | Int32
> cpc-unknown-pdp | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 220 (DCH, Unknown PDP address or PDP type). | Int32
> cpc-no-apn-subscription | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent because there was no apn subscription. | Int32
> cpc-auth-fail | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 201. | Int32
> cpc-sys-fail | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 204 (CCH, System failure). | Int32
> cpc-sem-tft | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 215 (D7H, Semantic error in the TFT operation). | Int32
> cpc-syn-tft | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 216 (D8H, Syntactic error in the TFT operation). | Int32
> cpc-sem-pktfilter | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 217 (D9H, Semantic error in packet filter(s)). | Int32
> cpc-syn-pktfilter | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 218 (DAH, Syntactic error in packet filter(s)). | Int32
> cpc-ie-err | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 201 (C9H, Mandatory IE incorrect). | Int32
> cpc-ie-missing | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 202 (CAH, Mandatory IE missing). | Int32
> cpc-opt-ie-err | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 203 (CBH, Optional IE incorrect). | Int32
> cpc-malformed | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 193 (C1H, Invalid message format). | Int32
> cpc-version | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 198 (C6H, version not supported). | Int32
> cpc-srv-not-supp | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 200 (C8H, service not Supported). | Int32
> disc-sgsn | The total number of sessions released by SGSN(s). | Int32
> disc-path-fail | The total number of session releases that occurred due to path failure. | Int32
> disc-smgr-dead | The total number of sessions released due to the termination of the session manager that was facilitating them. | Int32
> disc-admin | The total number of sessions administratively released. | Int32
> disc-other | The total number of sessions released due to other reasons. | Int32
> disc-teardown | The total number of sessions disconnected normally. | Int32
> disc-idle | The total number of sessions released due to the expiration of the idle timeout period as specified in the APN configuration. | Int32
> disc-absolute | The total number of sessions released due to the expiration of the absolute timeout period as specified in the APN configuration. | Int32
> disc-src-addr | The total number of sessions released due to source address violations. | Int32
> disc-flow-add | The total number of sessions released reason due to flow addition failures. | Int32
> disc-dhcp-renew-fail | The total number of sessions released due to failed DHCP lease renewal. | Int32
> disc-long-durn | The total number of sessions released due to the expiration of the long duration timeout period. | Int32
> disc-aborted | The total number of sessions released due to miscellaneous call abort conditions. | Int32
> disc-apn-rmvd | The total number of sessions released due to the removal of an APN’s configuration. | Int32
> pdu-notif | The total number of PDU Notification Request messages transmitted to the SGSN(s). | Int32
> pdu-notif-accept | The total number of PDU Notification Response messages received from the SGSN(s) containing a cause value of 128 (80H, Request accepted). | Int32
> pdu-notif-deny | The total number of “deny” PDU Notification Response messages received from the SGSN(s). | Int32
> pdu-notif-rej | The total number of PDU Notification Reject Request messages received from the SGSN(s). | Int32
> pdu-notif-rej-accept | The total number of PDU Notification Reject Response messaged transmitted to the SGSN(s) containing a cause value of 128 (80H, Request accepted). | Int32
> pdu-notif-rej-deny | The total number of “deny” PDU Notification Reject Response messages transmitted to the SGSN(s). | Int32
> pdu-notif-rej-discard | The total number of PDU Notification Reject Request messages discarded by the GGSN without any response transmitted to the SGSN(s). | Int32
> num-dt-established | The total number of direct tunnels established between SGSN and GGSN. | Int32
> num-dt-torn-by-sgsn | The total number of established direct tunnels between SGSN and GGSN torn by SGSN. | Int32
> num-dt-recv-err-ind | The total number of direct tunnels requests received from SGSN with error indication. | Int32
> sri-req | The total number of Send Routing Information (SRI) for GPRS messages transmitted to the HLR(s). | Int32
> sri-accept | The total number of Send Routing Info for GPRS Ack messages received from the HLR(s) containing a cause value of 128 (80H, Request accepted). | Int32
> sri-deny | The total number of “deny” Send Routing Info for GPRS Ack messages received from the HLR(s). | Int32
> fail-rep | The total number of Failure reports transmitted to the HLR(s). | Int32
> fail-rep-accept | The total number of Failure reports received from the HLR(s) containing a cause value of 128 (80H, Request accepted). | Int32
> fail-rep-deny | The total number of “deny” Failure reports received from the HLR(s). | Int32
> note-ms-gprs | The total number of Note MS GPRS Present messages received from the HLR(s). | Int32
> note-ms-gprs-accept | The total number of Note MS GPRS Present Response messages transmitted to the HLR(s) containing a cause value of 128 (80H, Request accepted). | Int32
> note-ms-gprs-deny | The total number of “deny” Note MS GPRS Present Response messages transmitted to the HLR(s). | Int32
> note-ms-gprs-discard | The total number of Note MS GPRS Present messages discarded with no response transmitted to the HLR(s). | Int32
> qosconv-bytes-in | The total number of Conversational Uplink Bytes Sent | Int64
> qosconv-pkts-in | The total number of Conversational Uplink Pkts Sent | Int64
> qosconv-bytes-out | The total number of Conversational Downlink Bytes Rcvd | Int64
> qosconv-pkts-out | The total number of Conversational Downlink Pkts Rcvd | Int64
> qosstrm-bytes-in | The total number of Streaming Uplink Bytes Sent | Int64
> qosstrm-pkts-in | The total number of Streaming Uplink Pkts Sent | Int64
> qosstrm-bytes-out | The total number of Streaming Downlink Bytes Rcvd | Int64
> qosstrm-pkts-out | The total number of Streaming Downlink Pkts Rcvd | Int64
> qosint1-bytes-in | The total number of Interactive 1 Uplink Bytes Sent | Int64
> qosint1-pkts-in | The total number of Interactive 1 Uplink Pkts Sent | Int64
> qosint1-bytes-out | The total number of Interactive 1 Downlink Bytes Rcvd | Int64
> qosint1-pkts-out | The total number of Interactive 1 Downlink Pkts Rcvd | Int64
> qosint2-bytes-in | The total number of Interactive 2 Uplink Bytes Sent | Int64
> qosint2-pkts-in | The total number of Interactive 2 Uplink Pkts Sent | Int64
> qosint2-bytes-out | The total number of Interactive 2 Downlink Bytes Rcvd | Int64
> qosint2-pkts-out | The total number of Interactive 2 Downlink Pkts Rcvd | Int64
> qosint3-bytes-in | The total number of Interactive 3 Uplink Bytes Sent | Int64
> qosint3-pkts-in | The total number of Interactive 3 Uplink Pkts Sent | Int64
> qosint3-bytes-out | The total number of Interactive 3 Downlink Bytes Rcvd | Int64
> qosint3-pkts-out | The total number of Interactive 3 Downlink Pkts Rcvd | Int64
> qosint-bytes-in | The total number of Interactive 1+2=3 Uplink Bytes Sent | Int64
> qosint-pkts-in | The total number of Interactive 1+2+3 Uplink Pkts Sent | Int64
> qosint-bytes-out | The total number of Interactive 1+2+3 Downlink Bytes Rcvd | Int64
> qosint-pkts-out | The total number of Interactive 1+2+3 Downlink Pkts Rcvd | Int64
> qosback-bytes-in | The total number of Background Uplink Bytes Sent | Int64
> qosback-pkts-in | The total number of Background Uplink Pkts Sent | Int64
> qosback-bytes-out | The total number of Background Downlink Bytes Rcvd | Int64
> qosback-pkts-out | The total number of Background Downlink Pkts Rcvd | Int64
> ctrl-num-bytes-in | The total number of bytes for control packets received on the Gn and/or Gp interface. | Int64
> ctrl-num-pkts-in | The total number of control packets received on the Gn and/or Gp interface. | Int64
> ctrl-num-bytes-out | The total number of bytes from control packets transmitted on the Gn and/or Gp interface. | Int64
> ctrl-num-pkts-out | The total number of control packets transmitted on the Gn and/or Gp interface. | Int64
> num-bytes-in | The total number of bytes received on the Gn and/or Gp interface. | Int64
> num-pkts-in | The total number of packets received on the Gn and/or Gp interface. | Int64
> num-bytes-out | The total number of bytes transmitted on the Gn and/or Gp interface. | Int64
> num-pkts-out | The total number of packets transmitted on the Gn and/or Gp interface. | Int64
> current-mbms-ue | The total number of current MBMS UE sessions. Type: Gauge | Int32
> current-mbms-mcast | The total number of current MBMS Multicast sessions. Type: Gauge | Int32
> current-mbms-bcast | The total number of current MBMS Broadcast sessions. Type: Gauge | Int32
> setup-mbms-ue | The total number of MBMS UE Sessions setup. | Int32
> setup-mbms-mcast | The total number of MBMS Multicast Sessions setup. | Int32
> setup-mbms-bcast | The total number of MBMS Broadcast Sessions setup | Int32
> chap-auth-attempt | The total number of CHAP Auth sessions attempted. | Int32
> chap-auth-success | The total number of CHAP Auth sessions successful | Int32
> chap-auth-failure | The total number of CHAP Auth sessions failed | Int32
> pap-auth-attempt | The total number of PAP Auth sessions attempted | Int32
> pap-auth-success | The total number of PAP Auth sessions successful | Int32
> pap-auth-failure | The total number of PAP Auth sessions failed | Int32
> no-auth | The total number of No-Auth sessions. | Int32
> err-ind | Total sessions released on Error Indication | Int32
> ctxt-replace | Total sessions released due to context replacement. | Int32
> purge-audit | Total sessions purged due to audit failure | Int32
> update-handoff-rej | Total sessions released due to handoff reject in UPC | Int32
> total-handoff-fail | Total path failure due to handoff | Int32
> sgsn-restart-cpc-req | Total path failure due to SGSN restart detected via CPC | Int32
> sgsn-restart-upc-req | Total path failure due to SGSN restart detected via UPC | Int32
> sgsn-restart-echo-rsp | Total path failure due to SGSN restart detected via Echo Rsp | Int32
> gtpc-echo-timeout | Total path failure due to SGSN restart detected via GTPC echo | Int32
> gtpu-echo-timeout | Total path failure due to SGSN restart detected via GTPU echo | Int32
> ggsn-req-timeout | Total path failure due to GGSN request timeout. | Int32
> version-not-sup-rx | Version not supported received | Int32
> version-not-sup-tx | Version not supported transmitted | Int32
> sup-ext-header-rx | Extension header supported received | Int32
> sup-ext-header-tx | Extension header supported transmitted | Int32
> cmc-total | The total number of Create MBMS Context request messages received. | Int32
> cmc-initial | The total number of initial Create MBMS Context request messages received. | Int32
> cmc-retrans | The total number of retransmitted Create MBMS Context request messages received. | Int32
> cmc-accept | The total number of Create MBMS Context request messages accepted by the GGSN. | Int32
> cmc-deny | The total number of Create MBMS Context request messages denied by the GGSN. | Int32
> cmc-discard | The total number of Create MBMS Context request messages discarded by the GGSN. | Int32
> umc-rx | The total number of Update MBMS Context request messages received. | Int32
> umc-rx-accept | The total number of Update MBMS Context request messages accepted by the GGSN. | Int32
> umc-rx-deny | The total number of Update MBMS Context request messages denied by the GGSN. | Int32
> umc-rx-discard | The total number of Update MBMS Context request messages discarded by the GGSN. | Int32
> dmc-rx | The total number of Delete MBMS Context request messages received. | Int32
> dmc-rx-accept | The total number of Delete MBMS Context request messages accepted by the GGSN. | Int32
> dmc-rx-deny | The total number of Delete MBMS Context request messages denied by the GGSN. | Int32
> dmc-rx-discard | The total number of Delete MBMS Context request messages discarded by the GGSN. | Int32
> dmc-tx | The total number of Delete MBMS Context request messages transmitted. | Int32
> dmc-tx-accept | The total number of Delete MBMS Context request messages accepted by the SGSN. | Int32
> dmc-tx-deny | The total number of Delete MBMS Context request messages denied by the SGSN. | Int32
> mbms-reg-req-total | The total number of MBMS Registration Request messages received. | Int32
> mbms-reg-req-initial | The total number of initial MBMS Registration Request messages received. | Int32
> mbms-reg-req-retrans | The total number of retransmitted MBMS Registration Request messages received. | Int32
> mbms-reg-req-accept | The total number of MBMS Registration Request messages accepted by the GGSN. | Int32
> mbms-reg-req-deny | The total number of MBMS Registration Request messages denied by the GGSN. | Int32
> mbms-reg-req-discard | The total number of MBMS Registration Request messages discarded by the GGSN. | Int32
> mbms-ses-start-tx | The total number of MBMS Session Start Request messages transmitted. | Int32
> mbms-ses-start-tx-accept | The total number of MBMS Session Start Request messages accepted by the SGSN. | Int32
> mbms-ses-start-tx-deny | The total number of MBMS Session Start Request messages denied by the SGSN. | Int32
> mbms-ses-stop-tx | The total number of MBMS Session Stop Request messages transmitted. | Int32
> mbms-ses-stop-tx-accept | The total number of MBMS Session Stop Request messages accepted by the SGSN. | Int32
> mbms-ses-stop-tx-deny | The total number of MBMS Session Stop Request messages denied by the SGSN. | Int32
> mbms-dereg-rx | The total number of MBMS De-Registration Request messages received. | Int32
> mbms-dereg-rx-accept | The total number of MBMS De-Registration Request messages accepted by the GGSN. | Int32
> mbms-dereg-rx-deny | The total number of MBMS De-Registration Request messages denied by the GGSN. | Int32
> mbms-dereg-rx-discard | mbms-dereg-rx-discard | Int32
> mbms-dereg-tx | The total number of MBMS De-Registration Request messages transmitted. | Int32
> mbms-dereg-tx-accept | The total number of MBMS De-Registration Request messages accepted by the SGSN. | Int32
> mbms-dereg-tx-deny | The total number of MBMS De-Registration Request messages denied by the SGSN. | Int32
> sess-in-preservation-mode | The total number of sessions in Preservation-Mode. This is a customer specific support only. | Int32
> transition-to-preservation-mode | The total number of sessions in transition from Non-Preservation mode (normal mode) to Preservation-Mode. This is a customer specific support only. | Int32
> transition-to-non-preservation-mode | The total number of sessions in transition from Preservation Mode to normal mode. This is a customer specific support only. | Int32
> sess-in-lorc | Indicates the number of GGSN session are in LORC state and subscriber is in out of radio coverage area. This counter is applicable when GGSN is enabled for overcharging protection for subscriber due to loss of radio coverage and SGSN notifies Update PDP Contexts for QOS change with GTP-C extension for LORC. | Int32
> transition-to-lorc | Indicates total number sessions in transitions state for overcharging protection support mode. This counter is applicable when GGSN is enabled for overcharging protection for subscriber due to loss of radio coverage and SGSN notifies Update PDP Contexts for QOS change with GTP-C extension for LORC. | Int32
> sess-in-focs | Total number of session Free of charge service. | Int32
> cnt-of-release-due-to-other | Total number of session release due to reasons other than listed in this table. | Int32
> cnt-of-release-due-to-violation | Total number of session release due to service violation. | Int32
> sess-in-odb | Indicates the total number of sessions with Operator Determined Barring enabled status. | Int32
> cnt-of-release-due-to-violation-odb | Indicates the statistics for sessions, with Operator Determined Barring enabled status, released due to violation of ODB conditions. | Int32
> cnt-of-release-due-to-other-odb | Indicates the total number of sessions, with Operator Determined Barring enabled status, released due to reasons not specified in this table. | Int32
> ipca-pdp-context-tx | Total number of PDP context activation requests sent for an Initiate PDP Context Activation. | Int32
> ipca-pdp-context-tx-accepted | Total number of PDP context activation requests sent and accepted for an Initiate PDP Context Activation. | Int32
> ipca-pdp-context-tx-denied | Total number of PDP context activation requests denied for an Initiate PDP Context Activation. | Int32
> ipca-reject-rx-no-resources | Total number of Initiate PDP Context Activation reject messages received due to no resource available on remote node. | Int32
> ipca-reject-rx-no-mem-avail | Total number of Initiate PDP Context Activation reject messages received due to no memory available on remote node. | Int32
> ipca-reject-rx-sys-failure | Total number of Initiate PDP Context Activation reject messages received due to system failure on remote node. | Int32
> ipca-reject-rx-non-existent | Total number of Initiate PDP Context Activation reject messages received due to non-existent session/subscriber on remote node. | Int32
> ipca-reject-rx-unsupported-service | Total number of Initiate PDP Context Activation reject messages received as service is not supported on on remote node. | Int32
> ipca-reject-rx-invalid-msg-format | Total number of Initiate PDP Context Activation reject messages received due to invalid message format. | Int32
> ipca-reject-rx-semantic-err-in-tft | Total number of Initiate PDP Context Activation reject messages received due to semantic error in Traffic Flow Template (TFT). | Int32
> ipca-reject-rx-syntactic-err-in-tft | Total number of Initiate PDP Context Activation reject messages received due to syntactic error in Traffic Flow Template (TFT) | Int32
> ipca-reject-rx-man-ie-incorrect | Total number of Initiate PDP Context Activation reject messages received due to incorrect information in mandatory information elements (IEs). | Int32
> ipca-reject-rx-semantic-err-in-pac-filter | Total number of Initiate PDP Context Activation reject messages received due to semantic error in PAC filter. | Int32
> ipca-reject-rx-man-ie-missing | Total number of Initiate PDP Context Activation reject messages received as mandatory information element (IE) is missing. | Int32
> ipca-reject-rx-optional-ie-incorrect | Total number of Initiate PDP Context Activation reject messages received due to incorrect information in optional information elements (IEs). | Int32
> ipca-reject-rx-syntactic-err-in-pac-filter | Total number of Initiate PDP Context Activation reject messages received due to syntactic error in PAC filter. | Int32
> ipca-reject-rx-ue-not-gprs-rsp | Total number of Initiate PDP Context Activation reject messages received as UE is not capable or subscribed to GPRS service. | Int32
> ipca-reject-rx-ue-refuses | Total number of Initiate PDP Context Activation reject messages received due to refusal from UE. | Int32
> ipca-reject-rx-invalid-correlation-id | Total number of Initiate PDP Context Activation reject messages received due to invalid correlation identifier. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883