> HNB-RN PLMN Configuration Mode Commands
> This HNB Radio Network PLMN configuration mode provides configuration to define the radio network PLMN parameters related to the HNB-GW connection with UMTS Femto radio network.
> associate cs-network
> This command associates a preconfigured circuit switched (CS) network within an HNB radio network PLMN with HNB-GW service.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] associate cs-network cs_name [ lac lac]
> no
> Disassociates/removes the configured CS network with an HNB radio network PLMN configured in HNB-GW service mode.
> cs_name
> Specifies the name of a preconfigured CS network in Global configuration mode with cs-network command and to be associated with an HNB radio network PLMN configured in HNB-GW service mode.
> To configure CS network, refer HNB-CS Configuration Mode Commands chapter.
> lac lac_id
> This keyword defines the granularity level of circuit switch network to a location area code (LAC) level to be associated with radio network PLMN in HNB-GW service.
> lac_id must be an integer between 1 and 65535.
> Usage
> Use this command to associate pre-defined CS networks with a radio network PLMN in an HNB-GW service.
> The circuit switched network comprises of one or more MSCs, where CS-domain IU-connections shall be routed. In a typical deployment HNB-GW is connected to only one MSC. However due to Iu-flex and networks-sharing requirements, HNB-GW can be connected to more than one MSCs as well.
> Another scenario when HNB-GW can be connected to multiple MSCs is when a set of HNBs should be connected to a particular MSC based on their UTRAN location or geographical location.
> This command provides configuration to have one or more MSCs such that these are used in load-shared (IuFlex) or network-shared mode. If location based distribution of HNBs to MSCs is desired then more than one circuit switched network configuration will be required.
> This configuration allows association of a circuit switched network with a radio network PLMN and granularity can either be at the PLMN level or at the level of a location area (LAC) in that PLMN.
> To configure CS network, refer HNB-CS Configuration Mode Commands chapter.
> Example
> The following command associates a CS network umts1 with radio network PLMN with a granularity of LAC 234:
> associate cs-network umts1 lac 234
> associate ps-network
> This command associates a preconfigured packet switched (PS) network within an HNB radio network PLMN with HNB-GW service.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] associate ps-network ps_name [ lac lac [ rac rac ] ]
> no
> Disassociates/removes the configured PS network with an HNB radio network PLMN configured in HNB-GW service mode.
> ps_name
> Specifies the name of a preconfigured PS network in Global configuration mode with ps-network command and to be associated with an HNB radio network PLMN configured in HNB-GW service mode.
> To configure PS network, refer HNB PS Configuration Mode Commands chapter.
> lac lac_id
> This keyword defines the granularity level of packet switched network to a location area code (LAC) level to be associated with radio network PLMN in HNB-GW service.
> lac_id must be an integer between 1 and 65535.
> rac rac_id
> This keyword defines the granularity level of packet switched network to a radio area code (RAC) level to be associated with radio network PLMN in HNB-GW service.
> rac_id must be an integer between 1 and 65535.
> Usage
> Use this command to associate pre-defined PS networks with HNB radio network PLMN in an HNB-GW service.
> The packet switched network comprises of one or more SGSNs where PS-domain IU-connections shall be routed. In a typical deployment HNB-GW is connected to only one SGSN. However with IuFlex and network-sharing functionality, HNB-GW can be connected to more than one SGSNs as well.
> Another scenario when HNB-GW can be connected to multiple SGSNs is when a set of HNBs should be connected to a particular SGSN based on their UTRAN location or geographical location.
> This command provides configuration to have one or more to have one or more SGSNs such that these are used in load-shared (iu-flex) or network-shared mode. If location based distribution of HNBs to SGSNs is desired then more than one packet switched network configuration will be required.
> This command allows association of a packet switched network with a radio network PLMN and granularity could either be at the PLMN level or at the level of a location area code (LAC) in that PLMN or at the level of a routing area code (RAC) in that LAC.
> To configure PS network, refer HNB-PS Configuration Mode Commands chapter.
> Example
> The following command associates a PS network umts_ps1 with radio network PLMN with a granularity of LAC 234 and RAC as 123:
> associate ps-network umts_ps1 lac 234 rac 123
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> rnc-id
> This command configures the Radio Network Concentrator (RNC) identifier in a Radio Network PLMN associated with HNB-GW service to provide RNC identifier to HNB during HNB-REGISTRATION procedure. Depending upon the requirement the RNC Identifier can be provided at the desired granularity.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] rnc-id rnc_id [ lac lac_id [ rac rac_id | cell-id cell_id ] ]
> no
> Deletes the LAC and RAC information from the system configuration.
> rnc-id
> Specified the RNC id to be configured in radio network PLMN associated with HNB-GW and to be provided to HNB during HNB-REGISTRATION procedure from HNB-GW. It also configures RNC Id for all HNBs operating in a particular PLMN.
> rnc_id must be an integer between 1 and 65535.
> lac lac_id
> This keyword defines the granularity level of location of HNB to a location area code (LAC) level and configures RNC ID for all HNBs operating in particular location-area.
> lac_id must be an integer between 1 and 65535.
> rac rac_id
> This keyword defines the granularity level of location of HNB to a routing area code (RAC) level and configures RNC ID for all HNBs operating in particular routing area.
> rac_id must be an integer between 1 and 65535.
> cell-id cell_id
> This keyword defines the granularity level of location of HNB to a UTRAN cell level and configures RNC ID for all HNBs operating in particular UTRAN cell area.
> cell_id must be an integer between 1 and 65535.
> Usage
> Use this command to configure RNC id for Radio Network PLMN which will be sent to HNBs from HNB-GW during HNB-REGISTRATION procedure. Depending upon the requirement the RNC Identifier can be provided at the desired granularity.
> When HNB-REGISTRATION request is received the RNC Id is looked up by matching the parameters received in the request. The most specific entry that matches the request shall have the highest priority, for example in the following configuration:
> rnc-id 257 lac 1 cell-id 3
> rnc-id 258 lac 1 rac 2
> rnc-id 259 lac 1
> rnc-id 260

> • | If request is received with LAC=1, RAC=2, and Cell-Id=3, the selected RNC id will be 257.

> • | If request is received with LAC=1, RAC=3, and Cell-Id != 3, the selected RNC id will be 258.

> • | If request is received with LAC=1 and any other values of RAC and Cell-id, the selected RNC id will be 259. For all other requests 260 will be returned.

> Example
> Following command will configure the HNB-GW service to return RNC id as 102 when HNB-REGISTRATION request is received with LAC 1, and RAC 2:
> rnc-id 102 lac 1 rac 2
> Following command will configure the HNB-GW service to return RNC id as 102 when HNB-REGISTRATION request is received with LAC 1 and cell-id 4:
> rnc-id 102 lac 1 cell-id 5

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883