> WEM Configuration File Parameters
> This appendix provides information about the configuration file parameters pertaining to the Web Element Manager. WEM provides a number of configuration files which can be modified to fine-tune the operation of the application. These files are located in the /<ems_dir>/server/etc directory by default.
> The following configuration files have been deprecated from WEM:

> • | fmcorelation.cfg

> • | description.cfg

> • | dbphy.cfg

> • | dblog.cfg

> This chapter provides information on the following configuration files:

> • | The alarmid.cfg File

> • | The audio.cfg File

> • | The blacklist.cfg File

> • | The bs.cfg File

> • | The bsparser.cfg File

> • | The bsserver.cfg File

> • | The bstca.cfg File

> • | The cf.cfg File

> • | The configupdate.cfg File

> • | The db.cfg File

> • | The emslic.cfg File

> • | The fm.cfg File

> • | The hwinv.cfg File

> • | The ism.cfg File

> • | The mcrdbs.cfg File

> • | The mdproxy.cfg File

> • | The nb.cfg File

> • | The nbserver.cfg File

> • | The nms.cfg File

> • | The pcrefgen.cfg File

> • | The processmonitor.cfg File

> • | The ps.cfg File

> • | The psmon.cfg File

> • | The res.cfg File

> • | The temip.cfg File

> • | The thr.cfg File

> • | The ua.cfg File

> • | The vacuum.cfg File

> • | The wblist.cfg File

> Important: Unless otherwise specified, all information in this chpater applies to both Sun Solaris- and RHEL-based WEM systems.
> The alarmid.cfg File
> This file provides parameters pertaining to the configuration of SNMP alarms received from managed devices.
> Important: This configuration file is customer-specific and is not operational without the appropriate license. Please contact your local sales representative for additional information.
> The audio.cfg File
> This file provides alarm severity associations to specific audio files. The audio files are in .WAV format and are played by the Web Element Manager when an alarm/trap of that severity is received. Additionally, this file can be used to associate an audio file to a specific alarm for further customizing.
> The following table describes the AUDIO file parameters.
> audio.cfg File Parameters

> Parameters
> AUDIO: This file contains the mapping of the alarm severity level and the corresponding audio file to be played when an alarm is received. The first field contains the severity level (number): The nth row in the SEVERITY section is n-1 in the fm.cfg file. Please use the fm.cfg file for the severity configuration information in detail. The second field contains the audio file name. The audio files are present in the audio sub-directory in the client installation directory. The format is as follows: Severity Number = WAV File Path For example: 1 = Blank Line - This means that no audio file is to be played when a first level (Indeterminate) severity alarm is received. 3 = audio/chord.wav - This means that the audio/chord.wav file is to be played when a third level (Major) severity alarm is received.
> audioPlayedFor: This option will decide the priority of alarm to play an audio. The default value is 0. Valid configurables are: 0 - Only STxx audio will be played as per severity and no audio will be played for WEM alarm. 1 - Audio for STxx and WEM will be played but severity will be given to STxx alarms. 2 - Audio for STxx and WEM will be played but first priority will be based on device and severity. 3 - Audio will be played strictly based on the severity irrespective of STxx/WEM.
> Severity No. | Severity Name | Audio Filename
> 1 | Critical | 1 = audio/notify.wav
> 2 | Major | 2 = audio/ding.wav
> 3 | Minor | 3 = audio/chord.wav
> 4 | Warning | 4 = audio/Alarmrng.wav

> ‌
> The following table describes the TRAPAUDIO file parameters.
> TRAPAUDIO File Parameters

> Parameters
> TRAPAUDIO: This section defines the mapping for Trap Number and the corresponding AUDIO file. This file is the default file to be played when the trap is received. If the filename field is kept empty then, the file associated with the severity of the trap will be played. Severity-AudioFilename relationship is defined in the AUDIO section. The format is as follows: Trap Number = File Path For example: 1 = This suggests that no audio file is associated with trap #1. So, the file associated with its severity will be played. 3 = audio/test01.wav - This file will be played whenever trap #3 comes.
> Trap Number | Trap Name
> Generic Alarms
> 1-1 | coldStart
> 1-2 | warmStart
> 1-3 | linkDown
> 1-4 | linkUp
> 1-5 | authenticationFailure
> 1-6 | egpNeighborLoss
> ST 16 Enterprise Alarms
> 2-1 | starCardTempOverheat
> 2-2 | starCardTempOK
> 2-3 | starCardReset
> 2-4 | starCardRebootRequest
> 2-5 | starCardUp
> 2-6 | starCardVoltageFailure
> 2-7 | starCardRemoved
> 2-8 | starCardInserted
> 2-9 | starCardBootFailed
> 2-12 | starCardRCCFailed
> 2-13 | starCardMismatch
> 2-14 | starCardFailureLEDOn
> 2-15 | starCardFailureLEDOff
> 2-16 | starCardPACMigrateStart
> 2-17 | starCardPACMigrateComplete
> 2-18 | starCardPACMigrateFailed
> 2-19 | starCardSPCSwitchoverStart
> 2-20 | starCardSPCSwitchoverComplete
> 2-21 | starCardSPCSwitchoverFailed
> 2-22 | starFanFailed
> 2-23 | starFanRemoved
> 2-24 | starFanInserted
> 2-25 | starLogThreshold
> 2-26 | starCPUBusy
> 2-27 | starCPUMemoryLow
> 2-28 | starCPUMemoryFailed
> 2-29 | starCPUFailed
> 2-30 | starCPUWatchDogExpired
> 2-31 | starNPUARPPoolExhausted
> 2-32 | starPowerFilterUnitUnavail
> 2-33 | starPowerFilterRemoved
> 2-34 | starPowerFilterAvail
> 2-37 | starAlertsDisabled
> 2-38 | starAlertsEnabled
> 2-39 | starAAAAuthServerUnreachable
> 2-40 | starAAAAuthServerReachable
> 2-41 | starAAAAuthServerMisconfigured
> 2-42 | starAAAAccServerUnreachable
> 2-43 | starAAAAccServerReachable
> 2-44 | starAAAAccServerMisconfigured
> 2-45 | starLogMsg
> 2-46 | starPDSNServiceStart
> 2-47 | starPDSNServiceStop
> 2-48 | starHAServiceStart
> 2-49 | starHAServiceStop
> 2-50 | starFAServiceStart
> 2-51 | starFAServiceStop
> 2-52 | starCLISessionStart
> 2-53 | starCLISessionEnd
> 2-54 | starCritTaskFailed
> 2-55 | starCardActive
> 2-56 | starLACServiceStart
> 2-57 | starLACServiceStop
> 2-58 | starLNSServiceStart
> 2-59 | starLNSServiceStop
> 2-60 | starCardDown
> 2-63 | starGGSNServiceStart
> 2-64 | starGGSNServiceStop
> 2-65 | starLicenseExceeded
> 2-66 | starSubscriberLimit
> 2-67 | starSessionRejectNoResource
> 2-68 | starLongDurTimerExpiry
> 2-69 | starClosedRPServiceStart
> 2-70 | starClosedRPServiceStop
> 2-71 | starGtpcPathFailure
> 2-72 | starGtpuPathFailure
> 2-73 | starManagerFailure
> 2-74 | starEISServerAlive
> 2-75 | starEISServerDead
> 2-76 | starCgfAlive
> 2-77 | starCgfDead
> 2-78 | starStorageServerAlive
> 2-79 | starStorageServerDead
> 2-80 | starGgsnInitiatedUpdtFailed
> 2-81 | starCongestion
> 2-82 | starCongestionClear
> 2-83 | starServiceLossPTACs
> 2-84 | starServiceLossLC
> 2-85 | starServiceLossSPIO
> 2-86 | starIPSPAllAddrsFree
> 2-87 | starPCFUnreachable
> 2-88 | starDhcpAlive
> 2-89 | starDhcpDead
> 2-90 | starNTPPeerUnreachable
> 2-91 | starNTPSyncLost
> 2-92 | starL2TPTunnelDownPeerUnreachable
> 2-93 | starCardStandby
> 2-94 | starLicenseUnderLimit
> 2-95 | starIPSECPriTunDown
> 2-96 | starIPSECPriTunUp
> 2-97 | starIPSECSecTunDown
> 2-98 | starIPSECSecTunUp
> 2-99 | starIPSECTunSwitchFail
> 2-100 | starIPSECTunSwitchComplete
> 2-101 | starNwReachServerAlive
> 2-102 | starNwReachServerDead
> 2-103 | starStorageServerUnackedGcdrVolPurge
> 2-104 | starStorageServerUnackedGcdrFileGen
> 2-200 | starThreshCPUUtilitization
> 2-201 | starThreshClearCPUUtilitization
> 2-202 | starThreshCPUMemory
> 2-203 | starThreshClearCPUMemory
> 2-204 | starThreshLicence
> 2-205 | starThreshClearLicence
> 2-206 | starThreshSubscriberTotal
> 2-207 | starThreshClearSubscriberTotal
> 2-208 | starThreshSubscriberActive
> 2-209 | starThreshClearSubscriberActive
> 2-210 | starThreshPortRxUtil
> 2-211 | starThreshClearPortRxUtil
> 2-212 | starThreshPortTxUtil
> 2-213 | starThreshClearPortTxUtil
> 2-214 | starThreshPortHighActivity
> 2-215 | starThreshClearPortHighActivity
> 2-216 | starThreshAAAAuthFail
> 2-217 | starThreshClearAAAAuthFail
> 2-218 | starThreshAAAAuthFailRate
> 2-219 | starThreshClearAAAAuthFailRate
> 2-220 | starThreshAAAAcctFail
> 2-221 | starThreshClearAAAAcctFail
> 2-222 | starThreshAAAAcctFailRate
> 2-223 | starThreshClearAAAAcctFailRate
> 2-224 | starThreshAAARetryRate
> 2-225 | starThreshClearAAARetryRate
> 2-226 | starThreshCallSetup
> 2-227 | starThreshClearCallSetup
> 2-228 | starThreshCallSetupFailure
> 2-229 | starThreshClearCallSetupFailure
> 2-230 | starThreshCallRejectNoResource
> 2-231 | starThreshClearCallRejectNoResource
> 2-232 | starThreshPacketsFilteredDropped
> 2-233 | starThreshClearPacketsFilteredDropped
> 2-234 | starThreshPacketsForwarded
> 2-235 | starThreshClearPacketsForwarded
> 2-236 | starThreshSessCPUThroughput
> 2-237 | starThreshClearSessCPUThroughput
> 2-238 | starThreshIPPoolAvail
> 2-239 | starThreshClearIPPoolAvail
> 2-240 | starThreshCPUUtilitization10Sec
> 2-241 | starThreshClearCPUUtilitization10Sec
> 2-242 | starThreshCPULoad
> 2-243 | starThreshClearCPULoad
> 2-244 | starThreshCPUMemUsage
> 2-245 | starThreshClearCPUMemUsage
> 2-246 | starThreshPDSNSessions
> 2-247 | starThreshClearPDSNSessions
> 2-248 | starThreshGGSNSessions
> 2-249 | starThreshClearGGSNSessions
> 2-250 | starThreshHASessions
> 2-251 | starThreshClearHASessions
> 2-252 | starThreshLNSSessions
> 2-253 | starThreshClearLNSSessions
> 2-254 | starThreshPerServicePDSNSessions
> 2-255 | starThreshClearPerServicePDSNSessions
> 2-256 | starThreshPerServiceGGSNSessions
> 2-257 | starThreshClearPerServiceGGSNSessions
> 2-258 | starThreshPerServiceHASessions
> 2-259 | starThreshClearPerServiceHASessions
> 2-260 | starThreshPerServiceLNSSessions
> 2-261 | starThreshClearPerServiceLNSSessions
> 2-262 | starThreshIPPoolHold
> 2-263 | starThreshClearIPPoolHold
> 2-264 | starThreshIPPoolUsed
> 2-265 | starThreshClearIPPoolUsed
> 2-266 | starThreshIPPoolRelease
> 2-267 | starThreshClearIPPoolRelease
> 2-268 | starThreshIPPoolFree
> 2-269 | starThreshClearIPPoolFree
> 2-270 | starThreshAAAAcctArchive
> 2-271 | starThreshClearAAAAcctArchive

> ‌
> The blacklist.cfg File
> This file contains the flag that is set to enable or disable the blacklisting feature in WEM. The file provides parameters for specifying information such as blacklist backup limit, time interval to poll the blacklist directory, and so on.
> blacklist.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> BLACKLIST: This section describes parameters that store information related to blacklisting.
> EnableBlackListFeature | Flag to enable/disable the blacklisting feature in WEM. Setting this flag to 1 will enable the blacklisting feature in WEM. Needs a WEM Server restart. Values: 1: Enable 0: Disable | -- | -- | 0
> BlacklistBackupLimit | Number of Blacklist backups to be maintained. | 5 | 15 | 10
> ExportBLtoCDPInterval | BlackList files Export interval. This specifies the time interval in hours for Content Filtering Server to export OPTCMDB-BL to CDP. | 1 hr | 5 hrs | 2 hrs
> BlPollInterval | BlackList directory poll interval. This specifies the time interval in minutes to poll the Blacklist directory. | 5 | 60 | 15
> EnableDNSLookup | Flag to enable/disable the DNS lookup functionality. Setting this flag to 1 will enable the DNS lookup functionality. Values: 1: Enable 0: Disable | -- | -- | 0
> ThreadPoolSize | Thread pool size. | 1 | 10 | 5
> NCMEC:
> EnableNCMEC | Flag to enable/disable the import of cumulative.csv from NCMEC. Setting this flag to 1 will enable the import of cumulative.csv from NCMEC. Values: 1: Enable - import cumulative.csv from NCMEC 0: Disable - assume cumulative.csv will be available in <EMS ServerPath>/flash/blacklist/blacklist/ Important: Do not change the value of configurable as functionality when this flag 0 is disabled | -- | -- | 1
> NCMECUrl | This specifies the cumulative.csv file path at NCMEC. | -- | -- | --
> NCMECAuthUserName | This specifies the username required for authentication at NCMEC site. | -- | -- | --
> NCMECAuthPassword | This specifies the password required for authentication at NCMEC site. | -- | -- | --
> BlacklistImportInterval | This specifies the cumulative.csv file import interval (in hours). | 1 | 168 (one week) | 24 (one day)
> BlacklistReImportInterval | This specifies the cumulative.csv file re-import interval (in minutes). | 1 | 30 | 5
> BLThreadPoolSize | Specifies the blacklist thread pool size. | 5 | 20 | 10

> ‌
> The bs.cfg File
> This file provides bulk statistic configuration information pertaining to schemas, formatting, and parameters for specifying time tolerances for searching bulk statistic records. This is a multi-section server configuration file for bulkstat module.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> Caution: To ensure proper operation of the Web Element Manager, bulk statistic schema and formatting configuration in this file should not be altered.
> bs.cfg File Parameters (Schemas)

> Key | Description | Default Value in Config File
> Schema: This section provides the schema format string for each subsystem. The parameter values in this section are internally used by the bulkstat server module and should not be changed.
> CardSch | Card Schema | EMS,Card,%date%,%time%,%card%,%cpubusy%,%cpuidle%,%numproc%,%memused%,%memtotal%,%numcpu%,%cpu0-cpubusy%,%cpu0-cpuidle%,%cpu0-numproc%,%cpu0-memused%,%cpu0-memtotal%,%cpu0-cpuused-user%,%cpu0-cpuused-sys%,%cpu0-cpuused-io%,%cpu0-cpuused-irq%,%cpu0-cpuused-idle%,%cpu1-cpubusy%,%cpu1-cpuidle%,%cpu1-numproc%,%cpu1-memused%,%cpu1-memtotal%,%cpu1-cpuused-user%,%cpu1-cpuused-sys%,%cpu1-cpuused-io%,%cpu1-cpuused-irq%,%cpu1-cpuused-idle%,%cpu2-cpubusy%,%cpu2-cpuidle%,%cpu2-numproc%,%cpu2-memused%,%cpu2-memtotal%,%cpu2-cpuused-user%,%cpu2-cpuused-sys%,%cpu2-cpuused-io%,%cpu2-cpuused-irq%,%cpu2-cpuused-idle%,%cpu3-cpubusy%,%cpu3-cpuidle%,%cpu3-numproc%,%cpu3-memused%,%cpu3-memtotal%,%cpu3-cpuused-user%,%cpu3-cpuused-sys%,%cpu3-cpuused-io%,%cpu3-cpuused-irq%,%cpu3-cpuused-idle%,%15avg-cpubusy%,%15peak-cpubusy%,%5avg-cpubusy%,%5peak-cpubusy%,%1avg-cpubusy%,%15avg-memused%,%15peak-memused%,%5avg-memused%,%5peak-memused%,%1avg-memused%,%cpu0-15avg-cpubusy%,%cpu0-15peak-cpubusy%,%cpu0-5avg-cpubusy%,%cpu0-5peak-cpubusy%,%cpu0-1avg-cpubusy%,%cpu0-15avg-memused%,%cpu0-15peak-memused%,%cpu0-5avg-memused%,%cpu0-5peak-memused%,%cpu0-1avg-memused%,%cpu1-15avg-cpubusy%,%cpu1-15peak-cpubusy%,%cpu1-5avg-cpubusy%,%cpu1-5peak-cpubusy%,%cpu1-1avg-cpubusy%,%cpu1-15avg-memused%,%cpu1-15peak-memused%,%cpu1-5avg-memused%,%cpu1-5peak-memused%,%cpu1-1avg-memused%,%cpu2-15avg-cpubusy%,%cpu2-15peak-cpubusy%,%cpu2-5avg-cpubusy%,%cpu2-5peak-cpubusy%,%cpu2-1avg-cpubusy%,%cpu2-15avg-memused%,%cpu2-15peak-memused%,%cpu2-5avg-memused%,%cpu2-5peak-memused%,%cpu2-1avg-memused%,%cpu3-15avg-cpubusy%,%cpu3-15peak-cpubusy%,%cpu3-5avg-cpubusy%,%cpu3-5peak-cpubusy%,%cpu3-1avg-cpubusy%,%cpu3-15avg-memused%,%cpu3-15peak-memused%,%cpu3-5avg-memused%,%cpu3-5peak-memused%,%cpu3-1avg-memused%,%task-sessmgr-num%
> CardSch2 | Card 2 Schema | EMS,Card2,%date%,%time%,%card%,%task-sessmgr-avgcpu%,%task-sessmgr-avgmem%,%task-sessmgr-maxcpu%,%task-sessmgr-maxmem%,%task-a11mgr-num%,%task-a11mgr-maxcpu%,%task-a11mgr-maxmem%,%task-l2tpmgr-num%,%task-l2tpmgr-maxcpu%,%task-l2tpmgr-maxmem%,%task-famgr-num%,%task-famgr-maxcpu%,%task-famgr-maxmem%,%task-hamgr-num%,%task-hamgr-maxcpu%,%task-hamgr-maxmem%,%task-acsmgr-num%,%task-acsmgr-avgcpu%,%task-acsmgr-avgmem%,%task-acsmgr-maxcpu%,%task-acsmgr-maxmem%,%task-vpnmgr-num%,%task-vpnmgr-maxcpu%,%task-vpnmgr-maxmem%
> PortSch | Port Schema | EMS,Port,%date%,%time%,%card%,%port%,%rxbytes%,%txbytes%,%ucast_inpackets%,%ucast_outpackets%,%mcast_inpackets%,%mcast_outpackets%,%bcast_inpackets%,%bcast_outpackets%,%rxpackets%,%txpackets%,%rxdiscbytes%,%rxdiscpackets%,%txdiscbytes%,%txdiscpackets%,%maxrate%,%frag-rcvd%,%pkt-reassembled%,%frag-tokernel%,%util-rx-curr%,%util-tx-curr%,%util-rx-5min%,%util-tx-5min%,%util-rx-15min%,%util-tx-15min%
> PDSNSystemSch | PDSN System Schema | EMS,PDSNSystem,%date%,%time%,%sess-ttlarrived%,%sess-ttlrejected%,%sess-ttlconnected%,%sess-ttlauthsucc%,%sess-ttlauthfail%,%sess-ttllcpup%,%sess-ttlipcpup%,%sess-ttlsrcviol%,%sess-ttlkeepfail%,%sess-curttlcalls%,%sess-cursipconn%,%sess-curmipconn%,%sess-curactcall%,%sess-curdormcall%,%sess-curarrived%,%sess-curlcpnegot%,%sess-curlcpup%,%sess-curauth%,%sess-curauthed%,%sess-curipcpup%,%sess-curdisc%,%a11-ttlarrived%,%a11-ttlrejected%,%a11-ttldemult%,%a11-ttldereg%,%a11-curactive%,%fa-ttlarrived%,%fa-ttlrejected%,%fa-ttldemult%,%fa-ttldereg%,%fa-curactive%,%ha-ttlarrived%,%ha-ttlrejected%,%ha-ttldemult%,%ha-ttldereg%,%ha-curactive%,%sess-calldur-1min%,%sess-calldur-2min%,%sess-calldur-5min%,%sess-calldur-15min%,%sess-calldur-1hour%,%sess-calldur-4hour%,%sess-calldur-12hour%,%sess-calldur-24hour%,%sess-calldur-over24hour%,%sess-setuptime-100ms%,%sess-setuptime-200ms%,%sess-setuptime-300ms%,%sess-setuptime-400ms%,%sess-setuptime-500ms%,%sess-setuptime-600ms%,%sess-setuptime-700ms%,%sess-setuptime-800ms%,%sess-setuptime-900ms%,%sess-setuptime-1sec%,%sess-setuptime-2sec%,%sess-setuptime-3sec%,%sess-setuptime-4sec%,%sess-setuptime-6sec%,%sess-setuptime-8sec%,%sess-setuptime-10sec%,%sess-setuptime-12sec%,%sess-setuptime-14sec%,%sess-setuptime-16sec%,%sess-setuptime-over16sec%,%incremental%,%enddate%,%endtime%,%localenddate%,%localendtime%,%sess-ttlfailed%,%uptime%,%uptimestr%,%lic-pdsn%,%lic-ha%,%lic-ggsn%,%lic-l2tplns%,%sess-txbytes%,%sess-rxbytes%,%sess-txpackets%,%sess-rxpackets%,%sess-siptxbytes%,%sess-siprxbytes%,%sess-miptxbytes%,%sess-miprxbytes%,%aaa-ttlreq%,%aaa-curreq%,%aaa-ttlauthreq%,%aaa-curauthreq%,%aaa-ttlauthprobe%,%aaa-curauthprobe%,%aaa-ttlacctreq%,%aaa-curacctreq%,%aaa-ttlauthsucc%,%aaa-ttlauthfail%,%aaa-ttlauthpurged%,%aaa-ttlauthcancelled%,%aaa-ttlauthdmuchal%,%aaa-ttlradauthreq%,%aaa-curradauthreq%,%aaa-ttlradauthreqretried%,%aaa-ttllclauthreq%,%aaa-curlclauthreq%,%aaa-ttlpseudoauthreq%,%aaa-curpseudoauthreq%,%aaa-ttlauthnulluser%,%aaa-ttlacctsucc%,%aaa-ttlacctpurged%,%aaa-ttlacctcancelled%,%aaa-ttlradacctreq%,%aaa-ttlradacctreqretried%,%disc-reason-summary%,%sess-curaaaactive%,%sess-curaaadeleting%,%sess-curaaaacctpending%,%sess-ttlemptyfwd%,%sess-ttlemptyrev%,%sess-ttlonlineprepaiderr%,%sess-ttlprepaidinitautherr%,%sess-ttlcrprpattempt%,%sess-ttlcrprpsuccess%,%sess-ttlrpcrpattempt%,%sess-ttlrpcrpsuccess%,%sess-curpmipconn%,%sess-curl2tplacconn%,%sess-curalwayson%,%sess-curbcmcsauth%,%sess-curbcmcsconn%,%sess-curhaipsecconn%,%sess-curl2tplacconnecting%,%sess-curpdptypeipconn%,%sess-curpdptypepppconn%,%sess-curprepaid%,%sess-rxpkt-1023%,%sess-rxpkt-127%,%sess-rxpkt-16%,%sess-rxpkt-2047%,%sess-rxpkt-255%,%sess-rxpkt-4095%,%sess-rxpkt-4500%,%sess-rxpkt-511%,%sess-rxpkt-64%,%sess-rxpkt-over4500%,%sess-ttldisconn%,%sess-ttlhandoff%,%sess-ttlonlineauthfail%,%sess-ttlonlineauthreq%,%sess-ttlonlineauthsucc%,%sess-ttlprepaid%,%sess-ttlproxydns-drop%,%sess-ttlproxydns-passthru%,%sess-ttlproxydns-redirect%,%sess-ttlrenewal%,%sess-txpkt-1023%,%sess-txpkt-127%,%sess-txpkt-16%,%sess-txpkt-2047%,%sess-txpkt-255%,%sess-txpkt-4095%,%sess-txpkt-4500%,%sess-txpkt-511%,%sess-txpkt-64%,%sess-txpkt-over4500%,%aaa-ttlauthkeepalive%,%aaa-curauthkeepalive%,%aaa-ttlacctkeepalive%,%aaa-curacctkeepalive%,%aaa-ttlauthkeepalivesuccess%,%aaa-ttlauthkeepalivefailure%,%aaa-ttlauthkeepalivepurged%,%aaa-ttlacctkeepalivesuccess%,%aaa-ttlacctkeepalivetimeout%,%aaa-ttlacctkeepalivepurged%,%ipsg-total-call-arrived%,%ipsg-total-call-rejected%,%ipsg-total-call-demult%,%ipsg-total-dereg-rep-sent%,%ipsg-cur-active-call%,%ipsg-total-active-serv%
> PDSNSystemSch2 | PDSN2 System Schema | EMS,PDSNSystem2,%date%,%time%,%asngw-cur-active-call%,%asngw-total-sess-setup%,%asngw-retriesexhaust%,%asngw.sfs%,%asngw.tidfail%,%asngw-handoffattempt%,%asngw-handoffdenied%,%asngw-handoffcomp%,%asngw.authsucc%,%asngw-authfailures%,%sess-ttlcallop%,%sess-curnonanchorconn%,%sess-curdhcppending%,%sess-ttlinterasngwattempt%,%sess-ttlinterasngwsuccess%,%sess-ttlintraasngwattempt%,%sess-ttlintraasngwsuccess%,%sess-ttlconnected-1xrtt%,%sess-txbytes-1xrtt%,%sess-rxbytes-1xrtt%,%sess-txpackets-1xrtt%,%sess-rxpackets-1xrtt%,%sess-ttlconnected-evdorev0%,%sess-txbytes-evdorev0%,%sess-rxbytes-evdorev0%,%sess-txpackets-evdorev0%,%sess-rxpackets-evdorev0%,%sess-ttlconnected-evdoreva%,%sess-txbytes-evdoreva%,%sess-rxbytes-evdoreva%,%sess-txpackets-evdoreva%,%sess-rxpackets-evdoreva%,%flow-ttlestab%,%flow-ttldisconn%,%flow-curdynamic%,%pdif-cursess%,%pdif-curactive%,%pdif-curdormant%,%pdif-ttlsetup%,%sess-15peak-curactcall%,%sess-15peak-curttlcall%,%sess-cursipactive%,%sess-15peak-cursipactive%,%sess-curmipactive%,%sess-15peak-curmipactive%,%a11-15peak-curactive%,%crp-curactive%,%crp-15peak-curactive%,%fa-15peak-curactive%,%ha-15peak-curactive%,%flow-15peak-curdynamic%,%sess-15min-usageactive%,%sess-15min-usageall%,%cc-cursess%,%cc-ttlecsadd%,%cc-ttlstart%,%cc-ttlsessupd%,%cc-ttlterm%,%cc-sessfailover%,%cc-msg-recv%,%cc-msg-sent%,%cc-msg-request%,%cc-msg-answer%,%cc-msg-ccrinit%,%cc-msg-ccainit%,%cc-msg-ccainitaccept%,%cc-msg-ccainitreject%,%cc-msg-ccainittimeout%,%cc-msg-ccrupdate%,%cc-msg-ccaupdate%,%cc-msg-ccaupdatetimeout%,%cc-msg-ccrfinal%,%cc-msg-ccafinal%,%cc-msg-ccafinaltimeout%,%cc-msg-asr%,%cc-msg-asa%,%cc-msg-rar%,%cc-msg-raa%,%cc-msg-ccadropped%,%cc-msgerr-proto%,%cc-msgerr-badanswer%,%cc-msgerr-unknownsess%,%cc-msgerr-unknowncomm%,%cc-msgerr-reqtimeout%
> PDSNSystemSch3 | PDSN3 System Schema | EMS,PDSNSystem3,%date%,%time%,%cc-msgerr-parse%,%cc-msgerr-unkratinggrp%,%cc-msgerr-unkrulebase%,%cc-msgerr-unkfailure%,%cc-upd-threshold%,%cc-upd-qht%,%cc-upd-final%,%cc-upd-quotaexhaust%,%cc-upd-validitytime%,%cc-upd-otherquota%,%cc-upd-ratingchange%,%cc-upd-forcedreauth%,%cc-term-diamlogout%,%cc-term-servnotprov%,%cc-term-badanswer%,%cc-term-admin%,%cc-term-linkbroken%,%cc-term-authexpired%,%cc-term-usermoved%,%cc-term-sesstimeout%,%cc-traf-catcreate%,%cc-traf-catdelete%,%cc-traf-catlookup%,%cc-traf-hits%,%cc-traf-misses%,%cc-traf-triggerevent%,%cc-traf-finalunit%,%cc-traf-catsuccess%,%cc-traf-ratingfail%,%cc-traf-servdenied%,%cc-traf-limitreached%,%cc-traf-authreject%,%cc-traf-othererror%,%cf-static-ratereq%,%cf-static-ratesucc%,%cf-static-rateblock%,%cf-static-ratefail%,%cf-static-ratefail-nr%,%cf-static-ratefail-notindb%,%cf-dyn-ratereq%,%cf-dyn-ratesucc%,%cf-dyn-rateblock%,%cf-dyn-ratefail%,%cf-ratereq%,%cf-ratesucc%,%cf-rateblock%,%cf-ratefail%,%ikev2-cursa%,%ikev2-cursainit%,%ikev2-cursaresp%,%ikev2-ttlsa%,%ikev2-ttlsainit%,%ikev2-ttlsaresp%,%ikev2-attempt%,%ikev2-attemptinit%,%ikev2-attemptresp%,%ikev2-rxpacket%,%ikev2-txpacket%,%ikev2-rxoctet%,%ikev2-txoctet%,%ikev2-initfail%,%ikev2-initfail-noresp%,%ikev2-initfail-resp%,%ikev2-invcookie%,%ikev2-nattkeepalive-recv%,%ikev2-nattkeepalive-send%,%ikev2-dpd-recv%,%ikev2-dpd-send%,%ikev2-dpd-recv-reply%,%ikev2-dpd-send-reply%,%ikev2-dpd-timeout%,%ikev2-dpd-disconnect%,%ikev2-dpd-p1rekey%,%lic-combo-phone%,%lic-ecsv2%,%lic-ipservices-gateway%,%lic-evdoreva-pdsn%,%lic-scm-proxyregistrar-ietfrfc3261%,%lic-scm-proxypcscf%,%lic-scm-servingscscf%,%lic-scm-interrogatingicscf%,%lic-asngw%,%lic-asnlr%,%cf-cache-hits%,%cf-cache-misses%,%cf-cache-has-path-hits%,%cf-cache-flushes%,%sess-curimsauthorized%
> PDSNSystemSch4 | PDSN4 System Schema | EMS,PDSNSystem4,%date%,%time%,%sess-curimsauthorizing%,%pdif-curchildsa%,%ikev2-ikesadel%,%ikev2-ikesadelrep-recv%,%ikev2-ikesadelrep-sent%,%ikev2-ikesadelreq-recv%,%ikev2-ikesadelreq-sent%,%ipsec-dpd-p1rekey%
> GGSNSystemSch | GGSN System Schema | EMS,GGSNSystem,%date%,%time%,%sess-ttlarrived%,%sess-ttlrejected%,%sess-ttlconnected%,%sess-ttlauthsucc%,%sess-ttlauthfail%,%sess-ttllcpup%,%sess-ttlipcpup%,%sess-ttlsrcviol%,%sess-ttlkeepfail%,%sess-curttlcalls%,%sess-cursipconn%,%sess-curmipconn%,%sess-curactcall%,%sess-curdormcall%,%sess-curarrived%,%sess-curlcpnegot%,%sess-curlcpup%,%sess-curauth%,%sess-curauthed%,%sess-curipcpup%,%sess-curdisc%,%sess-calldur-1min%,%sess-calldur-2min%,%sess-calldur-5min%,%sess-calldur-15min%,%sess-calldur-1hour%,%sess-calldur-4hour%,%sess-calldur-12hour%,%sess-calldur-24hour%,%sess-calldur-over24hour%,%sess-setuptime-100ms%,%sess-setuptime-200ms%,%sess-setuptime-300ms%,%sess-setuptime-400ms%,%sess-setuptime-500ms%,%sess-setuptime-600ms%,%sess-setuptime-700ms%,%sess-setuptime-800ms%,%sess-setuptime-900ms%,%sess-setuptime-1sec%,%sess-setuptime-2sec%,%sess-setuptime-3sec%,%sess-setuptime-4sec%,%sess-setuptime-6sec%,%sess-setuptime-8sec%,%sess-setuptime-10sec%,%sess-setuptime-12sec%,%sess-setuptime-14sec%,%sess-setuptime-16sec%,%sess-setuptime-over16sec%,%incremental%,%enddate%,%endtime%,%localenddate%,%localendtime%,%sess-ttlfailed%,%uptime%,%uptimestr%,%lic-ggsn%,%lic-l2tplns%,%sess-txbytes%,%sess-rxbytes%,%sess-txpackets%,%sess-rxpackets%,%sess-siptxbytes%,%sess-siprxbytes%,%sess-miptxbytes%,%sess-miprxbytes%,%aaa-ttlreq%,%aaa-curreq%,%aaa-ttlauthreq%,%aaa-curauthreq%,%aaa-ttlauthprobe%,%aaa-curauthprobe%,%aaa-ttlacctreq%,%aaa-curacctreq%,%aaa-ttlauthsucc%,%aaa-ttlauthfail%,%aaa-ttlauthpurged%,%aaa-ttlauthcancelled%,%aaa-ttlauthdmuchal%,%aaa-ttlradauthreq%,%aaa-curradauthreq%,%aaa-ttlradauthreqretried%,%aaa-ttllclauthreq%,%aaa-curlclauthreq%,%aaa-ttlpseudoauthreq%,%aaa-curpseudoauthreq%,%aaa-ttlauthnulluser%,%aaa-ttlacctsucc%,%aaa-ttlacctpurged%,%aaa-ttlacctcancelled%,%aaa-ttlradacctreq%,%aaa-ttlradacctreqretried%,%disc-reason-summary%,%sess-curaaaactive%,%sess-curaaadeleting%,%sess-curaaaacctpending%,%sess-ttlemptyfwd%,%sess-ttlemptyrev%,%sess-ttlonlineprepaiderr%,%sess-ttlprepaidinitautherr%,%sess-ttlcrprpattempt%,%sess-ttlcrprpsuccess%,%sess-ttlrpcrpattempt%,%sess-ttlrpcrpsuccess%,%sess-curpmipconn%,%sess-curl2tplacconn%,%sess-curalwayson%,%sess-curbcmcsauth%,%sess-curbcmcsconn%,%sess-curhaipsecconn%,%sess-curl2tplacconnecting%,%sess-curpdptypeipconn%,%sess-curpdptypepppconn%,%sess-curprepaid%,%sess-rxpkt-1023%,%sess-rxpkt-127%,%sess-rxpkt-16%,%sess-rxpkt-2047%,%sess-rxpkt-255%,%sess-rxpkt-4095%,%sess-rxpkt-4500%,%sess-rxpkt-511%,%sess-rxpkt-64%,%sess-rxpkt-over4500%,%sess-ttldisconn%,%sess-ttlhandoff%,%sess-ttlonlineauthfail%,%sess-ttlonlineauthreq%,%sess-ttlonlineauthsucc%,%sess-ttlprepaid%,%sess-ttlproxydns-drop%,%sess-ttlproxydns-passthru%,%sess-ttlproxydns-redirect%,%sess-ttlrenewal%,%sess-txpkt-1023%,%sess-txpkt-127%,%sess-txpkt-16%,%sess-txpkt-2047%,%sess-txpkt-255%,%sess-txpkt-4095%,%sess-txpkt-4500%,%sess-txpkt-511%,%sess-txpkt-64%,%sess-txpkt-over4500%,%aaa-ttlauthkeepalive%,%aaa-curauthkeepalive%,%aaa-ttlacctkeepalive%,%aaa-curacctkeepalive%,%aaa-ttlauthkeepalivesuccess%,%aaa-ttlauthkeepalivefailure%,%aaa-ttlauthkeepalivepurged%,%aaa-ttlacctkeepalivesuccess%,%aaa-ttlacctkeepalivetimeout%,%aaa-ttlacctkeepalivepurged%,%ipsg-total-call-arrived%,%ipsg-total-call-rejected%,%ipsg-total-call-demult%,%ipsg-total-dereg-rep-sent%,%ipsg-cur-active-call%,%ipsg-total-active-serv%,%asngw-cur-active-call%,%asngw-total-sess-setup%,%asngw-retriesexhaust%,%asngw.sfs%,%asngw.tidfail%,%asngw-handoffattempt%,%asngw-handoffdenied%,%asngw-handoffcomp%,%asngw.authsucc%,%asngw-authfailures%
> PPP1Sch | PPP1 Schema | EMS,PPP1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%init%,%reneg%,%success%,%failed%,%released%,%released-local%,%released-remote%,%lcp-fail-maxretry%,%lcp-fail-option%,%ipcp-fail-maxretry%,%ipcp-fail-option%,%fail-ccp%,%fail-auth%,%entered-lcp%,%entered-auth%,%entered-ipcp%,%reneg-pdsn%,%reneg-mobile%,%reneg-addrmis%,%reneg-other%,%auth-attempt-chap%,%auth-attempt-ppp%,%auth-attemp-mschap%,%auth-success-chap%,%auth-success-pap%,%auth-success-mschap%,%auth-fail-chap%,%auth-fail-pap%,%auth-fail-mschap%,%comp-stac%,%comp-mppc%,%comp-defl%,%rcverr-basfcs%,%rcverr-unknproto%,%rcverr-badaddr%,%rcverr-badctrl%,%comp-vjhdr%,%disc-lcp-remote%,%disc-rp-remote%,%disc-admin%,%disc-idle-timeout%,%disc-abs-timeout%,%disc-ppp-keepalive%,%disc-no-resource%,%disc-misc%,%remote-term%,%misc-fail%
> PPP2Sch | PPP2 Schema | EMS,PPP2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%fail-reneg%,%lcp-fail-unknown%,%ipcp-fail-unknown%,%abort-auth%,%rp-disc%,%success-lcp%,%success-auth%,%reneg-rp_handoff%,%reneg-update%,%auth-abort-chap%,%auth-abort-pap%,%auth-abort-mschap%,%sess-skip-auth%,%comp-sess-neg%,%comp-sess-neg-fail%,%disc-rp-local%,%disc-add-flow-fail%,%disc-maxretry-lcp%,%disc-maxretry-ipcp%,%disc-max-setup-time%,%disc-bad-dest-vpn%,%disc-opt-neg-lcp%,%disc-opt-neg-ipcp%,%disc-no-remoteaddr%,%disc-typedetect-fail%,%disc-bad-src-addr%,%disc-remote%,%disc-long-timeout%,%disc-auth-fail%,%lcpecho-req-total%,%lcpecho-req-resent%,%lcpecho-rep-recved%,%lcpecho-timeout%,%recverr-ctrl-field%,%recverr-bad-length%,%in-oct%,%in-ucast%,%in-nucast%,%in-pkt%,%in-discard%,%in-discard-oct%,%out-oct%,%out-ucast%,%out-nucast%,%out-pkt%,%out-discard%,%out-discard-oct%,%num-sessions%,%lcpvse-req-total%,%lcpvse-req-resent%,%lcpvse-rep-recved%,%lcpvse-proto-reject%,%lcpvse-req-maxreach%,%svctype%,%conn-sess-reneg%,%comp-rohchdr%,%altppp-connected%,%reneg-rp-handoff%,%auth-attempt-pap%,%auth-attempt-mschap%
> MIPFA1Sch | MIPFA1 Schema | EMS,MIPFA1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%advert-send%,%disc-expiry%,%disc-dereg%,%disc-admin%,%auth-attempt%,%auth-success%,%auth-failure%,%recv-total%,%recv-initial%,%recv-renewal%,%recv-dereg%,%accept-total%,%accept-initial%,%accept-renewal%,%accept-dereg%,%denied-total%,%denied-initial%,%denied-renewal%,%denied-dereg%,%discard-total%,%discard-initial%,%discard-renewal%,%discard-dereg%,%relayed-total%,%relayed-initial%,%relayed-renewal%,%relayed-dereg%,%authfail-total%,%authfail-initial%,%authfail-renewal%,%authfail-dereg%,%denied-pdsn-total%,%denied-pdsn-initial%,%denied-pdsn-renewal%,%denied-pdsn-dereg%,%denied-ha-total%,%denied-ha-initial%,%denied-ha-renewal%,%denied-ha-dereg%,%denied-pdsn-unspec%,%denied-pdsn-timeout%,%denied-pdsn-admin%,%denied-pdsn-resource%,%denied-pdsn-mnauth%,%denied-pdsn-haauth%,%denied-pdsn-lifetoolong%,%denied-pdsn-badreq%,%denied-pdsn-badreply%,%denied-pdsn-missnai%,%denied-pdsn-misshomeagent%,%denied-pdsn-misshomeaddr%,%denied-pdsn-unkchallange%,%denied-pdsn-misschallenge%,%denied-pdsn-stalechallenge%,%denied-pdsn-mntoodistant%,%denied-pdsn-styleunavail%,%denied-pdsn-hanetunreach%,%denied-pdsn-hahostunreach%
> MIPFA2Sch | MIPFA2 Schema | EMS,MIPFA2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%denied-pdsn-haportunreach%,%denied-pdsn-haunreach%,%denied-pdsn-invcoa%,%denied-pdsn-encapunavail%,%denied-pdsn-revtununavail%,%denied-pdsn-revtunmand%,%denied-ha-faauth%,%denied-ha-badreq%,%denied-ha-mismatchid%,%denied-ha-simulbind%,%denied-ha-unknownha%,%denied-ha-revtununavail%,%replyrcv-total%,%replyrcv-totalrelayed%,%replyrcv-errors%,%replyrcv-initial%,%replyrcv-initialrelayed%,%replyrcv-renewal%,%replyrcv-renewalrelayed%,%replyrcv-dereg%,%replyrcv-deregrelayed%,%replysent-total%,%replysent-acceptreg%,%replysent-acceptdereg%,%replysent-badreq%,%replysent-lifetoolong%,%replysent-mnauthfail%,%replysent-haauthfail%,%replysent-adminprohib%,%replysent-noresources%,%replysent-revtununavail%,%replysent-revtunmand%,%replysent-senderrors%,%replysent-mntoodistant%,%replysent-invcoa%,%replysent-hanetunreach%,%replysent-hahostunreach%,%replysent-haportunreach%,%replysent-haunreach%,%replysent-regtimeout%,%replysent-missnai%,%replysent-misshomeagent%,%replysent-misshomeaddr%,%replysent-unkchallenge%,%replysent-misschallenge%,%replysent-stalechallenge%,%replysent-badreply%,%reqsent-initial%,%reqsent-initial-resend%,%reqsent-initial-noresend%,%reqsent-renew%,%reqsent-renew-resend%,%reqsent-renew-noresend%,%reqsent-dereg%,%reqsent-dereg-resend%,%reqsent-dereg-noresend%,%denied-pdsn-unkchallenge%,%denied-pdsn-unknowncvse%,%replysent-unspecified%,%replysent-delstyleunavail%,%ttlprepaid%,%curprepaid%,%ttlonlineauthsucc%,%ttlonlineauthfail%,%revoc-sent%,%revoc-retry-sent%,%revoc-ack-recv%,%revoc-timeout%,%revoc-recv%,%revoc-ack-sent%
> MIPHASch | MIPHA Schema | EMS,MIPHA,%date%,%time%,%vpnname%,%vpnid%,%servname%,%disconnects%,%expiry%,%dereg%,%admindrop%,%recv-total%,%recv-initial%,%recv-renew%,%recv-dereg%,%accept-total%,%accept-reg%,%accept-renew%,%accept-dereg%,%denied-total%,%denied-initial%,%denied-renew%,%denied-dereg%,%discard-total%,%reply-total%,%reply-acceptreg%,%reply-acceptdereg%,%reply-denied%,%reply-badreq%,%reply-mismatchid%,%reply-adminprohib%,%reply-unspecerr%,%reply-noresource%,%reply-mnauthfail%,%reply-faauthfail%,%reply-simulbind%,%reply-unknownha%,%reply-revtununavail%,%reply-revtunmand%,%reply-encapunavail%,%reply-senderror%,%farevocation%,%accept-ho%,%denied-ho%,%reply-error%,%num-sessions%,%recv-ho%,%revoc-sent%,%revoc-retry-sent%,%revoc-ack-recv%,%revoc-timeout%,%revoc-recv%,%revoc-ack-sent%,%miscerror%,%auth-attempt%,%auth-failure%,%auth-success%,%auth-real-failure%,%auth-misc-failure%,%reply-unknowncvse%,%reply-cong-drop%,%reply-cong-adminprohib%,%reply-cong-unknownha%,%reply-udp-encapunavail%,%ttlprepaid%,%curprepaid%,%ttlonlineauthsucc%,%ttlonlineauthfail%,%paaa-query-total%,%paaa-query-accept%,%paaa-query-denied%,%paaa-resp-sent%,%paaa-resp-found%,%paaa-resp-notfound%,%paaa-resp-poolover%,%paaa-resp-misc%,%ipsec-esp-txpackets%,%ipsec-esp-txbytes%,%ipsec-ah-txpackets%,%ipsec-ah-txbytes%,%ipsec-error-txpackets%,%ipsec-error-txbytes%,%ipsec-esp-rxpackets%,%ipsec-esp-rxbytes%,%ipsec-ah-rxpackets%,%ipsec-ah-rxbytes%,%ipsec-error-packets%,%ipsec-error-bytes%,%ipsec-replay-packets%,%ipsec-replay-bytes%,%ipsec-decode-packets%,%ipsec-decode-bytes%,%ipsec-auth-packets%,%ipsec-auth-bytes%,%ipsec-tooshort-packets%,%ipsec-tooshort-bytes%,%ipsec-dpdreq-sent%,%ipsec-dpdreq-recv%,%ipsec-dpdreply-sent%,%ipsec-dpdreply-recv%,%ipsec-dpdtimeout%,%ipsec-dpddisconn%,%ipsec-dpdrekey%
> MIPHA2Sch | MIPHA2 Schema | EMS,MIPHA2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%ipsec-nattkeepalive-sent%,%ipsec-nattkeepalive-recv%,%ipsec-ike-udpflows%,%ipsec-ike-cookieflows%,%ipsec-ike-txpackets%,%ipsec-ike-rxpackets%,%ipsec-ike-reqrecv%,%ipsec-ike-udpflowpackets%,%ipsec-ike-cookieflowpackets%,%ipsec-cur-tun%,%ipsec-cur-tunestablished%,%ipsec-ike-fails%,%ipsec-ttl-tun%,%ipsec-ttl-tunestablished%,%ipsec-call-req-rej%
> RP Schema | RPSch | EMS,RP,%date%,%time%,%vpnname%,%vpnid%,%servname%,%recv-total%,%accept-total%,%denied-total%,%discard-total%,%accept-initial%,%accept-intrapdsn%,%accept-interpdsn%,%denied-initial%,%accept-renew%,%denied-renew%,%accept-dereg%,%denied-dereg%,%send-error%,%hash-error%,%decode-error%,%unhandled%,%seqerror%,%deny-unspec%,%deny-adminprohib%,%deny-noresource%,%deny-auth%,%deny-idmismatch%,%deny-badrequest%,%deny-unknownpdsn%,%deny-revtununavail%,%deny-revtunreq%,%deny-unrecogvend%,%upd-total%,%upd-accept%,%upd-denied%,%upd-unack%,%upd-trans%,%upd-retrans%,%upd-received%,%upd-discard%,%upd-senderror%,%upd-upltrinit%,%upd-other%,%upd-handoff%,%upddeny-unspec%,%upddeny-adminprohib%,%upddeny-auth%,%upddeny-idmismatch%,%upddeny-badrequest%,%sec-violations%,%sec-badauth%,%sec-badid%,%sec-badspi%,%sec-mnhaauth%,%sec-regupdate%,%disc-absent%,%disc-nomem%,%disc-malform%,%disc-authfail%,%disc-bounce%,%disc-inputq%,%disc-mismatchid%,%disc-invpktlen%,%disc-misc%,%reply-total%,%recv-initial%,%accept-active-intrapdsn%,%accept-dormant-intrapdsn%,%recv-renew%,%active-start-renew%,%active-stop-renew%,%recv-dereg%,%active-stop-dereg%,%upd-ttlnoretrans%,%upd-ack-received%,%num-sessions%,%deny-sessclosed%,%deny-cong-drop%,%deny-cong-adminprohib%,%deny-cong-unknownpdsn%,%sess-num-transmitted%,%sess-accepted%,%sess-denied%,%sess-not-acknowledged%,%sess-initial-update%,%sess-update-retransmitted%,%sess-update-ack-received%,%sess-update-ack-discarded%,%sess-update-send-error%,%sess-always-on-indication%,%sess-reason-unspecified%,%sess-PDSN-auth-fail%,%sess-ID-mismatch%,%sess-poorly-formed-update%,%sess-para-not-update%,%sess-absent%,%sess-no-memory%,%sess-malformed%,%sess-auth-fail%,%sess-ID-bounce-error%,%sess-input-Q-exceeded%,%sess-mismatched-ID%,%sess-invalid-packet-length%,%sess-misc-reasons%,%sess-gre-packet-sent-sdb%,%sess-gre-byte-sent-sdb%,%ttlprepaid%,%curprepaid%,%ttlonlineauthsucc%,%ttlonlineauthfail%,%discard-initial%,%recv-initial-setupstart%,%accept-initial-setupstart%,%denied-initial-setupstart%,%discard-initial-setupstart%,%discard-renew%,%recv-renew-noairlink%,%accept-renew-noairlink%,%denied-renew-noairlink%,%discard-renew-noairlink%,%recv-renew-activestart%,%accept-renew-activestart%,%denied-renew-activestart%,%discard-renew-activestart%,%recv-renew-activestop%,%accept-renew-activestop%,%denied-renew-activestop%,%discard-renew-activestop%,%discard-dereg%,%recv-dereg-noactivestop%,%accept-dereg-noactivestop%,%denied-dereg-noactivestop%,%discard-dereg-noactivestop%,%recv-dereg-activestop%,%accept-dereg-activestop%,%denied-dereg-activestop%,%discard-dereg-activestop%,%recv-intrapdsn-activeanidhandoff%,%accept-intrapdsn-activeanidhandoff%,%denied-intrapdsn-activeanidhandoff%,%discard-intrapdsn-activeanidhandoff%,%recv-intrapdsn-dormantanidhandoff%,%accept-intrapdsn-dormantanidhandoff%,%denied-intrapdsn-dormantanidhandoff%,%discard-intrapdsn-dormantanidhandoff%,%recv-interpdsn-activemeianidhandoff%,%accept-interpdsn-activemeianidhandoff%,%denied-interpdsn-activemeianidhandoff%,%discard-interpdsn-activemeianidhandoff%,%rx-pkt-xoff%,%rx-pkt-xon%,%xontoxoff%,%pkt-dropped-xoff%,%bytes-dropped-xoff%
> RPSch2 | RP2 Schema | EMS,RP2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%a10-cursetup%,%a10-ttlreleased%,%a10-ttlsetup%,%a10aux-cursetup%,%a10aux-ttlreleased%,%a10aux-ttlsetup%,%a10main-cursetup%,%a10main-ttlreleased%,%a10main-ttlsetup%,%deny-badrequest-alractive%,%deny-badrequest-alrdorm%,%deny-badrequest-authextn%,%deny-badrequest-fieldlen%,%deny-badrequest-flags%,%deny-badrequest-hoanonzero%,%deny-badrequest-miscoaaddr%,%deny-badrequest-other%,%deny-badrequest-pkttoolong%,%deny-badrequest-pkttooshort%,%deny-badrequest-setupabsent%,%deny-badrequest-sse%,%deny-badrequest-unkextn%,%deny-badrequest-vse%,%deny-noresource-a11mgrrej%,%deny-noresource-inputq%,%deny-noresource-nomem%,%deny-noresource-nosessmgr%,%deny-noresource-policy%,%deny-noresource-sessmgrrej%,%deny-noresource-sessmgrretried%,%deny-unspec-crphandoff%,%deny-unspec-intrahandoff%,%deny-unspec-lifezero%,%deny-unspec-noairlink%,%deny-unspec-notready%,%deny-unspec-nullpkt%,%reva-rrq-accept%,%reva-rrq-denied%,%reva-rrq-recv%,%reva-rrq-reply%,%rrqdiscard-adminprohib%,%rrqdiscard-authfail%,%rrqdiscard-bounce%,%rrqdiscard-grekey%,%rrqdiscard-inputq%,%rrqdiscard-invlen%,%rrqdiscard-maxsess%,%rrqdiscard-misc%,%rrqdiscard-nomem%,%rrqdiscard-nosessmgr%,%rrqdiscard-overload%,%rrqdiscard-smgrdead%,%rrqdiscard-smgrnotready%,%rrqdiscard-unkpdsn%,%sess-currevasetup%,%sess-cursetup%,%sess-release-dereg%,%sess-release-expiry%,%sess-release-grekey%,%sess-release-other%,%sess-release-pcfmonfail%,%sess-release-ppplayer%,%sess-ttlreleased%,%sess-ttlrevasetup%,%sess-ttlsetup%,%sess-updackdisc-pktnothand%,%sess-updackdisc-sessdisc%,%sess-upddenied-adminprohib%,%sess-upddenied-handoff%,%sess-upddenied-idnotsupp%,%sess-upddenied-noresource%,%sess-updreason-alwayson%,%sess-updreason-qosinfo%,%sess-updreason-qosoptrig%,%sess-updreason-qostftviol%,%sess-updreason-qostrafpol%,%sess-updreason-qostrafviol%,%upd-discard-unhpkt%,%upd-discard-unkpcf%,%upd-lifetime%,%upd-smgrexit%
> RPSch3 | RP3 Schema | EMS,RP3,%date%,%time%,%vpnname%,%vpnid%,%servname%,%sess-ttlrevareleased%,%sess-ttlrevadowngrade%,%deny-bsninfo%,%upd-uplyrinit%,%upd-discard-absent%,%upd-discard-nomem%,%upd-discard-malform%,%upd-discard-authfail%,%upd-discard-bounce%,%upd-discard-inputq%,%upd-discard-mismatchid%,%upd-discard-invpktlen%,%upd-discard-misc%,%sess-pdsn-auth-fail%,%sess-id-mismatch%,%sess-release-purged%
> GTPC1Sch | GTPC1 Schema | EMS,GTPC1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%setup-total%,%setup-ip%,%setup-ppp%,%released-total%,%cpc-total%,%cpc-v0%,%cpc-v1%,%cpc-sec%,%cpc-retrans%,%cpc-accept%,%cpc-deny%,%cpc-discard%,%upc-rx%,%upc-rx-accept%,%upc-rx-deny%,%upc-rx-discard%,%upc-tx%,%upc-tx-accept%,%upc-tx-deny%,%dpc-rx%,%dpc-rx-accept%,%dpc-rx-deny%,%dpc-rx-discard%,%dpc-tx%,%dpc-tx-accept%,%dpc-tx-deny%,%cpc-aa%,%cpc-aa-accept%,%cpc-aa-deny%,%cpc-aa-discard%,%dpc-aa-rx%,%dpc-aa-rx-accept%,%dpc-aa-rx-deny%,%dpc-aa-rx-discard%,%dpc-aa-tx%,%dpc-aa-tx-accept%,%dpc-aa-tx-deny%,%err-ind-rx%,%err-ind-tx%,%cpc-noresource%,%cpc-addr-occupied%,%cpc-nomem%,%cpc-missing-apn%,%cpc-unknown-pdp%,%cpc-auth-fail%,%cpc-sys-fail%,%cpc-sem-tft%
> GTPC2Sch | GTPC2 Schema | EMS,GTPC2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%cpc-syn-tft%,%cpc-sem-pktfilter%,%cpc-syn-pktfilter%,%cpc-ie-err%,%cpc-ie-missing%,%cpc-opt-ie-err%,%cpc-malformed%,%cpc-version%,%disc-sgsn%,%disc-path-fail%,%disc-smgr-dead%,%disc-admin%,%disc-other%,%disc-teardown%,%disc-idle%,%disc-absolute%,%disc-src-addr%,%disc-flow-add%,%disc-dhcp-renew-fail%,%disc-long-durn%,%disc-aborted%,%disc-apn-rmvd%,%pdu-notif%,%pdu-notif-accpet%,%pdu-notif-deny%,%pdu-notif-rej%,%pdu-notif-rej-accept%,%pdu-notif-rej-deny%,%pdu-notif-rej-discard%,%sri-req%,%sri-accept%,%sri-deny%,%fail-rep%,%fail-rep-accept%,%fail-rep-deny%,%note-ms-gprs%,%note-ms-gprs-accept%,%note-ms-gprs-deny%,%note-ms-gprs-discard%,%num-bytes-in%,%num-pkts-in%,%num-bytes-out%,%num-pkts-out%,%cpc-srv-not-supp%,%gtpu-echo-req-rx%,%gtpu-echo-req-tx%,%gtpu-echo-rsp-tx%,%gtpu-echo-rsp-rx%,%ctrl-num-bytes-in%,%ctrl-num-pkts-in%,%ctrl-num-bytes-out%,%ctrl-num-pkts-out%,%echo-req-rx%,%echo-req-tx%,%echo-rsp-tx%,%echo-rsp-rx%,%setup-current%,%current-ip%,%current-ppp%,%current-ipv6%,%current-ntwkinitd%,%setup-ipv6%,%setup-sgsn%,%setup-ggsn%,%qosconv-bytes-in%,%qosconv-pkts-in%,%qosconv-bytes-out%,%qosconv-pkts-out%,%qosstrm-bytes-in%,%qosstrm-pkts-in%,%qosstrm-bytes-out%,%qosstrm-pkts-out%,%qosint1-bytes-in%,%qosint1-pkts-in%,%qosint1-bytes-out%,%qosint1-pkts-out%,%qosint2-bytes-in%,%qosint2-pkts-in%,%qosint2-bytes-out%,%qosint2-pkts-out%,%qosint3-bytes-in%,%qosint3-pkts-in%,%qosint3-bytes-out%,%qosint3-pkts-out%,%qosint-bytes-in%,%qosint-pkts-in%,%qosint-bytes-out%,%qosint-pkts-out%,%qosback-bytes-in%,%qosback-pkts-in%,%qosback-bytes-out%,%qosback-pkts-out%,%dyn-ipv4-attempt%,%dyn-ipv6-attempt%,%dyn-ppp-attempt%,%dyn-ipv4-success%,%dyn-ipv6-success%,%dyn-ppp-success%,%cpc-no-apn-subscription%
> GTPPSch | GTPP Schema | EMS,GTPP,%date%,%time%,%vpnname%,%vpnid%,%echo-req-rx%,%echo-req-tx%,%echo-rsp-rx%,%echo-rsp-tx%,%redir-rcvd%,%redir-rsp%,%node-alive%,%node-alive-rsp%,%data-rec-trans%,%dup-data-rec-trans%,%send-data-rec%,%rel-data-rec%,%cancel-data-rec%,%data-rec-trans-rsp%,%delete-node%,%node-addr%,%req-accept%,%req-not-fulfil%,%req-malform%,%version-not-supp%,%serv-not-supp%,%mand-ie-err%,%mand-ie-miss%,%opt-ie-err%,%dup-already-fulfil%,%already-fulfil%,%no-resource%,%sys-fail%,%normal-close%,%abnormal-close%,%vol-limit-close%,%time-limit-close%,%open-req%,%aaa-acct-arch%,%rdir-sys-fail%,%rdir-txbuf-full%,%rdir-rxbuf-full%,%other-node-dn%,%self-node-dn%,%rdir-no-res%,%rdir-serv-no%,%rdir-version-not-supp%,%rdir-mand-ie-miss%,%rdir-mand-ie-err%,%rdir-opt-ie-err%,%rdir-malformed%,%rdir-rsp-sys-fail%,%gss-echo-req%,%gss-echo-rsp%,%gss-gtpp-req%,%gss-gtpp-req-ret%,%gss-gtpp-rsp%,%gss-gtpp-rsp-failed%,%gss-gcdr-req%,%gss-gcdr-req-ret%,%gss-gcdr-rsp%,%gss-gcdr-rsp-failed%,%gss-aaaproxy-rec-req%,%gss-aaaproxy-rec-ret%,%gss-aaaproxy-rec-rsp%,%gss-aaaproxy-rec-rsp-failed%,%gss-aaamgr-rec-req%,%gss-aaamgr-rec-ret%,%gss-aaamgr-rec-rsp%,%gss-aaamgr-rec-rsp-failed%,%gss-update-cgf-req%,%gss-update-cgf-req-ret%,%gss-update-cgf-rsp%,%gss-update-cfg-rsp-failed%,%gss-clear-db-req%,%gss-clear-db-req-ret%,%gss-clear-db-rsp%,%gss-clear-db-rsp-failed%,%gss-update-req%,%gss-invalid-req-rcvd%
> IPPoolSch | IPPool Schema | EMS,IPPOOL,%date%,%time%,%vpnname%,%vpnid%,%name%,%used%,%hold%,%release%,%free%,%type%,%priority%,%state%,%startaddr%,%groupname%
> APNSch | APN Schema | EMS,APN,%date%,%time%,%vpnname%,%vpnid%,%apn%,%uplnk-bytes%,%dnlnk-bytes%,%uplnk-pkts%,%dnlnk-pkts%,%uplnk-drop%,%dnlnk-drop%,%bad-hdr%,%ttl-excd%,%frag-sent%,%frag-fail%,%inacl-drop%,%outacl-drop%,%bad-src-addr%,%addr-stat%,%addr-lpool%,%addr-rad%,%addr-dhcp%,%addr-dhcp-rly%,%addr-no-alloc%,%sess-curr%,%sess-curr-all%,%sess-tot%,%sess-tot-all%,%uplnk-bytes-drop%,%dnlnk-bytes-drop%,%data-fromuseravg-bps%,%data-touseravg-bps%,%data-fromusersust-bps%,%data-tousersust-bps%,%data-fromuseravg-pps%,%data-touseravg-pps%,%data-fromusersust-pps%,%data-tousersust-pps%,%qosconv-pkts-uplnk%,%qosconv-pkts-dnlnk%,%qosstrm-pkts-uplnk%,%qosstrm-pkts-dnlnk%,%qosint1-pkts-uplnk%,%qosint1-pkts-dnlnk%,%qosint2-pkts-uplnk%,%qosint2-pkts-dnlnk%,%qosint3-pkts-uplnk%,%qosint3-pkts-dnlnk%,%qosint-pkts-uplnk%,%qosint-pkts-dnlnk%,%qosback-pkts-uplnk%,%qosback-pkts-dnlnk%,%att-pdp-ctxt%,%att-deact-pdp-ggsn%,%succ-deact-pdp-ggsn%,%att-deact-pdp-ms%,%succ-deact-pdp-ms%,%dyn-ipv4-attempt%,%dyn-ipv6-attempt%,%dyn-ipv4-success%,%dyn-ipv6-success%,%auth-req-sent%,%auth-acc-rcvd%,%auth-timeout%,%acc-req-sent%,%acc-rsp-rcvd%,%acc-req-timeout%
> LAC1Sch | LAC Schema 1 | EMS,LAC1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%tun-conn-attempt%,%tun-conn-success%,%tun-conn-fail%,%tun-conn-curactive%,%sess-attempts%,%sess-successful%,%sess-failed%,%sess-curactive%,%sess-intrapdsnho-attempt%,%sess-intrapdsnho-success%,%sess-intrapdsnho-failed%,%sess-interpdsnho-attempt%,%recv-err-malformed%,%recv-err-ctrlfield%,%recv-err-pktlen%,%recv-err-avplen%,%recv-err-protover%,%recv-err-md5%,%recv-err-invattr%,%recv-err-unkattr%,%recv-err-invsessid%,%recv-err-invstate%,%recv-err-unkmsg%,%recv-err-unmatchpktlen%,%recv-err-invtunid%,%tun-genclear%,%tun-ctrlconnexists%,%tun-unauth%,%tun-badproto%,%tun-reqshutdown%,%tun-statemacherr%,%tun-badlen%,%tun-oor%,%tun-noresource%,%tun-vendspec%,%tun-tryanotherlns%,%tun-unkavp%,%tun-ipsecdisc%,%tun-ipsecfail%,%tun-license%,%tun-newcallpoldisc%,%tun-maxretry%,%tun-syslimit%,%tun-miscerr%,%sess-nogeneral%,%sess-admin%,%sess-lossofcarr%
> LAC2Sch | LAC Schema 2 | EMS,LAC2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%sess-remoteadmin%,%sess-nofactemp%,%sess-nofacperm%,%sess-invdest%,%sess-nocarrier%,%sess-busysig%,%sess-nodialtime%,%sess-lactimeout%,%sess-noframing%,%sess-noctrlconn%,%sess-badlen%,%sess-oor%,%sess-noresource%,%sess-invsessid%,%sess-vendspec%,%sess-tryanotherlns%,%sess-unkavp%,%sess-maxtunnel%,%sess-ipsecfail%,%sess-ipsecdisc%,%sess-newcallpoldisc%,%sess-license%,%sess-servmismatch%,%sess-miscerr%
> CLOSEDRP1Sch | ClosedRP Schema 1 | EMS,CLOSEDRP1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%tun-conn-attempt%,%tun-conn-success%,%tun-conn-fail%,%tun-conn-curactive%,%sess-attempts%,%sess-successful%,%sess-failed%,%sess-curactive%,%sess-intrapdsnho-attempt%,%sess-intrapdsnho-success%,%sess-intrapdsnho-failed%,%sess-interpdsnho-attempt%,%recv-err-malformed%,%recv-err-ctrlfield%,%recv-err-pktlen%,%recv-err-avplen%,%recv-err-protover%,%recv-err-md5%,%recv-err-invattr%,%recv-err-unkattr%,%recv-err-invsessid%,%recv-err-invstate%,%recv-err-unkmsg%,%recv-err-unmatchpktlen%,%recv-err-invtunid%,%tun-genclear%,%tun-ctrlconnexists%,%tun-unauth%,%tun-badproto%,%tun-reqshutdown%,%tun-statemacherr%,%tun-badlen%,%tun-oor%,%tun-noresource%,%tun-vendspec%,%tun-tryanotherlns%,%tun-unkavp%,%tun-ipsecdisc%,%tun-ipsecfail%,%tun-license%,%tun-newcallpoldisc%,%tun-maxretry%,%tun-syslimit%,%tun-miscerr%,%sess-nogeneral%,%sess-admin%,%sess-lossofcarr%
> CLOSEDRP2Sch | ClosedRP Schema 2 | EMS,CLOSEDRP2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%sess-remoteadmin%,%sess-nofactemp%,%sess-nofacperm%,%sess-invdest%,%sess-nocarrier%,%sess-busysig%,%sess-nodialtime%,%sess-lactimeout%,%sess-noframing%,%sess-noctrlconn%,%sess-badlen%,%sess-oor%,%sess-noresource%,%sess-invsessid%,%sess-vendspec%,%sess-tryanotherlns%,%sess-unkavp%,%sess-maxtunnel%,%sess-ipsecfail%,%sess-ipsecdisc%,%sess-newcallpoldisc%,%sess-license%,%sess-servmismatch%,%sess-miscerr%,%sess-hocomplete%,%sess-invho%,%sess-duplsess%,%ttlprepaid%,%curprepaid%,%ttlonlineauthsucc%,%ttlonlineauthfail%
> RADIUSSch | RADIUS Schema | EMS,RADIUS,%date%,%time%,%vpnname%,%vpnid%,%servertype%,%ipaddr%,%auth-req-sent%,%auth-req-sentwdmu%,%auth-req-pending%,%auth-req-retried%,%auth-req-retriedwdmu%,%auth-chal-rcvd%,%auth-acc-rcvd%,%auth-rej-rcvd%,%auth-rej-rcvdwdmu%,%auth-timeout%,%auth-cons-fail%,%auth-rsp-badauth%,%auth-rsp-malformed%,%auth-rsp-malformedattr%,%auth-rsp-unktype%,%auth-rsp-dropped%,%auth-rsp-roundtripusec%,%probe-issued%,%probe-success%,%probe-failed%,%probe-roundtriptimeusec%,%acc-req-sent%,%acc-req-pending%,%acc-req-retried%,%acc-rsp-rcvd%,%acc-req-timeout%,%acc-req-cons-fail%,%acc-rsp-badresp%,%acc-rsp-malformed%,%acc-rsp-unktype%,%acc-rsp-dropped%,%acc-rsp-roundtripusec%,%port%,%acc-start-sent%,%acc-stop-sent%,%acc-interim-sent%,%acc-start-retries%,%acc-stop-retries%,%acc-interim-retries%,%group%,%acc-ttl-g1%,%acc-ttl-g2%,%online-acc-req-sent%,%online-acc-req-pending%,%online-acc-req-retried%,%online-acc-rsp-rcvd%,%online-acc-rej-rcvd%,%online-acc-req-timeout%,%online-acc-rsp-badauth%,%online-acc-rsp-malformed%,%online-acc-rsp-malformedattr%,%online-acc-rsp-unktype%,%online-acc-badmsgauth%,%online-acc-nomsgauth%,%nasipaddr%,%keepalive-auth-req-sent%,%keepalive-auth-retried%,%keepalive-auth-acc-rcvd%,%keepalive-auth-timeout%,%keepalive-auth-rej-rcvd%,%keepalive-acct-req-sent%,%keepalive-acct-retried%,%keepalive-acct-success%,%keepalive-acct-timeout%,%keepalive-acct-rsp-badauth%,%cons-fail%,%keepalive-auth-rsp-badauth%,%keepalive-auth-rsp-malformed%,%keepalive-auth-rsp-malformedattr%,%keepalive-auth-rsp-unktype%,%keepalive-auth-rsp-dropped%,%acc-on-sent%,%acc-off-sent%,%acc-on-retries%,%acc-off-retries%,%keepalive-acct-rsp-malformed%,%keepalive-acct-rsp-unktype%,%keepalive-acct-rsp-dropped%
> MISCSch | Miscellaneous Schema | %ipaddr%,%host%,%uptime%,%time%,%localdate%,%localtime%,%localtz%,%time2%,%localtime2%
> MISCSchForEMS | New Miscellaneous Schema | EMS,MISC,%date%,%time%,%ipaddr%,%host%,%uptime%,%localdate%,%localtime%,%localtz%,%time2%,%localtime2%,%swversion%,%swbuild%,%localtzoffset%
> ECS1Sch | ECS1 Schema | EMS,ECS1,%date%,%time%,%ecs-subscribers%,%ecs-subscribers-cur%,%gcdrs-generated%,%edrs-generated%,%udrs-generated%,%ip-flows%,%ip-flows-cur%,%ip-uplk-bytes%,%ip-dwnlk-bytes%,%ip-uplk-pkts%,%ip-dwnlk-pkts%,%ip-uplk-pkts-frag%,%ip-dwnlk-pkts-frag%,%ip-uplk-bytes-frag%,%ip-dwnlk-bytes-frag%,%udp-flows%,%udp-flows-cur%,%udp-uplk-bytes%,%udp-dwnlk-bytes%,%udp-uplk-pkts%,%udp-dwnlk-pkts%,%udp-inv-pkts%,%tcp-flows%,%tcp-flows-cur%,%tcp-uplk-bytes%,%tcp-dwnlk-bytes%,%tcp-uplk-pkts%,%tcp-dwnlk-pkts%,%tcp-uplk-bytes-retr%,%tcp-dwnlk-bytes-retr%,%tcp-uplk-pkts-retr%,%tcp-dwnlk-pkts-retr%,%tcp-uplk-pkts-ooo-analyzd%,%tcp-dwnlk-pkts-ooo-analyzd%,%tcp-uplk-pkts-ooo-fail%,%tcp-dwnlk-pkts-ooo-fail%,%tcp-uplk-pkts-ooo-retr%,%tcp-dwnlk-pkts-ooo-retr%,%icmp-flows%,%icmp-flows-cur%,%icmp-uplk-bytes%,%icmp-dwnlk-bytes%,%icmp-uplk-pkts%,%icmp-dwnlk-pkts%,%icmp-ech-req%,%icmp-ech-rep%,%icmp-dst-unrch%,%icmp-redir%,%icmp-tm-excd%,%icmp-trace-route%,%icmp-oth%,%http-flows%,%http-flows-cur%,%http-uplk-bytes%,%http-dwnlk-bytes%,%http-uplk-pkts%,%http-dwnlk-pkts%,%http-uplk-bytes-retr%,%http-dwnlk-bytes-retr%,%http-uplk-pkts-retr%,%http-dwnlk-pkts-retr%,%http-req-succ%,%http-req-fail%,%http-get-req%,%http-post-req%,%http-connect-req%,%http-inv-pkts%,%https-flows%,%https-flows-cur%,%https-uplk-bytes%,%https-dwnlk-bytes%,%https-uplk-pkts%,%https-dwnlk-pkts%,%https-uplk-bytes-retr%,%https-dwnlk-bytes-retr%,%https-uplk-pkts-retr%,%https-dwnlk-pkts-retr%,%wtp-trans%,%wtp-cls-zero%,%wtp-cls-one%,%wtp-cls-two%,%wtp-uplk-bytes%,%wtp-dwnlk-bytes%,%wtp-uplk-pkts%,%wtp-dwnlk-pkts%,%wtp-uplk-bytes-retr%,%wtp-dwnlk-bytes-retr%,%wtp-uplk-pkts-retr%,%wtp-dwnlk-pkts-retr%,%wtp-invk-pkts%,%wtp-invk-tcl-zero%,%wtp-invk-tcl-one%,%wtp-invk-tcl-two%,%wtp-invk-tid-new%,%wtp-rslt-pkts%,%wtp-ack-to-resp%,%wtp-ack-to-init%,%wtp-abrt-to-resp%,%wtp-abrt-to-init%,%wtp-seg-invk%,%wtp-seg-rslt%,%wtp-neg-ack%,%wtp-tid-vrf%,%wtp-noninit-invk%,%wtp-unk-pdu%,%wsp-flows%,%wsp-flows-cur%,%wsp-co-conn%,%wsp-cl-conn%,%wsp-uplk-bytes%,%wsp-dwnlk-bytes%,%wsp-uplk-pkts%,%wsp-dwnlk-pkts%,%wsp-uplk-bytes-retr%,%wsp-dwnlk-bytes-retr%,%wsp-uplk-pkts-retr%,%wsp-dwnlk-pkts-retr%,%wsp-co-req-succ%,%wsp-co-req-fail%,%wsp-cl-req-succ%,%wsp-cl-req-fail%,%wsp-conn-pdu%,%wsp-conn-rep%,%wsp-redir%,%wsp-disc%,%wsp-susp%,%wsp-resm%,%wsp-opt%,%wsp-head%,%wsp-del%,%wsp-trace%,%wsp-reply%,%wsp-put%,%wsp-get%,%wsp-push%,%wsp-conf-push%,%wsp-post%,%wsp-data-frag%,%wsp-rsrvd%,%wsp-inv-pkts%,%mms-send%,%mms-send-succ%,%mms-send-fail%,%mms-retrv%,%mms-retrv-succ%,%mms-retrv-fail%,%mms-uplk-bytes%,%mms-dwnlk-bytes%,%mms-uplk-pkts%,%mms-dwnlk-pkts%,%mms-uplk-bytes-retr%,%mms-dwnlk-bytes-retr%,%mms-uplk-pkts-retr%,%mms-dwnlk-pkts-retr%,%mms-snd-req%,%mms-snd-conf%,%mms-ntf-ind%,%mms-ntf-ind-imm%,%mms-ntf-ind-del%,%mms-ntf-rsp%,%mms-retrv-conf%,%mms-ack-ind%,%mms-delvry-ind%,%mms-unk-pdu%,%mms-inv-pkts%,%sip-flows%,%sip-flows-cur%,%sip-calls%,%sip-uplk-bytes%,%sip-dwnlk-bytes%,%sip-uplk-pkts%,%sip-dwnlk-pkts%,%sip-uplk-bytes-retr%,%sip-dwnlk-bytes-retr%,%sip-uplk-pkts-retr%,%sip-dwnlk-pkts-retr%,%sip-invite%,%sip-bye%,%sip-ack%,%sip-cancel%,%sip-register%,%sip-inv-pkts%,%rtsp-flows%,%rtsp-flows-cur%,%rtsp-sess%,%rtsp-uplk-bytes%,%rtsp-dwnlk-bytes%,%rtsp-uplk-pkts%,%rtsp-dwnlk-pkts%,%rtsp-uplk-bytes-retr%,%rtsp-dwnlk-bytes-retr%,%rtsp-uplk-pkts-retr%,%rtsp-dwnlk-pkts-retr%,%rtsp-play%,%rtsp-setup%,%rtsp-pause%,%rtsp-record%,%rtsp-option%,%rtsp-redir%,%rtsp-desc%,%rtsp-announ%,%rtsp-trdwn%,%rtsp-get-param%,%rtsp-set-param%,%rtsp-inv-pkts%
> ECS2Sch | ECS2 Schema | EMS,ECS2,%date%,%time%,%rtp-flows%,%rtp-flows-cur%,%rtp-uplk-bytes%,%rtp-dwnlk-bytes%,%rtp-uplk-pkts%,%rtp-dwnlk-pkts%,%ftp-flows%,%ftp-flows-cur%,%ftp-uplk-bytes%,%ftp-dwnlk-bytes%,%ftp-uplk-pkts%,%ftp-dwnlk-pkts%,%ftp-retr%,%ftp-stor%,%ftp-inv-pkts%,%smtp-flows%,%smtp-flows-cur%,%smtp-uplk-bytes%,%smtp-dwnlk-bytes%,%smtp-uplk-pkts%,%smtp-dwnlk-pkts%,%smtp-uplk-bytes-retr%,%smtp-dwnlk-bytes-retr%,%smtp-uplk-pkts-retr%,%smtp-dwnlk-pkts-retr%,%smtp-unk-cmd%,%smtp-unk-resp%,%smtp-req-succ%,%smtp-req-fail%,%smtp-helo%,%smtp-ehlo%,%smtp-mail-frm%,%smtp-rcpt-to%,%smtp-data%,%smtp-bdat%,%smtp-vrfy%,%smtp-expn%,%smtp-noop%,%smtp-rset%,%smtp-quit%,%smtp-inv-pkts%,%pop3-flows%,%pop3-flows-cur%,%pop3-uplk-bytes%,%pop3-dwnlk-bytes%,%pop3-uplk-pkts%,%pop3-dwnlk-pkts%,%pop3-uplk-bytes-retr%,%pop3-dwnlk-bytes-retr%,%pop3-uplk-pkts-retr%,%pop3-dwnlk-pkts-retr%,%pop3-retr%,%pop3-retr-succ%,%pop3-list%,%pop3-list-succ%,%pop3-inv-pkts%,%imap-uplk-bytes%,%imap-dwnlk-bytes%,%imap-uplk-pkts%,%imap-dwnlk-pkts%,%imap-uplk-bytes-retr%,%imap-dwnlk-bytes-retr%,%imap-uplk-pkts-retr%,%imap-dwnlk-pkts-retr%,%imap-req-succ%,%imap-req-fail%,%imap-reply-untag%,%imap-reply-commcont%,%imap-unk-command%,%imap-unk-reply%,%p2p-flows%,%p2p-flows-cur%,%p2p-skype-uplnk-bytes%,%p2p-skype-dwlnk-bytes%,%p2p-skype-uplnk-pkts%,%p2p-skype-dwlnk-pkts%,%p2p-bittorrent-uplnk-bytes%,%p2p-bittorrent-dwlnk-bytes%,%p2p-bittorrent-uplnk-pkts%,%p2p-bittorrent-dwlnk-pkts%,%p2p-edonkey-uplnk-bytes%,%p2p-edonkey-dwlnk-bytes%,%p2p-edonkey-uplnk-pkts%,%p2p-edonkey-dwlnk-pkts%,%p2p-msn-uplnk-bytes%,%p2p-msn-dwlnk-bytes%,%p2p-msn-uplnk-pkts%,%p2p-msn-dwlnk-pkts%,%p2p-yahoo-uplnk-bytes%,%p2p-yahoo-dwlnk-bytes%,%p2p-yahoo-uplnk-pkts%,%p2p-yahoo-dwlnk-pkts%
> ECS3Sch | ECS3 Schema | EMS,ECS3,%date%,%time%,%p2p-orb-uplnk-bytes%,%p2p-orb-dwlnk-bytes%,%p2p-orb-uplnk-pkts%,%p2p-orb-dwlnk-pkts%,%p2p-winny-uplnk-bytes%,%p2p-winny-dwlnk-bytes%,%p2p-winny-uplnk-pkts%,%p2p-winny-dwlnk-pkts%,%p2p-slingbox-uplnk-bytes%,%p2p-slingbox-dwlnk-bytes%,%p2p-slingbox-uplnk-pkts%,%p2p-slingbox-dwlnk-pkts%,%p2p-fasttrack-uplnk-bytes%,%p2p-fasttrack-dwlnk-bytes%,%p2p-fasttrack-uplnk-pkts%,%p2p-fasttrack-dwlnk-pkts%,%p2p-gnutella-uplnk-bytes%,%p2p-gnutella-dwlnk-bytes%,%p2p-gnutella-uplnk-pkts%,%p2p-gnutella-dwlnk-pkts%,%p2p-jabber-uplnk-bytes%,%p2p-jabber-dwlnk-bytes%,%p2p-jabber-uplnk-pkts%,%p2p-jabber-dwlnk-pkts%,%ecs-ttlsuccess%,%ecs-ttlfail%,%ecs-curactive%,%ecs-15peak-curactive%,%ecs-ruleshit%,%ecs-ttldlinkbytes%,%ecs-ttlulinkbytes%,%ecs-ttldlinkpackets%,%ecs-ttlulinkpackets%,%ecs-ttlflowconn%,%ecs-ttlflowdisc%,%ecs-curflow%,%ecs-15peak-curflow%,%ecs-15min-usage-flowall%,%dns-dwnlk-bytes%,%dns-dwnlk-pkts%,%dns-flows%,%dns-flows-cur%,%dns-inv-pkts%,%dns-over-tcp-dwnlk-bytes%,%dns-over-tcp-dwnlk-pkts%,%dns-over-tcp-uplk-bytes%,%dns-over-tcp-uplk-pkts%,%dns-req-a-query%,%dns-req-cname-query%,%dns-req-ns-query%,%dns-req-ptr-query%,%dns-req-unknown-query%,%dns-rsp-a-query%,%dns-rsp-cname-query%,%dns-rsp-ns-query%,%dns-rsp-ptr-query%,%dns-rsp-unknown-query%,%dns-unk-opcode%,%dns-uplk-bytes%,%dns-uplk-pkts%,%icmp-inv-pkts%,%p2p-applejuice-dwlnk-bytes%,%p2p-applejuice-dwlnk-pkts%,%p2p-applejuice-uplnk-bytes%,%p2p-applejuice-uplnk-pkts%,%p2p-ares-dwlnk-bytes%,%p2p-ares-dwlnk-pkts%,%p2p-ares-uplnk-bytes%,%p2p-ares-uplnk-pkts%,%p2p-directconnect-dwlnk-bytes%,%p2p-directconnect-dwlnk-pkts%,%p2p-directconnect-uplnk-bytes%,%p2p-directconnect-uplnk-pkts%,%p2p-feidian-dwlnk-bytes%,%p2p-feidian-dwlnk-pkts%,%p2p-feidian-uplnk-bytes%,%p2p-feidian-uplnk-pkts%
> ECS4Sch | ECS4 Schema | EMS,ECS4,%date%,%time%,%p2p-filetopia-dwlnk-bytes%,%p2p-filetopia-dwlnk-pkts%,%p2p-filetopia-uplnk-bytes%,%p2p-filetopia-uplnk-pkts%,%p2p-gadugadu-dwlnk-bytes%,%p2p-gadugadu-dwlnk-pkts%,%p2p-gadugadu-uplnk-bytes%,%p2p-gadugadu-uplnk-pkts%,%p2p-imesh-dwlnk-bytes%,%p2p-imesh-dwlnk-pkts%,%p2p-imesh-uplnk-bytes%,%p2p-imesh-uplnk-pkts%,%p2p-manolito-dwlnk-bytes%,%p2p-manolito-dwlnk-pkts%,%p2p-manolito-uplnk-bytes%,%p2p-manolito-uplnk-pkts%,%p2p-msn-non-voice-dwlnk-bytes%,%p2p-msn-non-voice-dwlnk-pkts%,%p2p-msn-non-voice-uplnk-bytes%,%p2p-msn-non-voice-uplnk-pkts%,%p2p-msn-voice-dwlnk-bytes%,%p2p-msn-voice-dwlnk-pkts%,%p2p-msn-voice-uplnk-bytes%,%p2p-msn-voice-uplnk-pkts%,%p2p-mute-dwlnk-bytes%,%p2p-mute-dwlnk-pkts%,%p2p-mute-uplnk-bytes%,%p2p-mute-uplnk-pkts%,%p2p-pando-dwlnk-bytes%,%p2p-pando-dwlnk-pkts%,%p2p-pando-uplnk-bytes%,%p2p-pando-uplnk-pkts%,%p2p-pplive-dwlnk-bytes%,%p2p-pplive-dwlnk-pkts%,%p2p-pplive-uplnk-bytes%,%p2p-pplive-uplnk-pkts%,%p2p-ppstream-dwlnk-bytes%,%p2p-ppstream-dwlnk-pkts%,%p2p-ppstream-uplnk-bytes%,%p2p-ppstream-uplnk-pkts%,%p2p-qq-dwlnk-bytes%,%p2p-qq-dwlnk-pkts%,%p2p-qqlive-dwlnk-bytes%,%p2p-qqlive-dwlnk-pkts%,%p2p-qqlive-uplnk-bytes%,%p2p-qqlive-uplnk-pkts%,%p2p-qq-uplnk-bytes%,%p2p-qq-uplnk-pkts%,%p2p-skinny-dwlnk-bytes%,%p2p-skinny-dwlnk-pkts%,%p2p-skinny-uplnk-bytes%,%p2p-skinny-uplnk-pkts%,%p2p-skype-non-voice-dwlnk-bytes%,%p2p-skype-non-voice-dwlnk-pkts%,%p2p-skype-non-voice-uplnk-bytes%,%p2p-skype-non-voice-uplnk-pkts%,%p2p-skype-voice-dwlnk-bytes%,%p2p-skype-voice-dwlnk-pkts%,%p2p-skype-voice-uplnk-bytes%,%p2p-skype-voice-uplnk-pkts%,%p2p-sopcast-dwlnk-bytes%,%p2p-sopcast-dwlnk-pkts%,%p2p-sopcast-uplnk-bytes%,%p2p-sopcast-uplnk-pkts%,%p2p-soulseek-dwlnk-bytes%,%p2p-soulseek-dwlnk-pkts%,%p2p-soulseek-uplnk-bytes%
> ECS5Sch | ECS5 Schema | EMS,ECS5,%date%,%time%,%p2p-soulseek-uplnk-pkts%,%p2p-yahoo-non-voice-dwlnk-bytes%,%p2p-yahoo-non-voice-dwlnk-pkts%,%p2p-yahoo-non-voice-uplnk-bytes%,%p2p-yahoo-non-voice-uplnk-pkts%,%p2p-yahoo-voice-dwlnk-bytes%,%p2p-yahoo-voice-dwlnk-pkts%,%p2p-yahoo-voice-uplnk-bytes%,%p2p-yahoo-voice-uplnk-pkts%,%p2p-zattoo-dwlnk-bytes%,%p2p-zattoo-dwlnk-pkts%,%p2p-zattoo-uplnk-bytes%,%p2p-zattoo-uplnk-pkts%
> IPSGSch | IPSG Schema | EMS,IPSG,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%rad-servaddr%,%rad-servport%,%total-start-req-rcv%,%total-interim-update-req-rcv%,%total-stop-req-rcv%,%total-unknown-req-rcv%,%total-rsp-sent%,%total-start-req-retrans-rcv%,%total-start-rsp-sent%,%total-discard-msgs-unknown-clnt%,%total-discard-msgs-ignore-interim%,%total-discard-msgs-ignore-stop%,%total-discard-msgs-incorrect-secret%,%total-discard-msgs-attr-missing%
> ASNGW1Sch | ASNGW1 Schema | EMS,ASNGW1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%peeripaddr%,%r6mspreattreq-totsent%,%r6mspreattreq-retranssent%,%r6mspreattreq-totrec%,%r6mspreattreq-totacc%,%r6mspreattreq-totdenied%,%r6mspreattreq-totdiscard%,%r6mspreattreq-badform%,%r6mspreattreq-decodeerr%,%r6mspreattreq-unspecerr%,%r6mspreattreq-missmandtlv%,%r6mspreattreq-tlvvalinval%,%r6mspreattreq-unknowntlv%,%r6mspreattreq-duptlvfound%,%r6mspreattreq-nosessfound%,%r6mspreattreq-transiderr%,%r6mspreattrsp-totsent%,%r6mspreattrsp-retranssent%,%r6mspreattrsp-totrec%,%r6mspreattrsp-totacc%,%r6mspreattrsp-totdenied%,%r6mspreattrsp-totdiscard%,%r6mspreattrsp-badform%,%r6mspreattrsp-decodeerr%,%r6mspreattrsp-unspecerr%,%r6mspreattrsp-missmandtlv%,%r6mspreattrsp-tlvvalinval%,%r6mspreattrsp-unknowntlv%,%r6mspreattrsp-duptlvfound%,%r6mspreattrsp-nosessfound%,%r6mspreattrsp-transiderr%,%r6mspreattack-totsent%,%r6mspreattack-retranssent%,%r6mspreattack-totrec%,%r6mspreattack-totacc%,%r6mspreattack-totdenied%,%r6mspreattack-totdiscard%,%r6mspreattack-badform%,%r6mspreattack-decodeerr%,%r6mspreattack-unspecerr%,%r6mspreattack-missmandtlv%,%r6mspreattack-tlvvalinval%,%r6mspreattack-unknowntlv%,%r6mspreattack-duptlvfound%,%r6mspreattack-nosessfound%,%r6mspreattack-transiderr%,%r6contextreq-totsent%,%r6contextreq-retranssent%,%r6contextreq-totrec%,%r6contextreq-totacc%,%r6contextreq-totdenied%,%r6contextreq-totdiscard%,%r6contextreq-badform%,%r6contextreq-decodeerr%,%r6contextreq-unspecerr%,%r6contextreq-missmandtlv%,%r6contextreq-tlvvalinval%,%r6contextreq-unknowntlv%,%r6contextreq-duptlvfound%,%r6contextreq-nosessfound%,%r6contextreq-transiderr%,%r6contextrepo-totsent%,%r6contextrepo-retranssent%,%r6contextrepo-totrec%,%r6contextrepo-totacc%,%r6contextrepo-totdenied%,%r6contextrepo-totdiscard%
> ASNGW2Sch | ASNGW2 Schema | EMS,ASNGW2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%peeripaddr%,%r6contextrepo-badform%,%r6contextrepo-decodeerr%,%r6contextrepo-unspecerr%,%r6contextrepo-missmandtlv%,%r6contextrepo-tlvvalinval%,%r6contextrepo-unknowntlv%,%r6contextrepo-duptlvfound%,%r6contextrepo-nosessfound%,%r6contextrepo-transiderr%,%r6contextack-totsent%,%r6contextack-retranssent%,%r6contextack-totrec%,%r6contextack-totacc%,%r6contextack-totdenied%,%r6contextack-totdiscard%,%r6contextack-badform%,%r6contextack-decodeerr%,%r6contextack-unspecerr%,%r6contextack-missmandtlv%,%r6contextack-tlvvalinval%,%r6contextack-unknowntlv%,%r6contextack-duptlvfound%,%r6contextack-nosessfound%,%r6contextack-transiderr%,%r6autheaptra-totsent%,%r6autheaptra-retranssent%,%r6autheaptra-totrec%,%r6autheaptra-totacc%,%r6autheaptra-totdenied%,%r6autheaptra-totdiscard%,%r6autheaptra-badform%,%r6autheaptra-decodeerr%,%r6autheaptra-unspecerr%,%r6autheaptra-missmandtlv%,%r6autheaptra-tlvvalinval%,%r6autheaptra-unknowntlv%,%r6autheaptra-duptlvfound%,%r6autheaptra-nosessfound%,%r6autheaptra-transiderr%,%r6autheaptra-outofordrcd%,%r6autheapsta-totrec%,%r6autheapsta-totacc%,%r6autheapsta-totdenied%,%r6autheapsta-totdiscard%,%r6autheapsta-badform%,%r6autheapsta-decodeerr%,%r6autheapsta-unspecerr%,%r6autheapsta-missmandtlv%,%r6autheapsta-tlvvalinval%,%r6autheapsta-unknowntlv%,%r6autheapsta-duptlvfound%,%r6autheapsta-nosessfound%,%r6autheapsta-transiderr%,%r6autheapsta-outofordrcd%,%r6autheapsta-noresourcedrop%,%r6autheapsta-bsinireauth%,%r6msattreq-totsent%,%r6msattreq-retranssent%,%r6msattreq-totrec%,%r6msattreq-totacc%,%r6msattreq-totdenied%,%r6msattreq-totdiscard%,%r6msattreq-badform%,%r6msattreq-decodeerr%,%r6msattreq-unspecerr%,%r6msattreq-missmandtlv%,%r6msattreq-tlvvalinval%,%r6msattreq-unknowntlv%
> ASNGW3Sch | ASNGW3 Schema | EMS,ASNGW3,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%peeripaddr%,%r6msattreq-duptlvfound%,%r6msattreq-nosessfound%,%r6msattreq-transiderr%,%r6msattrsp-totsent%,%r6msattrsp-retranssent%,%r6msattrsp-totrec%,%r6msattrsp-totacc%,%r6msattrsp-totdenied%,%r6msattrsp-totdiscard%,%r6msattrsp-badform%,%r6msattrsp-decodeerr%,%r6msattrsp-unspecerr%,%r6msattrsp-missmandtlv%,%r6msattrsp-tlvvalinval%,%r6msattrsp-unknowntlv%,%r6msattrsp-duptlvfound%,%r6msattrsp-nosessfound%,%r6msattrsp-transiderr%,%r6msattack-totsent%,%r6msattack-retranssent%,%r6msattack-totrec%,%r6msattack-totacc%,%r6msattack-totdenied%,%r6msattack-totdiscard%,%r6msattack-badform%,%r6msattack-decodeerr%,%r6msattack-unspecerr%,%r6msattack-missmandtlv%,%r6msattack-tlvvalinval%,%r6msattack-unknowntlv%,%r6msattack-duptlvfound%,%r6msattack-nosessfound%,%r6msattack-transiderr%,%r6datapathregreq-totsent%,%r6datapathregreq-retranssent%,%r6datapathregreq-totrec%,%r6datapathregreq-totacc%,%r6datapathregreq-totdenied%,%r6datapathregreq-totdiscard%,%r6datapathregreq-badform%,%r6datapathregreq-decodeerr%,%r6datapathregreq-unspecerr%,%r6datapathregreq-missmandtlv%,%r6datapathregreq-tlvvalinval%,%r6datapathregreq-unknowntlv%,%r6datapathregreq-duptlvfound%,%r6datapathregreq-nosessfound%,%r6datapathregreq-transiderr%,%r6datapathregrsp-totsent%,%r6datapathregrsp-retranssent%,%r6datapathregrsp-totrec%,%r6datapathregrsp-totacc%,%r6datapathregrsp-totdenied%,%r6datapathregrsp-totdiscard%,%r6datapathregrsp-badform%,%r6datapathregrsp-decodeerr%,%r6datapathregrsp-unspecerr%,%r6datapathregrsp-missmandtlv%,%r6datapathregrsp-tlvvalinval%,%r6datapathregrsp-unknowntlv%,%r6datapathregrsp-duptlvfound%,%r6datapathregrsp-nosessfound%,%r6datapathregrsp-transiderr%,%r6datapathregack-totsent%
> ASNGW4Sch | ASNGW4 Schema | EMS,ASNGW4,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%peeripaddr%,%r6datapathregack-retranssent%,%r6datapathregack-totrec%,%r6datapathregack-totacc%,%r6datapathregack-totdenied%,%r6datapathregack-totdiscard%,%r6datapathregack-badform%,%r6datapathregack-decodeerr%,%r6datapathregack-unspecerr%,%r6datapathregack-missmandtlv%,%r6datapathregack-tlvvalinval%,%r6datapathregack-unknowntlv%,%r6datapathregack-duptlvfound%,%r6datapathregack-nosessfound%,%r6datapathregack-transiderr%,%r6datapathderegreq-totsent%,%r6datapathderegreq-retranssent%,%r6datapathderegreq-totrec%,%r6datapathderegreq-totacc%,%r6datapathderegreq-totdenied%,%r6datapathderegreq-totdiscard%,%r6datapathderegreq-badform%,%r6datapathderegreq-decodeerr%,%r6datapathderegreq-unspecerr%,%r6datapathderegreq-missmandtlv%,%r6datapathderegreq-tlvvalinval%,%r6datapathderegreq-unknowntlv%,%r6datapathderegreq-duptlvfound%,%r6datapathderegreq-nosessfound%,%r6datapathderegreq-transiderr%,%r6datapathderegrsp-totsent%,%r6datapathderegrsp-retranssent%,%r6datapathderegrsp-totrec%,%r6datapathderegrsp-totacc%,%r6datapathderegrsp-totdenied%,%r6datapathderegrsp-totdiscard%,%r6datapathderegrsp-badform%,%r6datapathderegrsp-decodeerr%,%r6datapathderegrsp-unspecerr%,%r6datapathderegrsp-missmandtlv%,%r6datapathderegrsp-tlvvalinval%,%r6datapathderegrsp-unknowntlv%,%r6datapathderegrsp-duptlvfound%,%r6datapathderegrsp-nosessfound%,%r6datapathderegrsp-transiderr%,%r6keychadir-totsent%,%r6keychadir-retranssent%,%r6keychadir-totrec%,%r6keychadir-totacc%,%r6keychadir-totdenied%,%r6keychadir-totdiscard%,%r6keychadir-badform%,%r6keychadir-decodeerr%,%r6keychadir-unspecerr%,%r6keychadir-missmandtlv%,%r6keychadir-tlvvalinval%,%r6keychadir-unknowntlv%,%r6keychadir-duptlvfound%,%r6keychadir-nosessfound%,%r6keychadir-transiderr%
> ASNGW5Sch | ASNGW5 Schema | EMS,ASNGW5,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%peeripaddr%,%r6keychaack-totsent%,%r6keychaack-retranssent%,%r6keychaack-totrec%,%r6keychaack-totacc%,%r6keychaack-totdenied%,%r6keychaack-totdiscard%,%r6keychaack-badform%,%r6keychaack-decodeerr%,%r6keychaack-unspecerr%,%r6keychaack-missmandtlv%,%r6keychaack-tlvvalinval%,%r6keychaack-unknowntlv%,%r6keychaack-duptlvfound%,%r6keychaack-nosessfound%,%r6keychaack-transiderr%,%r6unknown-totrec%,%r6unknown-totacc%,%r6unknown-totdenied%,%r6unknown-totdiscard%,%r6unknown-badform%,%r6unknown-decodeerr%,%r6unknown-unspecerr%,%r6unknown-missmandtlv%,%r6unknown-tlvvalinval%,%r6unknown-unknowntlv%,%r6unknown-duptlvfound%,%r6unknown-nosessfound%,%r6unknown-transiderr%,%r6datagrerec-totpackrec%,%r6datagrerec-prottyperrror%,%r6datagrerec-totbytrec%,%r6datagrerec-grekeyabs%,%r6datagrerec-grechkerr%,%r6datagrerec-invpacklen%,%r6datagrerec-nosessfou%,%r6datagrerec-unspecerr%,%r6datagresend-totpacksent%,%r6datagresend-senderr%,%r6datagresend-totbytsent%,%r6datagresend-unspeerr%
> SGSN1Sch | SGSN1 Schema | EMS,SGSN1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%3G-attached%,%2G-attached%,%3G-home-subscribers%,%2G-home-subscribers%,%3G-visiting-national%,%2G-visiting-national%,%3G-visiting-foreign%,%2G-visiting-foreign%,%pmm-connected%,%pmm-idle%,%3G-IMSI-Attch%,%2G-IMSI-Attch%,%3G-ptmsi-Attch%,%2G-ptmsi-Attch%,%3G-attach-accept%,%2G-attch-accept%,%3G-attach-complete%,%2G-attach-complete%,%3G-attach-reject%,%2G-attach-reject%,%3G-intra-rau%,%2G-intra-rau%,%3G-periodic-rau%,%2G-periodic-rau%,%3G-inter-sgsn-rau%,%2G-inter-sgsn-rau%,%3G-rau-complete%,%2G-rau-complete%,%3G-rau-reject%,%2G-rau-reject%,%3G-ms-init-detach%,%2G-ms-init-detach%,%3G-nw-init-detach%,%2G-nw-init-detach%,%3G-ms-init-detach-accept%,%2G-ms-init-detach-accept%,%3G-nw-init-detach-accept%,%2G-nw-init-detach-accept%,%3G-signalling-service-request%,%2G-signalling-service-request%,%3G-data-service-request%,%2G-data-service-request%,%3G-service-response%,%2G-service-response%,%3G-service-reject%,%2G-service-reject%,%3G-paging-request%,%2G-paging-request%,%3G-gmm-status-sent%,%2G-gmm-status-sent%,%3G-gmm-status-rcvd%,%2G-gmm-status-rcvd%,%3G-auth-cipher-request%,%2G-auth-cipher-request%,%3G-auth-cipher-response%,%2G-auth-cipher-response%,%3G-auth-cipher-reject%,%2G-auth-cipher-reject%,%3G-auth-cipher-mac-fail%,%2G-auth-cipher-mac-fail%,%3G-auth-cipher-syn-fail%,%2G-auth-cipher-syn-fail%,%3G-ptmsi-realloc%,%2G-ptmsi-realloc%,%3G-ptmsi-realloc-complete%,%2G-ptmsi-realloc-complete%,%3G-imsi-identity-request%,%2G-imsi-identity-request%,%3G-imeisv-identity-request%,%2G-imeisv-identity-request%,%3G-imsi-identity-response%,%2G-imsi-identity-response%,%3G-imeisv-identity-response%,%2G-imeisv-identity-response%,%3G-unknown-identity-response%,%2G-unknown-identity-response%
> SGSN2Sch | SGSN2 Schema | EMS,SGSN2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%common-id-sent%,%sec-mode-command%,%sec-mode-complete%,%sec-mode-reject%,%Iu-release-request%,%Iu-release-command%,%Iu-release-complete%,%Reset-received%,%Retransmitted-reset-received%,%Reset-Ack-sent%,%Reset-sent%,%Retransmitted-reset-sent%,%Reset-Ack-received%,%Resource-reset-received%,%Resource-reset-ack-sent%,%Resource-reset-sent%,%Resource-reset-ack-received%,%Error-indication-rcvd%,%Relocation-required%,%Relocation-command%,%Relocation-request%,%Relocation-request-ack%,%Relocation-failure%,%Relocation-prep-failure%,%Relocation-cancel%,%Relocation-cancel-ack%,%Relocation-detect%,%Relocation-complete%,%Forward-srns-context%,%GMM-received-nas-pdu%,%GMM-sent-nas-pdu%,%SM-received-nas-pdu%,%SM-sent-nas-pdu%,%Unidentified-nas-pdu%,%3G-total-actv-req%,%3G-total-actv-accept%,%3G-ms-modify-req%,%3G-ms-modify-accept%,%3G-nw-modify-req%,%3G-nw-modify-accept%,%3G-ms-deactv-req%,%3G-ms-deactv-accept%,%3G-sgsn-init-deact-req%,%3G-sgsn-init-deact-acc%,%RNC-rab-modify-req%,%RNC-rab-rel-req%,%rab-assign-req%,%rab-assign-rsp%,%rab-set/mod-req%,%rab-set/mod-acc%,%rab-rel-req%,%rab-rel-accept%,%map-open-req-tx%,%map-open-req-rx%,%map-open-rsp-tx%,%map-open-rsp-rx%,%map-close-tx%,%map-close-rx%,%map-abort-tx%,%map-abort-rx%,%map-gprs-update-loc-req-tx%,%map-gprs-update-loc-rsp-tx%,%map-gprs-update-loc-err-tx%,%map-gprs-update-loc-timeouts-rx%,%map-cancel-loc-req-rx%,%map-cancel-loc-rsp-tx%,%map-cancel-loc-err-tx%,%map-del-subs-req-rx%,%map-del-subs-rsp-tx%,%map-del-subs-ret-tx%,%map-auth-timeouts-rcvd%,%map-purge-timeouts-rcvd%,%map-insert-subs-rcvd%,%map-standalone-isd-rcvd%,%map-isd-rsp-tx%,%map-isd-err-tx%,%map-auth-fail-rept-req-tx%,%map-auth-fail-rept-rsp-rx%,%map-auth-fail-rept-err-rx%
> SGSN3Sch | SGSN3 Schema | EMS,SGSN3,%date%,%time%,%vpnname%,%vpnid%,%servname%,%map-auth-fail-rept-timeouts-rcvd%,%map-hlr-reset-rcvd%,%tcap-total-active-trans%,%tcap-total-active-invoks%,%tcap-total-msg-drops%,%tcap-total-msg-rcvd%,%tcap-total-msg-sent%,%tcap-total-abort-rcvd%,%tcap-total-abort-sent%,%tcap-total-comp-rx%,%tcap-total-comp-tx%,%tcap-comp-reterr-rx%,%tcap-comp-reterr-tx%,%tcap-comp-retrej-rx%,%tcap-comp-retrej-tx%,%tcap-tran-incorrect-rx%,%tcap-tran-incorrect-tx%,%tcap-tran-badformed-rx%,%tcap-tran-badformed-tx%,%tcap-tran-unrecognised-rx%,%tcap-tran-unrecognised-tx%,%tcap-comp-incorrect-rx%,%tcap-comp-incorrect-tx%,%tcap-comp-badformed-rx%,%tcap-comp-badformed-tx%,%tcap-comp-unrec-invid-res-rx%,%tcap-comp-unrec-invid-res-tx%,%tcap-comp-unexp-res-rx%,%tcap-comp-unexp-res-tx%,%tcap-user-unrec-opcode-rx%,%tcap-user-unrec-opcode-tx%,%tcap-user-incorr-params-rx%,%tcap-user-incorr-params-tx%,%tcap-user-resourcelimit-rx%,%tcap-user-resourcelimit-tx%,%rab-set/mod-tmr-expired%,%rab-rel-tmr-expired%,%3G-rau-accept-intra%,%3G-rau-accept-inter%,%2G-rau-accept-intra%,%2G-rau-accept-inter%,%3G-attached-with-pdp%,%3G-attached-no-pdp%,%3G-gmm-info-sent%,%2G-gmm-info-sent%,%3G-auth-cipher-rsp-sres-mismatch%,%2G-auth-cipher-rsp-sres-mismatch%,%3G-auth-unacceptable%,%2G-auth-unacceptable%,%3G-imei-identity-request%,%2G-imei-identity-request%,%3G-imei-identity-response%,%2G-imei-identity-response%,%Initial-UE-Rcvd%,%Direct-Trans-Rcvd%,%Error-indication-sent%,%3G-total-num-actv-pdp%,%3G-primary-actv-req%,%3G-primary-actv-accept%,%3G-primary-actv-reject%,%3G-secondary-actv-req%,%3G-secondary-actv-acc%,%3G-secondary-actv-rej%,%3G-dupl-ti-pdpactive%,%3G-dupl-nsapi-pdpactv%,%3G-dupl-pdpaddr-apn-pdpactv%,%3G-dupl-ti-n-pdpactive%,%3G-dupl-pdpaddr-apn-n-pdpactv%,%3G-ms-modify-rej%,%3G-nw-modify-rej%,%3G-ms-deactv-reject%
> SGSN4Sch | SGSN4 Schema | EMS,SGSN4,%date%,%time%,%vpnname%,%vpnid%,%servname%,%3G-sgsn-init-deact-rej%,%3G-total-sm-status-req-rx%,%3G-total-sm-status-req-tx%,%RNC-rab-modify-num%,%RNC-rab-rel-num%,%rab-set/mod-fail%,%rab-rel-fail%,%rab-queued%,%total-rab-rej%,%SRNS-ctxt-req-sent%,%SRNS-ctxt-rsp-rcvd%,%SRNS-ctxt-req-tmr-expired%,%SRNS-ctxt-total-pdp-acc%,%SRNS-ctxt-total-pdp-rej%,%SRNS-data-fwd-cmd-sent%,%map-auth-req-tx%,%map-auth-succes%,%map-auth-fail%,%map-imei-req-tx%,%map-imei-succes%,%map-imei-fail%,%map-imei-timeout%,%map-purge-req-tx%,%map-purge-success%,%map-purge-fail%,%tcap-uni-dir-msg-rcvd%,%tcap-uni-dir-msg-sent%,%tcap-begin-msg-rcvd%,%tcap-begin-msg-sent%,%tcap-continue-msg-rcvd%,%tcap-continue-msg-sent%,%tcap-end-msg-rcvd%,%tcap-end-msg-sent%,%tcap-total-comp-invoke-rx%,%tcap-total-comp-invoke-tx%,%tcap-comp-retresult-rx%,%tcap-comp-retresult-tx%,%tcap-tran-unrec-msgtype-rx%,%tcap-tran-unrec-msgtype-tx%,%tcap-tran-resource-limit-rx%,%tcap-tran-resource-limit-tx%,%tcap-comp-unrecognised-rx%,%tcap-comp-unrecognised-tx%,%tcap-comp-unrec-linkid-rx%,%tcap-comp-unrec-linkid-tx%,%tcap-comp-unrec-invid-err-rx%,%tcap-comp-unrec-invid-err-tx%,%tcap-comp-unexp-err-rx%,%tcap-comp-unexp-err-tx%,%tcap-user-duplicate-invid-rx%,%tcap-user-duplicate-invid-tx%,%tcap-user-unexp-linked-resp-rx%,%tcap-user-unexp-linked-resp-tx%,%tcap-user-unexp-linked-oper-rx%,%tcap-user-unexp-linked-oper-tx%,%tcap-user-res-incorr-params-rx%,%tcap-user-res-incorr-params-tx%,%tcap-user-res-unrec-errcode-rx%,%tcap-user-res-unrec-errcode-tx%,%tcap-user-res-unexp-errcode-rx%,%tcap-user-res-unexp-errcode-tx%,%tcap-user-err-incorr-params-rx%,%tcap-user-err-incorr-params-tx%,%tcap-user-initiate-release-rx%,%tcap-user-initiate-release-tx%,%3G-dupl-nsapi-n-pdpactv%,%Direct-Trans-Sent%,%3G-T3350-expiry%
> SGSN5Sch | SGSN5 Schema | EMS,SGSN5,%date%,%time%,%vpnname%,%vpnid%,%servname%,%2G-T3350-expiry%,%3G-T3360-expiry%,%2G-T3360-expiry%,%3G-T3370-expiry%,%2G-T3370-expiry%,%3G-T3322-expiry%,%2G-T3322-expiry%,%3G-T3313-expiry%,%2G-T3313-expiry%,%mcc%,%mnc%,%lac%,%rac%,%2G-local-ptmsi-Attch%,%2G-paging-success%,%2G-remote-ptmsi-Attch%,%3G-actv-rej-apn-restriction-incompatible%,%3G-actv-rej-by-ggsn%,%3G-actv-rej-conditional-ie-err%,%3G-actv-rej-ie-non-existent%,%3G-actv-rej-insufficient-resources%,%3G-actv-rej-invalid-mandatory-info%,%3G-actv-rej-missing-or-unknown-apn%,%3G-actv-rej-msg-not-compatible-with-prot-state%,%3G-actv-rej-msg-type-non-existent%,%3G-actv-rej-network-failure%,%3G-actv-rej-odb%,%3G-actv-rej-pdp-notft-actv%,%3G-actv-rej-prot-err-unspecified%,%3G-actv-rej-recovery-on-timer-expiry%,%3G-actv-rej-semantically-incorrect%,%3G-actv-rej-semantic-err-in-pkt-filter%,%3G-actv-rej-semantic-error-tft-operation%,%3G-actv-rej-service-not-subscribed%,%3G-actv-rej-service-not-supported%,%3G-actv-rej-svc-opt-tmp-out-of-order%,%3G-actv-rej-syntax-err-in-pkt-filter%,%3G-actv-rej-syntax-err-in-tft-operation%,%3G-actv-rej-unknown-pdp-addr-type%,%3G-actv-rej-unknown-pdp-context%,%3G-actv-rej-unspecified-error%,%3G-actv-rej-usr-auth-failed%,%3G-attach-rej-congestion%,%3G-attach-rej-illegal-me%,%3G-attach-rej-illegal-ms%,%3G-attach-rej-implicitly-detach%,%3G-attach-rej-imsi-unknown-at-hlr%,%3G-attach-rej-network-failure%,%3G-attach-rej-plmn-not-allowed%,%3G-attach-rej-unknown-cause%,%3G-detached%,%3G-ggsn-init-deact-acc%,%3G-ggsn-init-deact-rej%,%3G-ggsn-init-deact-req%,%3G-gprs-and-non-gprs-service-not-allowed%,%3G-gprs-service-not-allowed%,%3G-gprs-service-not-allowed-in-this-plmn%,%3G-hlr-init-deact-acc%,%3G-hlr-init-deact-rej%,%3G-hlr-init-deact-req%,%3G-local-ptmsi-Attch%
> SGSN6Sch | SGSN6 Schema | EMS,SGSN6,%date%,%time%,%vpnname%,%vpnid%,%servname%,%3G-no-suitable-cells-in-location-area%,%3G-paging-success%,%3G-total-attach-req%,%exist-conn-proc-rej-overload%,%new-connection-rejected-overload%,%3G-total-actv-pdp-with-dir-tunnel%,%3G-remote-ptmsi-Attch%,%3G-roaming-not-allowed-in-this-location-area%,%3G-inter-rau-reject%,%3G-total-inter-rau-failure%,%3G-rau-accept-periodic%,%3G-periodic-rau-reject%,%3G-total-periodic-rau-failure%,%3G-intra-rau-reject%,%3G-total-intra-rau-failure%,%3G-total-attach-fail%,%3G-total-actv-reject%,%3G-total-actv-fail%,%3G-intra-rau-rej-imsi-unknown-hlr%,%2G-intra-rau-rej-imsi-unknown-hlr%,%3G-intra-rau-rej-illegal-ms%,%2G-intra-rau-rej-illegal-ms%,%3G-intra-rau-rej-illegal-me%,%2G-intra-rau-rej-illegal-me%,%3G-intra-rau-rej-gprs-svc-not-allw%,%2G-intra-rau-rej-gprs-svc-not-allw%,%3G-intra-rau-rej-nongprs-svc-not-allow%,%2G-intra-rau-rej-nongprs-svc-not-allow%,%3G-intra-rau-rej-msid-not-derived-by-nw%,%2G-intra-rau-rej-msid-not-derived-by-nw%,%3G-intra-rau-rej-implicitly-detach%,%2G-intra-rau-rej-implicitly-detach%,%3G-intra-rau-rej-plmn-not-allowed%,%2G-intra-rau-rej-plmn-not-allowed%,%3G-intra-rau-rej-loc-area-not-allow%,%2G-intra-rau-rej-loc-area-not-allow%,%3G-intra-rau-rej-roam-not-allow-larea%,%2G-intra-rau-rej-roam-not-allow-larea%,%3G-intra-rau-rej-gprs-svc-not-allow-plmn%,%2G-intra-rau-rej-gprs-svc-not-allow-plmn%,%3G-intra-rau-rej-no-cells-in-loc-area%,%2G-intra-rau-rej-no-cells-in-loc-area%,%3G-intra-rau-rej-msc-not-reachable%,%2G-intra-rau-rej-msc-not-reachable%,%3G-intra-rau-rej-network-failure%,%2G-intra-rau-rej-network-failure%,%3G-intra-rau-rej-mac-failure%,%2G-intra-rau-rej-mac-failure%,%3G-intra-rau-rej-syn-failure%,%2G-intra-rau-rej-syn-failure%,%3G-intra-rau-rej-congestion%,%2G-intra-rau-rej-congestion%
> SGSN7Sch | SGSN7 Schema | EMS,SGSN7,%date%,%time%,%vpnname%,%vpnid%,%servname%,%3G-intra-rau-rej-gsm-auth-unacceptable%,%2G-intra-rau-rej-gsm-auth-unacceptable%,%3G-intra-rau-rej-no-pdp-ctx-actv%,%2G-intra-rau-rej-no-pdp-ctx-actv%,%3G-intra-rau-rej-retry-from-new-cell%,%2G-intra-rau-rej-retry-from-new-cell%,%3G-intra-rau-rej-inval-mand-info%,%2G-intra-rau-rej-inval-mand-info%,%3G-intra-rau-rej-msg-type-non-exist%,%2G-intra-rau-rej-msg-type-non-exist%,%3G-intra-rau-rej-mtype-incompat-pstate%,%2G-intra-rau-rej-mtype-incompat-pstate%,%3G-intra-rau-rej-ie-non-existent%,%2G-intra-rau-rej-ie-non-existent%,%3G-intra-rau-rej-cond-ie-error%,%2G-intra-rau-rej-cond-ie-error%,%3G-intra-rau-rej-msg-incompat-prot-state%,%2G-intra-rau-rej-msg-incompat-prot-state%,%3G-intra-rau-rej-prot-error%,%2G-intra-rau-rej-prot-error%,%3G-intra-rau-rej-unknown-error%,%2G-intra-rau-rej-unknown-error%,%3G-intra-prau-rej-imsi-unknown-hlr%,%2G-intra-prau-rej-imsi-unknown-hlr%,%3G-intra-prau-rej-illegal-ms%,%2G-intra-prau-rej-illegal-ms%,%3G-intra-prau-rej-illegal-me%,%2G-intra-prau-rej-illegal-me%,%3G-intra-prau-rej-gprs-svc-not-allow%,%2G-intra-prau-rej-gprs-svc-not-allow%,%3G-intra-prau-rej-nongprs-svc-not-allow%,%2G-intra-prau-rej-nongprs-svc-not-allow%,%3G-intra-prau-rej-msid-not-derived-by-nw%,%2G-intra-prau-rej-msid-not-derived-by-nw%,%3G-intra-prau-rej-implicitly-detach%,%2G-intra-prau-rej-implicitly-detach%,%3G-intra-prau-rej-plmn-not-allowed%,%2G-intra-prau-rej-plmn-not-allowed%,%3G-intra-prau-rej-loc-area-not-allowed%,%2G-intra-prau-rej-loc-area-not-allowed%,%3G-intra-prau-rej-roam-not-allowed-larea%,%2G-intra-prau-rej-roam-not-allowed-larea%,%3G-intra-prau-rej-gprs-svc-not-allowed-plmn%,%2G-intra-prau-rej-gprs-svc-not-allowed-plmn%,%3G-intra-prau-rej-congestion%,%2G-intra-prau-rej-congestion%
> SGSN8Sch | SGSN8 Schema | EMS,SGSN8,%date%,%time%,%vpnname%,%vpnid%,%servname%,%3G-intra-prau-rej-gsm-auth-unacceptable%,%2G-intra-prau-rej-gsm-auth-unacceptable%,%3G-intra-prau-rej-no-pdp-ctx-actv%,%2G-intra-prau-rej-no-pdp-ctx-actv%,%3G-intra-prau-rej-retry-from-new-cell%,%2G-intra-prau-rej-retry-from-new-cell%,%3G-intra-prau-rej-sem-wrong-msg%,%2G-intra-prau-rej-sem-wrong-msg%,%3G-intra-prau-rej-inval-mand-info%,%2G-intra-prau-rej-inval-mand-info%,%3G-intra-prau-rej-msg-type-non-exist%,%2G-intra-prau-rej-msg-type-non-exist%,%3G-intra-prau-rej-mtype-incompat-pstate%,%2G-intra-prau-rej-mtype-incompat-pstate%,%3G-intra-prau-rej-ie-non-existent%,%2G-intra-prau-rej-ie-non-existent%,%3G-intra-prau-rej-cond-ie-error%,%2G-intra-prau-rej-cond-ie-error%,%3G-intra-prau-rej-msg-incompat-pstate%,%2G-intra-prau-rej-msg-incompat-pstate%,%3G-intra-prau-rej-prot-error%,%2G-intra-prau-rej-prot-error%,%3G-intra-prau-rej-unknown-error%,%2G-intra-prau-rej-unknown-error%,%3G-inter-rau-rej-imsi-unknown-hlr%,%2G-inter-rau-rej-imsi-unknown-hlr%,%3G-inter-rau-rej-illegal-ms%,%2G-inter-rau-rej-illegal-ms%,%3G-inter-rau-rej-illegal-me%,%2G-inter-rau-rej-illegal-me%,%3G-inter-rau-rej-gprs-svc-not-allow%,%2G-inter-rau-rej-gprs-svc-not-allow%,%3G-inter-rau-rej-nongprs-svc-not-allow%,%2G-inter-rau-rej-nongprs-svc-not-allow%,%3G-inter-rau-rej-msid-not-derived-by-nw%,%2G-inter-rau-rej-msid-not-derived-by-nw%,%3G-inter-rau-rej-implicitly-detach%,%2G-inter-rau-rej-implicitly-detach%,%3G-inter-rau-rej-plmn-not-allowed%,%2G-inter-rau-rej-plmn-not-allowed%,%3G-inter-rau-rej-loc-area-not-allowed%,%2G-inter-rau-rej-loc-area-not-allowed%,%3G-inter-rau-rej-roam-not-allowed-larea%,%2G-inter-rau-rej-roam-not-allowed-larea%,%3G-inter-rau-rej-gprs-svc-not-allowed-plmn%,%2G-inter-rau-rej-gprs-svc-not-allowed-plmn%
> SGSN9Sch | SGSN9 Schema | EMS,SGSN9,%date%,%time%,%vpnname%,%vpnid%,%servname%,%3G-inter-rau-rej-no-cells-in-location-area%,%2G-inter-rau-rej-no-cells-in-location-area%,%3G-inter-rau-rej-msc-not-reachable%,%2G-inter-rau-rej-msc-not-reachable%,%3G-inter-rau-rej-network-failure%,%2G-inter-rau-rej-network-failure%,%3G-inter-rau-rej-mac-failure%,%2G-inter-rau-rej-mac-failure%,%3G-inter-rau-rej-syn-failure%,%2G-inter-rau-rej-syn-failure%,%3G-inter-rau-rej-congestion%,%2G-inter-rau-rej-congestion%,%3G-inter-rau-rej-gsm-auth-unacceptable%,%2G-inter-rau-rej-gsm-auth-unacceptable%,%3G-inter-rau-rej-no-pdp-ctx-actv%,%2G-inter-rau-rej-no-pdp-ctx-actv%,%3G-inter-rau-rej-retry-from-new-cell%,%2G-inter-rau-rej-retry-from-new-cell%,%3G-inter-rau-rej-sem-wrong-msg%,%2G-inter-rau-rej-sem-wrong-msg%,%3G-inter-rau-rej-inval-mand-info%,%2G-inter-rau-rej-inval-mand-info%,%3G-inter-rau-rej-msg-type-non-exist%,%2G-inter-rau-rej-msg-type-non-exist%,%3G-inter-rau-rej-mtype-incompat-pstate%,%2G-inter-rau-rej-mtype-incompat-pstate%,%3G-inter-rau-rej-ie-non-existent%,%2G-inter-rau-rej-ie-non-existent%,%3G-inter-rau-rej-cond-ie-error%,%2G-inter-rau-rej-cond-ie-error%,%3G-inter-rau-rej-msg-not-compat-pstate%,%2G-inter-rau-rej-msg-not-compat-pstate%,%3G-inter-rau-rej-prot-error%,%2G-inter-rau-rej-prot-error%,%3G-inter-rau-rej-unknown-error%,%2G-inter-rau-rej-unknown-error%,%3G-intra-ra-upd-rau-fail-iu_release%,%3G-intra-ra-upd-rau-fail-ongoing-proc%,%2G-intra-ra-upd-rau-fail-ongoing-proc%,%3G-intra-perio-rau-fail-iu_release%,%3G-intra-perio-rau-fail-ongoing-proc%,%2G-intra-perio-rau-fail-ongoing-proc%,%3G-inter-rau-fail-iu_release%,%3G-inter-rau-fail-ongoing-proc%,%2G-inter-rau-fail-ongoing-proc%,%3G-attach-fail-iu_release%,%3G-attach-fail-ongoing-proc%,%2G-attach-fail-ongoing-proc%
> SGSNASch | SGSNA Schema | EMS,SGSNA,%date%,%time%,%vpnname%,%vpnid%,%servname%,%2G-total-attach-fail%,%3G-total-rau-failure%,%2G-total-rau-failure%,%2G-rau-accept-periodic%,%3G-ret-rau-accept-periodic%,%2G-ret-rau-accept-periodic%,%2G-intra-rau-reject%,%2G-periodic-rau-reject%,%2G-inter-rau-reject%,%2G-total-intra-rau-failure%,%2G-total-periodic-rau-failure%,%2G-total-inter-rau-failure%,%2G-total-actv-req%,%2G-total-actv-accept%,%2G-total-num-actv-pdp%,%2G-primary-actv-req%,%2G-primary-actv-accept%,%2G-total-actv-reject%,%2G-primary-actv-reject%,%2G-secondary-actv-req%,%2G-secondary-actv-acc%,%2G-secondary-actv-rej%,%2G-actv-rej-odb%,%2G-actv-rej-insufficient-resources%,%2G-actv-rej-network-failure%,%2G-actv-rej-missing-or-unknown-apn%,%2G-actv-rej-unknown-pdp-addr-type%,%2G-actv-rej-usr-auth-failed%,%2G-actv-rej-by-ggsn%,%2G-actv-rej-unspecified-error%,%2G-actv-rej-service-not-supported%,%2G-actv-rej-service-not-subscribed%,%2G-actv-rej-svc-opt-tmp-out-of-order%,%2G-actv-rej-apn-restriction-incompatible%,%2G-actv-rej-semantically-incorrect%,%2G-actv-rej-invalid-mandatory-info%,%2G-actv-rej-msg-type-non-existent%,%2G-actv-rej-ie-non-existent%,%2G-actv-rej-conditional-ie-err%,%2G-actv-rej-msg-not-compatible-with-prot-state%,%2G-actv-rej-recovery-on-timer-expiry%,%2G-actv-rej-prot-err-unspecified%,%2G-actv-rej-llc-sndcp-fail%,%2G-actv-rej-qos-not-acc%,%2G-actv-rej-semantic-error-tft-operation%,%2G-actv-rej-syntax-err-in-tft-operation%,%2G-actv-rej-unknown-pdp-context%,%2G-actv-rej-semantic-err-in-pkt-filter%,%2G-actv-rej-syntax-err-in-pkt-filter%,%2G-actv-rej-pdp-notft-actv%,%2G-dupl-ti-pdpactive%,%2G-dupl-nsapi-pdpactv%,%2G-dupl-pdpaddr-apn-pdpactv%,%2G-dupl-ti-n-pdpactive%,%2G-dupl-nsapi-n-pdpactv%,%2G-dupl-pdpaddr-apn-n-pdpactv%
> SGSNBSch | SGSNB Schema | EMS,SGSNB,%date%,%time%,%vpnname%,%vpnid%,%servname%,%2G-ms-modify-req%,%2G-ms-modify-accept%,%2G-ms-modify-rej%,%2G-nw-modify-req%,%2G-nw-ret-modify-req%,%2G-nw-modify-accept%,%2G-nw-modify-rej%,%2G-modify-rej-insufficient-resources%,%2G-modify-rej-service-opt-not-supported%,%2G-modify-rej-semantic-err-tft-operation%,%2G-modify-rej-syntax-err-tft-operation%,%2G-modify-rej-semnatic-err-pkt-filter%,%2G-modify-rej-syntax-err-pkt-filter%,%2G-modify-rej-semnatic-incorrect-message%,%2G-modify-rej-invalid-mand-info%,%2G-modify-rej-msg-non-existent%,%2G-modify-rej-ie-non-existent%,%2G-modify-rej-conditional-ie-err%,%2G-modify-rej-msg-not-compatible-prot-state%,%2G-modify-rej-rcvry-on-tmr-expiry%,%2G-modify-rej-prot-err-unspec%,%2G-ms-deactv-req%,%2G-ms-deactv-accept%,%2G-ms-deactv-reject%,%2G-ms-deactv-rej-rx-odb%,%2G-ms-deactv-rej-rx-mbms-cap-insuff-res%,%2G-ms-deactv-rej-rx-llc-sndcp-fail-gb%,%2G-ms-deactv-rej-rx-insuff-res%,%2G-ms-deactv-rej-rx-miss-unkwn-apn%,%2G-ms-deactv-rej-rx-unkwn-pdp-addr%,%2G-ms-deactv-rej-rx-usr-auth-fail%,%2G-ms-deactv-rej-rx-actv-rej-ggsn%,%2G-ms-deactv-rej-rx-actv-rej-unspec%,%2G-ms-deactv-rej-rx-service-opt-no-support%,%2G-ms-deactv-rej-rx-service-opt-no-subs%,%2G-ms-deactv-rej-rx-svc-opt-temp-out-order%,%2G-ms-deactv-rej-rx-nsapi-already-used%,%2G-ms-deactv-rej-rx-reg-deactv%,%2G-ms-deactv-rej-rx-qos-not-acc%,%2G-ms-deactv-rej-rx-nwt-fail%,%2G-ms-deactv-rej-rx-reactivation-req%,%2G-ms-deactv-rej-rx-no-feature-support%,%2G-ms-deactv-rej-rx-sem-err-tft-op%,%2G-ms-deactv-rej-rx-syn-err-tft-op%,%2G-ms-deactv-rej-rx-unknown-ctx%,%2G-ms-deactv-rej-rx-ctx-no-tft-already-actv%,%2G-ms-deactv-rej-rx-mcast-grp-mem-tout%,%2G-ms-deactv-rej-rx-sem-err-pkt-filter%,%2G-ms-deactv-rej-rx-syn-err-pkt-filter%,%2G-ms-deactv-rej-rx-invalid-trans-id%
> SGSNCSch | SGSNC Schema | EMS,SGSNC,%date%,%time%,%vpnname%,%vpnid%,%servname%,%2G-ms-deactv-rej-rx-sem-incorrect-msg%,%2G-ms-deactv-rej-rx-inval-mand-info%,%2G-ms-deactv-rej-rx-msg-non-existent%,%2G-ms-deactv-rej-rx-ie-non-existent%,%2G-ms-deactv-rej-rx-cond-ie-err%,%2G-ms-deactv-rej-rx-prot-err-unspec%,%2G-ms-deactv-rej-rx-apn-rest-incomap-actv-pdp%,%2G-ms-deactv-rej-rx-msg-not-compat-prot-state%,%2G-ms-deactv-rej-rx-rcvry-on-tmr-expiry%,%2G-sgsn-init-deact-req%,%2G-sgsn-init-deact-acc%,%2G-sgsn-init-deact-rej%,%2G-ggsn-init-deact-req%,%2G-ggsn-init-deact-acc%,%2G-ggsn-init-deact-rej%,%2G-hlr-init-deact-req%,%2G-hlr-init-deact-acc%,%2G-hlr-init-deact-rej%,%2G-nw-deactv-rej-tx-odb%,%2G-nw-deactv-rej-tx-mbms-cap-insuff-res%,%2G-nw-deactv-rej-tx-llc-sndcp-fail-gb%,%2G-nw-deactv-rej-tx-insuff-res%,%2G-nw-deactv-rej-tx-miss-unkwn-apn%,%2G-nw-deactv-rej-tx-unkwn-pdp-addr%,%2G-nw-deactv-rej-tx-usr-auth-fail%,%2G-nw-deactv-rej-tx-actv-rej-ggsn%,%2G-nw-deactv-rej-tx-actv-rej-unspec%,%2G-nw-deactv-rej-tx-service-opt-no-support%,%2G-nw-deactv-rej-tx-service-opt-no-subs%,%2G-nw-deactv-rej-tx-svc-opt-temp-out-order%,%2G-nw-deactv-rej-tx-nsapi-already-used%,%2G-nw-deactv-rej-tx-reg-deactv%,%2G-nw-deactv-rej-tx-qos-not-acc%,%2G-nw-deactv-rej-tx-nwt-fail%,%2G-nw-deactv-rej-tx-reactivation-req%,%2G-nw-deactv-rej-tx-no-feature-support%,%2G-nw-deactv-rej-tx-sem-err-tft-op%,%2G-nw-deactv-rej-tx-syn-err-tft-op%,%2G-nw-deactv-rej-tx-unknown-ctx%,%2G-nw-deactv-rej-tx-ctx-no-tft-already-actv%,%2G-nw-deactv-rej-tx-mcast-grp-mem-tout%,%2G-nw-deactv-rej-tx-sem-err-pkt-filter%,%2G-nw-deactv-rej-tx-syn-err-pkt-filter%,%2G-nw-deactv-rej-tx-invalid-trans-id%,%2G-nw-deactv-rej-tx-sem-incorrect-msg%,%2G-nw-deactv-rej-tx-inval-mand-info%,%2G-nw-deactv-rej-tx-msg-non-existent%,%2G-nw-deactv-rej-tx-ie-non-existent%
> SGSNDSch | SGSND Schema | EMS,SGSND,%date%,%time%,%vpnname%,%vpnid%,%servname%,%2G-nw-deactv-rej-tx-cond-ie-err%,%2G-nw-deactv-rej-tx-prot-err-unspec%,%2G-nw-deactv-rej-tx-apn-rest-incomap-actv-pdp%,%2G-nw-deactv-rej-tx-msg-not-compat-prot-state%,%2G-nw-deactv-rej-tx-rcvry-on-tmr-expiry%,%2G-total-sm-status-req-rx%,%2G-total-sm-status-req-tx%
> SGTPSch | SGTP Schema | EMS,SGTP,%date%,%time%,%vpn-name%,%vpn-id%,%service-name%,%sgtpc-cpc-req-v1-pri%,%sgtpc-cpc-req-v0-pri%,%sgtpc-cpc-req-sec%,%sgtpc-cpc-req-accept%,%sgtpc-cpc-rsp-v1-pri%,%sgtpc-cpc-rsp-v0-pri%,%sgtpc-cpc-rsp-sec%,%sgtpc-upc-req-v1-tx%,%sgtpc-upc-req-v0-tx%,%sgtpc-upc-req-v1-rx%,%sgtpc-upc-req-v0-rx%,%sgtpc-upc-req-accept-tx%,%sgtpc-upc-req-accept-rx%,%sgtpc-dpc-req-v1-tx%,%sgtpc-dpc-req-v0-tx%,%sgtpc-dpc-req-v1-rx%,%sgtpc-dpc-req-v0-rx%,%sgtpc-dpc-req-accept-tx%,%sgtpc-dpc-req-accept-rx%,%sgtpc-ident-req-v1-tx%,%sgtpc-ident-req-v0-tx%,%sgtpc-ident-req-v1-rx%,%sgtpc-ident-req-v0-rx%,%sgtpc-ident-req-accept-tx%,%sgtpc-ident-req-accept-rx%,%sgtpc-sgsn-ctxt-req-v1-tx%,%sgtpc-sgsn-ctxt-req-v0-tx%,%sgtpc-sgsn-ctxt-req-v1-rx%,%sgtpc-sgsn-ctxt-req-v0-rx%,%sgtpc-sgsn-ctxt-req-accept-tx%,%sgtpc-sgsn-ctxt-req-accept-rx%,%sgtpc-sgsn-ctxt-ack-accept-tx%,%sgtpc-sgsn-ctxt-ack-accept-rx%,%sgtpc-fwd-reloc-req-tx%,%sgtpc-fwd-reloc-req-rx%,%sgtpc-fwd-reloc-discard-tx%,%sgtpc-fwd-reloc-req-accept-tx%,%sgtpc-fwd-reloc-req-accept-rx%,%sgtpc-fwd-srnsctxt-req-tx%,%sgtpc-fwd-srnsctxt-req-rx%,%sgtpc-fwd-srnsctxt-discard-rx%,%sgtpc-fwd-srnsctxt-ack-tx%,%sgtpc-fwd-srnsctxt-ack-rx%,%sgtpc-fwd-reloc-compl-tx%,%sgtpc-fwd-reloc-compl-rx%,%sgtpc-reloc-cncl-req-tx%,%sgtpc-reloc-cncl-req-rx%,%sgtpc-reloc-cncl-req-accept-tx%,%sgtpc-reloc-cncl-req-accept-rx%,%sgtpc-v1-echo-req-tx%,%sgtpc-v1-echo-req-rx%,%sgtpc-v1-echo-rsp-tx%,%sgtpc-v1-echo-rsp-rx%,%sgtpu-ggsn-pkt-sent%,%sgtpu-rnc-pkt-sent%,%sgtpu-sgsn-pkt-sent%,%sgtpu-ggsn-pkt-rcvd%,%sgtpu-rnc-pkt-rcvd%,%sgtpu-sgsn-pkt-rcvd%,%sgtpu-echo-req-tx%,%sgtpu-echo-req-rx%,%sgtpu-echo-rsp-tx%,%sgtpu-echo-rsp-rx%,%sgtpu-ggsn-errind-sent%,%sgtpu-ggsn-errind-rcvd%,%sgtpu-rnc-errind-sent%,%sgtpu-rnc-errind-rcvd%,%sgtpu-total-active-ggsn%,%sgtpu-total-active-rnc%
> SGTP2Sch | SGTP2 Schema | EMS,SGTP2,%date%,%time%,%vpn-name%,%vpn-id%,%service-name%,%sgtpc-total-cpc-req%,%sgtpc-cpc-req-denied%,%sgtpc-total-upc-req%,%sgtpc-upc-req-denied-tx%,%sgtpc-upc-req-denied-rx%,%sgtpc-total-dpc-req%,%sgtpc-dpc-req-denied-tx%,%sgtpc-dpc-req-denied-rx%,%sgtpc-ident-req-denied-tx%,%sgtpc-ident-req-denied-rx%,%sgtpc-sgsn-ctxt-req-denied-tx%,%sgtpc-sgsn-ctxt-req-denied-rx%,%sgtpc-sgsn-ctxt-ack-denied-tx%,%sgtpc-sgsn-ctxt-ack-denied-rx%,%sgtpc-fwd-reloc-denied-tx%,%sgtpc-fwd-reloc-denied-rx%,%sgtpc-fwd-srnsctxt-ack-denied-tx%,%sgtpc-fwd-srnsctxt-ack-denied-rx%,%sgtpc-fwd-rel-compl-ack-accept-tx%,%sgtpc-fwd-rel-compl-ack-accept-rx%,%sgtpc-fwd-rel-compl-ack-denied-tx%,%sgtpc-fwd-rel-compl-ack-denied-rx%,%sgtpc-reloc-cncl-denied-tx%,%sgtpc-reloc-cncl-denied-rx%,%sgtpc-ver-not-supported-rx%,%sgtpc-ver-not-supported-tx%,%sgtpc-supp-extn-hdr-notif-rx%,%sgtpc-supp-extn-hdr-notif-tx%,%sgtpu-ggsn-byts-sent%,%sgtpu-rnc-byts-sent%,%sgtpu-sgsn-byts-sent%,%sgtpu-ggsn-byts-rcvd%,%sgtpu-ggsn-pkt-queued%,%sgtpu-ggsn-byts-queued%,%sgtpu-ggsn-pkt-queue-full%,%sgtpu-ggsn-byts-queue-full%,%sgtpu-ggsn-pkt-unkwn-sess%,%sgtpu-ggsn-byts-unkwn-sess%,%sgtpu-ggsn-pkt-suspended-st%,%sgtpu-ggsn-byts-suspended-st%,%sgtpu-ggsn-pkt-invalid-msg-length%,%sgtpu-ggsn-byts-invalid-msg-length%,%sgtpu-rnc-byts-rcvd%,%sgtpu-rnc-pkt-queued%,%sgtpu-rnc-byts-queued%,%sgtpu-rnc-pkt-queue-full%,%sgtpu-rnc-byts-queue-full%,%sgtpu-rnc-pkt-unkwn-sess%,%sgtpu-rnc-byts-unkwn-sess%,%sgtpu-rnc-pkt-sess-dealloc%,%sgtpu-rnc-byts-sess-dealloc%,%sgtpu-rnc-pkt-invalid-msg-length%,%sgtpu-rnc-byts-invalid-msg-length%,%sgtpu-rnc-pkt-source-ip-viol%,%sgtpu-rnc-byts-source-ip-viol%,%sgtpu-sgsn-byts-rcvd%,%sgtpu-sgsn-pkt-queued%,%sgtpu-sgsn-byts-queued%,%sgtpu-sgsn-pkt-queue-full%,%sgtpu-sgsn-byts-queue-full%
> SGTP3Sch | SGTP3 Schema | EMS,SGTP3,%date%,%time%,%vpn-name%,%vpn-id%,%service-name%,%sgtpu-sgsn-pkt-unkwn-sess%,%sgtpu-sgsn-byts-unkwn-sess%,%sgtpu-sgsn-pkt-iu-release%,%sgtpu-sgsn-byts-iu-release%,%sgtpu-sgsn-pkt-invalid-msg-length%,%sgtpu-sgsn-byts-invalid-msg-length%,%sgtpc-v0-echo-req-tx%,%sgtpc-v0-echo-req-rx%,%sgtpc-v0-echo-rsp-tx%,%sgtpc-v0-echo-rsp-rx%,%sgtpu-ggsn-pkt-sess-dealloc%,%sgtpu-ggsn-byts-sess-dealloc%,%sgtpu-ggsn-pkt-page-fail%,%sgtpu-ggsn-byts-page-fail%,%sgtpu-ggsn-pkt-v0-seq-num-nt-pres%,%sgtpu-ggsn-byts-v0-seq-num-nt-pres%,%sgtpu-rnc-pkt-rau-in-active-st%,%sgtpu-rnc-byts-rau_in_active-st%,%sgtpu-rnc-pkt-reg_in_rau%,%sgtpu-rnc-byts-reg_in_rau%,%sgtpu-rnc-pkt-suspended-st%,%sgtpu-rnc-byts-suspended-st%,%sgtpu-sgsn-pkt-inconsistent-tunnel-state%,%sgtpu-sgsn-byts-inconsistent-tunnel-state%,%sgtpu-sgsn-pkt-sess-dealloc%,%sgtpu-sgsn-byts-sess-dealloc%,%sgtpu-total-ggsn-pkt-drop%,%sgtpu-total-ggsn-byts-drop%,%sgtpu-total-sgsn-pkt-drop%,%sgtpu-total-sgsn-byts-drop%,%sgtpu-total-rnc-pkt-drop%,%sgtpu-total-rnc-byts-drop%,%sgtpu-ggsn-pkt-drop-suspend-dealloc-st%,%sgtpu-ggsn-byts-drop-suspend-dealloc-st%,%sgtpu-rnc-pkt-rau-in-active-reg-st%,%sgtpu-rnc-byts-rau_in_active-reg-st%,%sgtpu-rnc-pkt-drop-suspended-dealloc-st%,%sgtpu-rnc-byts-drop-suspended-dealloc-st%,%sgtpu-total-pkt-ctxt-preserved%,%sgtpu-total-byts-ctxt-preserved%,%sgtpc-paket-discarded%,%sgtpc-v1-retrnas-echo-req-tx%,%sgtpc-v0-retrnas-echo-req-tx%,%sgtpu-errors-payload-length-mismatch%,%sgtpu-rnc-byts-unknown-version%,%sgtpu-rnc-pkt-unknown-version%,%sgtpu-ggsn-byts-unknown-version%,%sgtpu-sgsn-byts-unknown-version%,%sgtpu-ggsn-pkt-unknown-version%,%sgtpu-sgsn-pkt-unknown-version%,%iups-service%,%rnc-address%,%ggsn-address%
> SCCPSch | SCCP Schema | EMS,SCCP,%date%,%time%,%sccp-nw-id%,%ssa-txed%,%ss-oos-grant-txed%,%ss-oos-req-txed%,%ssp-txed%,%ss-status-test-txed%,%ssa-rcvd%,%ss-oos-grant-rcvd%,%ss-oos-req-rcvd%,%ss-prohibit-rcvd%,%ss-status-test-rcvd%,%ss-congested-txed%,%ss-congested-rcvd%,%sccp-rtf-notrans-addr-nature%,%sccp-rtf-notrans-addr-specific%,%sccp-rtf-netwfail-pc-unavail%,%sccp-rtf-netw-conges%,%sccp-rtf-ssn-fail%,%sccp-rtf-ssn-conges%,%sccp-syntax-error%,%sccp-reassem-err-timer%,%sccp-reassem-err-sequence%,%sccp-reassem-err-space%,%sccp-hop-counter-violation%,%sccp-provider-ini-reset%,%sccp-provider-ini-rel%,%sccp-msg-toolarge-segment%,%sccp-segmentation-fail%,%sccp-total-msgs-handled%,%sccp-total-msgs-handl-local-ss%,%sccp-total-msgs-req-gtt%,%sccp-udt-sent%,%sccp-udt-rcvd%,%sccp-udts-sent%,%sccp-udts-rcvd%,%sccp-xudt-sent%,%sccp-xudt-rcvd%,%sccp-xudts-sent%,%sccp-xudts-rcvd%,%sccp-ludt-sent%,%sccp-ludt-rcvd%,%sccp-ludts-sent%,%sccp-ludts-rcvd%,%sccp-cr-sent%,%sccp-cr-rcvd%,%sccp-cc-sent%,%sccp-cc-rcvd%,%sccp-cref-sent%,%sccp-cref-rcvd%,%sccp-rsr-msg-sent%,%sccp-rsr-msg-rcvd%,%sccp-err-msg-sent%,%sccp-err-msg-rcvd%,%sccp-unequipped-user%,%sccp-reason-unknown%,%sccp-class-0-sent%,%sccp-class-0-rcvd%,%sccp-class-1-sent%,%sccp-class-1-rcvd%,%sccp-DT1-sent%,%sccp-DT1-rcvd%,%sccp-rel-compl-supv-fail%,%sccp-rel-disconn-req-rx%,%sccp-routing-fail-invalid-ins-routing-req%,%sccp-routing-fail-invalid-isni-routing-req%,%sccp-routing-fail-isni-constrained-routing%,%sccp-routing-fail-redundant-isni-routing-req%,%sccp-routing-fail-isni-identify-network%,%sccp-inactivity-rcv-tmr-expired%,%sccp-inactivity-test-sent%,%sccp-inactivity-test-received%
> SS7RD1Sch | SS7RD1 Schema | EMS,SS7RD1,%date%,%time%,%ss7rd-number%,%ss7rd-asp_instance%,%ss7rd-sctp-init-tx%,%ss7rd-sctp-init-rtx%,%ss7rd-sctp-init-rx%,%ss7rd-sctp-init-ack-tx%,%ss7rd-sctp-init-ack-rx%,%ss7rd-sctp-shutdown-tx%,%ss7rd-sctp-shutdown-rtx%,%ss7rd-sctp-shutdown-rx%,%ss7rd-sctp-shutdown-ack-tx%,%ss7rd-sctp-shutdown-ack-rtx%,%ss7rd-sctp-shutdown-ack-rx%,%ss7rd-sctp-cookie-tx%,%ss7rd-sctp-cookie-rtx%,%ss7rd-sctp-cookie-rx%,%ss7rd-sctp-cookie-ack-tx%,%ss7rd-sctp-cookie-ack-rx%,%ss7rd-sctp-data-tx%,%ss7rd-sctp-data-rtx%,%ss7rd-sctp-data-rx%,%ss7rd-sctp-sack-tx%,%ss7rd-sctp-sack-rx%,%ss7rd-sctp-shutdown-compl-tx%,%ss7rd-sctp-shutdown-compl-rx%,%ss7rd-sctp-heartbeat-tx%,%ss7rd-sctp-heartbeat-rx%,%ss7rd-sctp-heartbeat-ack-tx%,%ss7rd-sctp-heartbeat-ack-rx%,%ss7rd-sctp-abort-tx%,%ss7rd-sctp-abort-rx%,%ss7rd-sctp-bytes-tx%,%ss7rd-sctp-bytes-rx%,%ss7rd-mtp3-data-tx%,%ss7rd-mtp3-paused-tx%,%ss7rd-mtp3-resumed-tx%,%ss7rd-mtp3-congest-tx%,%ss7rd-mtp3-restrict-tx%,%ss7rd-mtp3-reset-begin-tx%,%ss7rd-mtp3-reset-end-tx%,%ss7rd-mtp3-reset-upu-tx%,%ss7rd-mtp3-data-rx%,%ss7rd-mtp3-paused-rx%,%ss7rd-mtp3-resumed-rx%,%ss7rd-mtp3-congest-rx%,%ss7rd-mtp3-restrict-rx%,%ss7rd-mtp3-reset-begin-rx%,%ss7rd-mtp3-reset-end-rx%,%ss7rd-mtp3-reset-upu-rx%,%ss7rd-m3ua-data-tx%,%ss7rd-m3ua-duna-tx%,%ss7rd-m3ua-dava-tx%,%ss7rd-m3ua-daud-tx%,%ss7rd-m3ua-scon-tx%,%ss7rd-m3ua-dupu-tx%,%ss7rd-m3ua-drst-tx%,%ss7rd-m3ua-regreq-tx%,%ss7rd-m3ua-regrsp-tx%,%ss7rd-m3ua-deregreq-tx%,%ss7rd-m3ua-deregrsp-tx%,%ss7rd-m3ua-aspup-tx%,%ss7rd-m3ua-aspup-ack-tx%,%ss7rd-m3ua-aspdn-tx%,%ss7rd-m3ua-aspdn-ack-tx%,%ss7rd-m3ua-aspac-tx%,%ss7rd-m3ua-aspac-ack-tx%,%ss7rd-m3ua-aspia-tx%,%ss7rd-m3ua-aspia-ack-tx%,%ss7rd-m3ua-hearbeat-tx%,%ss7rd-m3ua-hearbeat-ack-tx%,%ss7rd-m3ua-error-tx%,%ss7rd-m3ua-notify-tx%,%ss7rd-m3ua-data-rx%
> SS7RD2Sch | SS7RD2 Schema | EMS,SS7RD2,%date%,%time%,%ss7rd-number%,%ss7rd-asp_instance%,%ss7rd-m3ua-duna-rx%,%ss7rd-m3ua-dava-rx%,%ss7rd-m3ua-daud-rx%,%ss7rd-m3ua-scon-rx%,%ss7rd-m3ua-dupu-rx%,%ss7rd-m3ua-drst-rx%,%ss7rd-m3ua-regreq-rx%,%ss7rd-m3ua-regrsp-rx%,%ss7rd-m3ua-deregreq-rx%,%ss7rd-m3ua-deregrsp-rx%,%ss7rd-m3ua-aspup-rx%,%ss7rd-m3ua-aspup-ack-rx%,%ss7rd-m3ua-aspdn-rx%,%ss7rd-m3ua-aspdn-ack-rx%,%ss7rd-m3ua-aspac-rx%,%ss7rd-m3ua-aspac-ack-rx%,%ss7rd-m3ua-aspia-rx%,%ss7rd-m3ua-aspia-ack-rx%,%ss7rd-m3ua-hearbeat-rx%,%ss7rd-m3ua-hearbeat-ack-rx%,%ss7rd-m3ua-error-rx%,%ss7rd-m3ua-notify-rx%,%ss7rd-m3ua-lower-intf-pdu-tx%,%ss7rd-m3ua-lower-intf-pdu-rx%,%ss7rd-m3ua-upper-intf-pdu-tx%,%ss7rd-m3ua-upper-intf-pdu-rx%,%ss7rd-m3ua-down-no-route-found%,%ss7rd-m3ua-down-pc-unvailable%,%ss7rd-m3ua-down-msg-failed%,%ss7rd-m3ua-down-loadshare-failed%,%ss7rd-m3ua-up-no-route-found%,%ss7rd-m3ua-up-pc-unvailable%,%ss7rd-m3ua-up-msg-failed%,%ss7rd-m3ua-up-loadshare-failed%,%ss7rd-sctp-error-tx%,%ss7rd-sctp-error-rx%,%ss7rd-m3ua-lower-intf-pdusize-tx%,%ss7rd-m3ua-lower-intf-pdusize-rx%,%ss7rd-m3ua-upper-intf-pdusize-tx%,%ss7rd-m3ua-upper-intf-pdusize-rx%,%ss7rd-m3ua-down-pc-congested%,%ss7rd-m3ua-down-no-psp-avail%,%ss7rd-m3ua-down-no-nsap-avail%,%ss7rd-m3ua-down-data-conges-q%,%ss7rd-m3ua-down-data-as-pend-q%,%ss7rd-m3ua-up-pc-congested%,%ss7rd-m3ua-up-no-psp-avail%,%ss7rd-m3ua-up-no-nsap-avail%,%ss7rd-m3ua-up-data-conges-q%,%ss7rd-m3ua-up-data-as-pend-q%,%ss7rd-mtp3-user-part-unavail-tx%,%ss7rd-mtp3-traffic-restart-allowed-tx%,%ss7rd-mtp3-traffic-restart-waiting-tx%,%ss7rd-mtp3-user-part-unavail-rx%,%ss7rd-mtp3-traffic-restart-allowed-rx%,%ss7rd-mtp3-traffic-restart-waiting-rx%,%ss7rd-mtp3-msu-dropped-routing-err%
> SS7RD3Sch | SS7RD3 Schema | EMS,SS7RD3,%date%,%time%,%ss7rd-number%,%ss7rd-asp_instance%,%ss7rd-m3ua-psp-ps-id%,%ss7rd-m3ua-psp-instance%,%ss7-adjacent-point-code%,%ss7-adjacent-spc-not-accessible%,%ss7rd-m3ua-psp-aspac-ack-rx%,%ss7rd-m3ua-psp-aspac-ack-tx%,%ss7rd-m3ua-psp-aspac-rx%,%ss7rd-m3ua-psp-aspac-tx%,%ss7rd-m3ua-psp-aspdn-ack-rx%,%ss7rd-m3ua-psp-aspdn-ack-tx%,%ss7rd-m3ua-psp-aspdn-rx%,%ss7rd-m3ua-psp-aspdn-tx%,%ss7rd-m3ua-psp-aspia-ack-rx%,%ss7rd-m3ua-psp-aspia-ack-tx%,%ss7rd-m3ua-psp-aspia-rx%,%ss7rd-m3ua-psp-aspia-tx%,%ss7rd-m3ua-psp-aspup-ack-rx%,%ss7rd-m3ua-psp-aspup-ack-tx%,%ss7rd-m3ua-psp-aspup-rx%,%ss7rd-m3ua-psp-aspup-tx%,%ss7rd-m3ua-psp-congestion-count%,%ss7rd-m3ua-psp-congestion-duration%,%ss7rd-m3ua-psp-congestion-level1%,%ss7rd-m3ua-psp-congestion-level2%,%ss7rd-m3ua-psp-congestion-level3%,%ss7rd-m3ua-psp-congestion-queue-hw%,%ss7rd-m3ua-psp-congestion-queue-size%,%ss7rd-m3ua-psp-data-pdu-rx%,%ss7rd-m3ua-psp-data-pdusize-rx%,%ss7rd-m3ua-psp-data-pdusize-tx%,%ss7rd-m3ua-psp-data-pdu-tx%,%ss7rd-m3ua-psp-data-rx%,%ss7rd-m3ua-psp-data-tx%,%ss7rd-m3ua-psp-daud-rx%,%ss7rd-m3ua-psp-daud-tx%,%ss7rd-m3ua-psp-dava-rx%,%ss7rd-m3ua-psp-dava-tx%,%ss7rd-m3ua-psp-deregreq-rx%,%ss7rd-m3ua-psp-deregreq-tx%,%ss7rd-m3ua-psp-deregrsp-rx%,%ss7rd-m3ua-psp-deregrsp-tx%,%ss7rd-m3ua-psp-drst-rx%,%ss7rd-m3ua-psp-drst-tx%,%ss7rd-m3ua-psp-duna-rx%,%ss7rd-m3ua-psp-duna-tx%,%ss7rd-m3ua-psp-dupu-rx%,%ss7rd-m3ua-psp-dupu-tx%,%ss7rd-m3ua-psp-error-rx%,%ss7rd-m3ua-psp-error-tx%,%ss7rd-m3ua-psp-hearbeat-ack-rx%,%ss7rd-m3ua-psp-hearbeat-ack-tx%,%ss7rd-m3ua-psp-hearbeat-rx%,%ss7rd-m3ua-psp-hearbeat-tx%,%ss7rd-m3ua-psp-notify-rx%,%ss7rd-m3ua-psp-notify-tx%,%ss7rd-m3ua-psp-regreq-rx%,%ss7rd-m3ua-psp-regreq-tx%,%ss7rd-m3ua-psp-regrsp-rx%,%ss7rd-m3ua-psp-regrsp-tx%,%ss7rd-m3ua-psp-scon-rx%
> SS7RD4Sch | SS7RD4 Schema | EMS,SS7RD4,%date%,%time%,%ss7rd-number%,%ss7rd-asp_instance%,%ss7rd-m3ua-psp-scon-tx%,%ss7rd-m3ua-psp-unvailable-count%,%ss7rd-m3ua-psp-unvailable-duration%,%ss7rd-m3ua-psp-up-data-as-pend-q%,%ss7rd-m3ua-psp-up-data-conges-q%,%ss7rd-m3ua-psp-up-loadshare-failed%,%ss7rd-m3ua-psp-up-msg-failed%,%ss7rd-m3ua-psp-up-no-nsap-avail%,%ss7rd-m3ua-psp-up-no-psp-avail%,%ss7rd-m3ua-psp-up-no-route-found%,%ss7rd-m3ua-psp-up-pc-congested%,%ss7rd-m3ua-psp-up-pc-unvailable%
> MIPV6HASch | MIPV6HA Schema | EMS,MIPV6HA,%date%,%time%,%vpnname%,%vpnid%,%servname%,%servid%,%num-subscriber%,%aaa-attempt%,%aaa-success%,%aaa-totfail%,%aaa-actauthfail%,%aaa-misauthfail%,%bindupdrec-totrec%,%bindupdrec-totacc%,%bindupdrec-totdeny%,%bindupdrec-totdisc%,%bindupdrec-totcongdisc%,%ibindupdreq-receive%,%ibindupdreq-accept%,%ibindupdreq-deny%,%rbindupdreq-receive%,%rbindupdreq-accept%,%rbindupdreq-deny%,%deregreq-receive%,%deregreq-accept%,%deregreq-deny%,%horeq-receive%,%horeq-accept%,%horeq-deny%,%bindacksent-total%,%bindacksent-acceptreg%,%bindacksent-acceptdereg%,%bindacksent-deny%,%denyreason-badreq%,%denyreason-mismatchid%,%denyreason-mnauthfail%,%denyreason-admprohibit%,%denyreason-noresource%,%denyreason-simbindexceed%,%denyreason-senderror%,%denyreason-unspereason%,%denyreason-msgidrequire%,%denyreason-dadfail%,%denyreason-nothomesubnet%,%denyreason-seqoutwindow%,%denyreason-regchadisallow%,%rrqdeny-admprohibit%,%rrqdeny-unknownha%,%datareceive-totpkt%,%datareceive-totpkt6in6%,%datareceive-totbyte%,%datareceive-totbyte6in6%,%datareceive-errorprotocol%,%datareceive-errorinvpkt%,%datareceive-errornosess%,%datasent-totpkt%,%datasent-totpkt6in6%,%datasent-totbyte%,%datasent-totbyte6in6%,%disconnect-lifetimeexp%,%disconnect-deregistration%,%disconnect-admdrop%,%disconnect-othreason%,%icmpv6-toobigreceive%,%icmpv6-toobigforward%,%icmpv6-toobiggenerate%
> CONTEXTSch | CONTEXT Schema | EMS,CONTEXT,%date%,%time%,%vpnname%,%vpnid%,%sfw-total-rxpackets%,%sfw-total-rxbytes%,%sfw-total-txpackets%,%sfw-total-txbytes%,%sfw-total-injectedpkts%,%sfw-total-injectedbytes%,%sfw-dnlnk-droppkts%,%sfw-dnlnk-dropbytes%,%sfw-uplnk-droppkts%,%sfw-uplnk-dropbytes%,%sfw-total-malpackets%,%sfw-ip-discardpackets%,%sfw-ip-malpackets%,%sfw-icmp-discardpackets%,%sfw-icmp-malpackets%,%sfw-tcp-discardpackets%,%sfw-tcp-malpackets%,%sfw-udp-discardpackets%,%sfw-udp-malpackets%,%sfw-total-dosattacks%,%sfw-total-flows%
> CSCF1Sch | CSCF1 Schema | EMS,CSCF1,%date%,%time%,%vpnname%,%vpnid%,%svcname%,%svcid%,%curregusers%,%failedauth%,%regexp%,%callattrx%,%callatttx%,%callsuccrx%,%callsucctx%,%callfailrx%,%callfailtx%,%curcscfsess%,%callrejpdf%,%callrejloc%,%sesstimeexp%,%hssacc%,%emergcalls%,%tollfreecalls%,%premservcalls%,%internationalcalls%,%longDistancecalls%,%opassistcalls%,%dirassistcalls%,%regreqrx%,%regreqtx%,%invreqrx%,%invreqtx%,%ackreqrx%,%ackreqtx%,%byereqrx%,%byereqtx%,%cancreqrx%,%cancreqtx%,%optreqrx%,%optreqtx%,%prackreqrx%,%prackreqtx%,%subreqrx%,%subreqtx%,%notreqrx%,%notreqtx%,%refreqrx%,%refreqtx%,%inforeqrx%,%inforeqtx%,%updreqrx%,%updreqtx%,%msgreqrx%,%msgreqtx%,%pubreqrx%,%pubreqtx%,%tryrsprx%,%tryrsptx%,%rngrsprx%,%rngrsptx%,%fwdrsprx%,%fwdrsptx%,%quersprx%,%quersptx%,%prgrsprx%,%prgrsptx%,%200-regrsprx%,%200-regrsptx%,%200-invrsprx%,%200-invrsptx%,%200-byersprx%,%200-byersptx%,%200-cnlrsprx%,%200-cnlrsptx%,%200-optrsprx%,%200-optrsptx%,%200-prackrsprx%,%200-prackrsptx%,%200-subrsprx%,%200-subrsptx%,%200-notrsprx%,%200-notrsptx%,%200-infrsprx%,%200-infrsptx%,%200-updrsprx%,%200-updrsptx%,%200-pubrsprx%,%200-pubrsptx%,%200-refrsprx%,%200-refrsptx%,%200-msgrsprx%,%200-msgrsptx%,%202-refrsprx%,%202-refrsptx%,%202-subrsprx%,%202-subrsptx%,%mchrsprx%,%mchrsptx%,%mpersprx%,%mpersptx%,%mtersprx%,%mtersptx%,%upxrsprx%,%upxrsptx%,%altrsprx%,%altrsptx%,%brqerrrx%,%brqerrtx%,%uauerrrx%,%uauerrtx%,%forerrrx%,%forerrtx%,%nfderrrx%,%nfderrtx%,%mnaerrrx%,%mnaerrtx%,%nac406errrx%,%nac406errtx%,%parerrrx%,%parerrtx%,%rtoerrrx%,%rtoerrtx%,%gonerrrx%,%gonerrtx%,%crferrrx%,%crferrtx%,%relerrrx%,%relerrtx%,%rulerrrx%,%rulerrtx%,%umterrrx%,%umterrtx%,%uuserrrx%,%uuserrtx%,%bexerrrx%,%bexerrtx%,%exrerrrx%,%exrerrtx%,%itberrrx%,%itberrtx%,%tnaerrrx%,%tnaerrtx%,%tdnerrrx%,%tdnerrtx%,%ldterrrx%,%ldterrtx%
> CSCF2Sch | CSCF2 Schema | EMS,CSCF2,%date%,%time%,%vpnname%,%vpnid%,%svcname%,%svcid%,%tmherrrx%,%tmherrtx%,%adierrrx%,%adierrtx%,%amberrrx%,%amberrtx%,%bhrerrrx%,%bhrerrtx%,%rqcerrrx%,%rqcerrtx%,%namerrrx%,%namerrtx%,%trperrrx%,%trperrtx%,%udperrrx%,%udperrtx%,%ineerrrx%,%ineerrtx%,%nimerrrx%,%nimerrtx%,%bgterrrx%,%bgterrtx%,%suaerrrx%,%suaerrtx%,%gtterrrx%,%gtterrtx%,%bsverrrx%,%bsverrtx%,%mtlerrrx%,%mtlerrtx%,%pcferrrx%,%pcferrtx%,%bewerrrx%,%bewerrtx%,%decerrrx%,%decerrtx%,%neaerrrx%,%neaerrtx%,%nac606errrx%,%nac606errtx%,%callsetuptime%,%callscounted%
> SS7LINK1Sch | SS7LINK1 Schema | EMS,SS7LINK1,%date%,%time%,%ss7rd-number%,%ss7-linkset-id%,%ss7-link-id%,%ss7-dpc-point-code%,%ss7-link-mtp3-changeover-order-tx%,%ss7-link-mtp3-changeover-order-rx%,%ss7-link-mtp3-changeover-order-ack-tx%,%ss7-link-mtp3-changeover-order-ack-rx%,%ss7-link-mtp3-changeback-declaration-tx%,%ss7-link-mtp3-changeback-declaration-rx%,%ss7-link-mtp3-changeback-ack-tx%,%ss7-link-mtp3-changeback-ack-rx%,%ss7-link-mtp3-emergency-changeover-tx%,%ss7-link-mtp3-emergency-changeover-rx%,%ss7-link-mtp3-emergency-changeover-ack-tx%,%ss7-link-mtp3-emergency-changeover-ack-rx%,%ss7-link-mtp3-inhibit-tx%,%ss7-link-mtp3-inhibit-rx%,%ss7-link-mtp3-inhibit-ack-tx%,%ss7-link-mtp3-inhibit-ack-rx%,%ss7-link-mtp3-uninhibit-tx%,%ss7-link-mtp3-uninhibit-rx%,%ss7-link-mtp3-uninhibit-ack-tx%,%ss7-link-mtp3-uninhibit-ack-rx%,%ss7-link-mtp3-inhibit-deny-tx%,%ss7-link-mtp3-inhibit-deny-rx%,%ss7-link-mtp3-force-uninhibit-tx%,%ss7-link-mtp3-force-uninhibit-rx%,%ss7-link-mtp3-local-inhibit-test-tx%,%ss7-link-mtp3-local-inhibit-test-rx%,%ss7-link-mtp3-remote-inhibit-test-tx%,%ss7-link-mtp3-remote-inhibit-test-rx%,%ss7-link-mtp3-connection-order-tx%,%ss7-link-mtp3-connection-order-rx%,%ss7-link-mtp3-connection-order-ack-tx%,%ss7-link-mtp3-connection-order-ack-rx%,%ss7-link-mtp3-test-tx%,%ss7-link-mtp3-test-rx%,%ss7-link-mtp3-test-ack-tx%,%ss7-link-mtp3-test-ack-rx%,%ss7-link-mtp3-sif-octet-tx%,%ss7-link-mtp3-sif-octet-rx%,%ss7-link-mtp3-sio-octet-tx%,%ss7-link-mtp3-sio-octet-rx%,%ss7-link-mtp3-sio-msu-tx%,%ss7-link-mtp3-tx-msu-dropped%,%ss7-link-mtp3-tx-msu-congestion-dropped%,%ss7-link-mtp3-invalid-pdu-rx%,%ss7-link-mtp3-congestion-threshold1%,%ss7-link-mtp3-congestion-threshold2%,%ss7-link-mtp3-congestion-threshold3%,%ss7-link-mtp3-unavail-duration%,%ss7-link-mtp3-congested-duration%
> SS7LINK2Sch | SS7LINK2 Schema | EMS,SS7LINK2,%date%,%time%,%ss7rd-number%,%ss7-linkset-id%,%ss7-link-id%,%ss7-dpc-point-code%,%ss7-signalling-link-failure%,%ss7-dpc-route-set-test-msg-tx%,%ss7-dpc-route-set-congestion-test-msg-tx%,%ss7-dpc-transfer-prohibited-tx%,%ss7-dpc-transfer-restricted-tx%,%ss7-dpc-transfer-allowed-tx%,%ss7-dpc-transfer-controlled-tx%,%ss7-dpc-sif-octets-tx%,%ss7-dpc-sio-octets-tx%,%ss7-dpc-route-set-test-msg-rx%,%ss7-dpc-route-set-congestion-test-msg-rx%,%ss7-dpc-transfer-prohibited-rx%,%ss7-dpc-transfer-restricted-rx%,%ss7-dpc-transfer-allowed-rx%,%ss7-dpc-transfer-controlled-rx%,%ss7-dpc-usn-msg-rx%,%ss7-dpc-unavailable-duration%,%ss7-dpc-unavailable-count%,%ss7-link-sscf-mtp3-frames-tx%,%ss7-link-sscf-out-of-service-pdu-tx%,%ss7-link-sscf-processor-outage-tx%,%ss7-link-sscf-in-service-pdu-tx%,%ss7-link-sscf-normal-pdu-tx%,%ss7-link-sscf-emergency-pdu-tx%,%ss7-link-sscf-alignment-not-successfull-pdu-tx%,%ss7-link-sscf-management-initiated-pdu-tx%,%ss7-link-sscf-protocol-error-pdu-tx%,%ss7-link-sscf-proving-not-successfull-pdu-tx%,%ss7-link-sscf-mtp3-frames-rx%,%ss7-link-sscf-out-of-service-pdu-rx%,%ss7-link-sscf-processor-outage-rx%,%ss7-link-sscf-in-service-pdu-rx%,%ss7-link-sscf-normal-pdu-rx%,%ss7-link-sscf-emergency-pdu-rx%,%ss7-link-sscf-alignment-not-successfull-pdu-rx%,%ss7-link-sscf-management-initiated-pdu-rx%,%ss7-link-sscf-protocol-error-pdu-rx%,%ss7-link-sscf-proving-not-successfull-pdu-rx%,%ss7-link-qsaal-vpi%,%ss7-link-qsaal-vci%,%ss7-link-qsaal-req-initialization-tx%,%ss7-link-qsaal-req-ack-tx%,%ss7-link-qsaal-connection-reject-tx%,%ss7-link-qsaal-disconnect-command-tx%,%ss7-link-qsaal-disconnect-ack-tx%,%ss7-link-qsaal-resynchronization-command-tx%
> SS7LINK3Sch | SS7LINK3 Schema | EMS,SS7LINK3,%date%,%time%,%ss7rd-number%,%ss7-linkset-id%,%ss7-link-id%,%ss7-dpc-point-code%,%ss7-link-qsaal-resynchronization-ack-tx%,%ss7-link-qsaal-recovery-command-tx%,%ss7-link-qsaal-seq-connection-mode-data-tx%,%ss7-link-qsaal-poll-tx%,%ss7-link-qsaal-stat-tx%,%ss7-link-qsaal-ustat-tx%,%ss7-link-qsaal-unnumbered-user-data-tx%,%ss7-link-qsaal-unnumbered-management-data-tx%,%ss7-link-qsaal-unknown-pdu-type-tx%,%ss7-link-qsaal-tx-discarded-sdus%,%ss7-link-qsaal-tx-pdus-error-pdus%,%ss7-link-qsaal-tx-discarded-pdus%,%ss7-link-qsaal-tx-buffer-in-use-counter%,%ss7-link-qsaal-tx-buffer-in-use-gauge%,%ss7-link-qsaal-req-initialization-rx%,%ss7-link-qsaal-req-ack-rx%,%ss7-link-qsaal-connection-reject-rx%,%ss7-link-qsaal-disconnect-command-rx%,%ss7-link-qsaal-disconnect-ack-rx%,%ss7-link-qsaal-resynchronization-command-rx%,%ss7-link-qsaal-resynchronization-ack-rx%,%ss7-link-qsaal-recovery-command-rx%,%ss7-link-qsaal-recovery-ack-rx%,%ss7-link-qsaal-seq-connection-mode-data-rx%,%ss7-link-qsaal-poll-rx%,%ss7-link-qsaal-stat-rx%,%ss7-link-qsaal-ustat-rx%,%ss7-link-qsaal-unnumbered-user-data-rx%,%ss7-link-qsaal-unnumbered-management-data-rx%,%ss7-link-qsaal-unknown-pdu-type-rx%,%ss7-link-qsaal-rx-pdus-error-pdus%,%ss7-link-qsaal-rx-discarded-pdus%,%ss7-link-qsaal-rx-buffer-in-use-counter%,%ss7-link-qsaal-rx-buffer-in-use-gauge%
> GPRS1Sch | GPRS1 Schema | EMS,GPRS1,%date%,%time%,%vpnname%,%vpnid%,%servname%,%nse-id%,%ns-num-bytes-rvcd%,%ns-num-bytes-sent%,%ns-num-nsvc-failed%,%ns-num-nsvc-congest%,%ns-num-unit-data-msg-rcvd%,%ns-num-unit-data-msg-sent%,%ns-num-alive-pdu-rcvd%,%ns-num-alive-pdu-sent%,%ns-num-alive-ack-pdu-rcvd%,%ns-num-alive-ack-pdu-sent%,%ns-num-block-pdu-rcvd%,%ns-num-block-pdu-sent%,%ns-num-block-ack-pdu-rcvd%,%ns-num-block-ack-pdu-sent%,%ns-num-unblock-pdu-rcvd%,%ns-num-unblock-pdu-sent%,%ns-num-unblock-ack-pdu-rcvd%,%ns-num-unblock-ack-pdu-sent%,%ns-num-reset-pdu-rcvd%,%ns-num-reset-pdu-sent%,%ns-num-reset-ack-pdu-rcvd%,%ns-num-reset-ack-pdu-sent%,%ns-num-status-pdu-rcvd%,%ns-num-status-pdu-sent%,%num-sns-size-rcvd%,%num-sns-size-ack-sent%,%num-sns-size-fail-rcvd-unknown-nse%,%num-sns-config-rcvd%,%num-sns-config-sent%,%num-sns-config-ack-sent%,%num-sns-config-ack-rcvd%,%sns-config-fail-rcv-pdu-not-compat-state%,%sns-config-fail-sent-pdu-not-compat-state%,%sns-config-fail-rcv-inval-ipv4-endpt%,%sns-config-fail-sent-inval-ipv4-endpt%,%sns-config-fail-rcv-inval-ipv6-endpt%,%sns-config-fail-sent-inval-ipv6-endpt%,%sns-config-fail-rcv-prot-err-unspec%,%sns-config-fail-sent-prot-err-unspec%,%sns-config-fail-rcv-inval-essential-param%,%sns-config-fail-sent-inval-essential-param%,%sns-config-fail-rcv-internal-err%,%sns-config-fail-sent-internal-err%,%sns-config-fail-rcv-inval-weight%,%sns-config-fail-sent-inval-weight%,%sns-config-fail-sent-no-rsp-from-peer%,%num-sns-add-rcvd%,%num-sns-add-sent%,%sns-add-fail-rcv-pdu-not-compat-state%,%sns-add-fail-sent-pdu-not-compat-state%,%sns-add-fail-rcv-inval-ipv4-endpt%,%sns-add-fail-sent-inval-ipv4-endpt%,%sns-add-fail-rcv-inval-ipv6-endpt%,%sns-add-fail-sent-inval-ipv6-endpt%,%sns-add-fail-rcv-prot-err-unspec%
> GPRS2Sch | GPRS2 Schema | EMS,GPRS2,%date%,%time%,%vpnname%,%vpnid%,%servname%,%nse-id%,%sns-add-fail-sent-prot-err-unspec%,%sns-add-fail-rcv-inval-essential-param%,%sns-add-fail-sent-inval-essential-param%,%sns-add-fail-rcv-internal-err%,%sns-add-fail-sent-internal-err%,%sns-add-fail-rcv-inval-weight%,%sns-add-fail-sent-inval-weight%,%sns-add-fail-sent-no-rsp-from-peer%,%num-sns-delete-rcvd%,%num-sns-delete-sent%,%sns-delete-fail-rcv-pdu-not-compat-state%,%sns-delete-fail-sent-pdu-not-compat-state%,%sns-delete-fail-rcv-unknown-ip-endpt%,%sns-delete-fail-sent-unknown-ip-endpt%,%sns-delete-fail-rcv-unknown-ip-address%,%sns-delete-fail-sent-unknown-ip-address%,%sns-delete-fail-rcv-prot-err-unspec%,%sns-delete-fail-sent-prot-err-unspec%,%sns-delete-fail-rcv-inval-essential-param%,%sns-delete-fail-sent-inval-essential-param%,%sns-delete-fail-rcv-internal-err%,%sns-delete-fail-sent-internal-err%,%sns-delete-fail-sent-no-rsp-from-peer%,%num-sns-cw-rcvd%,%num-sns-cw-sent%,%sns-cw-fail-rcv-pdu-not-compat-state%,%sns-cw-fail-sent-pdu-not-compat-state%,%sns-cw-fail-rcv-inval-weight%,%sns-cw-fail-sent-inval-weight%,%sns-cw-fail-rcv-unknown-ip-endpt%,%sns-cw-fail-sent-unknown-ip-endpt%,%sns-cw-fail-rcv-unknown-ip-addr%,%sns-cw-fail-sent-unknown-ip-addr%,%sns-cw-fail-rcv-prot-err-unspec%,%sns-cw-fail-sent-prot-err-unspec%,%sns-cw-fail-rcv-inval-essential-param%,%sns-cw-fail-sent-inval-essential-param%,%sns-cw-fail-rcv-internal-err%,%sns-cw-fail-sent-internal-err%,%sns-cw-fail-sent-no-rsp-from-peer%,%sns-num-ack-rcvd%,%sns-num-ack-sent%,%sns-num-unknown-msg%,%sns-num-status-pdu-sent%,%bssgp-total-usr-req-drop%,%bssgp-usr-req-drop-unknown-bvci%,%bssgp-usr-req-drop-blocked-bvc%,%bssgp-usr-req-drop-encoding-fail%,%bssgp-usr-req-drop-bvc-flow-ctrl-rvcd%
> | GPRS3 Schema | EMS,GPRS3,%date%,%time%,%vpnname%,%vpnid%,%servname%,%nse-id%,%bssgp-usr-req-drop-bvc-flow-ctrl-ack-sent%,%bssgp-usr-req-drop-block-rvcd%,%bssgp-usr-req-drop-block-ack-sent%,%bssgp-usr-req-drop-unblock-rcvd%,%bssgp-usr-req-drop-unblock-ack-sent%,%bssgp-usr-req-drop-bvc-reset-sent%,%bssgp-usr-req-drop-bvc-reset-rcvd%,%bssgp-usr-req-drop-bvc-reset-ack-sent%,%bssgp-usr-req-drop-bvc-reset-ack-rcvd%,%bssgp-flush-llc-msg-sent%,%bssgp-flush-llc-ack-msg-rcvd%,%bssgp-cs-paging-msg-sent%,%bssgp-ps-paging-msg-sent%,%bssgp-ra-cap-update-msg-rcvd%,%bssgp-ra-cap-update-ack-msg-sent%,%bssgp-radio-status-msg-sent%,%bssgp-radio-status-msg-rcvd%,%bssgp-suspend-msg-rcvd%,%bssgp-suspend-ack-msg-sent%,%bssgp-suspend-nack-msg-sent%,%bssgp-resume-msg-rcvd%,%bssgp-resume-ack-msg-sent%,%bssgp-resume-nack-msg-sent%,%bssgp-downlink-unitdata-sent%,%bssgp-uplink-unitdata-rcvd%,%bssgp-llc-pdu-discard-msg-rcvd%,%bssgp-ms-flow-ctrl-msg-rcvd%,%bssgp-ms-flow-ctrl-ack-msg-sent%,%bssgp-bvc-status-msg-rcvd%,%bssgp-bvc-status-msg-sent%,%sndcp-xid-req-ms-init%,%sndcp-xid-ind-sgsn-init%,%sndcp-npdus-ack-rcvd-ms%,%sndcp-npdus-ack-sent-ms%,%sndcp-npdus-uack-rcvd-ms%,%sndcp-npdus-uack-sent-ms%,%sndcp-bytes-ack-rcvd-ms%,%sndcp-bytes-ack-sent-ms%,%sndcp-bytes-uack-rcvd-ms%,%sndcp-bytes-uack-sent-ms%,%sndcp-pdu-drop-rcvd-from-llc%,%sndcp-inval-ref-num-rcvd-from-llc%,%sndcp-npdu-sent-sgsn-irau%,%sndcp-npdu-rcvd-sgsn-irau%,%llc-data-req-rx%,%llc-data-cfm-tx%,%llc-data-ind-tx%,%llc-data-sent-ind-tx%,%llc-unit-data-req-rx%,%llc-unit-data-ind-tx%,%llc-discarded-frames-rx%,%llc-discarded-frames-tx%,%llc-error-frames-rx%,%llc-unrecog-frames-rx%,%llc-xid-collisions%,%llc-ciphering-errors%,%llc-fcs-errors%,%llc-frame-stats-ui-rx%,%llc-frame-stats-ui-tx%

> ‌
> bs.cfg File Parameters (Other)

> Directory | Description | Minimum Value | Maximum Value | Default Value
> Format: This section deals with the format string other than the subsystem schemas.
> RemoteFile | The parameter values should not be edited manually. Used by the WEM server. |  |  |
> Tolerance: These values indicate that the server will search records within a range (below and above the expected timestamp) if the exact record is not present. All values are in seconds.
> 5MinTolerance | 0 | 150 (2.5 mins) | 0
> 15MinTolerance | 0 | 450 (7.5 mins) | 0
> 30MinTolerance | 0 | 900 (15 mins) | 0
> 45MinTolerance | 0 | 1350 (22.5 mins) | 0
> HourTolerance | 0 | 1800 (30 mins) | 0
> DayTolerance | 0 | 43200 (12 hrs) | 0
> MonthTolerance | 0 | 1296000 (15 days) | 0
> StartDateTime: These values indicate the date and time for fetching the records in case of daily and monthly report type respectively.
> DailyStartTime | From this value, we can configure the time field for daily report type if DailyStartTime is set to 20, then record present at 08:00 PM of every day will be fetched from the database. | 23 (11:00 PM) | 0 (12:00 AM) | 12
> MonthlyStartDate | From this value, we can configure the day field for monthly report type if MonthlyStartDate is set to 15, then record present at day 15 of every month will be fetched from the database. | 1 | 31 | 15

> ‌
> The bsparser.cfg File
> This file provides parameters for specifying such information as the directories in which bulk statistics records received from the chassis are stored and archived after they are processed, in addition to time intervals for polling and record transfer.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> Caution: Several parameters contained in this file are configurable through the installation process.
> bsparser.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> Directory: This section contains the directory path required for bulk statistics.
> Ftp | Base directory for bulkstat FTP from the ASR 5000. The FTP directory entry can be changed to one of the available directories in the host file system. If the specified directory does not exist, then the bulkstats files will be configured for FTPing in <serverpath>/data/. Important: The FTP directory path entry should always be an absolute path and not a relative path. | -- | -- | <serverpath>/data/
> SecFtp | Base directory for bulkstat secondary FTP from the ASR 5000. The FTP directory entry can be changed to one of the available directories in the host file system. If the specified directory does not exist, then the bulkstats files will be configured for FTPing in <serverpath>/data/. Important: The FTP directory path entry should always be an absolute path and not a relative path. | -- | -- | <serverpath>/data/
> Archive | It is recommended that the WEM server installer/admin changes this entry to one of the available directories in the host file system. This directory contains the archive of the bulkstat files from the ASR 5000. If the directory pointed by this entry is inaccessible or does not exist, then the files FTPed by the ASR 5000 will not be archived. Important: The Archive directory path entry can be an absolute or relative path. | -- | -- | ./bulkstat_archive/
> FileArchiveEnable: This flag enables/disables the archiving of bulkstat files.
> • | 1 = Enables the archiving of bulkstat files
> • | 0 = Disables this functionality
> | -- | -- | 0
> Polling: This section contains parameters that are used for optimization of the bulkstatistics module in terms of polling.
> PollInterval | Poll interval in seconds. | 10 sec | 60 sec | 30 sec
> PoolEnable |
> • | 1 = Enables the thread pool
> • | 0 = Disables the thread pool
> | -- | -- | 1
> Size | Size of the thread pool. Important: This value should not be greater than the MaxDbConnPool parameter defined in the etc/db.cfg file. | 5 | 100 | 10
> FetchConfig | Fetch bulkstat configuration parameters from the ASR 5000.
> • | 1 = Fetch
> • | 0 = Do not fetch
> | -- | -- | 0
> LatencyPeriod | Tolerance period to be considered for Bulkstat FTP operation. | 0 min | 2 min | 2 min
> Queue: This section contains parameters that are used for optimization of the bulkstatistics module in terms of queuing.
> QueueInterval | Queue interval in seconds. | 10 sec | 60 sec | 10 sec
> DBSession: This section contains parameters that are used for optimization of the bulkstatistics module for database calls in terms of DB sessions.
> PermanentSession |
> • | PermanentSession 1 = DB actions performed using permanent database sessions
> • | PermanentSession 0 = DB actions performed using temporary database sessions
> | -- | -- | 0
> Parser: This section contains parameters that are used for connection to the Parser Server process.
> ParserPort | The TCP port to which the WEM server binds. | 1025 | 65535 | 22224

> ‌
> The bsserver.cfg File
> This file provides parameters pertaining to the XML-parsing of bulk statistic records received from the chassis. These parameters provide the ability to enable/disable XML parsing and to specify the directory, in which parsed records are to be stored, time intervals for checking for new records, and whether a single XML file should be generated for all subsystems or one XML file per subsystem in accordance with 3GPP TS 32.401 V4.1.0 and 3GPP TS 32.435 V6.2.0.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> Caution: Several parameters contained in this file are configurable through the installation process.
> bsserver.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> Port: This section contains the server port to which the BulkStat server binds.
> ServerPort | The TCP port to which the WEM server binds. | 1025 | 65535 | 22223
> Directory: This section contains the directory path required for the BulkStat server.
> XMLDir | Base directory path where the measurement files are to be generated. | -- | -- | <EMSServerInstallDir>/xmldata/
> FTP | Base directory for bulkstat FTP from the ASR 5000. The FTP directory entry can be changed to one of the available directories in the host file system. If the specified directory does not exist, then the bulkstats files will be configured for FTPing in <serverpath>/data/. | -- | -- | <serverpath>/data/
> PMFormat | This configurable states the PM table format. | -- | -- | ST16
> XMLDataEnable |
> • | 1 = Enables the XML Data Parsing
> • | 0 = Disables the XML Data Parsing
> | -- | -- | 0
> XMLFileType |
> • | 1 = XML file containing all the subsystem reports
> • | 0 = XML file containing a single subsystem report
> | -- | -- | 0
> ASCIIFileGeneration |
> • | 1 = Creates ASCII file as per the subsystem report
> • | 0 = Creates XML file as per the subsystem report
> | -- | -- | 0
> XMLFileFormat |
> • | 1 = Creates XML measurement report file using the enhanced 3GPP format (V6.2.0)
> • | 0 = Creates XML measurement report file using the old format
> | -- | -- | 0
> Interval: This section contains the interval parameters for polling operations.
> DataPollInterval | Polling interval in seconds to check the availability of new data samples in the WEM bulkstat database subsystem table. | 5 sec | 3600 sec | 60 sec
> SynchInterval | Synchronization interval in seconds to check the availability of new NE (ASR 5000) for polling the data samples in the WEM bulkstat database subsystem table. | 5 sec | 3600 sec | 120 sec
> GranularityPeriod | Granularity period to generate XML report files. The following values are only supported: 300 sec (5 min), 900 sec (15 min), 1800 sec (30 min), 3600 sec (60 min) All values other than the above will be ignored and the default value will be used. | 300 sec | 3600 sec | 300 sec
> Thread Pool: This section contains the configuration values for the thread pool.
> Size | Size of the thread pool. | 5 | 20 | 10
> Access TIme: This section contains the configuration values for overriding the bulkstat XML measurement generation timestamp.
> OverrideLastAccessFlag | The bulkstat server utility can be made to generate complete data from the Iast record by changing the Override Last Access Flag.
> • | OverideLastAccessFlag = 1 (Set to ON)
> • | OverrideLastAccessFlag = 0 (Set to OFF)
> | -- | -- | 0
> XML Data: The following values are the default data values for the XML Measurement file for the 3GPP recommended XML nodes. For more information, refer to the 3GPP TS 32.401 V4.1.0 (2001-12) document.
> ffv | File format version applied by the EM | -- | -- | --
> sn | Sender Name | -- | -- | --
> st | Sender Type | -- | -- | --
> vn | Vendor Name | -- | -- | --
> neun | NE User Name | -- | -- | --
> nedn | NE Distinguish Name | -- | -- | --
> nesw | NE Software | -- | -- | --
> rsf | Representative Suspect Flag: Used as an indication to stop collecting data from any NE in abnormal conditions.
> • | 0 (FALSE) in the case of normal condition
> • | 1 (TRUE) if not normal condition
> | -- | -- | 0
> sf | Suspect Flag: Used as an indication of quality for the scanned data.
> • | 0 (FALSE) in the case of reliable data
> • | 1 (TRUE) if not reliable
> | -- | -- | 0
> es | Error State: Used as an indication to state that the statistics data collection is not completed due to the error condition.
> • | 0 (FALSE) in the case of normal condition
> • | 1 (TRUE) if not normal condition
> | -- | -- | 0
> UseIpAddress | Use ASR 5000 IP address as an NE User Name.
> • | 0: Do not use IP address as a neun, that is, use host name as neun.
> • | 1: Use IP address as neun.
> | -- | -- | 0
> Timezone: This section contains the configuration values for overriding the bulkstat XML measurement generation timestamp.
> TimezoneOffsetToUTC | Configuration for time zone offset for XML file creation. NE generates data in UTC time zone. The timestamp values of the measurement data can be converted to specific time zone by applying the differential value of time in hhmm wrt UTC.TimezoneOffsetToUTC=signhhmm
> • | Sign (optional) indicates the sign of the local time differential from UTC (+ or -). '+' is considered if sign is not given.
> • | hh is the two digit number of hours of the local time differential from UTC (-12..+13).
> • | mm is the two digit number of minutes of the local time differential from UTC (00..59).
> For example:
> • | For IST: Use TimezoneOffsetToUTC=+0530 indicating 05 hours, 30 mins ahead of UTC
> • | For KST: Use TimezoneOffsetToUTC=+0900 indicating 09 hours, 00 mins ahead of UTC
> • | For EST: Use TimezoneOffsetToUTC=-0500 indicating 05 hours, 00 mins behind UTC
> | -- | -- | +0000
> TimezoneOffsetFromUTC | Use the TimezoneOffsetFromUTC parameter for all ASR 5000s to generate XML report file.UsePerNETimezone=0
> • | 0 = Use TimezoneOffsetFromUTC parameter as a time zone to generate report file.
> • | 1 = Use time zone from MISC table in database to generate report file.
> | -- | -- | +0000
> UsePerNETimezone | This parameter indicates whether to use time zone as per ASR 5000. | -- | -- | 0
> BSFTP: The bulkstat server transfers the generated XML file to NM using FTP. This section defines the default values for FTP.
> BSFTPPerformOperation | Flag to indicate whether bulkstat server should perform FTP operation of generated XML files or perform local storage. Values:
> • | 0 = Disable FTP operation
> • | 1 = Enable FTP operation
> | -- | -- | 0
> BSFTPUserName | User name field for FTP operation. | -- | -- |
> BSFTPPassword | Password field for FTP operation. | -- | -- |
> HostIPAddr | IP Address of the host system where the file is to be transferred. | -- | -- |
> HostBaseDir | FTP directory where the file is to be stored on the host system. | -- | -- |
> PoolSize | Pool size for threads. | -- | -- |
> • | 10 for FTP
> • | 3 for SFTP
> PollInterval | Poll interval | -- | -- |
> BSFTPMaxRetries | Maximum retries if FTP failed. | -- | -- |
> BSFTPRetryInterval | Interval between retries of FTP. | -- | -- |
> BSUseSFTP | Flag to indicate whether the bulkstat server should use SFTP/FTP to transfer the XML file to NM. Changing the value of BSUseSFTP requires bulkstat server restart. When BSUseSFTP is set to 0, increase the value of PoolSize to 10. When BSUseSFTP is set to 1, reduce the value of PoolSize to 3. Values:
> • | 0 = Disable SFTP
> • | 1 = Enable SFTP
> | -- | -- | 0

> ‌
> The bstca.cfg File
> This file contains parameters pertaining to the threshold configuration for bulk statistic counters. This file includes the threshold values, that is, clear threshold and set threshold to notify and clear SNMP traps accordingly. These threshold values are specified based on the threshold limit.
> bstca.cfg File Parameters

> Filename | Description
> bstca.cfg | This file specifies the threshold configuration for bulkstat counters.
> • | Needs a Bulkstat Parser restart
> • | Can be changed by the use
> The format is as follows: [schema name] counter name=clear threshold,set threshold Example of the threshold configuration: [mipha] expiry=10,20 recv-total=20,40 Threshold Value (Clear) is less than or equal to 10 for delta value of the bulkstat counter “expiry”. Threshold Value (Set) is more than or equal to 20 for delta value of the bulkstat counter “expiry”.

> ‌
> The cdp.cfg File
> This file contains CDP specific parameters that are configured for generation of ad-hoc reports. The parameters are also configured to export Optimized Customer Master Database (OPTCMDB) files to CDP.
> cdp.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> UNKNOWNURL: This section displays unknown URL database files Import interval related information.
> UnknownUrlImportInterval | This specifies time interval in hours for Content Filtering Configuration to import various databases from CDP | 1 hr | 720 hrs (30 days; 1 Month) | 24 hrs
> Reports: This section displays the report related information.
> MaxNumberOfReports | This specifies the maximum number of reports that can be present in the reports/cf/ directory. | 50 | 500 | 250
> ReportDirSizeLimit | This specifies the directory size of the reports in MB. | 100 | 1024 | 500

> ‌
> The cf.cfg File
> This file contains parameters pertaining to content filtering.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> cf.cfg File Parameters

> Directory | Description | Minimum Value | Maximum Value | Default Value
> ContentFiltering
> EnableCFFeature | Flag to enable/disable the CF features in WEM. Needs a WEM Server restart. Setting this flag to 1 will enable the CF features in WEM.Values:
> • | 1: Enable
> • | 0: Disable
> | -- | -- | 0
> CFStatistics
> CFStatsInterval | Time Interval for generating statistics. This is the time interval in seconds after which the statistics will be generated for CF. | 60 sec | 1800 sec | 300 sec
> CFBackupArchiveDatabase: This section contains the config variables related to archive operation of various CF databases.
> FullDbFilesBackupLimit | This specifies the number of backups to be maintained by Content Filtering Server for Full databases. | 1 | 10 | 4
> IncrementalDbFilesBackupLimit | This specifies the number of days incremental backup is to be maintained for incremental databases. | 1 day | 90 days | 30 days
> ArchiveDbFiles | This allows user to enable/disable archiving of database files once outdated. Possible values: ENABLE, DISABLE | -- | -- | DISABLE
> ArchivePath | This specifies the path where archive files are maintained. ArchivePath = ./flash/archive/ | -- | -- | --
> CFTRAP
> CFSnmpVersion | SNMP version for generation of WEM traps. The supported version is SNMPv1. | -- | -- | --
> CFTrapReceiverHost | Alarm receiver machine IP Address.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | --
> CFTrapReceiverPort | The port on which traps will be generated by the WEM server.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 65535 | 162
> CFThreadPool
> CFThreadPoolSize | This is the thread pool size for export content rating databases to the chassis. | 5 | 20 | 10
> UnkURLImportThreadPool
> UnkURLImportThreadPoolSize | This is the thread pool size for pulling unknown URL databases from the inPilot application. | 5 | 20 | 10

> ‌
> The configupdate.cfg File
> This file contains parameters pertaining to chassis software configuration updates using the Web Element Manager. It includes the directory in which the configuration files are stored and the directory to which configuration update log files can be stored.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> configupdate.cfg File Parameters

> Directory | Description | Minimum Value | Maximum Value | Default Value
> ConfigUpdate
> LogDirPath | The directory where all generated log files are stored. It can be changed by the user. If the specified directory does not exist, then the config files will be stored in ./flash/ConfigUpdate/log. Important: The config file directory path entry should always be an absolute path and not a relative path. | 1 | 80 | ./flash/ConfigUpdate/log
> ConfigFileDirPath | The directory where all configuration files to be loaded on the ASR 5000 are stored. It can be changed by the user. If the specified directory does not exist, then the config files will be stored in ./flash/ConfigUpdate/config. Important: The config file directory path entry should always be an absolute path and not a relative path. | 1 | 80 | ./flash/ConfigUpdate/config

> ‌
> The db.cfg File
> This file contains parameters pertaining to the WEM’s use of the Postgres database. It identifies the various databases and their locations.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> Caution: Improper configuration of this file can adversely affect WEM operation. To ensure proper operation of the Web Element Manager, do not edit the parameters in these files.
> db.cfg File Parameters

> Directory | Description | Minimum Value | Maximum Value | Default Value
> Database | This file contains parameters pertaining to the Database Name, Database type, Host IP Address, Port, User Name and Password of the Web Element Manager application. Here, Database means Postgres, Oracle, etc. and CommitRecTime is in seconds. Important: Any change in the configuration files will restart the server resulting in client restart. The format is as follows: DbName,Database,HostAddress,Port,UserName,Password
> • | CONFIGDBASE = configdb,postgres,127.0.0.1,5432,postgres,postgres
> • | TRAPDBASE = trapdb,postgres,127.0.0.1,5432,postgres,postgresMI
> • | BDBASE = mibdb,postgres,127.0.0.1,5432,postgres,postgresAU
> • | DITDBASE = auditdb,postgres,127.0.0.1,5432,postgres,postgresB
> • | SDBASE = bsdb,postgres,127.0.0.1,5432,postgres,postgresP2P
> • | DBASE = p2pdb,postgres,127.0.0.1,5432,postgres,postgresNB
> • | DBASE = nbdb,postgres,127.0.0.1,5432,postgres,postgres
> | -- | -- | --
> MaxDbConnPool | Size of the DB connection pool. | 1 | 50 | 25
> PostgresDIR | This specifies the path of the Postgres directory. PostgresDIR = /<ems_dir>/postgres | -- | -- | --

> ‌
> The emslic.cfg File
> This file contains license information for the WEM Server installation.
> emslic.cfg File Parameters

> Key | Description | Value | Default Value
> License: This is the WEM License file.
> LicenseKey | License key for using WEM.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | LicenseKey = Basic|Customer-EU2|Customer-EU4 | No default value

> ‌
> The fm.cfg File
> This file contains parameters pertaining to the handling of received alarms. It provides parameters for configuring color indicators for the various severities, E-mail server information for alert notifications, and SNMP operation.
> fm.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> SEVERITY: This section describes the severity configuration for traps that contain various priorities and the color in which the traps of that severity should be displayed.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Severity Name | The severity name is similar to the severity color. The format is as follows: Severity Name = Severity color Severity color should be specified in a CSV format. (Comma Separated Values: red, green, blue) Valid color values range from 0 to 255. The following are some usual colors with CSV format: 255,0,0 - red 0,255,0 - green 0,0,255 - blue 255,192,203 - pink 190,190,190 - gray 255,255,255 - white 0,0,0 - black 255,255,0 - yellow 0,255,255 - cyan 169,169,169 - darkgray 211,211,211 - lightgray 255,0,255 - magenta 255,165,0 - orange 165,42,42 - brown Color entry can be of a decimal, octal or hexadecimal form.
> • | A decimal constant begins with a non-zero digit, and consists of a sequence of decimal digits.
> • | An octal constant consists of the prefix 0 optionally followed by a sequence of the digits 0 to 7 only.
> • | A hexadecimal constant consists of the prefix 0x or 0X followed by a sequence of the decimal digits and letters a (or A) to f (or F) with values 10 to 15 respectively.
> | -- | -- | Default color (red, green, blue) value is 127
> Severity Level | The Severity level (number) for the nth row in the SEVERITY section is n. For example: Clear severity level is 6Minor severity level is 4 The severity levels are as follows:
> • | Severity level 1: This specifies “Indeterminate” alarm with color code “140,140,0”.
> • | Severity level 2: This specifies “Critical” alarm with color code “255,0,0”.
> • | Severity level 3: This specifies “Major” alarm with color code “255,0,255”.
> • | Severity level 4: This specifies “Minor” alarm with color code “204,153,0”.
> • | Severity level 5: This specifies “Warning” alarm with color code “0,145,145”.
> • | Severity level 6: This specifies “Clear” alarm with color code “0,145,0”.
> | -- | -- | --
> EMAIL: This section describes the E-mail configuration for traps.
> MailFrom | E-mail address of the e-mail notification originator.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | No default value
> MailServerAddr | Address in DNS or IP address format on which the SMTP (e-mail) server should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | No default value
> MailServerPort | Port number on which the e-mail server should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 65535 | 25
> DisconnectTime | Time out for mail server TCP connection in seconds.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 secs | 3600 secs | 10 secs
> URLPath | URL path on which the WEM server should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | No default value
> SCRIPT: This section describes the script configuration for traps.
> ScriptSrvPort | Port number on which the script server should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 65535 | 22225
> ScriptDirPath | Base directory in which the scripts to be executed are stored.
> • | Needs a WEM Server restart
> • | Must not be changed by the user - There is a separate directory that exists for the user.
> |  |  | <serverpath>/scripts
> UserScriptDirPath | Base directory in which the user scripts to be executed are stored. Needs a WEM Server restart |  |  | <serverpath>/alarmscripts
> TRAP: This section describes the flags for logging traps.
> SnmpTrapPort | The port on which traps will be received by the WEM server.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> • | Server must be run as root in order to receive traps on privileged ports (1 to 1024)
> | 1 | 65535 | 162
> SelectionFlag | Flag to enable or disable e-mail, notification, forwarding, script execution and syslog.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values: ALL, IMG ALL: Processing the traps when it is ASR 5000 or non-ASR 5000 IMG: Only ASR 5000 traps are processed | -- | -- | ALL
> LoggingFlag | Flag for logging traps.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values: ALL, IMG ALL: All traps are logged. IMG: Only ASR 5000 traps are logged. | -- | -- | ALL
> BroadCastFlag | Flag for receiving broadcast-traps (case insensitive).
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values: ENABLE, DISABLE ENABLE: Receiving broadcast traps DISABLE: Don't receive broadcast traps. | -- | -- | DISABLE
> GlobalOverride | Flag for global override.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values: ENABLE, DISABLE ENABLE: Disable sending e-mail and executing script DISABLE: Enable e-mail and script | -- | -- | DISABLE
> SupressEmsTraps | Flag for suppressing WEM-only Traps.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values: ENABLE, DISABLE ENABLE: Disable generation of WEM traps DISABLE: Enable generation of WEM traps | -- | -- | DISABLE
> SnmpVersion | SNMP Version for generation of WEM traps. The supported versions are:
> • | SNMPv1
> • | SNMPv2c
> | -- | -- | --
> ProxyFwd | Flag for configuring WEM server as proxy to forward the received SNMP traps. In case of forwarding the received SNMP traps as SNMPv2 traps, we need to - # translate the notification parameters to appropriate SNMPv2 parameters.Flag for suppressing WEM-only Traps.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values: ENABLE, DISABLE ENABLE: Disable generation of WEM traps DISABLE: Enable generation of WEM traps |  |  | ENABLE
> SYSLOG: This section describes the Syslog server configuration for traps.
> LogHost | Address of the machine on which syslog should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> |  |  | 127.0.0.1
> LogPort | Port number on which syslog should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 65535 | 514
> Facility | Syslog facility.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> FACILITY contains the following possible values: LOG_KERN,LOG_USER,LOG_MAIL, LOG_DAEMON, LOG_AUTH,LOG_SYSLOG, LOG_LPR,LOG_NEWS,LOG_UUCP,LOG_CRON,LOG_LOCAL0,LOG_LOCAL1, LOG_LOCAL2,LOG_LOCAL3,LOG_LOCAL4,LOG_LOCAL5,LOG_LOCAL6,LOG_LOCAL7 | -- | -- | LOG_LOCAL3
> Priority | Syslog priority.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> PRIORITY contains the following possible values: LOG_EMERG, LOG_ALERT, LOG_CRIT, LOG_ERR, LOG_WARNING, LOG_NOTICE, LOG_INFO, LOG_DEBUG | -- | -- | LOG_INFO
> EVENTSERVICE
> LogCLIShowCommands | Flag to enable(1)/disable(0) the logging of “show” CLI commands.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 0 | 1 | 1
> AUDIO
> AudioDir | Audio directory which contains audio files.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> |  |  | No default value
> GROUP | Alarm group configuration.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> The group number for nth row in the GROUP section is n. For example:
> • | “Communications Alarm” group number is 1
> • | “QOS Alarm” group number is 4
> The alarm groups are:
> • | Communications Alarm
> • | Processing Error Alarm
> • | Environmental Alarm
> • | QOS Alarm
> • | Equipment Alarm
> | -- | -- | No default value
> PROBABLECAUSE | Alarm probable cause configuration.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> The probable cause number for nth row in the PROBABLECAUSE section is n. For example:
> • | “Loss of multi frame sync” probable cause number is 1
> • | “Loss of frame sync” probable cause number is 4
> The probable causes are:
> • | Heating or ventilation system failure
> • | Equipment malfunction
> • | Manual configuration, software crash or voltage fluctuation
> • | Module inserted
> • | Module removed
> • | Software failure or crash
> • | Module slot mismatch
> • | Congestion
> • | Communication problem
> • | Configuration or customization error
> • | Manual configuration or threshold crossed
> • | Underlying resource unavailable
> | -- | -- | 0 (means empty)
> CLIInfoPolling: This section provides information needed for the configuration of Thread pool and Polling interval required for the FMCliInfoHandler module.
> CLIInfoPollInterval | Poll interval in seconds. Important: These value are dependent on the keepalive notification interval. | 1 sec | 30 sec | 15 sec
> CLIInfoThreadPoolSize | Size of the Thread Pool. | 5 | 20 | 10
> PENDINGALARM: This section describes the pending alarm related configuration.
> autoClearInterval | Time-out interval for pending alarms in days. If any alarm is in pending state for this configured interval, then it will be automatically cleared.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 30 | 3

> ‌
> The hwinv.cfg File
> This file provides the e-mail ID used when sending hardware change notifications.
> Important: The parameter in this file is configurable through the installation process.
> hwinv.cfg File Parameters

> Key | Description | Default Value
> HWEMAIL: This is the configuration file for Hardware Inventory.
> ChangeInHWMailFrom |
> • | E-mail address of the e-mail notification originator
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | No default value

> ‌
> The ism.cfg File
> This file contains parameters pertaining to communication between the Web Element Manager and managed chassis. These parameters include the security information used to access the chassis as well as the ports over which communication takes place.
> This file also contains a parameter that provides the ability to enable/disable the SSL encryption for client-to-server and server-to-boxer communication.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> ism.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> IMGSessMgt: This section describes the parameters that store ASR 5000 login information.
> ASID | Application Server ID that will be used by the WEM server to communicate with ASR 5000.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 10 | STARENT
> ASPasswd | Application Server Password for the ASR 5000 that will be used by the WEM server to communicate with the ASR 5000.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 35 | SN123
> IMGPort | Port number on which the ASR 5000 should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10000 | 65535 | 14132
> SSLConnect | Flag to enable or disable the SSL connection.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Currently, this feature is disabled and only IIOP connections will be used. | 0 | 1 | 0
> EnforceSSL | Flag to enforce SSL.
> • | Needs a WEM Server restart.
> • | Can be changed by the user.
> • | Overrides SSLConnect value, if set to 1.
> Change the value of ENFORCE_SSL parameter in ems/client/img.html and ems/client/imgdebug.html if this value is changed. If set to 1, then the sslflag field will be updated to 't' for all existing IMGs in the boxer table in ConfigDB at server restart. | 0 | 1 | 0
> SleepTime | Time for which the cleanup thread sleeps.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 5 | 300 | 60
> MaxIdleTime | Maximum time for which the servant reference can be idle.Needs a WEM Server restartCan be changed by the user | 30 | 1800 | 300
> IMGKeepAlive: This section describes parameters related to the ASR 5000 keep-alive.
> IcmpTimeout | Timeout value for ICMP requests in seconds. | 1 | 60 | 5
> IcmpRetries | Number of retries for ICMP requests. | 0 | 10 | 2
> IcmpKeepAliveInterval | Polling interval for ICMP requests in seconds. Important: The value must be greater than IcmpTimeout * (IcmpRetries + 1). | 5 | 300 | 30
> CorbaKeepAliveInterval | Polling interval for CORBA requests in seconds. Important: The value must be greater than or equal to IcmpKeepAliveInterval. | 10 | 600 | 2 * IcmpKeepAliveInterval

> ‌
> The mcrdbs.cfg File
> This file contains parameters that are configured to support the conversion of Vendor Format Master Database (VFMDB) to Starent Networks Format Master Database (SFMDB). This file also contains information on MCRDBS to handle the database files.
> mcrdbs.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> MCRDBS: This section describes parameters that store MCRDBS related information.
> FullDBFilesImportInterval | Database files Import interval: This specifies the time interval in hours for Content Filtering Server to import various databases from MCRDBS. (Databases: SFMDB) | 2 hrs | 4320 hrs (90 days; 6 months) | 24 hrs
> INCDBFilesImportInterval | Database files Import interval: This specifies the time interval in hours for Content Filtering Server to import various databases from MCRDBS. (Databases: SFMDB-INC) | 2 hrs | 720 hrs (30 days; 1 month) | 24 hrs
> StarentFormatDbFileImportPath | Starent format database file path: This specifies the path where SFMDB files are located in MCRDBS. Example: <Mcrdbs server path>/cfems/<cfems ip address>/sfmdb | -- | -- | --
> StarentFormatIncDbFileImportPath | Starent format incremental database file path: This specifies the path where SFMDB-INC files are located in MCRDBS. Example: <MCRDBS server path>/cfems/<cfems ip address>/sfmincdb | -- | -- | --
> MCRDBSInfo | This specifies the MCRDBS information in the following format:MCRDBS Host name, MCRDBS Ip address1, User name1, password1 Important: If the user does not want to enter any values, leave the fields blank separated by comma. Example: hostName, userName, password (OR), HostIPAddr, userName, Password | -- | -- | --

> ‌
> The mdproxy.cfg File
> This configuration file defines various properties used for the MD EMS Proxy functionality.
> mdproxy.cfg File Parameters

> Key | Description
> MDAUDIT
> MDAuditPath | The directory path to log the audit trail into file. The base is the WEM server's directory. MDAuditPath = log/RESP
> MDAuditSyncPath | MDAuditSyncPath = log/SYNC_RESP
> MDAlarmPath | MDAlarmPath = log/FM

> ‌
> The nb.cfg File
> This file contains parameters for NorthBound notifications from the WEM. The information in this file is used by the application for forwarding fault management information to other management devices on the NorthBound interface. This information includes such things as the device IP address and port number on which to forward notifications.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> nb.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> Fault Management: This section describes the parameters that store NorthBound Notification Service related configuration information.
> NSMode | Mode using WEM gets the Notification Service reference.Valid values: URL, IOR, NONE
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | NONE
> NSMode is URL� | Notification Service URL. The format is as follows: corbaloc:iiop:<NSAddr>:<NSPort>/<ChannelFactoryName> | -- | -- | corbaloc:iiop:127.0.0.1:5001/NOTIFY_SVC/CHANNEL_FACTORY
> NSAddr | Host IP Address on which the Notification Service should be running.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | 127.0.0.1
> NSPort | Port number on which the Notification Service should be running
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1000 | 65535 | 5001
> ChannelFactoryName | Names to be assigned to the channel factory created by the Notification Service daemon.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | NOTIFY_SVC/CHANNEL_FACTORY
> NSIORFILE | Path name of the Notification Service IOR (String field object reference) file. Here, the NSMode is IOR.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | No default value
> NSChannelId | Channel ID through which WEM notifies the events.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 0 | 1000 | 0

> ‌
> The nbserver.cfg File
> This file contains parameters for the configuration of NorthBound Server and Notification Service processes, and NorthBound interface.
> Important: The NorthBound Server and Notification Service processes are customer-specific and are not operational without the appropriate license. Please contact your local sales representative for additional information.
> The nms.cfg File
> This file contains parameters which control WEM access to the PostgreSQL database, client access to the server, and other properties used by the application for proper operation.
> Important: Many of the parameters contained in this file are configurable through the installation process.
> nms.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> DATABASE: This section describes parameters that store database configuration information.
> HostAddress | This specifies the host IP address. | -- | -- | 127.0.0.1
> UserName | This specifies the username to connect to the database. | -- | -- | postgres
> PassWord | This specifies the password to connect to the database. | -- | -- | postgres
> IOR
> Login |  | -- | -- | login.ior
> RESPath |  | -- | -- | res_path.ior
> SVPNIOR |  | -- | -- | svpn.ior
> ConfigAudit |  | -- | -- | audit.ior
> ClientSession: This section describes parameters related to client session management.
> UserLimit | Maximum number of user sessions allowed by the server at any time. | 1 | 100 | 10
> SecurityAdminLimit | Maximum number of Security Administrator sessions allowed by the server at any time. | 1 | UserLimit | 5
> ActiveToInactiveInterval | Time for activity time out in minutes. | 1 | -1 (infinite) | 15
> KeepAliveCallInterval | Keep alive polling time in seconds. | 0 | 86400 | 15
> KeepAliveRetryCnt | Retry count for keep alive: The minimum time for dismissing the client session if it is not reachable = KeepAliveCallInterval * KeepAliveRetryCnt | 1 | 5 | 2
> SessionInitTime | Time required for a typical session to initialize to ready state. Keep alive will be enabled after a specified time after client login. | KeepAliveCallInterval | 86400 | 120
> UserSessionLimit | Maximum number of sessions for a particular user. | 1 | UserLimit | 5
> ContextUserLimit | Maximum number of user sessions for a context. | 1 | UserLimit | 5
> Notification | Global flag to enable/disable the sending notification. Possible values: ENABLE, DISABLE | -- | -- | ENABLE
> Active timeout interval | This flag allows the user to login to the N+1st WEM Client and also, to cleanup any inactive / dead sessions. Session will get timed out after the given time (minutes) from the login time. Valid User: Security Administrator | -- | -- | --
> DenialService | Global Flag to enable/disable the Denial-Of-Service. Possible Values: ENABLE, DISABLE | -- | -- | DISABLE
> DefaultUPref | This is the default user preference configuration XML string. DefaultUPref = <xml version="1.0" encoding="UTF-8"> <screen id="SCR_ID_TOPOLOGY"> <dimension> <param name="RESOLUTION" value="1024X768"/> <param name="XPOS" value="137"/> <param name="YPOS" value="89"/> <param name="WIDTH" value="512"/> <param name="HEIGHT" value="384"/> </dimension> <information> <param name="MAP_COLOR" value="-1"/> <param name="MAP_IMAGE" value="none"/> <param name="LOOK_AND_FEEL"value="Metal"/> <param name="LAST_MAP_VISITED" value="true"/> <param name="LAST_MAP_NAME" value="default"/> <param name="LAST_IMG_VISITED" value="true"/> <param name="LAST_IMG_NAME" value="earth"/> <paramname="CLIENT_TIMEOUT" value="60"/> <param name="POLLING_INTERVAL" value="10"/> <param name="AUDIO_ALARMING" value="true"/> <param name="SHOW_TOOLBAR" value="true"/> <param name="TOOLBAR_POSITION" value="North"/> <param name="NOTIFICATION" value="true"/> </information> </screen> | -- | -- | --
> DefaultAppPath | This is the default Application Path XML string. DefaultAppPath=<xml version="1.0" encoding="UTF-8"> <screen id="SCR_ID_APPLICATION_PATH"> <dimension> <param name="RESOLUTION" value="1024X768"/> <param name="XPOS" value="272"/> <param name="YPOS" value="275"/> <param name="WIDTH" value="608"/> <param name="HEIGHT" value="313"/> </dimension> <os id="Windows 95"> <param name="telnet" value="cmd /c start c:\\telnet.exe"/> <param name="ftp" value="cmd /c start c:\\ftp.exe"/> <param name="ssh" value="cmd /c start c:\\ssh.exe"/> <param name="mibbrowser" value="cmd /c start c:\\mibbrowser.exe"/> </os> | -- | -- | --
> SWUpgrade: This section describes the parameters related to Software Upgrade.
> FTPSessLimit | Maximum number of FTP sessions. | -- | -- | 5
> FTPCallBackPeriod | Call back period in seconds with which the status of the FTP will be updated. | -- | -- | --
> NMSIMGBaseDir | Base directory for Software Upgrade Manager - Image files. | -- | -- | NMSIMGBaseDir = ./flash
> NMSIMGBaseDirForFileCompare | Base directory for Config file comparison - Image files. | -- | -- | NMSIMGBaseDirForFileCompare = ./flash
> FRV: This section describes the front/rear-view related parameters.
> PollInterval | Time interval used by the WEM Client for polling.
> • | Does not require WEM Server restart
> • | This value can be changed by the user
> | 10 secs | 60 secs | 30 secs
> Topology
> ClientBaseDir | Client base directory: This value is internally used by the Topology server module and should not be changed. | -- | -- | --
> MapImageDir | Directory Name which contains image files. This value can be changed and the subdirectory must exist in ClientBaseDir. | -- | -- | --
> POAPolicies: This section describes policies used for the POAs.
> ServerIIOPPort | Using this port, three sequential upward ports will be used to create POAs. Change the value of SERVER_BASE_PORT parameter in ems/client/img.html and ems/client/imgdebug.html if this value is changed. | 15000 | 15002 | 15000
> EMSLicense
> Mode | The mode in which WEM started. Valid values: PDSN, GGSN, BOTH The value must be specified otherwise, the server does not function. | -- | -- | --
> ConfigBackup
> FTPUserName | User name that will be used by the ASR 5000 to upload files on WEM server. This user account should be existing on the WEM server host machine.
> • | Needs server restart
> • | Can be changed by the user
> | 1 | 64 | guest
> FTPPassword | Password that will be used by the ASR 5000 while uploading files to WEM server. This user account should be existing on the WEM server host machine.
> • | Needs server restart
> • | Can be changed by the user
> | 1 | 64 | guest12
> EMSServer
> ServerIpAddress | This IP Address will be used by WEM server for generating IOR files. If the field has default loopback interface values then, WEM server will take the first active interface present on the machine. Change this IP value to change IP used for IOR generation. If the specified IP is not active, WEM server will not start. | -- | -- | 127.0.0.1
> ServerPort | The TCP port to which the WEM server binds. | 1025 | 65535 | 22222
> EMSORB: This section describes the parameters related to Object Request Broker.
> ORBReadTimeout | The read time out used for sockets in seconds. | 5 secs | 3600 secs | 30 secs
> ORBWriteTimeout | The write time out used for sockets in seconds. | 5 secs | 3600 secs | 30 secs
> EMSSSLORB
> SSLORBReadTimeout | The read time out used for sockets in seconds. | 5 secs | 3600 secs | 30 secs
> SSLORBWriteTimeout | The write time out used for sockets in seconds. | 5 secs | 3600 secs | 30 secs

> ‌
> The pcrefgen.cfg File
> Configuration file for 3GPP XML report generation of Camiant PCRF.
> pcrefgen.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> MPEManagerInfo: This section provides information required to configure the details of MPE Manager making the HTTP Post request.
> MPE Manager IP-address | EMS will make HTTP Post request to the configured address to fetch the MPE OM statistics periodically. Needs a PCRF Report generation restart. Needs a PCRF Report generation restart. | -- | -- | --
> MPE Manager host-name | EMS will use the configured name for generating 3GPP statistics for MPE Manager related counters. This name will be used as userLabel in the 3GPP XML file and also in the file name. This name should not be identical to any MPE name. Can be changed by the user. | -- | -- | Empty. In this case ip-address will be used.
> MPE Manager user-id | EMS will make HTTP Post request to the configured user-id for login to make HTTP Post request to MPE Manager. Can be changed by the user. | -- | -- | --
> MPE Manager password. | EMS will make HTTP Post request to the configured password for login to make HTTP Post request to MPE Manager. Needs a PCRF Report generation restart. Can be changed by the user. | -- | -- | --
> MPE Manager XML interface URL. | This URL, the ip-address and the userId-password will be used to construct the HTTP Post request URL. Needs a PCRF Report generation restart. Can be changed by the user. | -- | -- | mi/xmlInterfaceRequest.do
> XMLInterfaceUrl | -- | -- | -- | mi/xmlInterfaceRequest.do
> Report Generation
> Poll Interval | EMS will poll the MPE Manager as the configured poll-interval.This poll interval should be the same as the sample interval configured at MPEManager. Value in minutes. Can be changed by the user. PollInterval = 15 | -- | 5 | 15 minutes
> Latency Period. | This the latency (delay) in making the request to MPE Manager.So for fetching the statistics for time interval 12:15:00 to 12:30:00, the HTTPPOST request to MPE Manager will be made at 12:32:00 (endTime + LatencyPeriod). Value in seconds. Can be changed by the user. ReqLatencyPeriod = 120 | 0 | 900 (15 minutes). | 120 seconds.
> Initial offset for StartTime. | This is the offset in number of minutes before the utility's startup time to be used for fetching the PCRF statistics from the MPE Manager. e.g. if this value is set as 120 and the utility is started at 08:30:00 then the reports will be generated for statistics from 06:30:00. This value will be overridden by the next StartTime stored in database. Value in minutes. StartTimeOffset = 0 | 0 | 1400 | 0
> PCRFUseDoubleQuotes | 0 = Disable encapsulating all the values in the generated PCRF files in double quotes. 1 = Enable encapsulating all the values in the generated PCRF files in double quotes. PCRFUseDoubleQuotes=0 | -- | -- | 0
> PCRFFTP: The pcrfrepgen process transfers the generated 3GPP XML file to NM using ftp. This section defines the default values for ftp. The pcrfrepgen process uses the same host machine used by the bulkstat server for transferring the GGSN files. FTP configuration parameters 'HostIPAddr', BSFTPUserName', 'BSFTPPassword', 'BSFTPMaxRetries', 'BSFTPRetryInterval' and BSUseSFTP' from /etc/bsserver.cfg will be used to transfer the generated PCRF 3GPP XML files.
> PcrfFTPPort | Port number used to FTP/SFTP the PCRF XML files. This attribute can be changed by the user. When BSUseSFTP is set to 1, set BSFTPPort to 22. | -- | -- | 21 for FTP; 22 for SFTP.
> HostIPAddr | IP address of the host system where the file is to be transferred. | -- | -- | 127.0.0.1
> BSFTPUserName | User name field for ftp operation. | -- | -- | Anonymous.
> BSFTPPassword | Password field for ftp operation. | -- | -- | Guest.

> ‌
> The processmonitor.cfg File
> This file contains parameters used by the Process Monitor function. These include parameters such as the directories from which WEM-related processes are started, polling intervals, and maximum percentage thresholds.
> processmonitor.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> ProcessInfo: This section provides all the process information to be monitored by the module.
> ListServer | Lists all the servers to be monitored: 0 = WebServer 1 = DB 2 = EMSServer 3 = EMSScriptServer 4 = BulkstatServer 5 = BulkstatParser 6 = NBServer 7 = NotifyService | -- | -- | --
> WebServer | Web Server Process Information: In this case, it is the Apache Web Server.
> • | Name of the Process executable: ExeName=httpd
> • | Absolute or Relative path for executable file: ExePath=/<ems_dir>/apache/bin
> • | File name which contains the pid of the process: PidName=httpd.pid
> • | Absolute or Relative path for the pid file: PidPath=/<ems_dir>/apache/logs
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> DB | Database Process Information: In this case, it is Postgres.
> • | Name of the Process executable: ExeName=postmaster
> • | Absolute or Relative path for executable file: ExePath=/<ems_dir>/postgres/bin
> • | File name which contains the pid of the process: PidName=postmaster.pid
> • | Absolute or Relative path for the pid file: PidPath=/<ems_dir>/postgres/data
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> EMSServer | EMS Server Process Information.
> • | Name of the Process executable: ExeName=server
> • | Absolute or Relative path for executable file: ExePath=/<ems_dir>/server/bin
> • | File name which contains the pid of the process: PidName=server.pid
> • | Absolute or Relative path for the pid file: PidPath=/<ems_dir>/server
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> EMSScriptServer | EMS Script Server Process Information.
> • | Name of the Process executable: ExeName=scriptsrv
> • | Absolute or Relative path for executable file: ExePath=/<ems_dir>/server/bin
> • | File name which contains the pid of the process: PidName=script.pid
> • | Absolute or Relative path for the pid file: PidPath=/<ems_dir>/server
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> BulkstatServer | BulkstatServer Process Information.
> • | Name of the Process executable: ExeName=bulkstatserver
> • | Absolute or Relative path for executable file: ExePath=./bin
> • | File name which contains the pid of the process: PidName=bsserver.pid
> • | Absolute or Relative path for the pid file: PidPath=.
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> BulkstatParser | BulkstatParser Process Information.
> • | Name of the Process executable: ExeName=bulkstatparser
> • | Absolute or Relative path for executable file: ExePath=./bin
> • | File name which contains the pid of the process: PidName=bulkstatparser.pid
> • | Absolute or Relative path for the pid file: PidPath=.
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> NBServer | NBServer Process Information.
> • | Name of the Process executable: ExeName=nbserver
> • | Absolute or Relative path for executable file: ExePath=./bin
> • | File name which contains the pid of the process: PidName=nbserver.pid
> • | Absolute or Relative path for the pid file: PidPath=.
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> NotifyService | NotifyService Process Information.
> • | Name of the Process executable: ExeName=Notify_Service
> • | Absolute or Relative path for executable file: ExePath=./bin
> • | File name which contains the pid of the process: PidName=notify_service.pid
> • | Absolute or Relative path for the pid file: PidPath=.
> • | MultiProc: Flag indicating whether the process information should include the information of child processes or not.
> Valid values:
> • | 0: Disable
> • | 1: Enable
> | -- | -- | 0
> DirectoryInfo: This section provides information needed to monitor the directory size.
> DirEMSServer | EMS Server Directory Information. Path of EMS Server directory: DirPath=/<ems_dir>/server | -- | -- | --
> DirDB | Database Directory Information. Path of Database directory: DirPath=/<ems_dir>/postgres/data | -- | -- | --
> DirEMSFtp | EMS FTP Directory Information. Path of EMS FTP directory: DirPath=./data | -- | -- | --
> DirEMSBlkArch | EMS Bulkstat Archive Directory Information. Path of EMS Bulkstat archive directory: DirPath=./bulkstat_archive | -- | -- | --
> DirFTPCFDB | FTP CF DB Directory Information. Path of FTP directory for CF DB: DirPath=./flash/cf/cfdatabases | -- | -- | --
> Poll Information: This section provides information needed for the configuration of threshold poll interval in seconds. Each sub-module under monitor has its own poll interval defined to give fine tune support.
> ProcInfoPollInterval | The process which changes frequently can be monitored for threshold limits with a smaller poll interval, say 5 seconds. | 1 sec | 36000 sec | 5 sec
> DirInfoPollInterval | The directory size does not change suddenly and can be monitored with 1 Min OR greater than 1 Min poll interval for threshold limit. | 60 sec | 36000 sec | 300 sec
> IFInfoPollInterval | If information is constant, it can be monitored once in a Min. | 5 sec | 36000 sec | 60 sec
> Threshold Information: This section provides information needed for the configuration of default threshold values for various parameters monitored by the module. These values (if available to server successfully from this configuration file) are used for default configuration of the threshold values for the parameters.These values indicate the maximum percentage of threshold limits for the individual parameters as the default values. Note:
> • | WEM server will take the current configuration for the latest threshold values from the WEM Database saved in the last session of the server.
> • | The following values can be used as default configuration for the parameter(s) if no value(s) is/are available from the database. For example, first run of the server after a new installation or a database crash, etc.)
> To use the following values to override the database configurations with configuration values, WEM server administrator can turn on (set value to 1) the OverrideDBConfig flag.
> ThreshProcWebServer | This is the threshold value for disk utilization of Web Server process. | 0 | 100 | 25
> ThreshProcDB | This is the threshold value for disk utilization of DB Server process. | 0 | 100 | 25
> ThreshProcEMSServer | This is the threshold value for disk utilization of EMS Server process. | 0 | 100 | 25
> ThreshProcEMSScriptServer | This is the threshold value for disk utilization of EMS Script Server process. | 0 | 100 | 25
> ThreshProcBulkstatServer | This is the threshold value for disk utilization of Bulkstat Server process. | 0 | 100 | 25
> ThreshProcBulkstatParser | This is the threshold value for disk utilization of Bulkstat Parser process. | 0 | 100 | 25
> ThreshProcNBServer | This is the threshold value for disk utilization of NB Server process. | 0 | 100 | 25
> ThreshProcNotifyService | This is the threshold value for disk utilization of Notify Service process. | 0 | 100 | 25
> ThreshProcTotalCPU | This is the threshold value for total disk utilization of CPU. | 0 | 100 | 60
> ThreshProcTotalSwap | This is the threshold value for total disk utilization of swaps. | 0 | 100 | 75
> ThreshDirEMSServer | This is the threshold value for disk utilization of EMS Server Directory. | 0 | 100 | 25
> ThreshDirDB | This is the threshold value for disk utilization of Database Directory. | 0 | 100 | 25
> ThreshDirFTP | This is the threshold value for disk utilization of FTP Directory. | 0 | 100 | 25
> ThreshDirBlkArch | This is the threshold value for disk utilization of Bulkstat Archive Directory. | 0 | 100 | 25
> ThreshDirCFDB | This is the threshold value for disk utilization of CF DB Directory0. | 0 | 100 | 25
> OverrideDBConfig | Flag to override the current DB Configuration of the threshold values with the configuration values. Values:
> • | 1: True
> • | 0: False
> | -- | -- | 0
> CPU: This section describes the parameters used to calculate the CPU utilization.
> NumberofSample | This calculates the average of 'NumberofSample' given in the config file. | 1 | 360 | 5

> ‌
> The ps.cfg File
> This file contains parameters which control Web Element Manager polling intervals for managed chassis and database queries.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> ps.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> Polling: This section describes the parameters related to polling support.
> MinPollInterval | Minimum time interval used by the WEM server for polling.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 secs | 86400 secs | 10 secs
> MaxPollInterval | Maximum time interval used by the WEM server for polling.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 secs | 86400 secs | 86400 secs
> PoolEnable | Flag to enable/disable the thread pool.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Values:
> • | PoolEnable 1 = Thread pool enable
> • | PoolEnable 0 = Thread pool disable
> | 0 | 1 | 0
> Size | Size of the thread pool.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 | 100 | 10
> MaxSize | Maximum size of the thread pool.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 | 100 | 10
> ErrorCausingMethodRetries | Number of retries for error causing method. WEM server stops calling the error causing method after configurable successive method calls give the same error.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 1 | 10 | 3
> EnableInterval | Enabling interval for disabled fetch in seconds. The server periodically enables the disabled fetch.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 | 600 | 120
> Database: This section describes the parameters related to database information.
> QueryNameLimit | Number of queries to be stored in the database per user per context.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 100 | 200 | 100

> ‌
> The psmon.cfg File
> This file contains parameters for the operation of the PSMon (process monitor) function supported by the WEM.
> psmon.cfg File Parameters

> Key | Description | Default Value
> NotifyEmail | Defines the e-mail address where notification e-mails are to be sent. | root@localhost
> SmtpHost | Defines the IP address or hostname of the SMTP server to be used to send e-mail notifications. | localhost
> Frequency | Defines the frequency of process table queries. This is the polling interval. | 60 secs
> LastSafePID | When defined, psmon will never attempt to kill a process ID which is numerically less than or equal to the value defined by the last safepid. Important: Psmon will never attempt to kill a process ID lesser than or equal to 1, or itself. | 100
> ProtectSafePIDsQuietly | Accepts a boolean value of On or Off. Suppresses all notifications from preserved process IDs when used in conjunction with the last safepid directive. | Off
> DryRun | Forces this psmon to as if the --dryrun command line switch had specified. This is useful if you want to force a specific configuration file to only report and never actually take any automated action. This is enabled in this default distribution configuration to prevent people from blindly executing psmon “out of the box” and causing damage in live environments. The <Process *> scope is commented out by default. It should be used with extreme care. If used, run psmon in “DryRun” mode by adding the “DryRun” directive in this configuration file. Important: Read the config file thoroughly before enabling this feature. | Enabled
> For example: Use the following format to configure each process. Copy the following 6 lines for each WEM Process to monitor and modify according to the WEM Path: <Process /<ems_dir>/server/bin/server> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/server) pidfile /<ems_dir>/server/server.pid numretry 2 tmintval 300 </Process> Note: Do not remove the following statement as it is used to modify the config file while installing through the GUI Installer: <Process /<ems_dir>/postgres/bin/postmaster -i> spawncmd /<ems_dir>/server/scripts/postgresctl start pidfile /<ems_dir>/postgres/data/postmaster.pid numretry 10 tmintval 330 </Process> <Process /<ems_dir>/apache/bin/httpd -f /<ems_dir>/apache/conf/httpd.conf> spawncmd /<ems_dir>/apache/bin/apachectl start pidfile /<ems_dir>/apache/logs/httpd.pid numretry 10 tmintval 330 </Process> <Process /<ems_dir>/server/bin/server> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/server) pidfile /<ems_dir>/server/server.pid numretry 10 tmintval 330 </Process> <Process /<ems_dir>/server/bin/bulkstatserver> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/bulkstatserver) pidfile /<ems_dir>/server/bsserver.pid numretry 10 tmintval 330 </Process>
> <Process /<ems_dir>/server/bin/bulkstatparser> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/bulkstatparser) pidfile /<ems_dir>/server/bulkstatparser.pid numretry 10 tmintval 330 </Process> <Process /<ems_dir>/server/bin/Notify_Service> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/nbSrvr) pidfile /<ems_dir>/server/notify_service.pid numretry 10 tmintval 330 </Process> <Process /<ems_dir>/server/bin/nbserver> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/nbserver) pidfile /<ems_dir>/server/nbserver.pid numretry 10 tmintval 330 </Process> <Process /<ems_dir>/server/bin/scriptsrv> spawncmd (cd /<ems_dir>/server; /<ems_dir>/server/bin/scriptsrv) pidfile /<ems_dir>/server/script.pid numretry 10 tmintval 330 </Process> Where:
> • | numretry and tmintval are optional
> • | “tmintval” must be in seconds and greater than ('numretry' * 'Frequency’)
> • | Incase of wrong values, this will not work properly
> New Processes
> Do not edit these lines if you do not have enough information. The instances should not be 0. <Process /<ems_dir>/perl5.8.5/bin/perl -w ./psmon --daemon --cron> pidfile /<ems_dir>/server/psmon.pid instances 1 </Process>
> Sendmail SMTP Mail Daemon
> <Process sendmail> spawncmd /sbin/service sendmail start pidfile /var/run/sendmail.pid </Process>
> Apache Group HTTP Daemon
> <Process httpd> spawncmd /sbin/service httpd restart pidfile /var/run/httpd.pid instances 200 pctcpu 80 </Process>
> MySQL Database
> <Process mysqld> spawncmd /sbin/service mysqld restart killcmd /sbin/service mysqld stop pidfile /var/run/mysqld/mysqld.pid pctcpu 90 pctmem 60 </Process>

> ‌
> The res.cfg File
> This file contains parameters for associating resource-bundles to specific Web Element Manager dialogs. This is the configuration file for fetching screen-specific resource-bundle paths. Currently there are only two bundles. The resource-ids must be present in both the sections.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> Caution: To ensure proper operation of the Web Element Manager, do not edit the parameters in these files.
> res.cfg File Parameters

> Bundle 1 | Bundle 2
> GlobalCommonId = res.globalcommon.GlobalCommonCompFileChooserId = res.components.FileChooserCompColorChooserId = res.components.ColorChooserCompOptionPaneId = res.components.OptionPaneCompTableId=res.components.table.STableScrKeyExport = res.components.table.SExportFileScrKeyBoxerList = res.screens.boxerlist.GlobalListScrKeyUser = res.screens.useradm.UserAdminScrKeySubscriber = res.screens.subscriber.SubscriberScrKeyPPPSession = res.screens.ppp.SPPPScrKeyPPPConfig = res.screens.ppp.SPPPScrKeyPPPCounter = res.screens.ppp.SPPPScrKeyPPPSummary = res.screens.ppp.SPPPScrKeyPPPEchoTest = res.screens.ppp.SPPPScrKeyPPPStat = res.screens.ppp.SPPPScrKeyPPPInfo = res.screens.ppp.SPPPScrKeyAAATest = res.screens.aaa.SRADIUSScrKeyAAARADIUSTest = res.screens.aaa.SRADIUSScrKeyAAARADIUSCounter = res.screens.aaa.SRADIUSScrKeyAAARADIUSCounterDetails = res.screens.aaa.SRADIUSScrKeyAAARADIUSAuth = res.screens.aaa.SRADIUSScrKeyAAARADIUSAuthConfig = res.screens.aaa.SRADIUSScrKeyAAARADIUSAcct = res.screens.aaa.SRADIUSScrKeyAAARADIUSCharging = res.screens.aaa.SRADIUSScrKeyAAARADIUSChargingConfig = res.screens.aaa.SRADIUSScrKeyAAAContextConfig = res.screens.aaa.SRADIUSScrKeyModifyContextAAA = res.screens.aaa.SRADIUSScrKeyAAARADIUSResult = res.screens.aaa.SRADIUSScrKeyAAAGlobalConfig = res.screens.aaa.SRADIUSScrKeyModifyGlobalAAA = res.screens.aaa.SRADIUSScrKeySubsCriteria = res.screens.monitor.SMonitorFilterScrKeyFrontView = res.screens.csp.SCSPScrKeyRearView = res.screens.csp.SCSPScrKeySysInfo = res.screens.csp.SCSPScrKeyCardConfig = res.screens.csp.SCSPScrKeyPortConfig = res.screens.csp.SCSPScrKeyModifyPort = res.screens.csp.SCSPScrKeyPortInformation = res.screens.csp.SCSPScrKeyShowPortCounters = res.screens.csp.SCSPScrKeyIntfPortBind = res.screens.csp.SCSP | ScrKeyBoxerOperation = res.screens.boxerlist.BoxerOperationScrKeyNewMap = res.screens.boxerlist.NewMapScrKeySelectImage = res.screens.boxerlist.SelectImageScrKeyUserAdmin = res.screens.useradm.UserAdminScrKeyUser = res.screens.useradm.UserScrKeySubscriber = res.screens.subscriber.SubscriberScrKeyShowSubscriber = res.screens.subscriber.SShowSubscriberScrKeyShowSubscriberPDSNResult = res.screens.subscriber.SShowSubscriberPDSNResultScrKeyShowSubscriberGGSNResult = res.screens.subscriber.SShowSubscriberGGSNResultScrKeyAbout = res.topology.AboutDialogScrKeyTopology = res.topology.TopologyScrKeyPPPSession = res.screens.ppp.SPPPSessionScrKeyPPPConfig = res.screens.ppp.SPPPConfigScrKeyPPPCounter = res.screens.ppp.SPPPCounterScrKeyPPPSummary = res.screens.ppp.SPPPSummaryScrKeyPPPStat = res.screens.ppp.SPPPStatScrKeyPPPInfo = res.screens.ppp.SPPPInfoScrKeyContextAdministration = res.screens.contextlist.ContextAdministrationScrKeyContextAdd = res.screens.contextlist.ContextAddScrKeyContextModify = res.screens.contextlist.ContextModifyScrKeyAccessListUndefined = res.screens.contextlist.AccessListUndefinedScrKeyContextOperResults = res.screens.contextlist.ContextOperResultsScrKeyConfigPDSN = res.screens.pdsn.PDSNServiceScrKeyShowPDSN = res.screens.pdsn.PDSNServiceScrKeySPIBind = res.screens.pdsn.PDSNServiceScrKeyAddService = res.screens.pdsn.PDSNServiceScrKeyPDSNClosedRP = res.screens.pdsn.SPdsnClosedRPScrKeyPDSNClosedRPConfig = res.screens.pdsn.SPdsnClosedRPConfigScrKeyShowPcfStatus = res.screens.pdsn.SShowPcfStatusScrKeyUserPref = res.screens.userpreferences.UserPreferencesScrKeyAAATest = res.screens.aaa.SAAATestScrKeyAAARADIUSTest = res.screens.aaa.SRADIUSTestScrKeyAAARADIUSCounter = res.screens.aaa.SRADIUSCounter
> ScrKeyShowCardDiag = res.screens.csp.SCSPScrKeyCardHardware = res.screens.csp.SCSPScrKeyHardwareInventory = res.screens.csp.SCSPScrKeyHardwareVersion = res.screens.csp.SCSPScrKeyMacAddr = res.screens.csp.SCSPScrKeyMIPFA = res.screens.mip.SMIPScrKeyMIPFASess = res.screens.mip.SMIPScrKeyMIPFAStat = res.screens.mip.SMIPScrKeyMIPHA = res.screens.mip.SMIPScrKeyMIPHASess = res.screens.mip.SMIPScrKeyMIPHAStat = res.screens.mip.SMIPScrKeyAuditFilter = res.screens.audit.SAuditScrKeyAuditDetails = res.screens.audit.SAuditScrKeyCardMapping = res.screens.csp.SCSPScrKeySynch = res.screens.csp.SCSPScrKeyVLANDetails = res.screens.csp.SCSPScrKeySShowAlarm = res.screens.csp.SCSPScrKeyPortUtilization = res.screens.csp.SCSPScrKeyPrint = res.print.SPrintScrKey = res.screens.process.SProcessMonitorScrKeyProcessThreshold = res.screens.process.SProcessMonitorScrKeySAPNConfig = res.screens.apn.SAPNScrKeySAPNStat = res.screens.apn.SAPNScrKeyGTPPConf = res.screens.gtpp.SGTPPScrKeyGTPPStat = res.screens.gtpp.SGTPPScrKeyGTPPTest = res.screens.gtpp.SGTPPScrKeyIPSecMap = res.screens.ipsec.SIPSecScrKeyIsakmp = res.screens.ipsec.SIPSecScrKeyIsakmpSA = res.screens.ipsec.SIPSecScrKeyTransform = res.screens.ipsec.SIPSecScrKeyIPSecSA = res.screens.ipsec.SIPSecScrKeyIPSecStat = res.screens.ipsec.SIPSecScrKeyIPSecResult = res.screens.ipsec.SIPSecScrKeyPDSNClosedRPConfig = res.screens.pdsn.SPdsnClosedRPScrKeySPIOTiming=res.screens.csp.SCSP | ScrKeyAAARADIUSCounterDetails = res.screens.aaa.SRADIUSCounterScrKeyAAARADIUSAuth = res.screens.aaa.SRADIUSAuthScrKeyAAARADIUSAuthConfig = res.screens.aaa.SRADIUSAuthScrKeyAAARADIUSAcct = res.screens.aaa.SRADIUSAcctScrKeyAAAContextConfig = res.screens.aaa.SAAAContextConfigScrKeyModifyContextAAA = res.screens.aaa.SAAAContextConfigScrKeyAAARADIUSResult = res.screens.aaa.SRADIUSResultScrKeyAAAGlobalConfig = res.screens.aaa.SAAAGlobalConfigScrKeyModifyGlobalAAA = res.screens.aaa.SAAAGlobalConfigScrKeyRADIUSClientStatus = res.screens.aaa.SRADIUSClientStatusScrKeyAccessList = res.screens.vpn.AccessListScrKeyAccessListOpr = res.screens.vpn.AccessListScrKeyIPRoute = res.screens.vpn.IPRouteScrKeyIPRouteConf = res.screens.vpn.IPRouteScrKeySGetIntf = res.screens.vpn.IPRouteScrKeyIPPool = res.screens.vpn.IPPoolScrKeyIPPoolConf = res.screens.vpn.IPPoolScrKeyIPInterface = res.screens.vpn.IPInterfaceScrKeyIPInterfaceConf = res.screens.vpn.IPInterfaceScrKeyDNSConf = res.screens.vpn.SDNSConfScrKeyShowResult = res.screens.vpn.ResultCodeScrKeyIPInterfaceStats = res.screens.vpn.SIPInterfaceStatsScrKeyBusyoutRangeConf = res.screens.vpn.SBusyoutRangeConfScrKeyShowIPSP = res.screens.vpn.SShowIPSPScrKeyMonitorProtocols = res.screens.monitor.SMonitorScrKeyMonitorSubscribers = res.screens.monitor.SMonitorScrKeyProtoCriteria = res.screens.monitor.SMonitorFilterScrKeySubsCriteria = res.screens.monitor.SMonitorSubsFilterScrKeyFrontView = res.screens.csp.SIMGViewScrKeyRearView = res.screens.csp.SIMGViewScrKeySysInfo = res.screens.csp.SSysInfoScrKeyCardConfig = res.screens.csp.SCardConfig
> ScrKeyApplicationServerConfig=res.screens.vmg.SApplicationServerScrKeyAsAppDBConfig=res.screens.vmg.SAsAppDBScrKeyAsAppVimConfig=res.screens.vmg.SAsAppVimScrKeyAsAppChatConfConfig=res.screens.vmg.SAsAppChatConfScrKeyVmgMmsConfig=res.screens.vmg.SVmgMmsScrKeyAsDisConfig=res.screens.vmg.SAsDisScrKeyAsAppPttConfig=res.screens.vmg.SAsAppPttScrKeySTiming=res.screens.csp.SCSPScrKeyMultipleColSort = res.components.table.SMultipleColumnSortScrKeyIMGInfo = res.screens.hwinventory.SIMGInfoScrKeyProxyDns = res.screens.vpn.SProxyDnsScrKeyCscfPeerServer = res.screens.ims.SCscfPeerServerScrKeyCscfPolicy = res.screens.ims.SCscfPolicyScrKeyCscfService = res.screens.ims.SCscfServiceScrKeyCscfSessTemp = res.screens.ims.SCscfSessTempScrKeyCscfRoute = res.screens.ims.SCscfRouteScrKeyCscfACL = res.screens.ims.SCscfAclScrKeyCscfTranslation = res.screens.ims.SCscfTranslationScrKeyClassMap = res.screens.vpn.SClassMapScrKeyPolicyMap = res.screens.vpn.SPolicyMapScrKeyPolicyGroup = res.screens.vpn.SPolicyGroupScrKeyCscfURN = res.screens.ims.SCscfUrnScrKeyOnDemandReportConfig=res.screens.cf.SReportCommon | ScrKeyPortConfig = res.screens.csp.SPortConfigScrKeyModifyPort = res.screens.csp.SModifyPortScrKeyPortInformation = res.screens.csp.SPortInformationScrKeyShowPortCounters = res.screens.csp.SShowPortCountersScrKeySystem = res.screens.csp.SSysInfoScrKeyShowCardDiag = res.screens.csp.SShowCardDiagScrKeyCardHardware = res.screens.csp.SCardHardwareScrKeyHardwareInventory = res.screens.csp.SHardwareInventoryScrKeyHardwareVersion = res.screens.csp.SHardwareVersionScrKeyShowPower = res.screens.csp.SShowPowerScrKeySoftUpgrade = res.screens.softupgrade.SSoftUpgradeScrKeyShowVersion = res.screens.softupgrade.SShowVersionScrKeyOnlinePatchUpgrade = res.screens.softupgrade.SOnlinePatchUpgradeScrKeyFCFileSelection = res.screens.softupgrade.SFileSelectionScrKeyFCFileComparisonResult = res.screens.softupgrade.SFileComparisonResultScrKeyFCRemoteFileBrowser = res.screens.softupgrade.SRemoteFileBrowserScrKeyConfigurationFileEditor = res.screens.softupgrade.SConfigurationFileEditorScrKeyBootConfiguration = res.screens.softupgrade.SBootConfigurationScrKeyMIPFA = res.screens.mip.SMIPFAScrKeyMIPFASess = res.screens.mip.SMIPFASessScrKeyMIPFAStat = res.screens.mip.SMIPFAStatScrKeyMIPHA = res.screens.mip.SMIPHAScrKeyMIPHASess = res.screens.mip.SMIPHASessScrKeyMIPHAStat = res.screens.mip.SMIPHAStatScrKeyMIPFAContext = res.screens.mip.SMIPFAContextScrKeyMIPHAContext = res.screens.mip.SMIPHAContextScrKeySubsConfig = res.screens.subscriber.SubsConfigScrKeyChangePassword = res.screens.useradm.SChangePasswordScrKeyChangePasswordDialog = res.screens.useradm.SChangePasswordDialogScrKeyDefaultSubsConfig = res.screens.subscriber.SDefaultSubsConfigScrKeySysLog = res.screens.logging.SSysLogScrKeySysLogConf = res.screens.logging.SSysLog
> | ScrKeyLoggingConfig = res.screens.logging.SLoggingConfigScrKeyShowResultDialog = res.screens.logging.SResultDialogScrKeySNMPShow = res.screens.snmp.SSNMPScrKeySNMPConfig = res.screens.snmp.SSNMPConfigScrKeySNMPStatistics = res.screens.snmp.SSNMPStatisticsScrKeyUserSessInfo = res.screens.security.SUserSessInfoScrKeyInstall = res.screens.license.SInstallScrKeyLicense = res.screens.license.SLicenseScrKeyClock = res.screens.clock.SClockScrKeyAudit = res.screens.audit.SAuditScrKeyAuditFilter = res.screens.audit.SAuditFilterScrKeyAuditDetails = res.screens.audit.SAuditDetailsScrKeyBulkStat = res.screens.bulkstatistics.BulkStatsScrKeyBulkStatConf = res.screens.bulkstatistics.BulkStatsScrKeyBulkAnalysis = res.screens.bulkstatistics.performancestatScrKeyGraphScreenBulk = res.screens.bulkstatistics.performancestatScrKeyPerformanceStat = res.screens.bulkstatistics.performancestatScrKeyOrbemClientSession = res.screens.orbem.SOrbemClientSessionScrKeyOrbemConfig = res.screens.orbem.SOrbemConfigScrKeyModifyOrbemConfig = res.screens.orbem.SOrbemConfigScrKeyModifyOrbemClient = res.screens.orbem.SModifyOrbemClientScrKeyUCM = res.screens.ucm.SUCMScrKeyCardMapping = res.screens.csp.SCardMappingsScrKeySysInfoAdv = res.screens.csp.SAdvDataScrKeyHalt = res.screens.csp.SHaltScrKeyMigrate = res.screens.csp.SMigrateScrKeyPriority = res.screens.csp.SPriorityScrKeySynch = res.screens.csp.SSynchScrKeyVLANDetails = res.screens.csp.SVLANDetailsScrKeyMacAddr = res.screens.csp.SPortMacAddrScrKeyPortUtilization = res.screens.csp.SPortUtilizationScrKeyAllMgr = res.screens.session.SessionSubsystemScrKeySessRecovery = res.screens.session.SSessRecoveryScrKeyShowSessionProgress = res.screens.session.SShowSessionProgress
> | ScrKeySessProgressFilterDlg = res.screens.session.SShowSessionProgressScrKeyGenericRP = res.screens.rp.SGenericRPScrKeyGenericBCMCS = res.screens.bcmcs.SGenericBCMCSScrKeyMulticastSessions = res.screens.bcmcs.SMulticastSessionsScrKeyMulticastSessionFilter = res.screens.bcmcs.SMulticastSessionsFilterDialogScrKeyMulticastSessionsResult = res.screens.bcmcs.SShowMulticastSessionsResultScrKeySShowCpu = res.screens.cpu.SShowCpuScrKeySShowCpuDetails = res.screens.cpu.SShowCpuScrKeySShowTask = res.screens.cpu.SShowTaskScrKeyShowResources = res.screens.cpu.SShowResourcesScrKeyTaskConfig = res.screens.cpu.STaskConfigScrKeyProcessThreshold = res.screens.process.SThresholdScrKeyCOAlarms = res.screens.alarm.SCOAlarmsScrKeyAlarmStatFilters = res.screens.alarm.SAlarmStatFiltersScrKeyAlarmStat = res.screens.alarm.SAlarmStatFiltersScrKeyEventSetFilter = res.screens.alarm.SAlarmFilterScrKeyEventConfig = res.screens.alarm.SAlarmConfigScrKeyEvent = res.screens.alarm.SAlarmViewScrKeyEventDesc = res.screens.alarm.SDescScrKeySShowAlarm = res.screens.alarm.SShowAlarmScrKeyShowAlarmStat = res.screens.alarm.SShowAlarmStatScrKeyNTP = res.screens.system.SNTPScrKeyNetReqPDPCtxtConfig = res.screens.system.SNetReqPDPCtxtConfigScrKeyNetReqPDPCtxtConfigDlg = res.screens.system.SNetReqPDPCtxtConfigScrKeySAPN = res.screens.apn.SAPNScrKeySAPNConfig = res.screens.apn.SAPNConfigScrKeySAPNStat = res.screens.apn.SAPNStatScrKeyDhcpShow = res.screens.dhcp.SDHCPShowScrKeyDhcpConfig = res.screens.dhcp.SDHCPConfigScrKeyDhcpStat = res.screens.dhcp.SDHCPStatScrKeySDHCPStatus = res.screens.dhcp.SDHCPStatusScrKeyDhcpCache = res.screens.dhcp.SDHCPCacheScrKeyDhcpTest = res.screens.dhcp.SDHCPTestScrKeyLAC = res.screens.l2tp.L2tpScrKeyLACConfig = res.screens.l2tp.L2tp
> | ScrKeySShowL2TP = res.screens.l2tp.L2tpScrKeyLTTPTunnelFull = res.screens.l2tp.L2tpScrKeyLTTPTunnelCntrs = res.screens.l2tp.L2tpScrKeyLTTPTunnelSummary = res.screens.l2tp.L2tpScrKeyLTTPSessionFull = res.screens.l2tp.L2tpScrKeyLTTPSessionCntrs = res.screens.l2tp.L2tpScrKeyLTTPSessionSummary = res.screens.l2tp.L2tpScrKeyLTTPStat = res.screens.l2tp.L2tpScrKeyLNSShow = res.screens.l2tp.SLNSShowScrKeyLNSConfig = res.screens.l2tp.SLNSConfigScrKeyGTPPConf = res.screens.gtpp.SGTPPConfScrKeyGTPPStat = res.screens.gtpp.SGTPPStatScrKeyGTPPTest = res.screens.gtpp.SGTPPTestScrKeyGSNConf = res.screens.gtpp.SGSNScrKeyGTPPInterimNow = res.screens.gtpp.SGTPPInterimNowScrKeyShowGTPPCounters = res.screens.gtpp.SShowGTPPCountersScrKeyGTPPStorageSrvStat = res.screens.gtpp.SGTPPStorageServerStatisticsScrKeyGGSNService = res.screens.ggsn.SGGSNServiceScrKeyGGSNServiceInfo = res.screens.ggsn.SGGSNServiceInfoScrKeyGGSNServiceConfig = res.screens.ggsn.SGGSNServiceConfigScrKeyGTPCStat = res.screens.gtpc.SGTPCStatisticsScrKeyGTPCTest = res.screens.gtpc.SGTPCTestScrKeyIPSecMap = res.screens.ipsec.SIPSecMapScrKeyIsakmp = res.screens.ipsec.SIsakmpScrKeyIsakmpSA = res.screens.ipsec.SIsakmpSAScrKeyTransform = res.screens.ipsec.STransformScrKeyIPSecSA = res.screens.ipsec.SIPSecSAScrKeyIPSecStat = res.screens.ipsec.SIPSecStatScrKeyPeriodicSaveBoxerCfg = res.screens.configbackup.SPeriodicSaveBoxerCfgScrKeyIPRIPConfig = res.screens.rip.SIPRIPConfigScrKeyIPRIPConfigDlg = res.screens.rip.SIPRIPConfigScrKeyShowRouterRIPConfig = res.screens.rip.SRouterRIPConfigScrKeyModifyRouterRIPConfig = res.screens.rip.SRouterRIPConfigScrKeyKeyChainConfig = res.screens.rip.SKeyChainConfigurationScrKeyAddKeyChain = res.screens.rip.SKeyChainConfiguration
> | ScrKeyModifyKeyChainConfig = res.screens.rip.SModifyKeyChainConfigScrKeyExternalInlineServer = res.screens.vpn.SExternalInlineServerScrKeyIPPoolDefConfig = res.screens.vpn.SIPPoolDefaultConfigScrKeyAddBusyoutRangeConf = res.screens.vpn.SAddBusyoutRangeConfScrKeySFetchNonLocalInfo= res.globalcommon.FetchNonLocalInfoScrKeySThreshShow = res.screens.threshold.SThreshShowScrKeyThreshConfig = res.screens.threshold.SThreshConfigScrKeySCongestionControl = res.screens.threshold.SCongestionControlScrKeyCongestionControlStat = res.screens.threshold.SCongestionControlStatScrKeyShowNRPC = res.screens.system.SShowNRPCScrKeyNewCallPolicy = res.screens.system.SNewCallPolicyScrKeySBannerDisplay = res.screens.system.SBannerDisplayScrKeyShowSessionDuration = res.screens.session.SShowSessionDurationScrKeySessDurationFilterDlg = res.screens.session.SShowSessionDurationScrKeySessionDisconnectStatistics = res.screens.session.SessionDisconnectStatisticsScrKeySessionSetuptimeStat = res.screens.session.SSessionSetuptimeStatScrKeyPortMonitor = res.screens.portmonitor.SPortMonitorScrKeyNetworkReachability = res.screens.nr.SNetworkReachabilityScrKeyNrConfig = res.screens.nr.SNrConfigScrKeySShowVMGAll = res.screens.vmg.SShowVMGAllScrKeySShowVMGInterfaces = res.screens.vmg.SShowVMGInterfacesScrKeySShowVMGGCPStat = res.screens.vmg.SShowVMGGCPStatScrKeyVMGgpdsps = res.screens.vmg.SVMGgpdspsScrKeyGTPCInfo = res.screens.gtpc.SGTPCInfoScrKeyGTPCCounters = res.screens.gtpc.SGTPCCountersScrKeyGTPCSummary = res.screens.gtpc.SGTPCSummaryScrKeyGTPCSession = res.screens.gtpc.SGTPCSession
> | ScrKeyAlarmScheduler = res.screens.alarm.SAlarmSchedulerScrIDGraphConfig = res.graphs.SGraphConfigScrKeyGraphFilter = res.graphs.SGraphFilterScrKeyGraphScreen = res.graphs.SGraphScreenScrKeyIPPoolDetail = res.screens.vpn.IPPoolScrKeyIMGFileBrowser = res.screens.softupgrade.SIMGFileBrowserScrKeyShowGTPPStorageServerCounters = res.screens.gtpp.SSCounterDialogScrKeyOSPFExceptionHandler = res.screens.ospf.SOSPFExceptionHandlerScrKeyShowOSPFInformation = res.screens.ospf.SShowOSPFInformationScrKeyShowOSPFInterface = res.screens.ospf.SShowOSPFInterfaceScrKeyShowOSPFNeighbor = res.screens.ospf.SShowOSPFNeighborScrKeyOSPFConfiguration = res.screens.ospf.SOSPFConfigurationScrKeyModifyOSPFConfiguration = res.screens.ospf.SModifyOSPFConfigurationScrKeySDHCPExcpHandler = res.screens.dhcp.SDHCPExcpHandlerScrKeySDHCPServiceConfig = res.screens.dhcp.SDHCPServiceConfigScrKeySDHCPDetails = res.screens.dhcp.SDHCPDetailsScrKeySDHCPShowConfig = res.screens.dhcp.SDHCPShowConfigScrKeyUDR = res.screens.cdr.SCDRScrKeyUDRConfig = res.screens.cdr.SCDRConfigScrKeyShowOSPFBorderRouters = res.screens.ospf.SShowOSPFBorderRoutersScrKeyShowOSPFRoute = res.screens.ospf.SShowOSPFRouteScrKeyShowOSPFDatabase = res.screens.ospf.SShowOSPFDatabaseScrKeyShowOSPFDebugging = res.screens.ospf.SShowOSPFDebuggingScrKeySPIOTiming=res.screens.csp.SSPIOTimingScrKeyQosNpuStats=res.screens.npu.SQosNpuStatsScrKeyShowQoSNPUTrafficBanwidth = res.screens.npu.SShowQoSNPUTrafficBandwidthScrKeySQosnpuConfig = res.screens.npu.SQosnpuConfigScrKeyIPOSPFInterface = res.screens.ospf.SIPOSPFInterface
> | ScrKeyModifyIPOSPFInterface = res.screens.ospf.SModifyIPOSPFInterfaceScrKeySDHCPStatistics = res.screens.dhcp.SDHCPStatisticsScrKeyModifyOSPFDebugging = res.screens.ospf.SModifyOSPFDebuggingScrKeyOSPFAreaConfiguration = res.screens.ospf.SOSPFAreaConfigurationScrKeyVirtualLinks = res.screens.ospf.SVirtualLinksScrKeyModifyOSPFAreaConfiguration = res.screens.ospf.SModifyOSPFAreaConfigurationScrKeyBoundPortCounters = res.screens.csp.SBoundPortCountersScrKeyIsakmpKeepAlive = res.screens.ipsec.SIsakmpKeepAliveScrKeyCryptoGroupConfig = res.screens.ipsec.SCryptoGroupConfigScrKeyCryptoGroup = res.screens.ipsec.SShowCryptoGroupScrKeyModifySchema = res.screens.bulkstatistics.SModifySchemaScrKeyShowOSPFNeighborDetail = res.screens.ospf.SShowOSPFNeighborDetailScrKeySDHCPInfo = res.screens.dhcp.SDHCPInfoScrKeyModifyFileSystem = res.screens.softupgrade.SModifyFileSystemScrKeyChargingService = res.screens.chargingservice.SChargingServiceScrKeyModifyChargingServiceConfig = res.screens.chargingservice.SChargingServiceScrKeyCSService = res.screens.css.SCSServiceScrKeyCSServiceConfig =res.screens.css.SAddCSServiceScrKeyCSSServer =res.screens.css.SCSSServerScrKeyCSSServerConfig=res.screens.css.SCSSServerConfigScrKeyCSSDelSeq =res.screens.css.SCSSDeliverySequenceScrKeyCSSDelSeqConfig =res.screens.css.SCSSDeliverySequenceConfigScrKeySGlobalConfiguration =res.screens.chargingservice.SGlobalConfigurationScrKeySCSDetails=res.screens.chargingservice.SCSDetailsScrKeyChargingServiceFlows=res.screens.chargingservice.SChargingServiceFlowsScrKeyChargingServiceSessions = res.screens.chargingservice.SChargingServiceSessions
> | ScrKeyChargingServiceManagerStats = res.screens.chargingservice.SChargingServiceManagerStatsScrKeyIPAccessGroupStatistics=res.screens.vpn.SIPAccessGroupStatisticsScrKeyCommonClass=res.utils.SCommonClassScrKeySDataHandler=res.utils.SDataHandlerScrKeyAAARADIUSCharging = res.screens.aaa.SRADIUSChargingScrKeyAAARADIUSChargingConfig = res.screens.aaa.SRADIUSChargingScrKeyEDR = res.screens.cdr.SEDRScrKeyEDRConfig = res.screens.cdr.SEDRConfigScrKeyShowASInfo=res.screens.vmg.SShowASInfoScrKeyAsSigRoute=res.screens.vmg.SAsSigRouteScrKeyAsSigRouteConfig=res.screens.vmg.SAsSigRouteConfigScrKeyAsSigSIP=res.screens.vmg.SAsSigSIPScrKeyAsSigSIPConfig=res.screens.vmg.SAsSigSIPConfigScrKeyApplicationServer = res.screens.vmg.SApplicationServerScrKeyApplicationServerConfig = res.screens.vmg.SApplicationServerConfigScrKeyAsAppDB = res.screens.vmg.SAsAppDBScrKeyAsAppDBConfig = res.screens.vmg.SAsAppDBConfigScrKeyAsAppVim = res.screens.vmg.SAsAppVimScrKeyAsAppVimConfig=res.screens.vmg.SAsAppVimConfigScrKeyAsAppChatConf = res.screens.vmg.SAsAppChatConfScrKeyAsAppChatConfConfig=res.screens.vmg.SAsAppChatConfConfigScrKeySShowVMGPacketizers=res.screens.vmg.SShowVMGPacketizersScrKeyAsChatConfTable=res.screens.vmg.SAsChatConfTableScrKeyAsChatConfTableConfig=res.screens.vmg.SAsChatConfTableConfigScrKeyVMGCall=res.screens.vmg.SShowVMGCallScrKeySShowVMGConnections=res.screens.vmg.SShowVMGConnectionsScrKeyVMG=res.screens.vmg.SVMGScrKeyVMGConfig=res.screens.vmg.SVMGConfigScrKeySShowASAnnouncements=res.screens.vmg.SShowASAnnouncementsScrKeyVMGgpdsps= res.screens.vmg.SVMGgpdsps
> | ScrKeyVMGVop = res.screens.vmg.SVMGVopScrKeyVMGVopConfig = res.screens.vmg.SVMGVopConfigScrKeyVmgMms = res.screens.vmg.SVmgMmsScrKeyVmgMmsConfig=res.screens.vmg.SVmgMmsConfigScrKeyVMGres=res.screens.vmg.SVMGresScrKeyVMGGcp = res.screens.vmg.SVMGGcpScrKeyVMGGcpConfig = res.screens.vmg.SVMGGcpConfigScrKeyPrepaid3GPP2Statistics = res.screens.session.SPrepaid3GPP2StatisticsScrKeyRemoteServerList = res.screens.vpn.SRemoteServerListScrKeyConfigRemoteServerList = res.screens.vpn.SConfigRemoteServerListScrKeyAsDis = res.screens.vmg.SAsDisScrKeyAsDisConfig=res.screens.vmg.SAsDisConfigScrKeyShowAsConf=res.screens.vmg.SShowAsConfScrKeyAsAppPtt = res.screens.vmg.SAsAppPttScrKeyAsAppPttConfig=res.screens.vmg.SAsAppPttConfigScrKeyVMGchannel=res.screens.vmg.SVMGchannelScrKeyAsAppVinfo = res.screens.vmg.SAsAppVinfoScrKeyAsAppVinfoConfig=res.screens.vmg.SAsAppVinfoConfigScrKeyIpv4DnsProxy=res.screens.vpn.SDNSProxyCfgScrKeyORBStats=res.screens.security.SORBStatisticsScrKeyDeleteChargingService = res.screens.chargingservice.SChargingServiceScrKeyChargingServiceOprResult = res.screens.chargingservice.SChargingServiceScrKeySTiming=res.screens.vmg.STimingScrKeyDomainConfig=res.screens.contextlist.SDomainConfigScrKeySessionCounters=res.screens.session.SShowSessionCountersScrKeySROHCStatistics=res.screens.ppp.SROHCStatisticsScrKeyIPPolicyForward=res.screens.vpn.SIPPolicyForwardScrKeyModifyIPPolicyForward=res.screens.vpn.SModifyIPPolicyForwardScrKeyMIPIPAssignment=res.screens.mip.SMIPIPAssignmentScrKeyMIPIPAssignmentConfig=res.screens.mip.SMIPIPAssignmentConfigScrKeyEnforceImsi = res.screens.system.SEnforceImsi
> | ScrKeyIPv6Pool = res.screens.ipv6.SIPv6PoolScrKeyIPv6PoolConf = res.screens.ipv6.SIPv6PoolConfScrKeyIPv6PoolDetail = res.screens.ipv6.SIPv6PoolDetailScrKeyIPv6ShowResult = res.screens.ipv6.SShowResultScrKeySRPConfiguration = res.screens.srp.SSRPConfigurationScrKeyModifySRPConfiguration = res.screens.srp.SModifySRPConfigurationScrKeySRPStatistics = res.screens.srp.SSRPStatisticsScrKeySRPCheckPointInfo = res.screens.srp.SSRPCheckPointInfoScrKeySRPInfo = res.screens.srp.SSRPInfoScrKeySRPMonitorInformation = res.screens.srp.SSRPMonitorInformationScrKeySupportDetails = res.screens.system.SShowSupportDetailsScrKeyBatchJobs = res.screens.monitor.SBatchJobsScrKeyShowBGP = res.screens.bgp.ShowBGPScrKeyShowBGPDebugging = res.screens.bgp.ShowBGPDebuggingScrKeyShowBGPNeighbor = res.screens.bgp.ShowBGPNeighborScrKeyShowBGPSummary = res.screens.bgp.ShowBGPSummaryScrKeyConfigUpdateScheduler = res.screens.configupdate.SConfigSchedulerScrKeyScheduledConfigUpdate = res.screens.configupdate.SScheduledConfigScrKeyConfigUpdateFilter = res.screens.configupdate.SFilterScreenScrKeyFileTransfer = res.screens.configupdate.SFileTransferScrKeyBGPConfiguration = res.screens.bgp.SBGPConfigurationScrKeyModifyBGPConfiguration = res.screens.bgp.SModifyBGPConfigurationScrKeyClearIPBGPPeer = res.screens.bgp.SClearIPBGPPeerScrKeyAsPathAccessList = res.screens.bgp.AsPathAccessListScrKeyRouteMapConfiguration = res.screens.bgp.SRouteMapConfigurationScrKeyAddModifyRouteMapConfiguration = res.screens.bgp.SAddModifyRouteMapConfigurationScrKeySConfigCriteria = res.screens.showconfig.SConfigCriteriaScrKeySViewConfig = res.screens.showconfig.SViewConfig
> | ScrKeyShowSystemInfo = res.screens.system.SShowSystemInfoScrKeySearchIPPoolNames = res.screens.vpn.SSearchIPPoolNamesScrKeyAppConfig = res.topology.SApplicationConfigurationScrKeySCrashList = res.screens.crashlist.SCrashListScrKeySCrashInfo = res.screens.crashlist.SCrashInfoScrKeyAddressHoldTimerInformation = res.screens.vpn.SAddressHoldTimerInformationScrKeyPoolAddressInformation = res.screens.vpn.SPoolAddressInformationScrKeySShowSigSipDns = res.screens.vmg.SShowSigSipDnsScrKeyAcsAnalyzerStatistics = res.screens.acs.SAcsAnalyzerStatisticsScrKeyShowAcsSessions = res.screens.acs.ShowAcsSessionsScrKeyShowAcsSessionsFilter = res.screens.acs.ShowAcsSessionsFilterScrKeyShowAcsFlows = res.screens.acs.ShowAcsFlowsScrKeyAcsFlowsFliter = res.screens.acs.ShowAcsFlowsFilterScrKeyShowAcsSubsystem = res.screens.acs.ShowAcsSubsystemScrKeyAsAppVimProfile = res.screens.vmg.SAsAppVimProfileScrKeyAsAppVimProfileConfig = res.screens.vmg.SAsAppVimProfileConfigScrKeyAcsCommonClass=res.screens.acs.SAcsCommonClassScrKeyAcsConf=res.screens.acs.SAcsConfScrKeyAcsOperResults=res.screens.acs.SAcsOperResultsScrKeyAcsCFPolicyConfig=res.screens.acs.SAcsCFPolicyConfigScrKeyAcsRulebaseConfig=res.screens.acs.SAcsRuleBaseConfigScrKeyAcsRuledefConfig=res.screens.acs.SAcsRuleDefConfigScrKeyACS = res.screens.acs.SACSScrKeyACSDetails = res.screens.acs.SACSDetailsScrKeyACSGeneralConfig = res.screens.acs.SACSGeneralConfigScrKeyACSChargingActionConfig = res.screens.acs.SACSChargingActionConfigScrKeyACSEDRConfig = res.screens.acs.SACSEDRConfig
> | ScrKeyACSUDRConfig = res.screens.acs.SACSUDRConfigScrKeyConfirmAttributeDelete = res.screens.acs.SACSEDRConfigScrKeyShowDiameterRoute = res.screens.acs.SShowDiameterRouteScrKeyDHCPTest = res.screens.dhcp.SDHCPTestScrKeyAcsChargingActionStats = res.screens.acs.SAcsChargingActionStatsScrKeyAcsRulebaseStats = res.screens.acs.SAcsRulebaseStatsScrKeyAcsRuledefStats = res.screens.acs.SAcsRuledefStatsScrKeyGTPPStorageServerStatus = res.screens.gtpp.SShowGTPPStorageServerStatusScrKeyHardwareAudit = res.screens.hwinventory.SHardwareAuditScrKeyAddComment = res.screens.hwinventory.SAddCommentScrKeyHardwareFilter = res.screens.hwinventory.SHardwareFilterScrKeyHardwareDetails = res.screens.hwinventory.SHardwareDetailsScrKeyAcsDccaStats = res.screens.acs.SAcsDccaStatsScrKeyAcsDccaConfig = res.screens.acs.SAcsDccaConfigScrKeyRouteMapEntryDetails = res.screens.bgp.SRouteMapEntryDetailsScrKeyDiameter = res.screens.acs.SDiameterScrKeyDiameterConfig = res.screens.acs.SDiameterConfigScrKeyIMGInfo = res.screens.hwinventory.SIMGInfoScrKeyDiameterPeers = res.screens.acs.SDiameterPeersScrKeyDiameterEndpoint = res.screens.acs.SDiameterEndpointScrKeyDiameterStats = res.screens.acs.SDiameterStatsScrKeyProxyDns = res.screens.vpn.SProxyDnsScrKeySelectCounters = res.screens.bulkstatistics.SSelectCountersScrKeySROHCProfile = res.screens.rohc.SROHCProfileScrKeyPeriodicBackup = res.screens.periodicbackup.SPeriodicBackupScrKeyBackupHistory = res.screens.periodicbackup.SBackupHistoryScrKeyFilterScreen = res.screens.periodicbackup.SFilterScreenScrKeyShowRsvpStatistics = res.screens.rsvp.ShowRsvpStatistics
> | ScrKeyShowRsvpCounters = res.screens.rsvp.ShowRsvpCountersScrKeyAlarmInformation = res.screens.alarm.AlarmInformationScrKeyRouteAccessList = res.screens.vpn.RouteAccessListxListScrKeyTrapForwarding = res.screens.alarm.TrapForwardingScrKeySMIPFAHAStatus = res.screens.mip.SMIPFAHAStatusScrKeyIPPrefixList = res.screens.vpn.IPPrefixListScrKeyOfflineUpgrade = res.screens.softupgrade.SOfflineUpgradeScrKeyClassMap = res.screens.vpn.SClassMapScrKeyPolicyMap = res.screens.vpn.SPolicyMapScrKeyPolicyGroup = res.screens.vpn.SPolicyGroupScrKeyIpRoutingMaxPath = res.screens.vpn.IPRoutingMaxPathScrKeyAccessFlowStatistics = res.screens.subscriber.AccessFlowStatisticsScrKeySAcsCreditControlSessionStates = res.screens.acs.SAcsCreditControlSessionStatesScrKeyCscfPeerServer = res.screens.ims.SCscfPeerServerScrKeyCscfPolicy = res.screens.ims.SCscfPolicyScrKeyCscfService = res.screens.ims.SCscfServiceScrKeyCscfSessTemp = res.screens.ims.SCscfSessTempScrKeyCscfRoute = res.screens.ims.SCscfRouteScrKeyCscfACL = res.screens.ims.SCscfAclScrKeyCscfTranslation = res.screens.ims.SCscfTranslationScrKeySendBroadcastMessage = res.screens.security.SBroadcastMessageScrKeySendBroadcastMessageAlert = res.screens.security.SBroadcastMessageScrKeySProtocolConfig = res.screens.p2p.SProtocolConfigScrKeySProtocolAnalysis = res.screens.p2p.SProtocolAnalysisScrKeySP2PGraphView = res.screens.p2p.SP2PGraphViewScrKeySP2PTabularView = res.screens.p2p.SP2PGraphViewScrKeyCscfURN = res.screens.ims.SCscfUrnScrKeySyslog = res.screens.syslog.SSyslogScrKeySyslogConfig = res.screens.syslog.SSyslogConfigScrKeyShowMsg = res.screens.syslog.SShowMsg
> | ScrKeyShowSyslogConf = res.screens.syslog.SShowSyslogConfScrKeyShowSgsnTable = res.screens.ggsn.SGGSNServiceSgsnTableScrKeyShowOspfVirtualLinks=res.screens.ospf.SShowOSPFVirtualLinksScrKeySShowFirewallStatistics = res.screens.firewall.SShowFirewallStatisticsScrKeySRADIUSCounterSummary=res.screens.aaa.SRADIUSCounterSummaryScrKeyOnDemandReportConfig=res.screens.cf.SOnDemandReportConfigScrKeySearchFilter=res.screens.cf.SSearchFilterScrKeyViewStatusReportConfig=res.screens.cf.SViewReportStatusScrKeyReportDetails=res.screens.cf.SReportDetailsScrKeySSGSNMAPStats=res.screens.sgsn.SSGSNMAPStatsScrKeySSGTPUStats=res.screens.sgsn.SSGTPUStatsScrKeySSGTPCStats=res.screens.sgsn.SSGTPCStatsScrKeySSGSNOprPolicy=res.screens.sgsn.SSGSNOprPolicyScrKeySSGSNOprPolicyDetail=res.screens.sgsn.SSGSNOprPolicyScrKeySACSCFCateStatView=res.screens.acs.SACSCFCateStatView.javaScrKeySCFStatistics=res.screens.cf.SCFStatisticsScrKeySCFCategoryDb=res.screens.cf.SCFCategoryDbViewScrKeySSCCPStats=res.screens.sgsn.SSCCPStats

> ‌
> The temip.cfg File
> This configuration file is for a flat-file based interface between WEM and TEMIP.
> Important: This configuration file is customer-specific and is not operational without the appropriate license. Please contact your local sales representative for additional information.
> The thr.cfg File
> This file contains parameters pertaining to the WEM thread pool.
> Caution: To ensure proper operation of the WEM, do not edit the parameters in these files.
> thr.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> THREAD: This is the configuration file for Thread pool.
> PoolEnable | Flag for enable or disable the thread pool.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Values:
> • | 1 - Thread pool enable
> • | 0 - Thread pool disable
> | 0 | 1 | 0
> Size | Size of the thread pool.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 | 100 | 10
> MaxSize | Maximum size of the thread pool.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | 10 | 100 | 100

> ‌
> The ua.cfg File
> This file contains parameters pertaining to the WEM support for the ANSI T1.276 security specification. These include parameters granting and restricting access, login failures, password aging, and password complexity.
> Important: Any change in the configuration files will restart the server resulting in client restart.
> ua.cfg File Parameters

> Key | Description | Minimum Value | Maximum Value | Default Value
> Security: This file contains the list of security parameters for user access to WEM.
> AllowIpAddress | List of allowed IP addresses and mask.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> IP address 0.0.0.0: Allows all addresses Format: Allow IP address/subnet-mask number, IP address/subnet-mask number...Nothing: Allow nothing | -- | -- | --
> DenyIpAddress | List of deny IP addresses and mask.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> IP address 0.0.0.0: Deny all Addresses Format: Deny IP address/subnet-mask number, IP address/subnet-mask number...Nothing in list: Deny nothing | -- | -- | --
> ConsecutiveFailLogin | The system limit on consecutive failed login for a given user ID shall be configurable.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Value 0: No limit | 0 | 10 | 5
> LockOutInterval | Locked out login ID, automatically, following the crossing of a configurable timeframe. Value is in minutes.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Value 0: No lock out | 0 | 1440 | 60
> AlertExpiryThreshold | The account alert expiry threshold after WEM generates an alert. Value is in days.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Value 0: No alert | 0 | 30 | 10
> MinPasswordChangeInterval | Passwords will be user changeable at the user's discretion following a configurable minimum interval since the last change. Value is in seconds.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Value 0: No interval | 0 | 86400 | 86400
> NumOfPasswordInHistory | System will support a password history to prevent password reuse. The parameters will be configurable with a default of at least the past five password iterations.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Value 0: No password history | 0 | 10 | 5
> PasswordInHistoryAtLeast | System will support a password history to prevent password reuse. The parameters will be configurable with a default of at least the past 180 days.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Value 0: No expiry | 0 | 365 | 180
> EMSAdminMailId | E-mail address of the WEM account created/reset password notification originator.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | -- | -- | No default value
> PasswordComplexityRules | This flag indicates which rules should be used to verify password complexity.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values:
> • | 0: None
> • | 1: ANSI
> | -- | -- | 1
> PasswordMinLength | This flag sets the minimum length of a user-defined password.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | PasswordComplexityRules = None
> 1 | 63 | 8
> PasswordComplexityRules = ANSI
> 3 | 63 | 8
> PasswordMinCharChange | This flag defines the minimum number of characters that must be changed when a user changes the password.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> | If PasswordComplexityRules is None, then do not check this. (Value is 0) |  |
> |  | PasswordComplexityRules = ANSI |  |
> |  | 0 | 8 | 2
> ChangePasswordOnNextLogin | If this flag enabled then, on next login, the user will be required to change the password. Else, the user will not be required to change the password.
> • | Needs a WEM Server restart
> • | Can be changed by the user
> Possible values:
> • | 0: Password change will not be required
> • | 1: Password change will be required
> | -- | -- | 1

> ‌
> The vacuum.cfg File
> This file contains parameters pertaining to PostgreSQL database vacuuming.
> Configuring values for CompleteDB:

> • | If this value is 0, it means that vacuuming needs to be done on all the tables individually.

> • | If this value is 1, it means that vacuuming is done only to the database and not the tables individually.

> vacuum.cfg File Parameters

> Key | Description and Values
> Type: This section describes the type of vacuum to be done on database. |
> VACUUM | This parameter reclaims space and makes it available for re-use. This command can operate in parallel with normal reading and writing of the table, as an exclusive lock is not obtained. This is the default value.
> VACUUM ANALYZE | This parameter performs a VACUUM and then an ANALYZE for each selected table.
> VACUUM FULL | This parameter physically reorders the tables. This requires an exclusive lock on each table while it is being processed. Important: VACUUM FULL is not recommended for routine use.
> Database
> Database Name = hh,hh | First "hh" specifies the starting time to vacuum the database or table Second "hh" specifies the time interval for performing periodic vacuum after the starting time. Default value for database: 12,12Default value for table: 00, 00. This means that do not vacuum the database or table. It means midnight 12 as we have a separate value for the same, that is, 24. Any non-zero value for this will override the CompleteDB flag for this database. For example, if the ConfigDB value is 13 and CompleteDB value for ConfigDB is 0, means that the entire DB will be vacuumed along with all the tables. However, if the timestamp of start of vacuum for the DB and any of the tables conflicts, then, vacuum will not be started for that table, and the DB will get precedence in this case. Max value: 24,24 (24 is same as 12:00 AM) Important: It is not recommended to start table level vacuuming for all tables at the same time as it will increase number of transactions to the database. Database level vacuuming takes care of table level vacuuming, that means it vacuums whole database including all the tables present in that database so at critical point if we want to start vacuuming on all tables at the same time, at that point, we can start only database level vacuum. If we want to vacuum one or more (but not all) tables from the database, in that case we can use table level vacuuming by enabling vacuum for that tables.
> ConfigDB | TrapDB | AuditDB | BulkDB | P2PDB
> 12, 12 | 12, 12 | 12, 12 | 12, 12 | 12, 12
> Table Name = hh,hh | ConfigDB | TrapDB | AuditDB | BulkDB | P2PDB
> | CompleteDB= 1boxer = 00,00portmontable = 00,00boxeruserinfo = 00,00userpreference = 00,00processthreshold = 00,00ippooldefaults = 00,00scbrdefaults = 00,00csmsessioninfo = 00,00bkinfo = 00, 00graphscreeninfo = 00,00batchjobcleanup = 00,00batchjobinfo = 00,00boxeronmap = 00,00dbbackupinfo = 00,00maptable = 00,00p2pinfo = 00,00updateinfo = 00,00userinfo = 00,00dbcurrent = 00,00hostname = 00,00syslogkeywordlist = 00,00syslogmsgfileinfo = 00,00 | CompleteDB= 1trap = 00,00deletedtrap = 00,00forwardinginfo = 00,00forwardpurgeinfo = 00,00mailinfo = 00,00mailmessage = 00,00configure = 00,00schedule = 00,00forwardaddress = 00,00pendingtrap = 00,00trap_current = 00,00trapoperdetails = 00,00 | CompleteDB= 1auditlog = 00,00auditlog_current = 00,00chassisinfo = 00,00cpuinfo = 00,00daughtercardinfo = 00,00hardwareactivity = 00,00hardwareinfo = 00,00lcrccspioinfo = 00,00pactacinfo = 00,00rowcount = 00,00smcinfo = 00,00spccardinfo = 00,00imglastevtgentime = 00,00 | CompleteDB= 1card = 00,00card_current = 00,00port = 00,00port_current = 00,00system = 00,00system_current = 00,00ppp = 00,00ppp_current = 00,00mipfa = 00,00mipfa_current = 00,00mipha = 00,00mipha_current = 00,00rp = 00,00rp_current = 00,00gtpc = 00,00gtpc_current = 00,00gtpp = 00,00gtpp_current = 00,00ippool = 00,00ippool_current = 00,00apn = 00,00apn_current = 00,00lac = 00,00lac_current = 00,00closedrp = 00,00closedrp_current = 00,00 | CompleteDB= 1bwstat = 00,00bwstat_current = 00,00dailystat = 00,00dailystat_current = 00,00hourlystat = 00,00hourlystat_current = 00,00protocolstat = 00,00protocolstat_current = 00,00scbrdailystats = 00,00scbrdailystats_current = 00,00scbrhourlystats = 00,00scbrhourlystats_current = 00,00scbrstats = 00,00scbrstats_current = 00,00tempp2p = 00,00thresholdstats = 00,00
> |  |  |  | radius = 00,00radius_current = 00,00imgaccess = 00,00ecs = 00,00ecs_current = 00,00misc = 00,00misc_current = 00,00ipsg = 00,00ipsg_current = 00,00asngw = 00,00asngw_current = 00,00sgsn = 00,00sgsn_current = 00,00sgtp = 00,00sgtp_current = 00,00sccp = 00,00sccp_current = 00,00ss7rd = 00,00ss7rd_current = 00,00mipv6ha = 00,00mipv6ha_current = 00,00context = 00,00context_current = 00,00cscf = 00,00cscf_current = 00,00ss7link = 00,00ss7link_current = 00,00gprs = 00,00gprs_current = 00,00 |

> ‌
> The wblist.cfg File
> This file provides information on the white black list database file paths that are mainly used for content filtering.
> wblist.cfg File Parameters

> Key | Description
> WBLIST: This section describes the parameters that store Content Filtering Server information.
> WblistPath | White Black list file path: This specifies the path where white black list database files are located. WblistPath = ./flash/cf/cfdatabases/wblistdb/

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883