> PDG Schema Statistics
> The PDG schema provides operational statistics that can be used for monitoring and troubleshooting the following products: PDG/TTG
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the PDG Schema

> Variables | Description | Data Type
> vpnname | Description: The name of the context currently facilitating the service processing the subscriber session. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | String
> vpnid | Description: The identification number of the context currently facilitating the service processing the subscriber session. This is an internal reference number. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | Int32
> svcname | Description: The service name for which PDG statistics are being displayed. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | String
> svcid | Description: The service ID for which PDG statistics are being displayed. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | Int32
> bindaddress | Description: The bind IP address for this PDG service. This variable is proprietary. Availability: IPSec/SSL. | String
> state | Description: System-wide PDG state identified by the following codes:
> • | unknown(0)
> • | noservice(1): Chassis is not configured/licensed for PDG service.
> • | active(2): At least one PDG service is available.
> • | temporary(3): PDG service is running in a temporary capacity.
> • | outofservice(4): No PDG service is currently active, but one or more PDG services are configured.
> This variable is proprietary. Availability: IPSec/SSL. | String
> sess-ttlcursess | Description: Number of total current sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curact | Description: Number of currently active PDG sessions. This variable is proprietary. Trigger: Increments on receiving a new call request from the UE. For IPSec, it increments after receiving an IKE_INIT message from the UE. For SSL, it increments after the SSL tunnel is established. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curdorm | Description: Number of currently dormant PDG sessions. This variable is proprietary. Trigger: For SSL, it represents those subscribers wherein the TCP connection is up but the SSL tunnel is not yet up. Availability: SSL. Type: Gauge | Int32
> sess-curactipv4 | Description: Number of currently active IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curdormipv4 | Description: Number of currently dormant IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curactipv6 | Description: Number of currently active IPv6 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curdormipv6 | Description: Number of currently dormant IPv6 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curdiripipv4 | Description: Number of current direct IP IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-curttgipv4 | Description: Number of current TTG IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-ttldiripipv4 | Description: Total number of direct IP IPv4 sessions. This variable is proprietary. Trigger: Increments upon successful IPv4 PDG mode call setup. Availability: IPSec/SSL. Type: Gauge | Int32
> sess-ttlttgipv4 | Description: Total number of TTG IPv4 sessions. This variable is proprietary. Trigger: Increments upon successful IPv4 TTG mode call setup. Availability: IPSec/SSL. | Int32
> sess-diripipv4succ | Description: Number of direct IP IPv4 successful sessions. This variable is proprietary. Trigger: Increments upon successful IPv4 PDG mode call setup. Availability: IPSec/SSL. | Int32
> sess-diripipv4attempt | Description: Number of direct IP IPv4 attempted sessions. This variable is proprietary. Trigger: Increments upon receiving an IKE_INIT message from the UE in IPsec and a TCP SYN message from the UE in SSL. Availability: IPSec/SSL. | Int32
> sess-diripipv4attemptfail | Description: Number of direct IP IPv4 attempted sessions that failed. This variable is proprietary. Trigger: Increments upon a session setup timeout and authentication failure scenario in PDG mode IPv4 call setup. Availability: IPSec/SSL. | Int32
> sess-ttgipv4succ | Description: Number of direct TTG IPv4 successful sessions. This variable is proprietary. Trigger: Increments upon a successful IPv4 TTG mode call setup. Availability: IPSec/SSL. | Int32
> sess-ttgipv4attempt | Description: Number of direct TTG IPv4 attempted sessions. This variable is proprietary. Trigger: Increments upon receiving an IKE_INIT message from the UE in IPsec and a TCP SYN message from the UE in SSL TTG mode. Availability: IPSec/SSL. | Int32
> sess-ttgipv4attemptfail | Description: Number of direct TTG IPv4 attempted sessions that failed. This variable is proprietary. Trigger: Increments upon a session setup timeout and authentication failure scenario in PDG mode IPv4 call setup. Availability: IPSec/SSL. | Int32
> sess-ttlsetup | Description: Total number of sessions set up. This variable is proprietary. Trigger: Increments upon sending a successful IKE_AUTH CFG response to the UE in IPSec, and upon a successful call setup with an MT_CLOSE message sent to the UE in SSL. Availability: IPSec/SSL. | Int32
> sess-ttlattempt | Description: Total number of session attempted. This variable is proprietary. Trigger: Increments upon receiving an IKE_INIT message from the UE in IPsec and a TCP SYN message in SSL TTG mode. Availability: IPSec/SSL. | Int32
> sess-ttlattemptfail | Description: Total number of session attempts failed. This variable is proprietary. Trigger: Increments upon session setup timout and authentication failure scenario or a resource unavailable scenario where the subscriber allocation fails. Availability: IPSec/SSL. | Int32
> sess-ttldisc | Description: Total number of sessions disconnected. Trigger: Increments after call is up during re-authentication failure (IPSec only) and the SSL or IPSec tunnel goes down. This variable is proprietary. | Int32
> sess-ttldisclocal | Description: Total number of sessions disconnected locally. This variable is proprietary. Trigger: Increments by unavailable resources and session setup timeout. Availability: IPSec/SSL. | Int32
> sess-ttldiscremote | Description: Total number of sessions disconnected remotely. This variable is proprietary. Trigger: Increments on UE-initiated call tear down after call setup. Availability: IPSec/SSL. | Int32
> sess-discbeforeconn | Description: Sessions remotely disconnected before connected. This variable is proprietary. Trigger: Increments on UE-initiated call tear down before call setup. Availability: IPSec/SSL. | Int32
> sess-ttlfastreauthsucc | Description: Total fast re-authentication successes. This variable is proprietary. Trigger: Increments upon re-authetication success scenario. Includes both fast re-authentication and pseudoname re-authentication. Availability: IPSec. | Int32
> sess-ttlfastreauthattempt | Description: Total fast re-authentication attempts. This variable is proprietary. Trigger: Increments upon receiving the re-auth ID in the IKE-AUTH message from the UE. Includes both fast re-authentication and pseudoname re-authentication. Availability: IPSec. | Int32
> sess-ttlfastreauthattemptfail | Description: Total fast re-authentication attempts that failed. This variable is proprietary. Trigger: Increments upon a re-authentication success scenario from the AAA server. Includes both fast re-authentication and pseudoname re-authentication. Availability: IPSec. | Int32
> sess-ttlreauthorizesucc | Description: Total reauthorization attempts that succeeded. This variable is proprietary. Trigger: Increments upon receiving an authorize success message from the AAA server. Availability: IPSec. | Int32
> sess-ttlreauthorizeattempt | Description: Total reauthorization attempts. This variable is proprietary. Trigger: Increments upon sending an authorize request message to the AAA server. Availability: IPSec. | Int32
> sess-ttlreauthorizeattemptfail | Description: Total reauthorization attempts that failed. This variable is proprietary. Trigger: Increments upon an authorization failure with the AAA server or if the IPsec tunnel goes down during authorization. Availability: IPSec. | Int32
> sess-ttlprimaryaaasucc | Description: Total primary AAA sessions that succeeded. This variable is proprietary. Trigger: Increments upon receiving an access accept message from the AAA server. (Increments only during primary authentication if multiple authentication is supported in IPSec). Availability: IPSec/SSL. | Int32
> sess-ttlprimaryaaaattempt | Description: Total primary AAA sessions attempted. This variable is proprietary. Trigger: Increments upon receiving an IKE -AUTH message from the UE in IPSec and an MT-AUTH message from the UE in SSL. Availability: IPSec/SSL. | Int32
> sess-ttlprimaryaaaattemptfail | Description: Total primary AAA sessions that failed. This variable is proprietary. Trigger: Increments on an authentication failure and if the SSL or IPSec tunnel goes down during authentication. Availability: IPSec/SSL. | Int32
> sess-ttlexternalaaasucc | Description: Total external AAA sessions that succeeded. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server in a multiple authentication scenario. Availability: IPSec. | Int32
> sess-ttlexternalaaaattempt | Description: Total external AAA sessions that attempted. This variable is proprietary. Trigger: Increments upon receiving an IKE-AUTH (ANOTHER-AUTH-FOLLOWS) message from the UE in a multiple authentication scenario. Availability: IPSec. | Int32
> sess-ttlexternalaaaattemptfail | Description: Total external AAA sessions that failed. This variable is proprietary. Trigger: Increments upon receiving an authentication failure from the AAA server or an IPsec tunnel tear down in a multiple authentication scenario. Availability: IPSec. | Int32
> sess-ttleapauthsucc | Description: Total of successful EAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server for the second phase authentication using EAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
> sess-ttleapauthfail | Description: Total of failed EAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication failure message from the AAA server for the second phase authentication using EAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
> sess-ttlpapauthsucc | Description: Total of successful PAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server for the second phase authentication using PAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
> sess-ttlpapauthfail | Description: Total of failed PAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication failure message from the AAA server for the second phase authentication using PAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
> sess-ttlchapauthsucc | Description: Total of successful CHAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server for the second phase authentication using CHAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
> sess-ttlchapauthfail | Description: Total of failed CHAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication failure message from the AAA server for the second phase authentication using CHAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
> sess-discipsec | Description: Number of sessions terminated because of IPsec. This variable is proprietary. Trigger: A UE-initiated session disconnect (applicable in both ISec and SSL). This variable contains all sessions disconnected by a remote disconnect. Availability: IPSec/SSL. | Int32
> sess-discadmin | Description: Number of sessions terminated because of admin release. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discidletimeout | Description: Number of sessions terminated because of idle timer timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discabstimeout | Description: Number of sessions terminated because of absolute timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-disclongdur | Description: Number of sessions terminated because of long duration timer timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discsesssetuptimeout | Description: Number of sessions terminated because of Session Manager session setup timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discnonexistpcrf | Description: Number of sessions terminated because of non-existence of PCRF. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discnoresource | Description: Number of sessions terminated because of no resources. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discauthfail | Description: Number of sessions terminated because of AAA authentication failure. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discflowaddfail | Description: Number of sessions terminated because of flow add failure. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discinvdestctx | Description: Number of sessions terminated because of invalid destination context. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discsourceviol | Description: Number of sessions terminated because of source IP address violation. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discgtp | Description: Number of sessions terminated because of GTP. This variable is proprietary. Trigger: Triggered by a GGSN-initiated teardown. Availability: IPSec/SSL (TTG only). | Int32
> sess-discdupreq | Description: Number of sessions terminated because of duplicate requests. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discaddrfail | Description: Number of sessions terminated because of an address assignment failure. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-discmisc | Description: Number of sessions terminated because of miscellaneous reasons. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-ttlbytessent | Description: Total number of bytes sent. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-ttlbytesrcvd | Description: Total number of bytes received. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-ttlpktsent | Description: Total number of packets sent. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-ttlpktrcvd | Description: Total number of packets received. This variable is proprietary. Availability: IPSec/SSL. | Int32
> sess-ttlpktviolations | Description: Total number of packet violations. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-rxttlsrvrpassthru | Description: Total number of EAP messages received from the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-rxsuccsrvrpassthru | Description: Total number of EAP-Success messages received from the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-rxfailsrvrpassthru | Description: Total number of EAP-Failure messages received from the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-rxchalsrvrpassthru | Description: Total number of EAP challenge messages sent to the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-txttlsrv | Description: Total number of EAP messages transmitted to the EAP server. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-txinitrequest | Description: Total number of EAP request messages forwarded to the EAP server for initial request. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-txreqfwd | Description: Total number of EAP messages transmitted to the EAP server for forward request. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-rxmobilepassthru | Description: Total number of EAP messages transmitted to the EAP server in pass-through mode for mobile node. This variable is proprietary. Availability: IPSec/SSL. | Int32
> eap-rxmobilediscarded | Description: Total number of EAP messages transmitted to the EAP server that were discarded. This variable is proprietary. Availability: IPSec/SSL. | Int32
> mt-txdatabyteuplink | Description: SSL micro-tunneling: Uplink data bytes sent. This variable is proprietary. Availability: SSL. | Int64
> mt-databyteuplinkdropped | Description: SSL micro-tunneling: Uplink data bytes dropped. This variable is proprietary. Availability: SSL. | Int64
> mt-uldroppedd-nonconnectedstate | Description: SSL micro-tunneling: Uplink data bytes dropped due to non-connected state. This variable is proprietary. Availability: SSL. | Int64
> mt-uldroppedd-transstackbuffoverflow | Description: SSL micro-tunneling: Uplink data bytes dropped due to transport stack buffer over flow. This variable is proprietary. Availability: SSL. | Int64
> mt-uldroppedd-incorrectdestip | Description: SSL micro-tunneling: Uplink data bytes dropped due to incorrect destination IP address. This variable is proprietary. Availability: SSL. | Int64
> mt-uldroppedd-transtackfailed | Description: SSL micro-tunneling: Uplink data bytes dropped due to transport stack failed to send. This variable is proprietary. Availability: SSL. | Int64
> mt-uldroppedd-sessnotfoundforsockid | Description: SSL micro-tunneling: Uplink data bytes dropped due to session not found for sock-id. This variable is proprietary. Availability: SSL. | Int64
> mt-txdatabytedownlink | Description: SSL micro-tunneling: Downlink data bytes sent. This variable is proprietary. Availability: SSL. | Int64
> mt-rxttlopenreq | Description: SSL micro-tunneling: Total OPEN requests received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxopenreqprocessed | Description: SSL micro-tunneling: OPEN requests processed. This variable is proprietary. Availability: SSL. | Int32
> mt-rxopenreqdropped | Description: SSL micro-tunneling: OPEN requests dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlopenresp | Description: SSL micro-tunneling: Total OPEN responses sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txopenrespaccept | Description: SSL micro-tunneling: OPEN responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-txopenresprej | Description: SSL micro-tunneling: OPEN responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxopenresp | Description: SSL micro-tunneling: OPEN responses received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlnamreq | Description: SSL micro-tunneling: Total NAM requests received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxnamreqprocessed | Description: SSL micro-tunneling: NAM requests processed. This variable is proprietary. Availability: SSL. | Int32
> mt-rxnamreqdropped | Description: SSL micro-tunneling: NAM requests dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlnamresp | Description: SSL micro-tunneling: Total NAM responses sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txnamrespaccept | Description: SSL micro-tunneling: NAM responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-txnamresprej | Description: SSL micro-tunneling: NAM responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxnamresp | Description: SSL micro-tunneling: NAM responses received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlauthreq | Description: SSL micro-tunneling: Total AUTH requests received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxauthreqprocessed | Description: SSL micro-tunneling: AUTH requests processed. This variable is proprietary. Availability: SSL. | Int32
> mt-rxauthreqdropped | Description: SSL micro-tunneling: AUTH requests dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlauthresp | Description: SSL micro-tunneling: Total AUTH responses sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txauthrespaccept | Description: SSL micro-tunneling: AUTH responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-txauthresprej | Description: SSL micro-tunneling: AUTH responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxauthresp | Description: SSL micro-tunneling: AUTH responses received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlrecvreq | Description: SSL micro-tunneling: Total RECV requests received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxrecvreqprocessed | Description: SSL micro-tunneling: RECV requests processed. This variable is proprietary. Availability: SSL. | Int32
> mt-rxrecvreqdropped | Description: SSL micro-tunneling: RECV requests dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlrecvresp | Description: SSL micro-tunneling: Total RECV responses sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txrecvrespaccept | Description: SSL micro-tunneling: RECV responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-txrecvresprej | Description: SSL micro-tunneling: RECV responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxrecvresp | Description: SSL micro-tunneling: RECV responses received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlclosereq | Description: SSL micro-tunneling: Total CLOSE requests received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxclosereqprocessed | Description: SSL micro-tunneling: CLOSE requests processed. This variable is proprietary. Availability: SSL. | Int32
> mt-rxclosereqdropped | Description: SSL micro-tunneling: CLOSE requests dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlclosereq | Description: SSL micro-tunneling: Total CLOSE requests sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txclosereqdispatch | Description: SSL micro-tunneling: CLOSE requests dispatched. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlcloseresp | Description: SSL micro-tunneling: Total CLOSE responses received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxcloserespaccept | Description: SSL micro-tunneling: CLOSE responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-rxcloseresprej | Description: SSL micro-tunneling: CLOSE responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxcloserespdropped | Description: SSL micro-tunneling: CLOSE responses dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlcloseresp | Description: SSL micro-tunneling: Total CLOSE responses sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txcloserespaccept | Description: SSL micro-tunneling: CLOSE responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-txcloseresprej | Description: SSL micro-tunneling: CLOSE responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlsendreq | Description: SSL micro-tunneling: Total SEND requests received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxsendreqprocessed | Description: SSL micro-tunneling: SEND requests processed. This variable is proprietary. Availability: SSL. | Int32
> mt-rxsendreqdropped | Description: SSL micro-tunneling: SEND requests dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlsendreq | Description: SSL micro-tunneling: Total SEND requests sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txsendreqdispatch | Description: SSL micro-tunneling: SEND requests dispatched. This variable is proprietary. Availability: SSL. | Int32
> mt-rxttlsendresp | Description: SSL micro-tunneling: Total SEND responses received. This variable is proprietary. Availability: SSL. | Int32
> mt-rxsendrespaccept | Description: SSL micro-tunneling: SEND responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-rxsendresprej | Description: SSL micro-tunneling: SEND responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-rxsendrespdropped | Description: SSL micro-tunneling: SEND responses dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-txttlsendresp | Description: SSL micro-tunneling: Total SEND responses sent. This variable is proprietary. Availability: SSL. | Int32
> mt-txsendrespaccept | Description: SSL micro-tunneling: SEND responses accepted. This variable is proprietary. Availability: SSL. | Int32
> mt-txsendresprej | Description: SSL micro-tunneling: SEND responses rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-cannotcreatconn | Description: SSL micro-tunneling: OPEN Reject sent: cannot create connection. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-protonotsupported | Description: SSL micro-tunneling: OPEN Reject sent: protocol not supported. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-permdenied | Description: SSL micro-tunneling: OPEN Reject sent: permission denied. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-cannotcreatesockid | Description: SSL micro-tunneling: OPEN Reject sent: cannot create sock-id. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-badparam | Description: SSL micro-tunneling: OPEN Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-addrport-alreadyused | Description: SSL micro-tunneling: OPEN Reject sent: address or port already used. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-cannotconnectserver | Description: SSL micro-tunneling: OPEN Reject sent: cannot connect the server. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-hostnameunknown | Description: SSL micro-tunneling: OPEN Reject sent: hostname is unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-authrequired | Description: SSL micro-tunneling: OPEN Reject sent: authentication required. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-undefined | Description: SSL micro-tunneling: OPEN Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-openrejtx-reserved | Description: SSL micro-tunneling: OPEN Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-namrejtx-versionnotsupported | Description: SSL micro-tunneling: OPEN Reject sent: version not supported. This variable is proprietary. Availability: SSL. | Int32
> mt-namrejtx-servercannotcreateauth | Description: SSL micro-tunneling: OPEN Reject sent: server cannot create an authentication process. This variable is proprietary. Availability: SSL. | Int32
> mt-namrejtx-badparameters | Description: SSL micro-tunneling: OPEN Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-namrejtx-undefined | Description: SSL micro-tunneling: NAM Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-namrejtx-reserved | Description: SSL micro-tunneling: NAM Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-authrejtx-authidunknown | Description: SSL micro-tunneling: AUTH Reject sent: the auth-id is unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-authrejtx-cannotconntoauthserver | Description: SSL micro-tunneling: AUTH Reject sent: cannot connect to authentication server. This variable is proprietary. Availability: SSL. | Int32
> mt-authrejtx-badparam | Description: SSL micro-tunneling: AUTH Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-authrejtx-undefined | Description: SSL micro-tunneling: AUTH Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-authrejtx-reserved | Description: SSL micro-tunneling: AUTH Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-recvrejtx-sockidunknown | Description: SSL micro-tunneling: RECV Reject sent: the sock-id is unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-recvrejtx-connlost | Description: SSL micro-tunneling: RECV Reject sent: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
> mt-recvrejtx-permissiondenied | Description: SSL micro-tunneling: RECV Reject sent: permission denied. This variable is proprietary. Availability: SSL. | Int32
> mt-recvrejtx-badparameters | Description: SSL micro-tunneling: RECV Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-recvrejtx-undefined | Description: SSL micro-tunneling: RECV Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-recvrejtx-unreserved | Description: SSL micro-tunneling: RECV Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejtx-sockidunknown | Description: SSL micro-tunneling: RECV Reject sent: the sock-id is unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejtx-connlost | Description: SSL micro-tunneling: CLOSE Reject sent: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejtx-badparameters | Description: SSL micro-tunneling: CLOSE Reject sent: the bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejtx-undefined | Description: SSL micro-tunneling: CLOSE Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejtx-unreserved | Description: SSL micro-tunneling: CLOSE Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejrx-sockidunknown | Description: SSL micro-tunneling: CLOSE Reject received: sock-id unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejrx-connlost | Description: SSL micro-tunneling: CLOSE Reject received: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejrx-badparameters | Description: SSL micro-tunneling: CLOSE Reject received: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejrx-undefined | Description: SSL micro-tunneling: CLOSE Reject received: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-closerejrx-unreserved | Description: SSL micro-tunneling: CLOSE Reject received: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejtx-sockidunknown | Description: SSL micro-tunneling: SEND Reject sent: sock-id unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejtx-connlost | Description: SSL micro-tunneling: SEND Reject sent: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejtx-permissiondenied | Description: SSL micro-tunneling: SEND Reject sent: permission denied. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejtx-badparam | Description: SSL micro-tunneling: SEND Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejtx-undefined | Description: SSL micro-tunneling: SEND Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejtx-reserved | Description: SSL micro-tunneling: SEND Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejrx-sockidunknown | Description: SSL micro-tunneling: SEND Reject received: sock-id unknown. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejrx-connlost | Description: SSL micro-tunneling: SEND Reject received: connection is lost. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejrx-permissiondenied | Description: SSL micro-tunneling: SEND Reject received: permission denied. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejrx-badparam | Description: SSL micro-tunneling: SEND Reject received: bad parameters. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejrx-undefined | Description: SSL micro-tunneling: SEND Reject received: undefined. This variable is proprietary. Availability: SSL. | Int32
> mt-sendrejrx-reserved | Description: SSL micro-tunneling: SEND Reject received: reserved. This variable is proprietary. Availability: SSL. | Int32
> mt-pktdiscardstat-unknownversion | Description: SSL micro-tunneling: Packets discarded statistics: unknown version. This variable is proprietary. Availability: SSL. | Int32
> mt-pktdiscardstat-unknownmsgtype | Description: SSL micro-tunneling: Packets discarded statistics: unknown message type. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-open-decodefaildropped | Description: SSL micro-tunneling: Packets discarded statistics: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-open-decodefailrej | Description: SSL micro-tunneling: Packets discarded statistics: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-open-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: OPEN: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-open-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: OPEN: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respopen-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP OPEN: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respopen-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP OPEN: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-close-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-close-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-close-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-close-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respclose-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP CLOSE: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respclose-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP CLOSE: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-nam-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: NAM: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-nam-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: NAM: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-nam-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: NAM: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-nam-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: NAM: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respnam-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP NAM: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respnam-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP NAM: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-auth-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: AUTH: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-auth-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: AUTH: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-auth-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: AUTH: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-auth-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: AUTH: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respauth-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP AUTH: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respauth-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP AUTH: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-recv-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RECV: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-recv-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: RECV: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-recv-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RECV: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-recv-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: RECV: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-resprecv-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP RECV: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-resprecv-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP RECV: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-send-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: SEND: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-send-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: SEND: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-send-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: SEND: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-send-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: SEND: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respsend-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP SEND: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respsend-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP SEND: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
> mt-msgdenied-respunknowncommdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP to unknown command dropped. This variable is proprietary. Availability: SSL. | Int32
> Important: See the “Bulk Statistics Overview” chapter for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883