> SCCP Network Configuration Mode Commands
> The SCCP Network Configuration Mode is used to configure properties for Signaling Connection Control Part (SCCP) services for SS7.
> In this mode, the command prompt should be similar to:
> [local]hostname(config-sccp-network-<sccp_id>)#
> Signaling Connection Control Part (SCCP) is a routing protocol in the SS7 protocol suite in layer 4, which provides end-to-end routing for TCAP messages to their proper database.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> associate
> Associates an SS7 routing domain with the SCCP network.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> associate ss7-routing-domain rd_id
> no associate
> no
> Removes the association with the SS7 routing domain from the system configuration.
> rd_id
> This number identifies an already defined SS7 routing domain.
> rd_id: enter an integer from 1 through 12.
> Usage
> Use this command to associate SS7 routing domain configurations with SCCP network configurations.
> Example
> The following command associates the SCCP network with SS7 routing domain 2:
> associate ss7-routing-domain 2
> description
> This command defines a string that describes the SCCP network. The description is used for operator reference.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> description string
> no description
> string
> This is a string to describe the SCCP network.
> string must be an alphanumeric string from 1 through 127 characters in length. If there are spaces in the string the string must be enclosed in double-quotes. For example; “This is a Description”.
> no
> Removes the description from the system configuration.
> Usage
> Use this command to configure a description of this SCCP service for operator reference.
> Example
> The following command sets the description to “This is the SCCP Service Number 1”:
> description ”This is the SCCP Service Number 1.”
> destination
> This command configures the SCCP network destination information. Use this command multiple times to set all of the destination information required.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> destination dpc pt_code { name route_name | next-hop pt_code [ priority priority ] | ssn subsys_num | version sccp_ver }
> no destination dpc p_code [ name route_name | ssn ssn_num | version sccp_ver ]
> no
> Deletes the specified destination information from the SCCP network configuration.
> dpc pt_code
> Specifies the SCCP destination point code.
> pt_code: Must be in SS7 point code dotted-decimal ###.###.### format or decimal ######## format.
> name route_name
> The name of the SCCP destination route.
> route_name: enter an alphanumeric string from 1 through 64 characters in length.
> next-hop pt_code [ priority priority
> Associates the next destination defined in the SS7 routing domain and assigns the next-hop a priority for use.
> pt_code: Must be in SS7 point code dotted-decimal ###.###.### format or decimal ######## format.
> priority: Must be an integer from 0 to 15, with 0 setting the highest priority.
> ssn subsys_num
> The destination subsystem number.
> subsys_num: enter an integer from 1 through 255.
> version sccp_ver
> sccp_ver: enter one of the following to select the SCCP variant:

> • | ANSI88

> • | ANSI92

> • | ANSI96

> • | BELL05

> • | CHINA

> • | GSM0806

> • | ITU88

> • | ITU92

> • | ITU96

> Usage
> Use this command to configure the destination information for the SCCP network.
> Example
> The following commands set the name of the destination route to default_route, the subsystem number to 1, and the variant version to ITU96, all with a destination point code of 1:
> destination dpc 1 name default_routedestination dpc 1 ssn 1destination dpc version ITU96
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> SGSN , HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the global configuration mode.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the global configuration mode.
> global-title-translation
> This command associates a GTT address-map with this SCCP network.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> global-title-translation address-map instance instance
> no global-title-translation address-map instance instance
> no
> Deletes the GTT address-map instance associated with this SCCP network.
> instance
> This value uniquely identifies a specific previously defined instance of a GTT address-map.
> instance: enter an integer from 1 to 4096.
> Usage
> Use this command to link a GTT address-map, configured with the GTT Address Map configuration mode, to a specific SCCP network configuration.
> Example
> global-title-translation address-map instance gtt-map1
> hop-count
> This command specifies the hop count for this SCCP network.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> hop-count hop_cnt
> default hop-count
> default
> Resets the hop-count value to the system default of 5.
> hop_cnt
> The hop count to assign to this SCCP network.
> hop_cnt: enter an integer from 1 to 15.
> Usage
> Use this command to define the hop count for this SCCP network.
> Example
> The following command sets the hop count to 3:
> hop-count 3
> self-point-code
> This command specifies the SS7 point code for this SCCP service.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> self-point-code point_code
> no self-point-code
> no
> Deletes the configured self point code.
> point_code
> Defines the point code to assign to this SCCP network service.
> point_code: value entered must adhere to the point code variant selected when the SCCP network instance was defined:

> • | ITU Range 0.0.1 to 7.255.7

> • | ANSI Range 0.0.1 to 255.255.255

> • | TTC Range 0.0.1 to 15.31.255

> • | a string of 1 to 11 combined digits ad period.

> Usage
> Use this command to assign the self point code to use for this SCCP service.
> Example
> The following command sets an ITU-based point code for this SCCP service:
> self-pointcode 4.121.5
> The following command removes the configured self-point code:
> no self-pointcode
> timeout
> This command configures the timeout parameters for this SCCP network.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> timeout { attack-timer | congestion-timer | conn-est-timer | crd-timer | decay-timer | iar-timer | ias-timer | interval-timer | reassembly-timer | release-timer | repeat-release-timer | reset-timer | sst-timer } +
> default timeout
> no timeout timer
> attack-timer time
> Defines the time before the attack timer expires.
> time: enter an integer between 1 and 10.
> congestion-timer time
> Defines the time before the congestion timer expires.
> time: enter an integer between 1 and 10.
> conn-est-timer time
> Defines the time before the connection timer expires.
> time: enter an integer between 6 and 12.
> crd-timer time
> Defines the time before the coordinated-state-change timer expires.
> time: enter an integer between 60 and 120.
> decay-timer time
> Defines the time before the decay timer expires.
> time: enter an integer between 1 and 10.
> iar-timer time
> Defines the time before the inactivity-receive timer expires.
> time: enter an integer between 60 and 120.
> ias-timer time
> Defines the time before the inactivity-send timer expires.
> time: enter an integer between 30 and 60.
> interval-timer time
> Defines the time before the interval timer expires.
> time: enter an integer between 6 and 12
> reassembly-timer time
> Defines the time before the reassembly-timer expires.
> time: enter an integer between 10 and 20.
> release-timer time
> Defines the time before the release-assembly timer expires.
> time: enter an integer between 1 and 2.
> repeat-release-timer time
> Defines the time before repeat-release timer expires.
> time: enter an integer between 1 and 2
> reset-timer time
> Defines the amount of time before the reset timer expires.
> time: enter an integer between 1 and 2
> sst-timer time
> Defines the amount of time before the subsystem status test timer expires.
> time: enter an integer between 5 and 1200.
> default
> Resets the timeout parameter to the system default.
> no
> Deletes the specified timer configuration.
> Usage
> Use this command to assign timeout timers and timeout values for this SCCP service.
> Example
> timeout reset-timer 75

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883