> show hardware card
> show hardware card Command Output Descriptions

> Field | Applicable Card(s) | Description
> Card Type | All | The type of card installed.
> Card Description | All | Displays the description assigned to the card during software configuration.
> Part Number | All | The card’s part number. Cards of the same type and revision will have the same part number.
> Serial Number | All | The card’s serial number.
> Switch Fabric Modes | SMC, Processing Cards | Which Switch Fabric modes the card can do. Possible values are:
> • | control plane
> • | switch fabric
> MAC Addresses | SMC, SPIO, and line cards | The media access control addresses supported by the interfaces on the cards.
> Card Programmables | All | This field indicates if the software on any of the programmable components on the card is not at the current revision.
> • | If all software is current, Up To Date is displayed.
> • | If one or more components do not have the most current software, Out of Date is displayed, along with the component(s) requiring the newer code.
> • | If one or more components have experimental or unreleased software, Experimental/Unreleased is displayed.
> NPU Microcode | Processing Cards | The version of the software running (currently operational) on the Network Processing Unit (NPU).
> Slave SCB | Processing Cards, SPIO, RCC, and line cards | The firmware version of the component that allows non-SMC cards to communicate with the SMC over the system control bus (SCB). on-card: Indicates the version of the firmware that is on the boot flash for the component.
> SRM | SMC | The firmware version of the Status, Reset, and Monitoring component.
> CIF FPGA | SMC | The firmware version of the Chassis Information (CIF) Field Programmable Gate Array (FPGA).
> • | on-card: Indicates the version of the firmware that is on the boot flash for the component.
> • | running: The firmware version that is currently operational.
> PSR | Processing Cards | The firmware version of the Power, Status, and Reset component.
> BIOS | Processing Cards, SMC | The version of the Basic Input/Output System (BIOS). on-card indicates the version of the firmware that on the boot flash for the component.
> DT FPGA | Processing Cards | The firmware version of the Data Transport (DT) Field Programmable Gate Array (FPGA).
> • | on-card: Indicates the version of the firmware that is on the boot flash for the component.
> • | running: The firmware version that is currently operational.
> FPGA | SPIO and line cards | The Field Programmable Gate Arrays that allow the SPIOs and other line cards to communicate with the SMC and Processing Cards respectively. on-card: Indicates the version of the firmware that is on the boot flash for the component.
> CPU 0 through 3 Type / Memory | Processing Cards and SMC | The CPU’s pass (revision), speed and memory. The SMC only indicates CPU 0 because it has only one CPU. The Processing Cards display CPUs 0 and 1 because each card has two CPUs.
> CPU 0 through 3 CFE / Diags | Processing Cards and SMC | The CPU’s Common Firmware Environment (CFU) and diagnostic software version.
> • | on-card: Indicates the version of the firmware that is on the boot flash for the component.
> • | running: The firmware version that is currently operational.
> The SMC only indicates CPU 0 because it has only one CPU. The Processing Cards display CPUs 0 and 1 because each card has two CPUs.
> SFP Info | SPIO and Ethernet 1000 line cards and Quad Gig-E line card, 10 Gig Ethernet line card | Indicates information pertaining to the small form-factor pluggable (SFP) modules installed on the card. Among the information provided is the Manufacturer name, ID number, the module part and serial numbers, and the production date.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883