> show sgtp
> This chapter describes the outputs of the show sgtp command.
> show sgtp-service ggsn-table
> show sgtp-service ggsn-table Command Output Descriptions

> Field | Description
> GTP | Indicates the GTP version. Possible values are:
> • | 0: GTP-v0
> • | 1: GTP-v1
> Status | Indicates the status of the GTP session. Possible values are:
> • | I: Inactive
> • | A: Active
> GTPC Echo | Indicates the status of the GTPC echo. Possible values are:
> • | D: Disabled
> • | E: Enabled
> PLMN Type | Indicates the type of Public Land Mobile Network area. Possible values are:
> • | H: Home networks
> • | F: Foreign networks
> • | U: Unknown networks
> SGTPC Stats | Indicates the availability of the SGTPC statistics. Possible values are:
> • | A: Available
> • | U: Unavailable
> Service ID | Indicates the SGTP service identifier.
> GGSN Address | Indicates the IP address of GGSN service.
> Restart Counter | Indicates the restart counter of SGTP service.
> No. of restart | Indicates the total number of restarts happened for SGTP session.
> Curr sessions | Total number of SGTP session currently running.
> Max sessions | Indicates the maximum number of SGTP session allowed.

> ‌
> show sgtp-service sgsn-table
> show sgtp-service sgsn-table Command Output Descriptions

> Field | Description
> GTP | Indicates the GTP version. Possible values are:
> • | 0: GTP-v0
> • | 1: GTP-v1
> GTPC Echo | Indicates the status of the GTPC echo. Possible values are:
> • | D: Disabled
> • | E: Enabled
> PLMN Type | Indicates the type of Public Land Mobile Network area. Possible values are:
> • | H: Home networks
> • | F: Foreign networks
> • | U: Unknown networks
> SGTPC Stats | Indicates the availability of the SGTPC statistics. Possible values are:
> • | A: Available
> • | U: Unavailable
> Service ID | Indicates the SGTP service identifier.
> SGSN Address | Indicates the IP address of SGGSN service.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883