> show pdif-service
> This chapter describes the output of the show pdif-service command.
> show pdif-service statistics
> show pdif-service statistics Command Output Descriptions

> Field | Description
> Session Statistics
> Current sessions total | Total number of current sessions.
> Simple-IPv4 current | Number of current Simple-IPv4 sessions.
> Mobile-IPv4 current | Number of current Mobile-IPv4 sessions.
> Proxy-Mobile-IPv4 current | Number of current Proxy-Mobile-IPv4 sessions.
> Data-Clients | Total number of subscriber sessions originating from data clients.
> Active current | Total number of currently active sessions.
> Dormant current | Total number of currently dormant sessions.
> Active IPv4 current | Total number of currently active IPv4 sessions.
> Active IPv6 current | Total number of currently active IPv6 sessions.
> Dormant IPv4 current | Total number of currently dormant IPv4 sessions.
> Dormant IPv6 current | Total number of currently dormant IPv6 sessions.
> Total Simple-IP IPv4 | Total number of Simple-IP IPv4 sessions.
> Total Mobile-IP IPv4 | Total number of Mobile-IP IPv4 sessions.
> Total Proxy-Mobile-IP IPv4 | Total number of Proxy-Mobile-IP IPv4 sessions.
> Mobile-IP IPv4 attempts | Total number of Mobile-IP IPv4 session attempts.
> Mobile-IP IPv4 successes | Number of successful Mobile-IP IPv4 session attempts.
> Mobile-IP IPv4 failures | Number of failed Mobile-IP IPv4 session attempts.
> Proxy-Mobile-IP IPv4 attempts | Total number of Proxy-Mobile-IP IPv4 session attempts.
> Proxy-Mobile-IP IPv4 succ | Number of successful Proxy-Mobile-IP IPv4 session attempts.
> Proxy-Mobile-IP IPv4 fails | Number of failed Proxy-Mobile-IP IPv4 session attempts.
> Simple-IP-Fallback attempts | Total number of Simple-IP fallback attempts.
> successes | Number of successful Simple-IP fallback sessions.
> failures | Number of failed Simple-IP fallback sessions.
> Simple-IP-Fallback Failure Reasons
> No Mobile-IP RRQ Rx | Mobile-IP RRQ request not received.
> Not allowed | Simple-IP fallback not allowed by configuration.
> Tagged Pool Address | Address is in a pool and tagged not to allow Simple-IP fallback.
> Misc
> Simple-IP IPv4 attempts | Total number of Simple-IP IPv4 session attempts.
> Simple-IP IPv4 successes | Number of successful Simple-IP IPv4 attempts.
> Simple-IP IPv4 failures | Number of failed Simple-IP IPv4 attempts.
> Total setup attempts | Total number of session setup attempts.
> Total setup success | Number of successful session setup attempts.
> Total Attempts Failed | Number of failed session setup attempts.
> Total disconnected | Total number of disconnected sessions.
> Disconnected locally | Number of sessions disconnected locally.
> Disconnected remotely | Number of sessions disconnected remotely.
> Disconnect remotely before connect | Number of sessions disconnected remotely before the session was fully connected.
> Session Disconnect Reasons
> Remote disconnect ipsec | Number of sessions disconnected because of remote party (mobile) hang-up.
> Admin disconnect | Number of sessions disconnected by the Admin.
> Idle timeout | Number of sessions disconnected because the Idle timer has timed out.
> Absolute timeout | Number of sessions disconnected because the Absolute timer has timed out.
> Long duration timeout | Number of sessions disconnected because the Long Duration timer has timed out.
> Session setup timeout | Number of sessions disconnected because the Session Setup timer has timed out.
> No resource | Number of sessions disconnected because the system has run out of resources (flows, memory, etc.).
> Auth failure | Number of sessions disconnected because of an authentication failure.
> Flow add failure | Number of sessions disconnected because flow could not be added on NPU.
> Invalid dest-context | Number of sessions disconnected because the destination context coming from AAA server is invalid.
> Source address violation | Number of sessions disconnected because the source IP address is invalid.
> MIP Remote | Number of Mobile-IP sessions disconnected because of remote mobile user hang-up.
> MIP Local | Number of Mobile-IP sessions disconnected locally.
> Duplicate Request | Number of sessions disconnected because of a duplicate request when there is already a session with the same NAI.
> MAC validation failure | Number of sessions disconnected because the HSS cannot validate MAC address from remote user.
> Addr assign failure | Number of sessions disconnected because no address has been assigned.
> Miscellaneous reasons | Number of Mobile-IP sessions disconnected for other reasons.
> MAC Address Validation Statistics
> Validation attempted | Total number of MAC address validation attempts.
> Validation succeeded | Number of successful MAC address validation attempts.
> Validation failed | Number of failed MAC address validation attempts.
> MAC Address Validation Successes
> MAC Address matches | Number of successful HSS server MAC address matches.
> HSS failure continued | HSS is configured to continue the session after a failure is registered.
> MAC Address Validation Failure Reasons
> Diameter Error | Validation failed because of a problem with the Diameter server.
> User Unknown | Validation failed because of an unknown user.
> Malformed MAC Address | Validation failed because of a malformed MAC address from the mobile subscriber.
> No MAC Address provided | Validation failed because the mobile subscriber does not supply a MAC address.
> Unauthorized MAC Address | Validation failed because the MAC address is not authorized by the HSS.
> Sh Interface unavailable | Validation failed because of a problem with the interface to the HSS.
> Others | Validation failed because of other reasons.
> Data Stats
> Total Bytes Sent | Total number of bytes sent.
> Total Packets Sent | Total number of packets sent.
> Total Bytes Rcvd | Total number of bytes received.
> Total Packets Rcvd | Total number of packets received.
> Total Pkts Violations | Total number of packets received from UEs and destined for the Internet that do not match any of the configured traffic selectors.
> EAP Server Statistics
> Total Received | Total number of EAP Success+ EAP Challenge + EAP Failures, coming from EAP server.
> Success Received | Number of EAP successes received.
> Challenge Received | Number of EAP challenges received.
> Failures Received | Number of EAP failures received.
> Discarded | Number of EAP server messages discarded.
> Total Sent | Total number of EAP server messages sent.
> Initial Requests | Number of initial requests.
> Requests Forwarded | Number of requests forwarded.
> EAP Mobile Statistics
> Total Received | Total number of EAP Requests coming from mobile subscriber.
> Discarded | Number of EAP mobile messages discarded.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883