> Local Policy Actiondef Configuration Mode Commands
> The Local Policy Actiondef Configuration Mode is used to configure the action definitions to be used for local QoS policies.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> action
> This command configures the action priority for an actiondef.
> Product
> P-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> action priority priority action_name arguments
> no action priority priority
> priority priority
> Specifies a priority for the specified action.
> priority must be unique and an integer from 1 to 2048.
> action_name arguments
> The following actions are supported. arguments specifies a set of parameters to be used when invoking the action.

> • | activate-ambr uplink bandwidth downlink bandwidth

> Sets the AMBR for the APN.
> Configure uplink and downlink bandwidth. bandwidth must be an integer from 1 to 1000000000.

> • | activate-flow-detection { initiation | termination } ruledef ruledef_name

> Detects a flow and takes action.
> initiation ruledef: Checks for flow initiation and adds a rule definition.
> termination ruledef: Checks for flow termination and adds a rule definition.
> ruledef_name must be an existing ruledef.

> • | activate-policy-group

> Not supported in this release.

> • | activate-rule name rule_name

> Activates a rule within ECS rulebase for a subscriber.
> rule_name must be an existing rule within this local QoS policy service.

> • | activate-rulebase name rulebase_name

> Associates the session with a specific rulebase.
> rulebase_name must be an existing rulebase within this local QoS policy service.

> • | allow-requested-qos

> Allow a specific UE initiated QoS request.

> • | allow-session

> Allows the session to continue.

> • | create-bearer qci value arp value uplink-mbr mbr_rate downlink-mbr mbr_rate [ uplink-gbr gbr_rate ] downlink-gbr gbr_rate

> Creates a bearer with a specific QCI and BANDWIDTH.
> qci value must be an integer from 1 to 254.
> arp value must be an integer from 1 to 15.
> uplink-mbr: Uplink maximum bitrate. mbr_rate must be an integer from 1 to 1000000000.
> downlink-mbr: Downlink maximum bitrate. mbr_rate must be an integer from 1 to 1000000000.
> uplink-gbr: Uplink guaranteed bitrate. gbr_rate must be an integer from 1 to 1000000000.
> downlink-gbr: Downlink guaranteed bitrate. gbr_rate must be an integer from 1 to 1000000000.

> • | deactivate-ambr

> Removes AMBR control for the specific session.

> • | deactivate-flow-detection { initiation | termination } ruledef ruledef_name

> Deactivates detection of flow and takes action.
> initiation ruledef: Checks for flow initiation and adds a rule definition.
> termination ruledef: Checks for flow termination and adds a rule definition.
> ruledef_name must be an existing ruledef.

> • | deactivate-policy-group

> Not supported in this release.

> • | deactivate-rule name rule_name

> Deactivates a rule within ECS.
> rule_name must be an existing rule within this local QoS policy service.

> • | deactivate-rulebase name rulebase_name

> Disassociates the rulebase from a session.
> rulebase_name must be an existing rulebase within this local QoS policy service.

> • | default-qos qci value arp value

> Sets the default QoS parameters for the session
> qci value must be an integer from 1 to 254.
> arp value must be an integer from 1 to 15.

> • | reject-requested-qos

> Rejects the requested QoS.

> • | delete-bearer qci value arp value

> Delete a bearer
> qci value must be an integer from 1 to 254.
> arp value must be an integer from 1 to 15.

> • | reject-requested-qos

> Reject UE QoS resource request.

> • | terminate-session

> Terminates the session.
> no action priority priority
> Deletes the specified action.
> Usage
> Use this command to enable the setting of parameters to be used when invoking actions. Actions are a series of operations that are triggered by activated rules.
> This command can be entered multiple times to configure multiple actions for an actiondef. The actions are examined in priority order until a match is found and the corresponding action is applied.
> Example
> The following command creates an action to allow a session to continue with priority set to 125:
> action priority 125 allow-session
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883