> eGTP Service Configuration Mode Commands
> The eGTP Service Configuration Mode is used to create and manage eGTP interface types and associated parameters.
> associate
> Configures an association with a GTP-U service where parameters are applied to the GTP-U data flow.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> associate gtpu-service name
> no associate gtpu-service
> no
> Removes the association to the configured GTP-U service from this service.
> gtpu-service name
> Associates a GTP-U service with this eGTP service. name must be from 1 to 63 alpha and/or numeric characters.
> Usage
> Use this command to associate a GTP-U service with this eGTP service.
> Example
> The following command associates this eGTP service with a GTP-U service named gtpu3:
> associate gtpu-service gtpu3
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> gtpc
> Configure the GPRS Tunneling Protocol Control (GTP-C) plane settings for this service.
> Product
> MME, P-GW, S-GW
> Privilege
> Administrator
> Syntax
> gtpc { bind { ipv4-address ipv4_address [ ipv6-address ipv6_address ] | ipv6-address ipv6_address [ ipv4-address ipv4_address ] } | echo-interval seconds | ip qos-dscp { forwarding_type } | max-retransmissions num | retransmission-timeout seconds }
> no gtpc { bind { ipv4-address ipv4_address [ ipv6-address ipv6_address ] | ipv6-address ipv6_address [ ipv4-address ipv4_address ] } | echo-interval }
> default gtpc { echo-interval | ip qos-dscp | max-retransmissions | retransmission-timeout }
> no
> Disables or removes the configured GTP-C setting.
> default
> Resets the specified parameter to its default value.
> bind { ipv4-address ipv4_address [ ipv6-address ipv6_address ] | ipv6-address ipv6_address [ ipv4-address iv4p_address ] }
> Binds the service to an interface with an IPv4 address, IPv6 address or both.
> ipv4-address ipv4_address [ ipv6-address ipv6_address ]: Binds this service to the IPv4 address of a configured interface. Optionally, bind the service to a configured interface with an IPv6 address. ipv4_address must be entered as a standard IPv4 address in dotted decimal notation. ipv6_address must be entered as a standard IPv6 address in colon-separated notation.
> ipv6-address ipv6_address [ ipv4-address ipv4_address ]: Binds this service to the IPv6 address of a configured interface. Optionally, bind the service to a configured interface with an IPv4 address. ip6_address must be entered as a standard IPv6 address in colon-separated notation. ipv4_address must be entered as a standard IPv4 address in dotted decimal notation.
> echo-interval seconds
> Default: 60
> Configures the duration between the sending of echo messages. seconds must be an integer value from 60 to 3600.
> ip qos-dscp { forwarding_type }
> Default: af11
> Specifies the IP QoS DSCP per-hop behavior to be marked on the outer header of signalling packets originating from the LTE component. This is a standards-based feature (RFC 2597). The following forwarding types are supported:
> af11: Designates the use of Assured Forwarding 11 per-hop behavior
> af12: Designates the use of Assured Forwarding 12 per-hop behavior
> af13: Designates the use of Assured Forwarding 13 per-hop behavior
> af21: Designates the use of Assured Forwarding 21 per-hop behavior
> af22: Designates the use of Assured Forwarding 22 per-hop behavior
> af23: Designates the use of Assured Forwarding 23 per-hop behavior
> af31: Designates the use of Assured Forwarding 31 per-hop behavior
> af32: Designates the use of Assured Forwarding 32 per-hop behavior
> af33: Designates the use of Assured Forwarding 33 per-hop behavior
> af41: Designates the use of Assured Forwarding 41 per-hop behavior
> af42: Designates the use of Assured Forwarding 42 per-hop behavior
> af43: Designates the use of Assured Forwarding 43 per-hop behavior
> be: Designates the use of Best Effort forwarding per-hop behavior
> ef: Designates the use of Expedited Forwarding per-hop behavior typically dedicated to low-loss, low-latency traffic.
> The assured forwarding behavior groups are listed in the table below.

> | Class 1 | Class 2 | Class 3 | Class 4
> Low Drop | AF11 | AF21 | AF31 | AF41
> Medium Drop | AF12 | AF22 | AF32 | AF42
> High Drop | AF13 | AF23 | AF33 | AF43

> ‌
> Traffic marked with a higher class is given priority during congestion periods. If congestion occurs to traffic with the same class, the packets with the higher AF value are dropped first.
> max-retransmissions num
> Default: 4
> Configures the maximum number of retries for packets. num must be an integer from 0 through 15.
> retransmission-timeout seconds
> Default: 5
> Configures the control packet (echo message) retransmission timeout in GTP, in seconds. seconds must be an integer value from 1 through 20.
> Usage
> Use this command to configure GTP-C settings for the current service. This interface assumes the characteristics of an S11 reference point on the S-GW or MME.
> Example
> The following command binds the service to a GTP-C interface with an IP address of 112.334.556.778:
> gtpc bind address 112.334.556.778
> interface-type
> Configures the interface type used by this service.
> Product
> MME, P-GW, S-GW
> Privilege
> Administrator
> Syntax
> interface-type { interface-mme | interface-pgw-ingress | interface-sgsn | interface-sgw-egress | interface-sgw-ingress }
> { interface-mme | interface-pgw-ingress | interface-sgsn | interface-sgw-egress | interface-sgw-ingress }
> interface-mme: Specifies that the interface has the characteristics of an eGTP MME S11 reference point to/from an S-GW or an eGTP MME Sv reference point to/from a Mobile Switching Center (MSC).
> interface-pgw-ingress: Specifies that the interface has the characteristics of an eGTP P-GW S5/S8 reference point from an S-GW. The interface assumes the characteristics of either a GTP-C (control Plane) or GTP-U (user plane) reference point.
> interface-sgsn: Specifies that the interface has the characteristics of an eGTP S-GW S4 reference point to/from an SGSN.
> interface-sgw-egress: Specifies that the interface has the characteristics of an eGTP S-GW S5/S8 reference point to an eGTP P-GW. The interface assumes the characteristics of either a GTP-C (control Plane) or GTP-U (user plane) reference point.
> interface-sgw-ingress: Specifies that the interface has the characteristics of:

> • | an eGTP-C S-GW S11 reference point from the MME.

> • | an eGTP-U S-GW S1-U reference point from the eNodeB.

> Usage
> Use this command to specify the type of interface this service uses. By configuring this command, the interface takes on the characteristics of the selected type.
> Example
> The following command configures the interface bound to this service to maintain the characteristics of an eGTP-C S-GW S11 reference point from an MME:
> interface-type interface-sgw-ingress
> validation-mode
> Configures the type of validation to be performed on messages received by this service.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> validation-mode { custom1 | standard }
> default validation-mode
> default
> Returns the command to the default setting of standard.
> { custom1 | standard }
> custom1: Specifies that the message should be validated based on a vendor-specific set of mandatory elements.
> standard: Specifies that the message should be validated based on the set of mandatory elements as defined in 3GPP 29.274.
> Usage
> Use this command to specify the type of validation performed on messages received by this service. The information elements contained in messages have mandatory elements and conditional elements. The standard set of elements, as defined by 3GPP 29.274 is checked if this command is set to “standard”. The custom1 setting is for a vendor-specific set of mandatory elements.
> Example
> The flowering command sets the validation mode for incoming messages to standard:
> validation-mode standard

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883