> GT-Format1 Configuration Mode Commands
> The GT-Format1 configuration mode is a sub-mode for either the Global Title Translation Association configuration mode or the Global Title Translation Address-Map configuration mode. This sub-mode configures a set of rules used in the global title translation (GTT) process.
> Upon accessing this mode, your prompt should look similar to the following:
> [local]<hostname>(config-gtt-1-format1)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> nature-of-address
> Configures the indicator to identify the nature of the address.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> nature-of-address { international | national | subscriber )
> international
> Identifies the numbers as international.
> national
> Identifies the numbers as matching the national configuration.
> subscriber
> Identifies the numbers as subscriber numbers.
> Usage
> Configure the identify of the GT format as national.
> Example
> nature-or-address national
> odd-even-indicator
> Configures the bits for matching the global title translation.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> odd-even-indicator type
> type

> • | odd: Sets the odd bit for matching the GTT.

> • | even: Sets the even bit for matching the GTT.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883