> GTPP Schema Statistics
> The GTPP schema provides operational statistics that can be used for monitoring and troubleshooting the following products: GGSN, P-GW, SGSN
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the GTPP Schema

> Variables | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the GTPP configuration. This is a key variable. Type: Information | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the GTPP configuration. This is an internal reference number. This is a key variable. Type: Information | Int32
> echo-req-rx | The total number of Echo Request messages received. | Int32
> echo-req-tx | The total number of Echo Request messages transmitted. | Int32
> echo-rsp-rx | The total number of Echo Response messages received. | Int32
> echo-rsp-tx | The total number of Echo Response messages transmitted. | Int32
> redir-rcvd | The total number of Redirection Request messages received. | Int32
> redir-rsp | The total number of Redirection Response messages transmitted. | Int32
> node-alive | The total number of Node Alive Request messages received. | Int32
> node-alive-rsp | The total number of Node Alive Response messages transmitted. | Int32
> data-rec-trans | The total number of Data Record Transfer Request messages transmitted to the CGF(s). | Int32
> dup-data-rec-trans | The total number of data records transmitted marked as potential duplicates. | Int32
> send-data-rec | The total number of Data Record Transfer Request messages transmitted containing a Packet Transfer Command information element of 1 (Send Data Record Packet). | Int32
> rel-data-rec | The total number of Data Record Transfer Request messages transmitted containing a Packet Transfer Command information element of 4 (Release Data Record Packet). | Int32
> cancel-data-rec | The total number of Data Record Transfer Request messages transmitted containing a Packet Transfer Command information element of 3 (Cancel Data Record Packet). | Int32
> data-rec-trans-rsp | The total number of Data Record Transfer Response messages received from the CGF(s). | Int32
> delete-node | The total number of Delete Node Address Request messages sent to the CGF(s). | Int32
> node-addr | The total number of Set Node Address Request messages sent to the CGF(s). | Int32
> req-accept | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 128 (80H, Request accepted). | Int32
> req-not-fulfil | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 255 (FFH, Request not fulfilled). | Int32
> req-malform | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 193 (C1H, Invalid message format). | Int32
> version-not-supp | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 198 (C6, Version not supported). | Int32
> serv-not-supp | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 200 (C8H, Service not supported). | Int32
> mand-ie-err | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 201 (C9H, Mandatory IE incorrect). | Int32
> mand-ie-miss | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 202 (CAH, Mandatory IE missing). | Int32
> opt-ie-err | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 203 (CBH, Optional IE incorrect). | Int32
> dup-already-fulfil | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 252 (FCH, Request related to possibly duplicated packets already fulfilled). | Int32
> already-fulfil | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 253 (FDH, Request already fulfilled). | Int32
> no-resource | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 199 (C7H, No resources available). | Int32
> sys-fail | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 204 (CCH, System failure). | Int32
> cdr-dec-error | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 177 (B1H, CDR Decoding Error). | Int32
> seq-no-incorrect | The total number of Data Record Transfer Response messages received from the CGF(s) containing a cause information element of 254 (FEH, Incorrect Seq No). | Int32
> unknown-cause | The total number of Data Record Transfer Response messages received from the CGF with Unknown Cause Code. | Int32
> normal-close | The total number of CDRs sent containing a Cause for Record Closing information element of 0 ( normal release). | Int32
> abnormal-close | The total number of CDRs sent containing a Cause for Record Closing information element of 4 (abnormal termination). | Int32
> vol-limit-close | The total number of CDRs sent containing a Cause for Record Closing information element of 16 (10H, volume limit). | Int32
> time-limit-close | The total number of CDRs sent containing a Cause for Record Closing information element of 17 (11H, time limit). | Int32
> open-req | The total number of Start-Accounting Request messages received. | Int32
> aaa-acct-arch | The total number of requests currently archived by the system’s AAA subsystem. | Int32
> rdir-sys-fail | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 59 (3BH, System failure). | Int32
> rdir-txbuf-full | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 60 (3CH, The transmit buffers are becoming full). | Int32
> rdir-rxbuf-full | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 61 (3DH, The receive buffers are becoming full). | Int32
> other-node-dn | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 62 (3EH, Another node is about to go down). | Int32
> self-node-dn | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 63 (3FH, This node is about to go down). | Int32
> rdir-no-res | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 199 (C7H, No resources available). | Int32
> rdir-serv-no | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 200 (C8H, Service not supported). | Int32
> rdir-version-not-supp | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 198 (C6H, Version not supported). | Int32
> rdir-mand-ie-miss | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 202 (CAH, Mandatory IE missing). | Int32
> rdir-mand-ie-err | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 201 (C9H, Mandatory IE incorrect). | Int32
> rdir-opt-ie-err | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 203 (CBH, Optional IE incorrect). | Int32
> rdir-malformed | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 193 (C1H, Invalid message format). | Int32
> rdir-rsp-sys-fail | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 204 (CCH, System failure). | Int32
> mgmt-int-close | indicates that the CDR is generated with cause for record closing as management intervention. e.g when the user does the “clear sub” or “gtpp interim now”. | Int32
> sgsn-chng-close | This stat is used to indicate that the CDR is generated at the OLD sgsn with "causeForRecClosing" as SGSN change. This will happen during ISRAU (Inter SGSN Routing Area Update) scenario wherein the call in old SGSN is transferred to new SGSN and the CDR is generated at the old SGSN indicating that MM context/PDP context is released with causeForRecClosing as SGSN Change. This is applicable only for SGSN. | Int32
> max-chng-close | This indicates that the CDR is released because the container changes are more than the configured value. For example, in SGSN for QOS or tariff time changes a container is added. By default, max change is set to 4. If 4 containers are added then the CDR is released with causeForRecClosing as max change condition. | Int32
> rat-chng-close | This indicates that the partial CDR is released at the GGSN due to the RAT (Radio Access Technology) change. This will happen whenever the user moves from GPRS to UMTS and vice versa. This is applicable only for G-CDR. | Int32
> ms-tz-chng-close | This indicates that the partial CDR is released at the GGSN due to the MS Time zone change. This is applicable only for G-CDR. | Int32
> list-down-stream-chng-close | The total number of CDRs sent containing a Cause for Record Closing information element of 59 (List Of Downstream Node Change). | Int32
> focs-close | Indicates the total number of FOCS enabled sessions closed due to ACL rule violation received for FOCS and/or ODB. | Int32
> inactivity-close | Indicates the total number of FOCS enabled sessions closed due to inactivity timeout. | Int32
> total-gcdr-xmit | This indicates the total number of G-CDRs transmitted to the mediation system. | Int32
> total-scdr-xmit | This indicates the total number of S-CDRs transmitted to the mediation system. | Int32
> total-mcdr-xmit | This indicates the total number of M-CDRs transmitted to the mediation system. | Int32
> total-smbmscdr-xmit | The total number of S-MB-CDR transmitted between SGSN and MBMS service. | Int32
> total-gmbcdr-xmit | The total number of G-MB-CDR transmitted between GGSN and MBMS service. | Int32
> total-gcdr-rexmit | This indicates the total number of G-CDRs re-transmitted to the mediation system. This will happen whenever SGSN/GGSN is not getting the response from the mediation server in a stipulated period of time. | Int32
> total-scdr-rexmit | This indicates the total number of S-CDRs re-transmitted to the mediation system. his will happen whenever SGSN/GGSN is not getting the response from the mediation server in a stipulated period of time. | Int32
> total-mcdr-rexmit | This indicates the total number of M-CDRs re-transmitted to the mediation system. his will happen whenever SGSN/GGSN is not getting the response from the mediation server in a stipulated period of time. | Int32
> total-smbmscdr-rexmit | The total number of S-MB-CDR retransmitted between SGSN and MBMS service. | Int32
> total-gmbcdr-rexmit | The total number of G-MB-CDRs retransmitted between GGSN and MBMS service. | Int32
> total-gcdr-accept | This indicates the total number of G-CDRs successfully sent to the mediation server for which the SGSN/GGSN received the positive response. | Int32
> total-scdr-accept | This indicates the total number of S-CDRs successfully sent to the mediation server for which the SGSN/GGSN received the positive response. | Int32
> total-mcdr-accept | This indicates the total number of M-CDRs successfully sent to the mediation server for which the SGSN/GGSN received the positive response. | Int32
> total-gmbcdr-accept | The total number of G-MB-CDR accepted between GGSN and MBMS service. | Int32
> total-gcdr-fail | This indicates the total number of G-CDRs transmission failures. | Int32
> total-scdr-fail | This indicates the total number of S-CDRs transmission failures. | Int32
> total-mcdr-fail | This indicates the total number of M-CDRs transmission failures. | Int32
> total-gmbcdr-fail | The total number of G-MB-CDR failed between GGSN and MBMS service. | Int32
> cc-char-hot | This indicates the CDR released with charging characteristics set as Hot Billing. | Int32
> cc-char-normal | This indicates the CDR released with charging characteristics set as Normal Billing. | Int32
> cc-char-prepaid | This indicates the CDR released with charging characteristics set as Prepaid Billing. | Int32
> cc-char-flat | This indicates the CDR released with charging characteristics set as Flat Billing. | Int32
> cc-char-unknown | This indicates the CDR released with charging characteristics set as Unknow charging characteristics. | Int32
> data-rec-ret-send | The total number of Data Record Transfer Request messages retried containing a Packet Transfer Command information element of 1 (Send Data Record Packet). | Int32
> data-rec-ret-poss-dup | The total number of data records retried marked as potential duplicates with IE of 2. (Send Possibly Duplicate Data Record) | Int32
> data-rec-ret-cancel | The total number of Data Record Transfer Request messages retried containing a Packet Transfer Command information element of 3 (Cancel Data Record Packet). | Int32
> data-rec-ret-rel | The total number of Data Record Transfer Request messages retried containing a Packet Transfer Command information element of 4 (Release Data Record Packet). | Int32
> data-rec-ret-emp | The total number of empty Data Record Transfer Request messages retried containing a Packet Transfer Command information element of 1 (Send Data Record Packet). | Int32
> data-rec-success-send | The total number of successful Data Record Transfer Response messages for Send Data Record Packet Transfer command. | Int32
> data-rec-success-poss-dup | The total number of Successful Data Record Transfer Response messages for Send Poss Dup Data Record Packet Transfer command. | Int32
> data-rec-success-cancel | The total number of Successful Data Record Transfer Response messages for Cancel Data Record Packet Transfer command. | Int32
> data-rec-success-rel | The total number of Successful Data Record Transfer Response messages for Release Data Record Packet Transfer command. | Int32
> data-rec-success-emp | The total number of Successful Data Record Transfer Response messages for Empty Send Data Record Packet Transfer command. | Int32
> invalid-msg-seq-num | The total number of requests with invalid sequence number. | Int32
> invalid-msg-unknown-cgf | The total number of requests with an unknown CGF. | Int32
> invalid-msg-unknown-msg | The total number of requests with an unknown message. | Int32
> gss-echo-req | The total echo request from GSS. | Int32
> gss-echo-rsp | The total echo request response to GSS. | Int32
> gss-gtpp-req | The total GTPP request sent to GSS. | Int32
> gss-gtpp-req-ret | The total GTPP request retried to GSS. | Int32
> gss-gtpp-rsp | The total successful GTPP request response. | Int32
> gss-gtpp-rsp-failed | The total GTPP request response failed. | Int32
> gss-gcdr-req | The total GCDR request sent. | Int32
> gss-gcdr-req-ret | The total GCDR request retried. | Int32
> gss-gcdr-rsp | The total successful GCDR request response. | Int32
> gss-gcdr-rsp-failed | The total GCDR request response failed. | Int32
> gss-aaaproxy-rec-req | The total AAA proxy recover request sent. | Int32
> gss-aaaproxy-rec-ret | The total AAA proxy recover request retried. | Int32
> gss-aaaproxy-rec-rsp | The total successful AAA proxy recover request response. | Int32
> gss-aaaproxy-rec-rsp-failed | The total AAA proxy recover request response failed. | Int32
> gss-aaamgr-rec-req | The total AAA MGR recover request sent. | Int32
> gss-aaamgr-rec-ret | The total AAA MGR recover request retried. | Int32
> gss-aaamgr-rec-rsp | The total successful AAA MGR recover request response. | Int32
> gss-aaamgr-rec-rsp-failed | The total AAA MGR recover request response failed. | Int32
> gss-update-cgf-req | The total CGF update request sent. | Int32
> gss-update-cgf-req-ret | The total CGF update request retried. | Int32
> gss-update-cgf-rsp | The total successful CGF update request response. | Int32
> gss-update-cfg-rsp-failed | The total CGF update request response failed. | Int32
> gss-clear-db-req | The total database clear request sent. | Int32
> gss-clear-db-req-ret | The total database clear request retried. | Int32
> gss-clear-db-rsp | The total successful database clear request response. | Int32
> gss-clear-db-rsp-failed | The total database clear request response failed. | Int32
> gss-update-req | The total update request received. | Int32
> gss-invalid-req-rcvd | The total invalid request received from. | Int32
> gss-cdr-loss | The total number of CDRs lost due to failure of remote CDR file streaming. | Int32
> gss-cdr-loss-traps | The total number of traps generaed for loss of CDRs due to failure of remote CDR file streaming. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883