> MME LAC Pool Area Configuration Mode Commands
> The MME LAC Pool Area Configuration Mode is used to create and manage the Local Area Code (LAC) pool areas.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> hash-value
> Configures the Visitor Location Register hash value mapping for this pool area.
> Product
> MME
> Privilege
> Administrator
> Syntax
> hash-value { value | non-configured-values | range value to value } use-vlr vlr_name
> no hash-value { value | non-configured-values | range value to value }
> no
> Removes the configured hash-value from the pool-area configuration.
> value
> Specifies the VLR hash value to be used with the configured VLR. value must be and integer from 0 to 999.
> non-configured-values
> Specifies that the VLR configured in this command is to be used non-configured hash values.
> range value to value vlr_name
> Specifies a range of hash values to use with the configured VLR. value must be an integer from 0 to 999.
> use-vlr
> Specifies the VLR to be used with the hash value configuration in this command.
> Usage
> Use this command to configure hash values to be used with VLRs.
> Example
> The following command configures all hash values within a range of 0 to 500 to use a VLR named vlr1:
> hash-value range 0 to 500 use-vlr vlr1
> The following command configures hash values of 501 to use a VLR named vlr2:
> hash-value 501 use-vlr vlr2
> The following command configures all non-configured hash values to use a VLR named vlr3:
> hash-value non-configured-values use-vlr vlr3
> lac
> Configures a 3G location area code or area codes that define this pool area.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] lac { area_code } +
> no
> Removes a configured forbidden handover area code or area codes from this policy. If no location area code is specified, then all location area codes are removed.
> area_code
> Specifies an area code or area codes from which UEs are restricted from participating in a handover. area_code must be an integer value from 0 to 65535. Multiple area codes can be entered (up to 128 in a single line).
> Usage
> Use this command to configure 3G location-based area codes that define this pool area.
> Example
> The following command configures eight location-based area codes (1, 2, 3, 4, 5, 6, 7, 8) that define this pool area:
> lac 1 2 3 4 5 6 7 8

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883