> Linkset Configuration Mode Commands
> The Linkset configuration mode defines the MTP3 linkset parameters for a specific SS7 routing domain instance.
> In this mode, the prompt will appear similar to:
> [local]hostname(config-ss7-rd-linkset-<#>)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> adjacent-point-code
> This command defines the point-code for the adjacent (next) network element in the SS7 network.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> adjacent-point-code point-code
> no adjacent-point-code
> point-code
> Point-code is an SS7 address for an element in the SS7 network. Point-codes must be defined in dotted-decimal format in a string of 1 to 11 digits. Format options include:

> • | 0.0.1 to 7.255.7 for point-code in the ITU range.

> • | 0.0.1 to 255.255.255 for point-code in the ANSI range.

> • | 0.0.1 to 15.31.255 for point-code in the TTC range.

> • | a string of 1 to 11 digits in dotted-decimal to represent a point-code in a different range.

> no
> Removes the adjacent-point-code configuration for this linkset in the SS7 routing domain
> Important: Removing the linkset configuration will result in the termination of all of the links within the linkset.
> Usage
> Use this command to define the point-code for the adjacent element in the SS7 network.
> Example
> adjacent-point-code 6.202.7
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> link
> This command creates an MTP3 link configuration for the SS7 linkset and enters the Link configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> link id id [ link-type [ atm-broadband | highspeed-narrowband | lowspeed-narrowband ]
> no link id id
> no
> Disables the specified link configuration.
> Important: Removing the link configuration will result in the termination of traffic on the specified link.
> #_octets
> Sets the number of octets for the length of the LSSU.
> id
> This number uniquely identifies the link in the linkset.
> id: an integer between 1 and 16.
> link-type
> Identifies the signalling type for this link; options include:

> • | ATM broadband -- ATM AAL5 over an optical line card (OLC2)

> • | high speed-narrowband -- 64 kbps over a channelized optical line card (CLC2)

> • | low speed-narrowband -- 4.8 kbps over a channelized optical line card (CLC2)

> Important: Be default link-type is ATM-broadband. To support narrowband SS7, one of the other options must be set.
> Usage
> Access the Link configuration mode to configure the parameters for the the link.
> Example
> Access configuration for link 4:
> link id 4
> self-point-code
> This command defines the SS7 network point-code to identify this SGSN.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> self-point-code point-code
> no self-point-code
> point-code
> Point-code is an SS7 address for an element in the SS7 network. Point-codes must be defined in dotted-decimal format in a string of 1 to 11 digits. Format options include:

> • | 0.0.1 to 7.255.7 for point-code in the ITU range.

> • | 0.0.1 to 255.255.255 for point-code in the ANSI range.

> • | 0.0.1 to 15.31.255 for point-code in the TTC range.

> • | a string of 1 to 11 digits in dotted-decimal to represent a point-code in a different range.

> no
> Removes the self-point-code configuration for this linkset in the SS7 routing domain.
> Important: Removing the self-point-code will result in the termination of all traffic on this link.
> Usage
> Use this command to define the SS7 point-code to identify this system.
> Example
> self-point-code 6.192.7

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883