> HD Storage Policy Configuration Mode Commands
> The HD Storage Policy Configuration Mode is used to configure directory name and file parameters for Diameter record files being stored on the HD storage device.
> directory
> Configures the name of the directory on the HD storage drive where Diameter records are stored.
> Product
> HSGW, P-GW, S-GW
> Privilege
> Administrator
> Syntax
> directory name dir_name
> default directory name
> default
> Returns the command to its default setting of using the policy name as the directory name.
> name dir_name
> Specifies the name to be applied to the directory. dir_name must be an alpha and or numeric string from 1 to 63 characters.
> When configured, the actual directory path is:
> /hd-raid/records/<record-type>/<dir_name>/
> So if the directory name variable is entered as “sgwpgw”, the path is:
> /hd-raid/records/acr/sgwpgw
> Usage
> Use this command to name a directory on the HD storage drive where Diameter records are to be stored.
> Example
> The following command configures a directory named cdr1:
> directory name cdr1
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> file
> Configures file parameters for Diameter records being stored on the HD storage device.
> Product
> HSGW, P-GW, S-GW
> Privilege
> Administrator
> Syntax
> file { format acr { custom1...custom10 } | name { extension string | prefix string } | rotation { record-count num | time-interval sec | volume mb mbytes } }
> default file { format acr | name prefix | rotation { record-count | time-interval | volume } }
> no file ( extension | rotation { record-count | time-interval } }
> default
> Returns the command to the default settings for the specified keywords.
> no
> Removes the configuration for the specified parameters.
> format acr { custom1...custom10 }
> Default: custom1
> Specifies the file format used when storing records on the HD storage device. custom1 is a vendor-specific file format.
> name { extension string | prefix string }
> Specifies a string to be pre-pended or appended to the filenames. By default, the policy name is used for the prefix.
> extension string: Specifies a file extension to append to the filename. string must be an alpha and/or numeric string from 1 to 10 characters.
> prefix string: Specifies a file prefix to append to the filename. string must be an alpha and/or numeric string from 1 to 63 characters. This parameter replaces the policy name used by default.
> rotation { record-count num | time-interval sec | volume mb mbytes }
> Specifies the triggers that prompt file rotation on the HD storage drive. All options can be configured and upon reaching any of the thresholds, file rotation is initiated.
> record-count num: Specifies that file rotation is to occur when the number of records reaches the number configured in this keyword. num must be an integer value from 1000 tom 65000. Default = 10000
> time-interval sec: Specifies that file rotation is to occur a time intervals configure in this keyword. sec must be an integer value from 30 to 86400. Default = 3600 (1 hour)
> volume mb mbytes: Specifies that file rotation is to occur when the record volume exceeds the value configured in the keyword. mbytes must be an integer value from 2 to 40. Default = 4 (mb)
> Usage
> Use this command to configure file parameters for Diameter records being stored on the HD storage device.
> Example
> The following command set the file rotation thresholds for files being stored on the HD storage device:
> file rotation volume mb 4
> file rotation record-count 15000
> file rotation time-interval 7200
> The following command replaces the policy name as the prefix of all files being stored through this policy with the prefix sgw:
> file name prefix sgw

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883