> Configuration Management
> This chapter identifies new, modified, and obsoleted configuration commands in Releases 12.0 or 12.1.
> Topics covered in this chapter are:

> l | New Configuration Commands

> l | Modified Configuration Commands

> l | Obsoleted Commands

> l | GTPP Storage Server (GSS)

> l | Web Element Manager Changes

> New Configuration Commands
> This section identifies configuration commands that are new in .

> l | Common Commands - New in Release 12.0

> l | Application Detection and Control - New in Release 12.0

> l | ASN GW Commands - New in Release 12.0

> l | Content Filtering Commands - New in Release 12.0

> l | ECS Commands - New in Release 12.0

> l | Firewall Commands - New in Release 12.0

> l | GGSN Commands - New in Release 12.0

> l | HA Commands - New in Release 12.0

> l | HNB-GW Commands - New in Release 12.1

> l | HSGW Commands - New in Release 12.0

> l | Mobility Management Entity Commands - New in Release 12.0

> l | NAT Commands - New in Release 12.0

> l | Packet Data Network Gateway Commands - New in Release 12.0

> l | PDIF Commands - New in Release 12.0

> l | PDSN Commands - New in Release 12.0

> l | Serving Gateway Commands - New in Release 12.0

> l | Session Control Manager Commands - New in Release 12.0

> l | SGSN Commands - New in Release 12.0

> l | SGSN Commands - New in Release 12.1

> Common Commands - New in Release 12.0
> This section provides information on new commands that are common to products in Release 12.0.
> aaa secondary-group
> This command enables to configure secondary AAA group for the APN. This supports the RADIUS Fire-and-Forget feature in conjunction with GGSN for secondary accounting (with different RADIUS accounting group configuration) to the RADIUS servers without expecting acknowledgement from the server, in addition to standard RADIUS accounting. This secondary accounting will be an exact copy of all the standard RADIUS accounting message (RADIUS Start / Interim / Stop) sent to the standard AAA RADIUS server.
> CLI (APN Configuration Mode)
> aaa secondary-group aaa_group_name
> { default | no } aaa secondary-group
> aaa tacacs+
> Enables TACACS+ AAA services that have been configured on the ASR 5000.
> CLI (Global Configuration Mode)
> aaa tacacs+
> aaa secondary-group
> This command enables to configure secondary AAA group for the subscriber template. This supports the No-ACK RADIUS Targets feature in conjunction with PDSN and HA for secondary accounting (with different RADIUS accounting group configuration) to the RADIUS servers without expecting the acknowledgement from the server, in addition to standard RADIUS accounting. This secondary accounting will be an exact copy of all the standard RADIUS accounting message (RADIUS Start / Interim / Stop) sent to the standard AAA RADIUS server.
> CLI (Subscriber Configuration Mode)
> aaa secondary-group aaa_group_name
> { default | no } aaa secondary-group
> accounting
> Enables or disables the recording of the start and stop time of each command issued during a TACACS+ authenticated session.
> CLI (TACACS+ Configuration Mode)
> [no] accounting {start-stop | command}
> app-level-retransmission
> This command enables application-level retransmissions with “T” bit set.
> CLI (Credit Control Configuration Mode)
> app-level-retransmission { set-retransmission-bit | unset-retransmission-bit }
> default app-level-retransmission
> arp-priority-level
> This command enables to map ARP priority-level value received from PCRF to inter-user-priority value and be sent in A11 session update.
> CLI (Policy Control Configuration Mode)
> arp-priority-level map-to inter-user-priority
> { default | no } arp-priority-level map-to
> authorization
> Enables or disables the authorization of TACAS+ users on a command-by-command, command + argument, or command prompt basis.
> CLI (TACACS+ Configuration Mode)
> [no] authorization {command | prompt | arguments}
> credit-control-group
> This command enables to configure Credit Control Group in subscriber template.
> CLI (Subscriber Configuration Mode)
> credit-control-group cc_group_name
> no credit-control-group
> diameter ignore-service-id
> This command enables to accept/ignore service ID in Service-Identifier AVP defined in the Diameter dictionaries for Gy interface implementation.
> CLI (Credit Control Configuration Mode)
> [ default | no ] diameter ignore-service-id
> diameter service-context-id
> This command configures the value to be sent in the Service-Context-Id AVP, which identifies the context in which DCCA is used.
> CLI (Credit Control Configuration Mode)
> diameter service-context-id service_context_id
> default diameter service-context-id
> diameter update-dictionary-avps
> This command enables dictionary control of the AVPs that need to be added based on the version of the specification to which the OCS is compliant with. This command is applicable to all products that use the dcca-custom8 dictionary for Gy interface implementation.
> CLI (Credit Control Configuration Mode)
> diameter update-dictionary-avps { 3gpp-rel8 | 3gpp-rel9 }
> { default | no } diameter update-dictionary-avps
> diameter update-dictionary-avps
> This command enables dictionary control of the AVPs that need to be added based on the version of the specification to which the PCEF is compliant with. This command is applicable only to Diameter dictionaries that support standard based volume reporting over Gx feature.
> CLI (Policy Control Configuration Mode)
> diameter update-dictionary-avps { 3gpp-r8 | 3gpp-r9 }
> { default | no } diameter update-dictionary-avps
> destination-host-avp
> This command controls encoding of the Destination-Host AVP in initial/retried requests.
> CLI (Diameter Endpoint Configuration Mode)
> destination-host-avp { session-binding | always | initial-request | retried-request }
> default destination-host-avp
> dynamic-peer-failure-retry-count
> This command configures the number of times the system attempts to connect to a dynamically discovered Diameter peer.
> CLI (Diameter Endpoint Configuration Mode)
> dynamic-peer-failure-retry-count value
> default dynamic-peer-failure-retry-count
> dynamic-route
> This command configures the expiration time for dynamic routes created after a Diameter destination host is reached.
> CLI (Diameter Endpoint Configuration Mode)
> dynamic-route expiry-timeout value
> default dynamic-route expiry-timeout
> egcdr cdr-encoding
> This command configures the eG-CDR encoding type.
> CLI (ACS Rulebase Configuration Mode)
> egcdr cdr-encoding { ascii [ delimiter { colon | comma | pipe } ] | asn.1 }
> default egcdr cdr-encoding
> link-aggregation port switch to
> When a link aggregation group (LAG) contains two sets of ports, each connecting to a different Ethernet switch, this command allows you to change the status of the active distributing ports.
> CLI (Global Configuration Mode)
> link-aggregation port switch to <slot/port>
> load-balancing-algorithm
> This command configures the behavior for load balancing Diameter peers in the event of a failure of an active server.
> CLI (Diameter Endpoint Configuration Mode)
> load-balancing-algorithm { highest-weight | lowest-weight-borrowing min-active-servers number }
> default load-balancing-algorithm
> lsp ping
> This command checks the Multi Protocol Label Switching (MPLS) LSP connectivity for the specified forwarding equivalence class (FEC). It must be followed by an IPv4 prefix.
> CLI (Exec Mode)
> lsp-ping ip_prefix_FEC [ count ping-packets ] [ | verbose ] [ | grep grep_options ]
> lsp-traceroute
> This command discovers MPLS LSP routes that packets actually take when traveling to their destinations. It must be followed by an IPv4 prefix.
> CLI (Exec Mode)
> lsp-traceroute ip_prefix_FEC [ maxttl time_to_live ] [ | verbose ] [ | grep grep_options ]
> on-authen-fail
> Defines system behavior when an administrative login fails due to a TACACS+ authentication failure.
> CLI (TACACS+ Configuration Mode)
> on-authen-fail {continue | stop} [tty console]
> on-network-error
> Defines system behavior when a TACACS+ login fails due to a network error.
> CLI (TACACS+ Configuration Mode)
> on-network-error {continue | stop} [tty console]
> on-unknown-user
> Configures system behavior when a TACACS+ server cannot authenticate a given user name.
> CLI (TACACS+ Configuration Mode)
> on-unknown-user {continue | stop} [tty console]
> post-processing policy
> This command configures the post-processing policy to be applied on Limit-Reached packets. This allows to enable post-processing priority based rules for content in blacklisted state.
> The post-processing policy always CLI command will enable post-processing on Limit-Reached packets. If there are post-processed priority based rules, it will check for any redirection rules, else will discard the packets by default. No other post-processing actions like forward, next-hop, xheader-insertion, etc. will be applied on these limit-reached packets. If no post-processing priority rules are present, the packets will be dropped by default.
> The post-processing policy not-for-dynamic-discard will directly discard the limit-reached context and will not apply post-processing priority based rules. This is the default setting.
> Also, refer to the configuration changes required in the New Feature Summary chapter.
> CLI (ACS Rulebase Configuration Mode)
> post-processing policy { always | not-for-dynamic-discard }
> default post-processing policy
> pptp any-match
> This command defines rule expressions to match all PPTP packets. This is used in conjunction with ADC, Stateful Firewall, and NAT in-line services.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] pptp any-match operator condition
> pptp ctrl-msg-type
> This command defines rule expressions to analyze and charge user traffic based on control message type for PPTP packets. This is used in conjunction with ADC, Firewall, and NAT inline services.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] pptp ctrl-msg-type = { call-clear-request | call-disconnect-notify | echo-reply | echo-request | incoming-call-connected | incoming-call-reply | incoming-call-request | outgoing-call-reply | outgoing-call-request | set-link-info | start-control-connection-reply | start-control-connection-request | stop-control-connection-reply | stop-control-connection-request | wan-error-notify
> pptp gre
> This command defines rule expressions based on GRE to match all PPTP packets. This is used in conjunction with ADC, Firewall, and NAT in-line services.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] pptp gre any-match = condition
> radius accounting fire-and-forget
> This feature enables to configure the Fire-and-Forget feature. The accounting request sent to a RADIUS accounting server configured under the AAA group with this CLI command configured in it will not expect a response from the server.
> CLI (AAA Group Configuration Mode)
> [ default | no ] radius accounting fire-and-forget
> require ecs credit-control subscriber-mode
> This command configures DCCA/Gy to work in per subscriber-PDN level Gy mode, wherein one Diameter session is created per subscriber PDN rather than per bearer, and only one DCCA/Gy session is created for multi-bearer PDNs. This command is applicable to all products using the Gy interface.
> CLI (Global Configuration Mode)
> [ no ] require ecs credit-control subscriber-mode
> server
> Configures TACACS+ AAA service-related parameters for use in authenticating ASR 5000 administrative users via a TACACS+ server.
> CLI (TACACS+ Configuration Mode)
> [no] server priority <priority_number> ip-address <ip_address> [service {authentication | authorization | accounting}] [port <port_number>] [{encrypted password <shared_secret > | password <text_password>}] [timeout <seconds>] [retries <num_retries>] [nas-source-address <ip_address>]
> server-mode
> This command configures the Diameter endpoint to establish the system as the server side endpoint of the connection.
> CLI (Diameter Endpoint Configuration Mode)
> server-mode [ demux-mode ]
> servers-unreachable
> This command configures whether to continue/terminate calls when Diameter server(s)/OCS become unreachable.
> CLI (Credit Control Configuration Mode)
> servers-unreachable { initial-request { continue | terminate [ after-timer-expiry timeout_period ] } | update-request { continue | terminate [ after-quota-expiry | after-timer-expiry timeout_period ] } }
> no servers-unreachable { initial-request | update-request }
> Application Detection and Control - New in Release 12.0
> This section provides information on new ADC commands available in Release 12.0.
> None for this release.
> ASN GW Commands - New in Release 12.0
> This section provides information on new ASN GW commands available in Release 12.0.
> asn-policy ms-requested-classifiers
> This command allows an operator to allow or decline the dynamic addition of classifiers during MS-initiated service flow creation/modification.
> CLI (Subscriber Configuration Mode)
> [no] asn-policy ms-requested-classifiers {allow | disallow}
> asn-policy notification-handoff
> This command allows an operator to enable/disable the reporting of the BSID in the Accounting Interim Update during the handoff and location update.
> CLI (Subscriber Configuration Mode)
> [no] asn-policy notification-handoff {allow | disallow}
> asn-policy hotlining wimax
> This command allows an operator to enable or disable WiMAX hotlining capability in the ASNGW and WiMAX HA. The command applies to both profile id-based and rule-based hotlining.
> CLI (Subscriber Configuration Mode)
> [no] asn-policy hotlining-wimax
> asngw-service priority vlan
> This command allows an operator to enable or disable 802.1P priority marking for WiMAX control traffic over an R6/R4 interface.
> CLI (Service Configuration Mode)
> asngw-service <asngw_serviceName> priority vlan <priority >
> The default is to disallow.
> schedule-type
> This command allows an operator to configure the 802.1 priority based on the schedule type for WiMAX data traffic.
> CLI (ASN QoS Descriptor Configuration Mode)
> (no] schedule-type [be | ertvr | nrtvr | rtvr | ugs] priority < 0-7 >
> If the policy is set to allow, only the priority value is used for WiMAX data traffic.
> Content Filtering Commands - New in Release 12.0
> This section provides information on new CF commands available in Release 12.0.
> None for this release.
> ECS Commands - New in Release 12.0
> This section provides information on new ECS commands available in Release 12.0.
> egcdr cdr-encoding
> This command configures the eG-CDR encoding type. When configuring the eG-CDR encoding type as ASCII, the delimiter character can be specified as either “:” (colon), “,” (comma), or “|” (pipe). The default delimiter character is “|” (pipe).
> CLI (ACS Rulebase Configuration Mode)
> egcdr cdr-encoding { ascii [ delimiter { colon | comma | pipe } ] | asn.1 }
> default egcdr cdr-encoding
> http domain
> This command enables to define rule expressions to match domain portion of the URI in HTTP packets.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] http domain [ case-sensitive ] operator domain
> tcp proxy-prev-state
> This command defines rule expressions to match TCP previous state on the ingress side of the TCP proxy.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] tcp proxy-prev-state operator previous_state
> tcp proxy-state
> This command defines rule expressions to match TCP state on the ingress side of the TCP proxy.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] tcp proxy-state operator previous_state
> tftp any-match
> This command defines rule expressions to match all TFTP packets.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] tftp any-match operator condition
> tftp data-any-match
> This command defines rule expressions to match all TFTP data packets.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] tftp data-any-match operator condition
> wsp domain
> This command enables to define rule expressions to match domain portion of the URI in WSP packets.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] wsp domain [ case-sensitive ] operator domain
> www domain
> This command enables to define rule expressions to match domain portion of the URI for WSP/HTTP packets.
> CLI (ACS Ruledef Configuration Mode)
> [ no ] www domain [ case-sensitive ] operator domain
> Firewall Commands - New in Release 12.0
> This section provides information on new Stateful Firewall commands available in Release 12.0.
> icmpv6 any-match
> This command configures an access ruledef to match any ICMPv6 traffic for the user.
> CLI (Access Ruledef Configuration Mode)
> [ no ] icmpv6 any-match operator condition
> icmpv6 code
> This command configures an access ruledef to analyze user traffic based on ICMPv6 code.
> CLI (Access Ruledef Configuration Mode)
> [ no ] icmpv6 code operator code
> icmpv6 type
> This command configures an access ruledef to analyze user traffic based on ICMPv6 type.
> CLI (Access Ruledef Configuration Mode)
> [ no ] icmpv6 type operator type
> ip version
> This command defines rule expressions to match version number in IP header.
> CLI (Access Ruledef Configuration Mode)
> [ no ] ip version = { ipv4 | ipv6 }
> GGSN Commands - New in Release 12.0
> This section provides information on new GGSN commands available in Release 12.0.
> ikev1 disable-initial-contact
> From the Context Configuration Mode, this command disables the sending of an INITIAL-CONTACT message in the IKEv1 protocol after the node creates a new Phase 1 SA, caused either by Dead Peer Detection or by a rekey.
> CLI (Context Configuration Mode)
> [ no ] ikev1 disable-initial-contact
> HA Commands - New in Release 12.0
> This section provides information on new HA commands available in Release 12.0.
> None for this release.
> HNB-GW Commands - New in Release 12.1
> This section provides information on new commands for HNB-GW available in Release 12.1.
> map lac
> This command configures the mapping of Location Area Code (LAC) received from UE to MSC point code. This is an important configuration for CS network resource sharing without Iu-Flex interface configuration.
> Support for multiple MSC selection in a CS core network is provided with this command.
> CLI (HNB-CS Configuration Mode)
> map lac range lac_start to lac_end point-code msc_point_code
> no map lac range lac_start to lac_end
> ecmp-lag hash
> This command is added to the Global Configuration Mode to configure the system to select source Boxer Internal Address (SBIA) as the input to the hashing function for ECMP-LAG distribution.
> This command allows the operator to change the way hashing works in deciding which link to use for ECMP and Link Aggregation. In the default hashing algorithm the IP Source Address, IP Destination Address, IP Protocol and Source BIA are used in the hashing function. When “use-sbia-only” option is selected, only the Source BIA is used in the hashing function.
> CLI (Global Configuration Mode)
> [no] ecmp-lag hash use-sbia-only
> CAUTION: While using ECMP-LAG on a HNB-GW, this configuration is mandatory for standalone HNB-GW deployment and highly recommended in other deployment scenarios where HNB-GW is used in combination with other services.
> HSGW Commands - New in Release 12.0
> This section provides information on new HSGW commands available in Release 12.0.
> a11-signalling-packets
> This command enables the DSCP marking feature for IP headers carrying outgoing A11-signalling A11 packets (such as RRP, RU, SU).
> CLI (HSGW Service Configuration Mode)
> a11-signalling-packets ip-header-dscp value
> [ default | no ] a11-signalling-packets ip-header-dscp
> mobility-option-type-value
> This command changes the mobility option type value used in mobility messages.
> CLI (MAG Service Configuration Mode)
> mobility-option-type-value { custom1 | standard )
> default mobility-option-type-value
> rsvp
> This command configures resource reservation protocol (RSVP) parameters for this HSGW service in support of the network initiated QoS feature.
> CLI (HSGW Service Configuration Mode)
> rsvp { max-retransmissions count | retransmission-timeout seconds }
> [ default | no ] rsvp { max-retransmissions | retransmission-timeout }
> signalling-packets
> This command enables the DSCP marking feature for IP headers carrying outgoing signalling packets.
> CLI (MAG Service Configuration Mode)
> signalling-packets ip-header-dscp value
> [ default | no ] signalling-packets ip-header-dscp
> LNS Service Configuration Mode Commands
> This section provides information on new LNS commands available in Release 21.2
> newcall
> The following command configures new call related behavior
> CLI (LNS Service Configuration Mode)
> newcall duplicate-subscriber-requested-address { accept | reject }
> default newcall duplicate-subscriber-requested-address
> Mobility Management Entity Commands - New in Release 12.0
> This section provides information on new MME commands available in Release 12.0.
> csfb
> The csfb command configures Circuit-Switched FallBack options for the configured call control profile. This command sets the CSFB option as only supporting short message service (SMS).
> CLI (Call Control Profile Configuration Mode)
> [ remove ] csfb sms-only
> lte-policy
> This command is a direct replacement for the obsolete mme-policy command and contains the same command set as the MME Policy mode.
> CLI (Global Configuration Mode)
> lte-policy
> sctp-param-template
> This command creates a new, or enters an existing SCTP parameter template configuration. SCTP parameter templates configure SCTP associations.
> CLI (Global Configuration Mode)
> sctp-param-template name
> This command enters the following mode:
> CLI (SCTP Parameter Template Configuration Mode)
> The following commands are located in the new SCTP Parameter Template Configuration mode:
> sctp-alpha value
> sctp-alt-accept-flag { diable | enable }
> sctp-beta value
> sctp-checksum-type { adler32 | crc32 }
> sctp-cookie-life value
> sctp-max-assoc-retx value
> sctp-max-in-strms value
> sctp-max-init-retx value
> sctp-max-mtu-size bytes
> sctp-max-out-strms value
> sctp-max-path-retx value
> sctp-min-mtu-size bytes
> sctp-rto-initial value
> sctp-rto-max value
> sctp-rto-min value
> sctp-sack-frequency value
> sctp-sack-period { value | units-10ms value }
> sctp-start-mtu-size bytes
> timeout { sctp-bundle value | sctp-heart-beat value }
> peer-sgsn
> This command statically configures peer SGSN environments to facilitate MME-to-SGSN relocations over an S3 or Gn/Gp interface. In prior releases, before this command was created, the MME relied on the DNS setting in the SCTP Service mode for peer SGSN discovery/selection. The order of selection is peer SGSN configuration through MME Service mode first and DNS selection through the SCTP Service mode second.
> CLI (MME Service Configuration Mode)
> peer-sgsn rai mcc number mnc number [ nri value ] rac value lac value address ip_address capability [ gn ] [ s16 ] [ s3 ]
> policy inter-rat
> This command enables the establishment of indirect data forwarding tunnels for Gn/Gp-based SRNS relocations.
> CLI (MME Service Configuration Mode)
> policy inter-rat indirect-forwarding-tunnels always
> s1-mme ip
> This command configures the quality of service QoS differentiated service code point (DSCP) used when sending data packets of a particular 3GPP QoS class over the S1-MME interface.
> CLI (MME Service Configuration Mode)
> s1-mme ip qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef }
> NAT Commands - New in Release 12.0
> This section provides information on new NAT commands available in Release 12.0.
> h323 time-to-live
> This command configures registration lifetime to maintain NAT binding.
> CLI (ACS Configuration Mode)
> h323 time-to-live timeout
> default h323 time-to-live
> h323 timeout
> This command configures the timeout interval for H323 requests.
> CLI (ACS Configuration Mode)
> h323 timeout { admission adm_timeout | discovery disc_timeout | location loc_timeout | registration reg_timeout | unregistration unreg_timeout }
> default h323 timeout { admission | discovery | location | registration | unregistration }
> h323 tpkt
> This command configures the Transport Protocol Data Unit Packet (TPKT).
> CLI (ACS Configuration Mode)
> h323 tpkt timeout
> default h323 tpkt
> h323 version
> This command configures the supported H323 versions.
> CLI (ACS Configuration Mode)
> h323 version version_num
> default h323 version
> Packet Data Network Gateway Commands - New in Release 12.0
> This section provides information on new P-GW commands available in Release 12.0.
> action
> This command configures the action priority for an actiondef.
> CLI (Local Policy Actiondef Configuration Mode)
> action priority priority action_name arguments
> no action priority priority
> actiondef
> This command enables creating, configuring, or deleting action definitions within a local policy service.
> CLI (Local Policy Service Configuration Mode)
> actiondef actiondef_name [ -noconfirm ]
> no actiondef actiondef_name
> This command enters the following mode:
> CLI (Local Policy Actiondef Configuration Mode)
> The following commands are located in the new Local Policy Actiondef Configuration mode:
> action priority priority action_name arguments
> end
> exit
> condition
> This command is used to configure the conditions which trigger the ruledef event.
> CLI (Local Policy Ruledef Configuration Mode)
> condition priority priority { variable { eq | ge | gt | le | lt | match | ne | nomatch } regex | string_value | int_value | set }
> no condition priority priority
> eventbase
> This command enables creating, configuring, or deleting an event base within a local policy service.
> CLI (Local Policy Service Configuration Mode)
> eventbase eventbase_name [ -noconfirm ]
> no eventbase eventbase_name
> This command enters the following mode:
> CLI (Local Policy Eventbase Configuration Mode)
> The following commands are located in the new Local Policy Eventbase Configuration mode:
> end
> exit
> rule priority priority [ event list_of_events ] ruledef ruledef_name actiondef actiondef_name [continue]
> local-policy-service
> This command enables creating, configuring, or deleting a local QoS policy.
> CLI (Global Configuration Mode)
> local-policy-service name [ -noconfirm ]
> This command enters the following mode:
> CLI (Local Policy Service Configuration Mode)
> The following commands are located in the new Local Policy Service Configuration mode:
> actiondef actiondef_name [ -noconfirm ]
> eventbase eventbase_name [ -noconfirm ]
> end
> exit
> ruledef ruledef_name [ -noconfirm ]
> mobility-option-type-value
> This command changes the mobility option type value used in mobility messages.
> CLI (LMA Service Configuration Mode)
> mobility-option-type-value { custom1 | standard )
> default mobility-option-type-value
> permission
> This command enables the ability to use network mobility service (NEMO) for the current APN. NEMO is disabled by default.
> CLI (APN Configuration Mode)
> [ no ] permission nemo
> default permission
> policy
> This command configures the Mobile IPv6 policy to decide on action to be taken when IPv4/IPv6 subscriber packets need to be tunneled, however, the encapsulated packets exceed tunnel MTU size.
> CLI (APN Configuration Mode)
> policy ipv6 tunnel mtu exceed { fragment [ inner ] | notify-sender }
> [ default | no ] policy ipv6 tunnel mtu exceed
> rule
> This command enables the setting of event rules. An event is something that occurs in the system which would trigger a set of actions to take place, such as new-call or rat-change.
> CLI (Local Policy Eventbase Configuration Mode)
> rule priority priority [ event list_of_events ] ruledef ruledef_name actiondef actiondef_name [continue]
> no rule priority priority
> ruledef
> This command enables creating, configuring, or deleting a rule definition within a local policy service.
> CLI (Local Policy Service Configuration Mode)
> ruledef ruledef_name [ -noconfirm ]
> no ruledef ruledef_name
> This command enters the following mode:
> CLI (Local Policy Ruledef Configuration Mode)
> The following commands are located in the new Local Policy Ruledef Configuration mode:
> condition priority priority { variable { eq | ge | gt | le | lt | match | ne | nomatch } regex | string_value | int_value | set }
> end
> exit
> signalling-packets
> This command enables the DSCP marking feature for IP headers carrying outgoing signalling packets.
> CLI (LMA Service Configuration Mode)
> signalling-packets ip-header-dscp value
> [ default | no ] signalling-packets ip-header-dscp
> PDIF Commands - New in Release 12.0
> This section provides information on new PDIF commands available in Release 12.0.
> None for this release.
> PDSN Commands - New in Release 12.0
> This section provides information on new PDSN commands available in Release 12.0.
> bgp
> The following command has been added.

> l | bgp extended-asn-cap

> CLI (Context Configuration Mode)
> [ no ] bgp extended-asn-cap
> maximum-paths ebgp
> The following command has been added.

> l | maximum-paths ebgp

> CLI (Router Bgp Mode)
> maximum-paths ebgp value
> [ no ] maximum-paths ebgp
> a11-signalling-packets
> The following command is added.

> l | a11-signalling-packets

> CLI (Pdsn-service Mode)
> a11-signalling-packets ip-header-dscp value
> [ no | default ] a11-signalling-packets ip-header-dscp
> fa-spi-list / ha-spi-list
> The following commands are added.

> l | fa-spi-list

> l | ha-spi-list

> CLI (Config Mode)
> fa-spi-list list
> ha-spi-list list
> aaa nas-ip-address IPv4
> The following commands are added.

> l | aaa nas-ip-address IPv4

> l | aaa 3gpp2-service-option

> CLI (PDSN Service Config Mode)
> aaa nas-ip-address ip-address
> aaa 3gpp2-service-option service option
> show ipv6 ospf
> Following command shows ipv6 ospf options and its results
> CLI (Context configuration mode)
> show ipv6 ospf [ database [ adv-router IPv4-Address ] [ls-type { external | inter-prefix | inter-router | intra-prefix | link | network | router } ] [ verbose ] [ | { grep grep_options | more } ] ] [ debugging ] [ interface ] [ neighbor [ details ] ] [ route [ summary ] ] [ virtual-links ] [ | { grep grep_options | more } ]
> Serving Gateway Commands - New in Release 12.0
> This section provides information on new commands available in Release 12.0.
> apn-profile
> The S-GW now supports the use of the APN Profile Configuration Mode commands. The apn-profile name command is located in the Global Configuration Mode.
> CLI (APN Profile Configuration Mode)
> The following commands in this mode are supported by the S-GW:
> cc { local-value-for-scdrs behavior bit_value profile index_bit | prefer { hlrvalue-for-scdrs | local-value-for-scdrs } }
> description description
> idle-mode-acl { ipv4 | ipv6 } access-group group_name
> ip { qos-dscp { { downlink | uplink } { background forwarding | conversational forwarding | interactive traffic-handling-priority priority_forwarding | streaming forwarding } + } | source-violation { deactivate [ all-pdp | excludefrom accounting | linked-pdp | tolerance-limit } | discard [ exclude-fromaccounting ] | ignore }
> call-control-profile
> The S-GW now supports the use of the Call Control Profile Configuration Mode commands. The call-control-profile name command is located in the Global Configuration Mode.
> CLI (Call Control Profile Configuration Mode)
> The following commands in this mode are supported by the S-GW:
> attach access-type { gprs | umts } { all | location-area-list instance list_id }{ failure-code code | user-device-release { before-r99 failure code code | r99-or-later failure code code }
> attach allow access-type { eps | gprs | umts } location-area-list instance list_id
> attach restrict access-type { eps | gprs | umts } { all | location-area-list instance list_id }
> attach imei-query-type { imei | imei-sv | none } [ [ verify-equipment-identity ] [ deny-greylisted ]
> attach imei-query-type
> authenticate { activate [ access-type { gprs | umts } ] | first [ access-type { gprs | umts } ] | frequency frequency | primary [ access-type { gprs | umts } ] | all-events [ access-type { gprs | umts } | frequency frequency | attach [ access-type { gprs | umts } | attach-type { combined | gprs-only } [ access-type { gprs | umts } | frequency frequency ] | frequency frequency | inter-rat [ access-type { gprs | umts } ] ] | detach [ access-type { gprs | umts } ] | rau | service-request | sms | tau }
> description description
> equivalent-plmn radio-access-technology { 2G | 3g | 4g | any } plmnid mcc mcc_number mnc_number priority priority
> treat-as-hplmn
> operator-policy
> The S-GW now supports the use of the Operator Policy Configuration Mode commands. The operator-policy name command is located in the Global Configuration Mode.
> CLI (Operator Policy Configuration Mode)
> The following commands in this mode are supported by the S-GW:
> apn { default-apn-profile apn_profile_name | network-identifier apn_net_id apn-profile apn_profile_name | operator-identifier apn_op_id apn-profile apn_profile_name }
> associate { apn-remap-table table_id | call-control-profile profile_id }
> description description
> imei range IMEI_number to IMEI_number { imei-profile profile_name | sv ## imeiprofile profile_name }
> lte-policy
> This command is a direct replacement for the obsolete mme-policy command and contains the same command set as the MME Policy mode. The S-GW now supports the following modes in the LTE Policy Configuration Mode: LTE Subscriber Map Configuration Mode and LTE TAI Management Database Configuration Mode.
> CLI (Global Configuration Mode)
> lte-policy
> Session Control Manager Commands - New in Release 12.0
> This section provides information on new SCM commands available in Release 12.0.
> bgcf-proxy
> This command enables SIP BGCF proxy for the service.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> bgcf-proxy [ port value | transport { tcp | udp } port value ] ]
> [ default | no ] bgcf-proxy
> core-reg-expiry-time
> This command configures Registration Expiry Timer Handling in P-CSCF/A-BG to keep pin holes open in B2BUA mode.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> core-reg-expiry-time sec
> [ default | no ] core-reg-expiry-time
> emergency-call-mode
> This command enables the P-CSCF/A-BG service to add “P-Emergency-Call-Mode-Preference” header in 200OK to REGISTER message. By default, this command is disabled.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> emergency-call-mode { 3gpp-cs | 3gpp-ims }
> [ default | no ] emergency-call-mode
> lawful-intercept
> This command enables Lawful Intercept (LI) in this CSCF service. Feature is disabled by default.
> CLI (CSCF Service Configuration Mode)
> [ no ] lawful-intercept
> pcrf-policy-control
> This command enables external policy control via PCRF through the Rx Diameter interface and enters the PCRF-Policy-Control Configuration Mode. Default is disabled.
> CLI (Proxy-CSCF Configuration Mode)
> [ no ] pcrf-policy-control
> This command enters the following mode:
> CLI (CSCF PCRF-Policy-Control Configuration Mode)
> The following commands are located in the new PCRF-Policy-Control Configuration Mode:
> [ no ] authorization mediatype { application | audio | control | data | message | others | text | video }
> end
> exit
> [ no ] signaling-bearer-loss subscription
> signaling-bearer-loss
> This command replaces the subscribe command in the CSCF Proxy-CSCF Configuration Mode. Use this command to enable subscription to Notification of Signaling Transmission Path Status, as well as IPCAN Change type notification.
> When enabled (default), the P-CSCF/A-BG sends AAR to the external PCRF via the Rx interface after UE registration. When disabled, the P-CSCF/A-BG will not subscribe to any event during Registration with PCRF and no diameter session will be established.
> CLI (CSCF PCRF-Policy-Control Configuration Mode)
> [ no ] signaling-bearer-loss subscription
> ca-certificate
> This command specifies a list of ca-certificates.
> CLI (SSL Template Configuration Mode)
> ca-certificate list name
> certificate
> This command is used to bind an X.509 trusted certificate to the SSL template.
> CLI (SSL Template Configuration Mode)
> certificate name
> cipher-suite
> This command creates a new SSL cipher suite or specifies an existing cipher suite and enters the Cipher Suite Configuration Mode.
> CLI (Context Configuration Mode)
> [ no ] cipher-suite name
> This command enters the following mode:
> CLI (Cipher Suite Configuration Mode)
> The following commands are located in the new Cipher Suite Configuration mode:
> encryption { 3des | aes-128 | null | rc4 }
> end
> exit
> hmac { sha1 }
> key-exchange { rsa }
> cipher-suites
> This command specifies a list of SSL cipher suites. Currently, the system supports only one SSL cipher suite per SSL template.
> CLI (SSL Template Configuration Mode)
> cipher-suites list name
> clear ssl statistics
> This command deletes all previously gathered SSL statistics for a specific P-CSCF service or all P-CSCF services, either system-wide or within a context.
> CLI (Exec Mode)
> clear ssl statistics [ service-name name ]
> encryption
> This command specifies the encryption algorithm for the SSL cipher suite.
> CLI (Cipher Suite Configuration Mode)
> encryption { 3des | aes-128 | null | rc4 }
> default encryption
> hmac
> This command specifies the HMAC (keyed-Hash Message Authentication Code) for the SSL cipher suite.
> The default and only currently available option is SHA-1 (Secure Hash Algorithm-1).
> CLI (Cipher Suite Configuration Mode)
> hmac { sha1 }
> default hmac
> key-exchange
> This command specifies the key exchange algorithm for the SSL cipher suite. The key exchange algorithm provides the means by which the cryptographic keys for conventional encryption and MAC calculations are exchanged.
> The default and only currently available option is RSA (Rivest, Shamir, and Adleman).
> CLI (Cipher Suite Configuration Mode)
> key-exchange { rsa }
> default key-exchange
> require cipher ssl resource-percentage
> This command assigns the 8 processing cores on the PSC2 card and splits the hardware acceleration resources between SSL protocol and IPSec protocol processing.
> CLI (Global Configuration Mode)
> require cipher ssl resource-percentage percentage_value
> default require cipher ssl resource-percentage
> show ssl cipher-suite
> This command displays information related to SSL cipher suites since the last restart or clear command. A cipher suite contains the cryptographic algorithms supported by the client.
> CLI (Exec Mode)
> show ssl cipher-suite [ name name ] [ | { grep grep_options | more } ]
> show ssl connection
> This command displays information pertaining to SSL connections on the P-CSCF.
> CLI (Exec Mode)
> show ssl connection [ list | summary [ service-name name ] ] [ name name ] [ | { grep grep_options | more } ]
> show ssl map
> This command displays information related to configured SSL maps/templates since the last restart or clear command.
> CLI (Exec Mode)
> show ssl map [ map-type ssl-subscriber-template ] [ name name ] [ | { grep grep_options | more } ]
> show ssl statistics
> This command displays statistics for SSL since the last restart or clear command.
> CLI (Exec Mode)
> show ssl statistics [ service-name name ] [ | { grep grep_options | more } ]
> ssl
> This command creates a new SSL template or specifies an existing one and enters the SSL Template Configuration Mode.
> CLI (Context Configuration Mode)
> [ no ] ssl template name { ssl-subscriber }
> This command enters the following mode:
> CLI (SSL Template Configuration Mode)
> The following commands are located in the new SSL Template Configuration mode:
> ca-certificate list name
> certificate name
> cipher-suites list name
> end
> exit
> version list { tlsv1 }
> version
> This command specifies the supported version(s) of SSL protocol on the P-CSCF/A-BG. Currently, there is only one supported version of SSL protocol, which is TLS v0.1.
> CLI (SSL Template Configuration Mode)
> version list { tlsv1 }
> default version
> SGSN Commands - New in Release 12.0
> This section provides information on new SGSN commands available in Release 12.0.
> access-restriction-data
> This new command enables the operator to assign a failure code to be included in reject messages if attach rejection is due to access restriction data (ARD) checking in incoming subscriber data (ISD) messages. As well, the operator can disable the ARD checking behavior.
> CLI (Call Control Profile Configuration Mode)
> access-restriction-data { failure-code <cause_code> | no-check }
> remove access-restriction-data failure-code
> aggregate-ipc-msg
> New command enables/disables aggregation of IPC messages in linkmgr and sessmgr.
> CLI (SGSN-Global Configuration Mode)
> aggregate-ipc-msg { linkmgr | sessmgr } { flush-frequency <frequency> | num-msgs <number_msgs> }
> default aggregate-ipc-msg { linkmgr | sessmgr }
> associate-dscp-template
> This new command in the GPRS Service configuration mode associates a specific DSCP template with a specific GPRS service configuration.
> CLI (GPRS Service Configuration Mode)
> associate-dscp-template downlink <template_name>
> no associate-dscp-template downlink
> bssgp-message
> A new command determines the SGSN response to MS-Flow-Control messages received from an unknown MS.
> CLI (SGSN Global Configuration Mode)
> bssgp-message ms-flow-control-from-unknown-ms { discard-message | send-ack | send-status }
> [default] bssgp-message ms-flow-control-from-unknown-ms
> check-zone-code
> Command enables/disables a mechanism to check zone codes.
> CLI (Call-Control Profile Configuration Mode)
> [ no | remove ] check-zone-code
> control-packet
> This command in the new DSCP template mode configure handling of downlink control packets.
> CLI (DSCP TemplateConfiguration Mode)
> control-packet qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | cs1 | cs2 | cs3 | cs4 | cs5 | cs6 | cs7 | ef }]
> default control-packet
> data-packiet
> This command in the new DSCP template mode configure handling of downlink data packets.
> CLI (DSCP TemplateConfiguration Mode)
> data-packet { background | conversational | interactive { priority1 |
> priority2 | priority3 } | streaming } qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | cs1 | cs2 | cs3 | cs4 | cs5 | cs6 | cs7 | ef }]
> default data-packet { background | conversational | interactive { priority1 | priority2 | priority3 } | streaming }
> disable-remote-restart-counter-verification
> This new command disables the SGSN's default behavior for verification of remote peer's restart counter change values.
> CLI (SGTP Service Configuration Mode)
> [ no | default ] disable-remote-restart-counter-verification
> dscp-template
> Use this new command to create or delete DSCP templates and to gain access to the new DSCP templates configuration mode. The new DSCP template mode provides commands to configure control and data-packet handling:

> l | control-packet command configures DSCP values for downlink control packets

> l | data-packet command configures DSCP values for downlink data packets

> CLI (SGSN Global Configuration Mode)
> [ no ] dscp-template <template_name> [-noconfirm]
> ggsn-fail-retry-timer
> Sets the amount of time that a GGSN will be unavailable/blacklisted.
> CLI (SGTP Service Configuration Mode)
> ggsn-fail-retry-timer <value>
> no ggsn-fail-retry-timer
> gn-delay-monitoring
> New command enables monitoring of the delay of packets over Gn/Gp between the SGSN and GGSN.
> CLI (SGTP Service Configuration Mode)
> gn-delay-monitoring [ num-delay <number_delayed> | num-no-delay-for-clear <number_normal> | tolerance-seconds <number_seconds> ]
> default gn-delay-monitoring [ num-delay | num-no-delay-for-clear | tolerance-seconds ]
> no gn-delay-monitoring
> max-remote-restart-counter-change
> This command sets a restart counter change window to avoid the resulting service deactivations and activations causing large bursts of network traffic if the restart counter change messages from the GGSN are erroneous.
> CLI (SGTP Service Configuration Mode)
> max-remote-restart-counter-change <value 1 - 255>
> default max-remote-restart-counter-change
> mtp2-max-outstand-frames
> A new command provides a new default (7) for the number of outstanding packets sent by the linkmgr and also enables the operator to configurable a specific number of outstanding packets sent by the linkmgr. These configurations are applicable for both highspeed and lowspeed narrowband links.
> CLI (Link Configuration Mode)
> mtp2-max-outstand-frames <5 - 10>
> default mtp2-max-outstand-frames
> mtp3-msg-size
> The default number (272) of outstanding packets sent by the linkmgr (MTP2), for both highspeed and lowspeed narrowband SS7 links, has been altered with the addition of this new command. As well, it is now possible to configure a preferred number of outstanding packets.
> CLI (Link Configuration Mode)
> mtp3-msg-size <1-272>
> default mtp3-msg-size
> pdp-deactivation-rate
> Set the rate at which the SGSN deactivates PDP connections per second per SessMgr when a GPT-C path failure is detected.
> CLI (SGSN-Global Configuration Mode)
> pdp-deactivation-rate { connected-ready <rate> | idle-standby <rate> }
> default pdp-deactivation-rate { connected-ready | idle-standby }
> ptmsi-signature-reallocate
> A new command enables configuration of P-TMSI signature reallocation for Attach/RAU procedures.
> CLI (SGTP Service Configuration Mode)
> ptmsi-signature-reallocate { attach | frequency <frequency> | interval <minutes> | ptmsi-reallocation-command | routing-area-update [ update-type [ combined-update | imsi-combined-update | periodic | ra-update ] } [ access-type { gprs | umts } ] [ frequency <frequency> ]
> regional-subscription-restriction
> This command enables the operator to define the cause code for subscriber rejection when it is due to regional subscription information failure.
> CLI (Call-Control Profile Configuration Mode)
> [ remove ] regional-subscription-restriction [ failure-code <code> | user-device-release { before-r99 failure-code <code> | r99-or-later failure-code <code> } ]
> relocation-alloc-timeout
> A new command defines the amount of time (in seconds) that the SGSN waits for a Relocation Request message. The range is 1 to 60 with a default of 5.
> CLI (IuPS Service Configuration Mode)
> relocation-alloc-timeout <time>
> default relocation-alloc-timeout
> sgsn retry-unavailable-ggsn
> Marks the GGSN as available for further activation.
> CLI (Exec Mode)
> sgsn retry-unavailable-ggsn <IPv4 or IPv6>
> smsc-address-restriction-list
> A new command allows the operator to restrict forwarding of SMS messages on the basis of a defined list of SMS-C addresses.
> CLI Short-Message-Service Configuration Mode
> smsc-address-restriction-list <isdn-no> +
> no smsc-address-restriction-list <isdn-no>
> IMPORTANT: The smsc-address-restriction-list command only takes effect if the smsc-address-restriction-type command has also been configured.
> target-offloading algorithm
> Configure the number of subscribers to be off-loaded.
> CLI (SGSN-Global Configuration Mode)
> target-offloading algorithm [ optimized-for-speed | optimized-for-target-count ]
> SGSN Commands - New in Release 12.1
> This section provides information on new SGSN commands available in Release 12.1.
> access-restriction-data
> This new command enables the operator to assign a failure code to be included in reject messages if attach rejection is due to access restriction data (ARD) checking in incoming subscriber data (ISD) messages. As well, the operator can disable the ARD checking behavior.
> CLI (Call Control Profile Configuration Mode)
> access-restriction-data { failure-code <cause_code> | no-check }
> remove access-restriction-data failure-code
> aggregate-ipc-msg
> New command enables/disables aggregation of IPC messages in linkmgr and sessmgr.
> CLI (SGSN-Global Configuration Mode)
> aggregate-ipc-msg { linkmgr | sessmgr } { flush-frequency <frequency> | num-msgs <number_msgs> }
> default aggregate-ipc-msg { linkmgr | sessmgr }
> bssgp-message
> A new command determines the SGSN response to MS-Flow-Control messages received from an unknown MS.
> CLI (SGSN Global Configuration Mode)
> bssgp-message ms-flow-control-from-unknown-ms { discard-message | send-ack | send-status }
> [default] bssgp-message ms-flow-control-from-unknown-ms
> check-zone-code
> Command enables/disables a mechanism to check zone codes.
> CLI (Call-Control Profile Configuration Mode)
> [ no | remove ] check-zone-code
> ggsn-fail-retry-timer
> Sets the amount of time that a GGSN will be unavailable/blacklisted.
> CLI (SGTP Service Configuration Mode)
> ggsn-fail-retry-timer <value>
> no ggsn-fail-retry-timer
> gn-delay-monitoring
> New command enables monitoring of the delay of packets over Gn/Gp between the SGSN and GGSN.
> CLI (SGTP Service Configuration Mode)
> gn-delay-monitoring [ num-delay <number_delayed> | num-no-delay-for-clear <number_normal> | tolerance-seconds <number_seconds> ]
> default gn-delay-monitoring [ num-delay | num-no-delay-for-clear | tolerance-seconds ]
> no gn-delay-monitoring
> ignore-remote-restart-counter-change
> A new command instructs the SGSN to ignore (not process) restart counters received from remote nodes. Default is to process the restart counters.
> CLI (SGTP Service Configuration Mode)
> ignore-remote-restart-counter-change
> [ default | no ] ignore-remote-restart-counter-change
> mtp2-max-outstand-frames
> A new command provides a new default (7) for the number of outstanding packets sent by the linkmgr and also enables the operator to configurable a specific number of outstanding packets sent by the linkmgr. These configurations are applicable for both highspeed and lowspeed narrowband links.
> CLI (Link Configuration Mode)
> mtp2-max-outstand-frames <5 - 10>
> default mtp2-max-outstand-frames
> mtp3-msg-size
> The default number (272) of outstanding packets sent by the linkmgr (MTP2), for both highspeed and lowspeed narrowband SS7 links, has been altered with the addition of this new command. As well, it is now possible to configure a preferred number of outstanding packets.
> CLI (Link Configuration Mode)
> mtp3-msg-size <1-272>
> default mtp3-msg-size
> ptmsi-signature-reallocate
> A new command enables configuration of P-TMSI signature reallocation for Attach/RAU procedures.
> CLI (SGTP Service Configuration Mode)
> ptmsi-signature-reallocate { attach | frequency <frequency> | interval <minutes> | ptmsi-reallocation-command | routing-area-update [ update-type [ combined-update | imsi-combined-update | periodic | ra-update ] } [ access-type { gprs | umts } ] [ frequency <frequency> ]
> regional-subscription-restriction
> This command enables the operator to define the cause code for subscriber rejection when it is due to regional subscription information failure.
> CLI (Call-Control Profile Configuration Mode)
> [ remove ] regional-subscription-restriction [ failure-code <code> | user-device-release { before-r99 failure-code <code> | r99-or-later failure-code <code> } ]
> relocation-alloc-timeout
> A new command defines the amount of time (in seconds) that the SGSN waits for a Relocation Request message. The range is 1 to 60 with a default of 5.
> CLI (IuPS Service Configuration Mode)
> relocation-alloc-timeout <time>
> default relocation-alloc-timeout
> sgsn retry-unavailable-ggsn
> Marks the GGSN as available for further activation.
> CLI (Exec Mode)
> sgsn retry-unavailable-ggsn <IPv4 or IPv6>
> smsc-address-restriction-list
> A new command allows the operator to restrict forwarding of SMS messages on the basis of a defined list of SMS-C addresses.
> CLI Short-Message-Service Configuration Mode
> smsc-address-restriction-list <isdn-no> +
> no smsc-address-restriction-list <isdn-no>
> IMPORTANT: The smsc-address-restriction-list command only takes effect if the smsc-address-restriction-type command has also been configured.
> target-offloading algorithm
> Configure the number of subscribers to be off-loaded.
> CLI (SGSN-Global Configuration Mode)
> target-offloading algorithm [ optimized-for-speed | optimized-for-target-count ]
> TPO Commands - New in Release 12.0
> This section provides information on new TPO commands available in Release 12.0.
> p2p-detected
> This command allows to disable/continue TPO optimizations when a P2P flow is detected.
> CLI (ACS TPO Profile Configuration Mode)
> p2p-detected { cease-tpo | continue-tpo }
> default p2p-detected
> tpo default-policy
> This command configures the default TPO policy for a rulebase. For subscribers using a particular rulebase, the default TPO policy configured in it will be used only if in the APN/subscriber profile no TPO policy is configured, and a policy to use is not received from the AAA.
> CLI (ACS Rulebase Configuration Mode)
> tpo default-policy tpo_policy_name
> no tpo default-policy
> tpo profile
> This command configures the TPO profile for the charging action. This enables the specified TPO profile to be applied when a flow matches the charging action.
> CLI (ACS Charging Action Configuration Mode)
> tpo profile tpo_profile_name
> no tpo profile
> Modified Configuration Commands
> This section identifies configuration commands that have been modified in:

> l | Common Commands - Modified in Release 12.0

> l | Application Detection and Control - Modified in Release 12.0

> l | Content Filtering Commands - Modified in Release 12.0

> l | ECS Commands - Modified in Release 12.0

> l | Firewall Commands - Modified in Release 12.0

> l | GGSN Commands - Modified in Release 12.0

> l | HA Commands - Modified in Release 12.0

> l | HSGW Commands - Modified in Release 12.0

> l | Mobility Management Entity Commands - Modified in Release 12.0

> l | NAT Commands - Modified in Release 12.0

> l | Packet Data Network Gateway Commands - Modified in Release 12.0

> l | PDIF Commands - Modified in Release 12.0

> l | PDSN Commands - Modified in Release 12.0

> l | Serving Gateway Commands - Modified in Release 12.0

> l | Session Control Manager Commands - Modified in Release 12.0

> l | SGSN Commands - Modified in Release 12.0

> l | SGSN Commands - New in Release 12.1

> l | TPO Commands Modified in Release 12.0

> Common Commands - Modified in Release 12.0
> This section provides information on common commands modified for Release 12.0.
> authentication
> This command configures authentication for subscribers or gateways accessing a service using the crypto template. Two new keywords and their respective supporting keywords and variables were added to the authentication command in the Crypto Template Configuration Mode: local and remote.
> CLI (Crypto Template Configuration Mode)
> authentication { eap-profile name [ second-phase eap-profile name ] | gateway { encrypted key value | key clear_text } | local { certificate | pre-shared-key { encrypted key value | key clear_text } | pre-shared-key { encrypted key value | key clear_text } | remote { certificate | eap-profile name [ second-phase eap-profile name ] | pre-shared-key { encrypted key value | key clear_text } }
> diameter dictionary
> This command configures the Diameter Credit Control dictionary for the Active Charging Service. In release 12.0, the dcca-custom21 through dcca-custom30 options were added to this command.
> CLI (Credit Control Configuration Mode)
> diameter dictionary { dcca-custom1 | dcca-custom10 | dcca-custom11 | dcca-custom12 | dcca-custom13 | dcca-custom14 | dcca-custom15 | dcca-custom16 | dcca-custom17 | dcca-custom18 | dcca-custom19 | dcca-custom2 | dcca-custom20 | dcca-custom21 | dcca-custom22 | dcca-custom23 | dcca-custom24 | dcca-custom25 | dcca-custom26 | dcca-custom27 | dcca-custom28 | dcca-custom29 | dcca-custom3 | dcca-custom30 | dcca-custom4 | dcca-custom5 | dcca-custom6 | dcca-custom7 | dcca-custom8 | dcca-custom9 | standard }
> default diameter dictionary
> ikev2-ikesa
> The allow-empty-ikesa keyword is new in the ikev2-ikesa command allowing the retention of an IKE SA even after its child SAs have been deleted.
> CLI (Crypto Template Configuration Mode)
> ikev2-ikesa { allow-empty-ikesa | keepalive-user-activity | max-retransmissions number | retransmission-timeout msec | policy error-notification [ invalid-message-id | invalid-syntax ] rekey | setup-timer sec | transform-set list name }
> ip address
> This command now allows the configuration of a 31-bit subnet mask for IPv4 addresses per RFC 3021.
> CLI (Ethernet Interface Configuration Mode)
> ip address ip_address ip_mask
> link-aggregation
> This command is used to aggregate ports on a Quad Gig-E line card (QGLC) and set related parameters. Several keywords have been added.
> CLI (Ethernet Port Configuration Mode)
> link-aggregation { distribution { block | random | rotate | simple } | lacp { active | passive } [ rate { auto | fast | slow } ] [ timeout { long | short } ] | master { global group group_number | group group_number | local group group_number } | member { global group group_number | group group_number | local group group_number } | redundancy { standard | switched } [ hold-time sec ] [ preferred slot { card_number | none } ] | toggle-link }
> no link-aggregation [ toggle-link ]
> default link-aggregation { distribution | lacp | redundancy | toggle-link }
> For link-aggregation redundancy standard mode, hold-time and preferred slot settings are now accepted and processed. Previously these setting were only observed for link-aggregation redundancy switched mode.
> match ip pool
> The keyword destination-network has been added to this command. An IP pool attached to the crypto map can have multiple IPSec tunnels according to the destination of the packet being forwarded to internet.
> CLI (Crypto Map IKEv1 Configuration Mode)
> [ no ] match ip pool pool-name pool_name[ destination-network ip_address { / mask | mask ip_mask } ]
> pending-traffic-treatment
> This command controls the pass/drop treatment of traffic while waiting for definitive credit information from the server. The limted-pass keyword was added to this command. This enables limited access for subscribers when the OCS is unreachable by provisioning a default quota to use until there is a response from the OCS.
> CLI (Credit Control Configuration Mode)
> pending-traffic-treatment { { { forced-reauth | trigger | validity-expired } drop | pass } | { { noquota | quota-exhausted } buffer | drop | limited-pass volume | pass } }
> default pending-traffic-treatment { forced-reauth | noquota | quota-exhausted | trigger | validity-expired }
> rule-variable
> This command specifies the order of fields in the EDR. The following new TPO-related fields are now supported in the EDR format:

> l | TCP flow related:

> l | tpo-enabled

> l | HTTP transaction related:

> l | ad-delivered

> l | ad-replaced

> l | compression-bytes-in

> l | compression-bytes-out

> l | dns-resolution-locally

> l | dns-resolution-remotely

> l | tpo-enabled

> CLI (ACS EDR Format Configuration Mode)
> rule-variable protocol rule priority priority [ in-quotes ]
> no rule-variable protocol rule [ priority priority ]
> use-proxy
> This command enables a Diameter proxy for the Diameter endpoint. A server-mode keyword is added in the 12.0 release to specify that the Diameter proxy should be treated as if it is the server side of the endpoint connection.
> CLI (Diameter Endpoint Configuration Mode)
> use-proxy [ server-mode [ demux-mode ] ]
> Application Detection and Control - Modified in Release 12.0
> This section provides information on ADC commands modified in Release 12.0.
> p2p-detection protocol
> This command configures the system to detect peer-to-peer (P2P) protocols. The following keywords were added to this command:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (ACS Configuration Mode)
> [ no ] p2p-detection protocol [ actsync | aimini | all | applejuice | ares | armagettron | battlefld | bittorrent | blackberry | citrix | clubpenguin | crossfire | ddlink | directconnect | dofus | edonkey | facebook | facetime | fasttrack | feidian | fiesta | filetopia | florensia | freenet | fring | funshion | gadugadu | gamekit | gnutella | gmail | gtalk | guildwars | halflife2 | hamachivpn | iax | icecast | imesh | iptv | irc | isakmp | iskoot | itunes | jabber | kontiki | manolito | maplestory | meebo | mgcp | msn | mute | myspace | nimbuzz | octoshape | off | oovoo | openft | orb | oscar | paltalk | pando | pandora | popo | pplive | ppstream | ps3 | qq | qqgame | qqlive | quake | rdp | rfactor | rmstream | secondlife | shoutcast | skinny | skype | slingbox | sopcast | soulseek | splashfighter | ssdp | stealthnet | steam | stun | teamspeak | teamviewer | thunder | tor | truphone | tvants | tvuplayer | twitter | uusee | veohtv | viber | vpnx | vtun | warcft3 | wii | winmx | winny | wmstream | wofkungfu | wofwarcraft | xbox | xdcc | yahoo | yourfreetunnel | zattoo + ]
> p2p protocol
> This command configures the system to detect specific P2P protocols for charging purposes. This release now supports the following protocols:

> l | Blackberry

> l | Gmail

> l | iTunes

> l | MySpace

> l | TeamViewer

> l | Twitter

> l | Viber

> CLI (ACS Ruledef Configuration Mode)
> [ no ] p2p protocol operator protocol
> p2p traffic-type
> This command defines rule expressions to match traffic type—audio, video, and unclassified. The following keywords were added to this command:

> l | audio

> l | video

> l | unclassified

> CLI (ACS Ruledef Configuration Mode)
> [ no ] p2p traffic-type operator traffic_type
> Content Filtering Commands - Modified in Release 12.0
> This section provides information on Content Filtering commands modified in Release 12.0.
> analyze
> This command specifies the action to take for the indicated result after content filtering analysis. The following options are additionally supported for the category keyword:

> l | BACKUP

> l | CDN

> l | PHOTO

> l | PLAG

> CLI (Content Filtering Policy Configuration Mode)
> analyze priority priority { all | category category | x-category string } action { allow | content-insert content_string | discard | redirect-url url | terminate-flow | www-reply-code-and-terminate-flow reply_code } [ edr edr_format_name ]
> ECS Commands - Modified in Release 12.0
> This section provides information on ECS commands modified in Release 12.0.
> group-of-ruledefs-application
> This command specifies the purpose of setting up a group-of-ruledefs. In support for the GX Alias feature the gx-alias keyword was added to this command. This enables to specify that a group-of-ruledefs is for Gx-alias purposes.
> CLI (ACS Group-of-Ruledefs Configuration Mode)
> group-of-ruledefs-application { charging | content-filtering | gx-alias | post-processing }
> no group-of-ruledefs-application
> insert
> This command configures the x-header fields to be inserted in HTTP/WSP GET and POST request packets. The qos and s-mcc-mnc keywords were added to this command. This enables inserting bearer QoS and serving node MCC + MNC in x-headers.
> CLI (ACS x-header Format Configuration Mode)
> insert xheader_field_name { string-constant xheader_field_value | variable { bearer { 3gpp { apn | charging-characteristics | charging-id | imei | imsi | qos | rat-type | s-mcc-mnc | sgsn-address } | acr | customer-id | ggsn-address | mdn | radius-calling-station-id | session-id | sn-rulebase | subscriber-ip-address | username } [ encrypt ] | http { host | url } }
> no insert xheader_field_name
> rule-variable
> This command configures the order of fields in the EDR. This command now enables to configure HTTP domain and WSP domain fields in the EDR. For this, from the URL, after http:// (if it is present) is removed, everything until the first “/” is used as the domain.
> CLI (ACS EDR Ruledef Configuration Mode)
> rule-variable protocol rule priority priority [ in-quotes ]
> no rule-variable protocol rule [ priority priority ]
> Firewall Commands - Modified in Release 12.0
> This section provides information on Stateful Firewall commands modified in Release 12.0.
> firewall dos-protection
> This command configures Stateful Firewall protection for subscribers from Denial-of-Service (DoS) attacks. The following keywords have been added to this command to support IPv6 firewall:
> ipv6-dst-options [ invalid-options | unknown-options ] | ipv6-extension-hdrs [ limit extension_limit ] | ipv6-frag-hdr nested-fragmentation | ipv6-hop-by-hop [ invalid-options | jumbo-payload | router-alert | unknown-options ]
> CLI (Firewall-and-NAT Policy Configuration Mode)
> [ no ] firewall dos-protection { all | flooding { icmp | tcp-syn | udp } | ftp-bounce | ip-unaligned-timestamp | ipv6-dst-options [ invalid-options | unknown-options ] | ipv6-extension-hdrs [ limit extension_limit ] | ipv6-frag-hdr nested-fragmentation | ipv6-hop-by-hop [ invalid-options | jumbo-payload | router-alert | unknown-options ] | mime-flood | port-scan | source-router | tcp-window-containment | teardrop | winnuke }
> default firewall dos-protection
> firewall ip-reassembly-failure
> This command configures Stateful Firewall action on IPv4/IPv6 packets involved in IP Reassembly Failure scenarios. In this release, support for IPv6 firewall is added.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall ip-reassembly-failure { drop | permit }
> default firewall ip-reassembly-failure
> firewall max-ip-packet-size
> This command configures the maximum IPv4/IPv6 packet size (after IP reassembly) allowed over Stateful Firewall. In this release, support for IPv6 firewall is added.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall max-ip-packet-size packet_size protocol { icmp | non-icmp }
> default firewall max-ip-packet-size protocol { icmp | non-icmp }
> firewall policy
> This command enables/disables Stateful Firewall support in a Firewall-and-NAT policy. In this release, support to enable/disable IPv4 and IPv6 firewall is added.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall policy { ipv4-and-ipv6 | ipv4-only | ipv6-only }
> { default | no } firewall policy
> ip max-fragments
> This command limits the maximum number of IPv4/IPv6 fragments per fragment chain. In this release, support for IPv6 firewall is added.
> CLI (ACS Configuration Mode)
> ip max-fragments max_fragments
> default ip max-fragments
> route priority
> This command controls routing of packets to protocol analyzers. The basic-and-advanced option is added to sip keyword for SIP packets to route through SIP analyzer and SIP ALG.
> CLI (ACS Rulebase Configuration Mode)
> route priority route_priority ruledef ruledef_name analyzer { dns | file-transfer | ftp-control | ftp-data | h323 | http | imap | mms | p2p | pop3 | pptp | rtcp | rtp | rtsp | sdp | secure-http | sip [ advanced | basic-and-advanced ] | smtp | tftp | wsp-connection-less | wsp-connection-oriented } [ description description ]
> no route priority route_priority
> GGSN Commands - Modified in Release 12.0
> This section provides information on GGSN commands modified in Release 12.0.
> virtual-apn
> Virtual APN selection is based on configuration parameters like roaming mode, bearer access service etc. Three more parameters ‘cc-profile’, ‘msisdn-range’, and ‘rat-type’ are added based on them virtual-apn will be selected. ‘CC-profile option specifies the APN for charging characteristics (CC)-profile index. The APN selection will be applied to all subscribers that have msisdn in the configured ‘msisdn-range’. The range has lower and upper limit configured as ‘from’ and ‘to’ respectively. The ‘rat-type’ option configures the APN for rat-type (gan, geran, hspa, utran, wlan) received in the message.
> Another addition is the ‘msin-range from <start_refix> to <end_prefix>’ keywords have been added to the MCC-MNC in this command to enable the IMSI prefix based prepaid/postpaid subscribers selection on GGSN. This enhancement extends the MCC+MNC based virtual APN selection to MCC+MNC+MSIN Range based virtual APN selection.
> CLI (APN Configuration Mode)
> virtual-apn { gcdr apn-name-to-be-included { gn | virtual } | preference priority apn apn_name { access-gw-address { ip_address | ip_address/mask } | bearer-access-service svc_name | cc-profile cc_profile_index | domain domain_name | mcc mcc_number mnc mnc_number { msin-range from msin_range_from to msin_range_to } | msisdn-range from msisdn_start_range to msisdn_to_range | rat-type { gan | geran | hspa | utran | wlan } | roaming-mode { home | visiting | roaming } } }
> authentication
> This command configures the APN’s authentication parameters. A new option ‘prefer-chap-pco’ has been added to be used along with msisdn-auth/imsi-auth parameter. With this option, if enabled, GGSN performs CHAP authentication if CHAP parameters are received in Protocol Configuration Options (PCO). However, chap username would be constructed as msisdn@apn / imsi@apn and chap challenge, chap response parameters should be used as it is from CHAP parameters received in PCO IE. If CHAP parameters are not received in PCO IE of CPC Request, GGSN should do normal PAP authentication with PAP username as msisdn@apn / imsi@apn (ignoring any PAP username if received).
> IMPORTANT: This change is applicable for 10.2 and above versions.
> CLI (APN Configuration Mode)
> authentication { [ msid-auth | imsi-auth [ password-use-pco | username-strip-apn | prefer-chap-pco ] | msisdn-auth [ password-use-pco | username-strip-apn | prefer-chap-pco ] | eap initial-access-request [ authenticate-authorize | authenticate-only ] | [ allow-noauth ] [ chap preference ] [ mschap preference ] [ pap preference ] }
> ip user-datagram-tos copy
> This command controls copying of IP TOS octet value from user IPv4/IPv6 datagrams to header of GTP tunnel encapsulation. Earlier the “data-tunnel” option appeared after this command, but it was removed to match with the same command in Subscriber Configuration Mode command.
> CLI (APN Configuration Mode)
> [ no | default ] ip user-datagram-tos copy
> crypto ipsec transform-set
> From the Context Configuration Mode, this command creates IPSec transform sets. A new aes-cbc-256 cipher has been added to the existing list of supported cipher options.
> CLI (Context Configuration Mode)
> [ no ] crypto ipsec transform-set transform_name [ ah { hmac { md5-96 | none | sha1-96 } { esp { hmac { { md5-96 | sha1-96 } { cipher { 3des-cbc | aes-cbc-128 | aes-cbc-256 | des-cbc } } | none } } } } ]
> sgsn mcc-mnc
> From the GGSN Service Configuration Mode, the sgsn command configures the SGSNs allowed to connect to this GGSN. A new option ‘mcc-mnc’ has been added to this command to configure the sgsn mcc-mnc to the GGSN service. This implementation gives first preference to “User Location Information” IE in Create PDP Context Request Message (to be sent to PCRF) for determining 3GPP-SGSN-MCC-MNC attribute. For backward compatibility with this old behavior, CLI controlled implementation has been done so that existing deployments are not affected with this change in behavior.
> CLI (GGSN Service Configuration Mode)
> sgsn mcc-mnc { prefer rai | prefer uli }
> default sgsn mcc-mnc
> HA Commands - Modified in Release 12.0
> This section provides information on HA commands modified in Release 12.0.
> None for this release.
> HSGW Commands - Modified in Release 12.0
> This section provides information on HSGW commands modified in Release 12.0.
> None for this release.
> Mobility Management Entity Commands - Modified in Release 12.0
> This section provides information on MME commands modified in Release 12.0.
> apn-selection-default
> The apn-selection-default command enables and configures the Default APN feature for use when the normal APN selection process fails. A new keyword, first-in-subscription, has been added in this release and specifies that the first APN in the subscription record matching the PDN type is used if the UE APN is absent and the default APN is not a match.
> CLI (APN Remap Table Configuration Mode)
> apn-selection-default { first-in-subscription | network-identifier apn_net_id [ fallback-apn apn_net_id | reject-blank-apn | require-dns-fail-wildcard | require-subscription-apn ] }
> authenticate
> The authenticate command enables authentication for a variety of procedures within services using the configure call control profile. The authentication of SMS procedures has been added in this release.
> CLI (Call Control Profile Configuration Mode)
> authenticate sms [ access-type { gprs | umts } | frequency frequency | sms-type { mo-sms | mt-sms } ]
> associate
> The associate command configures association between the MME service and other services such as the HSS peer service and the SGs service. An sctp-param-template keyword and associated variable has been added to this command. The sctp-param-template keyword allows the MME service to be associated with a configured SCTP parameter template. SCTP parameter templates are configured through the Global Configuration Mode.
> Also, the associate sgs-service command now allows the SGs context to be configured.
> CLI (MME Service Configuration Mode)
> associate { { egtp-service egtp_svc_name | hss-peer-service hss_svc_name | sctp-param-template template_name | sgs-service sgs_svc_name | sgtpc-service sgtpc_svc_name } [ context ctx_name ] | subscriber-map map_name | tai-mgmt-db database_name }
> bind s1-mme
> The bind s1-mme command connects the MME service to the S1-MME interface. In this release, the ability to configure node-to-node IP security has been added. An optional crypto template keyword and associated variable has been added to this command.
> CLI (MME Service Configuration Mode)
> bind s1-mme ipv4-address address [ ipv4-address secondary_address ] | ipv6-address address [ ipv6-address secondary_address ] } [ crypto-template name ] [ max-subscribers number ]
> IMPORTANT: Crypto templates can only be associated with IPv4 addresses on the S1-MME in this release.
> dns
> The dns command configures association between the MME service and a named context where a DNS client resides allowing for DNS queries to peer servers or other EPC entities. An peer-sgsn keyword has been added to this command. The peer-sgsn keyword allows the MME service to be associated with a context where a DNS client provides DNS queries to locate a peer SGSN.
> CLI (MME Service Configuration Mode)
> dns { peer-mme | peer-sgsn | pgw | sgw | [ context ctx_name ]
> NAT Commands - Modified in Release 12.0
> This section provides information on NAT commands modified in Release 12.0.
> firewall nat-alg
> This command enables/disables all/specified NAT Application Level Gateways (ALG). The h323 keyword is added to this command to enables/disable H23 processing.
> CLI (ACS Configuration Mode)
> [ default | no ] firewall nat-alg { all | ftp | h323 | pptp | rtsp | sip }
> route priority
> This command controls routing of packets to protocol analyzers. The h323 keyword is added to this command to route the H323 analyzer for the ruledef.
> CLI (ACS Rulebase Configuration Mode)
> route priority route_priority ruledef ruledef_name analyzer { dns | file-transfer | ftp-control | ftp-data | h323 | http | imap | mms | p2p | pop3 | pptp | rtcp | rtp | rtsp | sdp | secure-http | sip [ advanced ] | smtp | tftp | wsp-connection-less | wsp-connection-oriented } [ description description ]
> no route priority route_priority
> Packet Data Network Gateway Commands - Modified in Release 12.0
> This section provides information on P-GW commands modified in Release 12.0.
> diameter
> The keyword service-context-id has been added to this command.
> CLI (Credit Control Configuration Mode)
> diameter service-context-id service_context_id
> default diameter service-context-id
> gtpp attribute
> This command enables the specification of some of the optional fields in the CDRs that the GSN (GGSN, P-GW, or SGSN) generates and/or how the information is to be presented. Several keywords have been added.
> CLI (GTPP Server Group Configuration Mode)
> gtpp attribute { camel-info | cell-plmn-id | diagnostics | duration-ms | imei | local-record-sequence-number | msisdn | node-id-suffix STRING | plmn-id | rat | record-extensions rat | sms { destination-number | recording-entity | service-centre } } +
> default gtpp attribute { cell-plmn-id | diagnostics | duration-ms | imei | local-record-sequence-number | msisdn | plmn-id | rat | record-extensions rat | sms
> { destination-number | recording-entity | service-centre } }
> no gtpp attribute { cell-plmn-id | diagnostics | duration-ms | imei | local-record-sequence-number | msisdn | node-id-suffix | plmn-id | rat | record-extensions rat | sms { destination-number | recording-entity | service-centre } }
> insert
> Support has been added for the following charging-characteristics:

> l | Service Data Volume Limit

> l | Service Data Time Limit

> CLI (ACS x-header Format Configuration Mode)
> insert xheader_field_name { string-constant xheader_field_value | variable { bearer { 3gpp { apn | charging-characteristics | charging-id | imei | imsi | rat-type | sgsn-address } | acr | customer-id | ggsn-address | mdn | radiuscalling-station-id | session-id | sn-rulebase| subscriber-ip-address | username } [ encrypt ] | http { host | url } }
> no insert xheader_field_name
> trigger type
> Support has been added for serving-node trigger type.
> CLI (Credit Control Configuration Mode)
> [ no ] trigger type { cellid | lac | qos | rat | serving-node | sgsn } +
> default trigger type
> PDIF Commands - Modified in Release 12.0
> This section provides information on PDIF commands modified in Release 12.0.
> None for this release.
> PDSN Commands - Modified in Release 12.0
> This section provides information on PDSN commands modified in Release 12.0.
> neighbor fall-over bfd multihop
> The following keyword has been added to the command.

> l | fall-over bfd multihop

> CLI (Router bgp Mode)
> [ no ] neighbor ip_address fall-over bfd multihop
> neighbor password / encrypted password
> The following keywords have been added to the command.

> l | password

> l | encrypted password

> CLI (Router bgp Mode)
> neighbor ip_addres password password
> neighbor ip_addres encrypted password encrypted_password
> [ no ] neighbor ip_addres password
> neighbor srp-activated-soft-clear
> The following keyword has been added to the command.

> l | srp-activated-soft-clearp

> CLI (Router bgp Mode)
> [ no ] neighbor ip_address srp-activated-soft-clear
> show rp statistics pcf-summary
> The following keyword has been added to the command.

> l | pcf-summary

> CLI (Config Mode)
> show rp statistics pcf-summary
> Serving Gateway Commands - Modified in Release 12.0
> This section provides information on commands modified in Release 12.0.
> associate
> The associate command in the S-GW Service Configuration Mode is updated with the new subscriber-map keyword. This new keyword allows the S-GW service to be associated with a subscriber map configured through the LTE Policy Configuration Mode, and thus, to an operator policy.
> CLI (S-GW Service Configuration Mode)
> associate subscriber-map name
> cc
> The S-GW now supports the charging characteristics (cc) commands in the APN Profile and Call Control Profile Configuration Modes.
> CLI (APN Profile Configuration Modes)
> cc { local-value-for-scdrs behavior bit_value profile index_bit | prefer { hlr-value-for-scdrs | local-value-for-scdrs } }
> CLI (Call Control Profile Configuration Modes)
> cc { behavior-bit no-records bit_value | local-value behavior bit_value profile index_bit | prefer { hlr-value | local-value } }
> accounting context
> The S-GW now supports the accounting context command in the Call Control Profile Configuration Mode.
> CLI (S-GW Service Configuration Mode)
> accounting context ctxt_name [ gtpp group grp_name ]
> Session Control Manager Commands - Modified in Release 12.0
> This section provides information on SCM commands modified in Release 12.0.
> authorization
> This command functionality has been moved from the CSCF Proxy-CSCF Configuration Mode and expanded.
> CLI (CSCF PCRF-Policy-Control Configuration Mode)
> [ no ] authorization mediatype { application | audio | control | data | message | others | text | video }
> bind
> The keyword tls-crypto-template and its options have been added to this command.
> CLI (CSCF Service Configuration Mode)
> bind address ip_address [ cscf-hostname host_name ] [ ipsec-crypto-template template ] [ max-sessions max# ] [ port number ] [ reserved-call-capacity percentage ] [ tls-crypto-template template [ tls-port number ] ] [ transport tcp ] [ use-serviceport-towards-network ]
> no bind address
> nat-pool
> The keyword signalling-pool has been added to this command. Specifies the name of an existing IP pool from where IP addresses will be used to fill in signalling headers only.
> CLI (CSCF Service Configuration Mode)
> nat-pool name pool_name [ signalling-pool signalling_pool_name ]
> no nat-pool name pool_name
> policy
> The keyword overload and its options have been moved from the CSCF Policy Rules Configuration Mode. The keyword ibcf-capability has also been added to this command.
> CLI (CSCF Service Configuration Mode)
> policy { accounting interim-interval value | allow-early-media | ibcf-capability domain domain/name | overload [ drop | redirect IPv4_address1 [ weight weight1 ] [ IPv4_address2 [ weight weight2 ] ] ... | reject ] | threshold congestion-control { system-cpu-utilization percent | tolerance percent } }
> default policy { allow-early-media | overload | threshold congestion-control { system-cpu-utilization | tolerance } }
> no policy { accounting interim-interval | allow-early-media | ibcf-capability domain domain/name | overload [ redirect IPv4_address1 ] [ IPv4_address2 ] ... | threshold congestion-control { system-cpu-utilization | tolerance } }
> threshold
> This command enables thresholds alerting and configuration of thresholds for CSCF Service. This functionality has been moved from the Global Configuration Mode.
> CLI (CSCF Service Configuration Mode)
> threshold { { call-setup-failures | call-total-active | error-no-resource | error-presence | error-reg-auth | error-tcp | invite-rcvd-rate | reg-rcvd-rate | reg-total-active | route-failures } high_thresh [ clear low_thresh ] | monitoring }
> [ default | no ] monitoring
> timeout
> The keyword cleanup-timer has been added to this command. This timer is used to control how often to check for idle TCP connections.
> CLI (CSCF Service Configuration Mode)
> timeout { hss-wait sec | no-answer sec | policy-interface sec | sip { 3gpp-d sec | 3gpp-t1 msec | 3gpp-t2 sec | 3gpp-t4 sec | d sec | idle-tcp-connection msec [ cleanup-timer msec ] | invite-expiry sec | t1 msec | t2 sec | t4 sec } }
> default timeout { hss-wait | no-answer | policy-interface | sip { 3gpp-d | 3gpp-t1 | 3gpp-t2 | 3gpp-t4 | d | idle-tcp-connection | invite-expiry | t1 | t2 | t4 } }
> trusted-domain-entity
> The keyword private-network has been added to this command.
> CLI (CSCF Service Configuration Mode)
> trusted-domain-entity address [ foreign-network ] [ private-network ]
> no trusted-domain-entity address
> SGSN Commands - Modified in Release 12.0
> This section provides information on SGSN commands modified in Release 12.0.
> apn-selection-default
> New keyword ‘fallback-apn’ allows definition of a dummy APN to use when default APN is not available.
> CLI (APN-Remap-Table Configuration Mode)
> apn-selection-default network-identifier <apn_net_id> [ fallback-apn <apn_net_id> | reject-blank-apn | require-dns-fail-wildcard | require-subscription-apn ] }
> no apn-selection
> apn-selection-default
> Three new keywords have been added to support flexible new options for using default APNs in the APN selection process:

> l | first-in-subscription - option instructs the SGSN to use the APN in the first subscription record as a default APN.

> l | fallback-to-first-in-subscription - option instructs the SGSN to use the APN in the first subscription record when configured default APN is not available.

> l | prefer-single-subscription - option instructs the SGSN to use the APN in subscription record if it is the only record available and normal APN selection fails.

> CLI (APN-Remap-Table Configuration Mode)
> apn-selection-default { first-in-subscription | network-identifier <> [ fallback-apn network-identifier <> | fallback-to-first-in-subscription | prefer-single-subscription | reject-blank-apn | require-dns-fail-wildcard | require-subscription-apn ] }
> no apn-selection
> authenticate
> New keywords enable/disable authentication for the SMS procedure.
> CLI (Call-Control Profile Configuration Mode)
> authenticate sms [ sms-type ( mo-sms | mt-sms } ] [ frequency <frequency> | access-type { umts | gprs } ]
> no authenticate sms [ sms-type ( mo-sms | mt-sms } ] {access-type [umts/gprs]}
> default authenticate sms [ sms-type ( mo-sms | mt-sms } ] {access-type [umts/gprs]}
> bssgp-timer
> The range of the BSSGP MS flow control timer ‘th’ has been expanded (per TS 48.018) to 6 to 5999 seconds:
> CLI (SGSN-Global Configuration Mode)
> bssgp-timer th <6 to 5999>
> default bssgp-timer th
> ciphering algorithm
> New keywords - negotiation-failure-action - have been added to configure the SGSN's action if there is not a match between the MS and SGSN ciphering algorithm configurations. As well, the call Attach/RAU Rejection message may include a configurable GMM failure code.
> CLI (GPRS Service Configuration Mode)
> ciphering-algorithm { negotiation-failure-action { reject [ failure-code ] | use-geo0 } | priority <priority> }
> default ciphering-algorithm negotiation-failure-action
> dns-extn
> New keyword in the command enables the SGSN to append geographical information to the APN string that is being sent in the DNS query.
> CLI (APN-Profile Configuration Mode)
> dns-extn { lac-rac | msisdn start-offset <start_digits> end-offset <end_digits>
> dns-extn
> If the DNS is configured to support, then inclusion of two new keywords - charg-id and rnc-id - facilitate GGSN selection.
> CLI (APN-Profile Configuration Mode)
> dns-extn { charg-id { binary | decimal | hexadecimal } | lac-rac | msisdn | rnc-id [ charg-id { binary | decimal | hexadecimal } ] }
> remove dns-extn { charg-id | rnc-id [ charg-id ] }
> gateway-address
> New keyword assigns GGSN to a secondary pool of GGSNs.
> CLI (APN-Profile Configuration Mode)
> gateway-address <IPv4 or IPv6> weight <1-100> secondary-pool
> gtpc
> Configures the diffserv code point marking to be used when sending GTP-C messages originating from the session manager and SGTPC manager.
> CLI (SGTP Service Configuration Mode)
> gtpc ip qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef }
> default gtpc ip qos-dscp
> gtpp dictionary
> The custom33 keyword has been enabled to allow inclusion of the custom33 dictionary in the billing context configuration and to associate the dictionary with the GTPP server group for the billing context.
> CLI (Context Configuration Mode Commands)
> gtpp dictionary custom33
> CLI (GTPP Server Group Configuration Mode Commands)
> gtpp dictionary custom33
> gtpp storage-server local file
> New keyword "file-name-pattern" defines a pattern for the file name that will be used to match against the files to be purged.
> CLI (GTPP Server Group Configuration Mode Commands)
> gtpp storage-server local file purge-processed-files file-name-pattern <name_pattern>
> gtp send
> The rai keyword has been added to configure the SGSN to include the RAI of the SGSN in CPCQ and UPCQ messages to the GGSN.
> CLI (GTPP Server Group Configuration Mode Commands)
> gtp send { imeisv | ms-timezone | rai | rat | uli }
> [ no | remove ] gtp send rai
> hop-count
> The configurable number of hop counts for an SCCP network instance has been expanded to 15.
> CLI (SCCP-Network Configuration Mode)
> hop-count <1-15>
> imsi-range
> The description keyword has been added to the IMSI range configuration to clarify use of the ranges when Release 9.0 Operator Policy configurations are converted for use with the Operator Policy functionality of Release 12.0.
> CLI (SGSN-Global Configuration Mode Commands)
> imsi-range mcc <mcc> mnc <mnc> msin first <msin> last <msin> operator-policy <policy_name> description <description>
> link-aggregation redundancy
> New keywords enable the operator to provision port link aggregation across multiple side-by-side XGLCs -- horizontal link aggregation.
> CLI (Port Ethernet Configuration Mode Commands)
> link-aggregation redundancy { standard | switched } [ hold-time <seconds> ] [ preferred slot { none | <slot#>} ]
> link id <id> link-type {highspeed-narrowband | lowspeed-narrowband}
> Ranges and defaults for various MTP2 timers have been modified for ANSI and ITU variants for both SS7 lowspeed-narrowband and SS7 highspeed-narrowband links.
> CLI (Link Configuration Mode Commands)
> Lowspeed, ITU and ANSI; new defaults below:

> l | mtp2-tmr-t1 - ITU default value is 40s and ANSI default value is 13s

> l | mtp2-tmr-t2 - ITU default value is 5s, ANSI default value is 11.5s

> l | mtp2-tmr-t3 - ITU default value is 1.5s, ANSI default value is 11.5s

> l | mtp2-tmr-t4e - ITU default value is 500ms, ANSI default value is 600ms

> l | mtp2-tmr-t4n - ITU default value is 8.2s, ANSI default value is 2.3s

> Lowspeed, ITU and ANSI; new ranges below:

> l | mtp2-tmr-t1 - ITU & ANSI ranges are 120 - 500

> l | mtp2-tmr-t3 - ITU & ANSI ranges are 10 - 140

> l | mtp2-tmr-t4n - ITU & ANSI ranges are 20 - 95

> l | mtp2-tmr-t6 - ITU & ANSI ranges are 10 - 60

> Highspeed, ITU and ANSI; new defaults below:

> l | mtp2-tmr-t1 - ITU default value is 300s and ANSI default value is 170s

> l | mtp2-tmr-t2 - ITU default value is 5s, ANSI default value is 23s

> l | mtp2-tmr-t3 - ITU default value is 1.5s, ANSI default value is 11.5s

> l | mtp2-tmr-t4e - ITU default value is 500ms, ANSI default value is 5s

> Highspeed, ITU and ANSI; new ranges below:

> l | mtp2-tmr-t1 - ITU & ANSI ranges are 160 - 3500

> l | mtp2-tmr-t2 - ITU & ANSI ranges are 50 - 1500

> l | mtp2-tmr-t3 - ITU & ANSI ranges are 10 - 140

> l | mtp2-tmr-t4e - ITU & ANSI ranges are 4 - 60

> l | mtp2-tmr-t6 - ITU & ANSI ranges are 10 - 60

> network-initiated-pdp-activation
> In support of NRPCA, new keywords identify a predefined location area code list and define a GTPP failure cause code for inclusion in activation Reject messages.
> CLI (Call-Control Profile Configuration Mode)
> network-initiated-pdp-activation { allow { primary | secondary } | restrict { primary | secondary } } access type { gprs | umts } { all | location-area-list instance <instance> } failure-code <code>
> qos class
> New mbr-map-down and mbr-map-up keywords enable override mapping to replace a maximum bit rate (MBR) received from the HLR with locally configured MBR.
> CLI (APN-Profile Configuration Mode)
> qos class { background | conversational | interactive | streaming } [ mbr-map-down from from_kbps to to_kbps | mbr-map-up from from_kbps to to_kbps ]
> qos class
> The following keywords have been removed from the command:

> l | default

> l | no

> The following keywords have been added to the command:

> l | all-values

> l | arp

> l | mbr-map-down

> l | mbr-map-up

> l | thp

> l | remove

> CLI (APN-Profile Configuration Mode)
> [ remove ] qos class { background | conversational | interactive | streaming } [ all-values | arp | gbr-down | gbr-up | mbr-down | mbr-map-down | mbr-map-up | mbr-up | min-transfer-delay | residual-bit-error-rate | sdu | thp ]
> sctp-rto-min / sctp-sack-period
> Include this keyword with the following commands in the PSP configuration mode. Enter it before entering a value. This enables configuration with finer granuality - in 10 millisecond units.
> CLI (PSP Configuration Mode)
> sctp-rto-min units-10ms <1-500>
> sctp-sack-period units-10ms <1-500>
> sgsn offload
> Enable targeting an SGSN for offloading.
> CLI (Exec Mode)
> sgsn offload [ gprs-service srvc_name | sgsn-service srvc_name } srvc_name { activating | connecting [ nri-value <nri_value> | stop [ target-nri <target_nri> target-count <target_count> ] | t3312-timeout <seconds> [ target-nri <target_nri> target-count <target_count>] | target-nri <target_nri> target-count <target_count> }
> service timers changed
> Four timers have had changes to their ranges and two timers have had changes to their defaults:
> CLI (IuPS Service Configuration Mode)

> l | • reset ack-timeout range has been expanded from 5 - 10 to 5 - 60 seconds. Default has increased to 20 seconds.

> l | • reset guard-timeout range has been expanded from 5 - 10 to 5 - 60 seconds.

> l | • tigoc-timeout range has been expanded from 1 - 10 to 1 - 60 seconds

> l | • tintc-timeout range has been expanded from 1 - 10 to 1 - 60 seconds and the default has been increased to 30 seconds.

> sndcp reassembly-timeout
> The default (now 30 seconds) and maximum range of seconds (now 1 to 300) configurable for the SNDCP reassembly timer have been changed to facilitate support for the reordering of sub-network dependent convergence protocol N-PDU segments that arrive out-of-order.
> CLI (GPRS Service Configuration Mode)
> sndcp reassembly-timeout seconds
> default sndcp reassembly-timeout
> SGSN Commands - Modified in Release 12.1
> This section provides information on SGSN commands modified in Release 12.1.
> apn-selection-default
> New keyword ‘fallback-apn’ allows definition of a dummy APN to use when default APN is not available.
> CLI (APN-Remap-Table Configuration Mode)
> apn-selection-default network-identifier <apn_net_id> [ fallback-apn <apn_net_id> | reject-blank-apn | require-dns-fail-wildcard | require-subscription-apn ] }
> no apn-selection
> apn-selection-default
> Three new keywords have been added to support flexible new options for using default APNs in the APN selection process:

> l | first-in-subscription - option instructs the SGSN to use the APN in the first subscription record as a default APN.

> l | fallback-to-first-in-subscription - option instructs the SGSN to use the APN in the first subscription record when configured default APN is not available.

> l | prefer-single-subscription - option instructs the SGSN to use the APN in subscription record if it is the only record available and normal APN selection fails.

> CLI (APN-Remap-Table Configuration Mode)
> apn-selection-default { first-in-subscription | network-identifier <> [ fallback-apn network-identifier <> | fallback-to-first-in-subscription | prefer-single-subscription | reject-blank-apn | require-dns-fail-wildcard | require-subscription-apn ] }
> no apn-selection
> authenticate
> New keywords enable/disable authentication for the SMS procedure.
> CLI (Call-Control Profile Configuration Mode)
> authenticate sms [ sms-type ( mo-sms | mt-sms } ] [ frequency <frequency> | access-type { umts | gprs } ]
> no authenticate sms [ sms-type ( mo-sms | mt-sms } ] {access-type [umts/gprs]}
> default authenticate sms [ sms-type ( mo-sms | mt-sms } ] {access-type [umts/gprs]}
> bssgp-timer
> The range of the BSSGP MS flow control timer ‘th’ has been expanded (per TS 48.018) to 6 to 5999 seconds:
> CLI (SGSN-Global Configuration Mode)
> bssgp-timer th <6 to 5999>
> default bssgp-timer th
> ciphering algorithm
> New keywords - negotiation-failure-action - have been added to configure the SGSN's action if there is not a match between the MS and SGSN ciphering algorithm configurations. As well, the call Attach/RAU Rejection message may include a configurable GMM failure code.
> CLI (GPRS Service Configuration Mode)
> ciphering-algorithm { negotiation-failure-action { reject [ failure-code ] | use-geo0 } | priority <priority> }
> default ciphering-algorithm negotiation-failure-action
> dns-extn
> New keyword in the command enables the SGSN to append geographical information to the APN string that is being sent in the DNS query.
> CLI (APN-Profile Configuration Mode)
> dns-extn { lac-rac | msisdn start-offset <start_digits> end-offset <end_digits>
> gateway-address
> New keyword assigns GGSN to a secondary pool of GGSNs.
> CLI (APN-Profile Configuration Mode)
> gateway-address <IPv4 or IPv6> weight <1-100> secondary-pool
> gtpc
> Configures the diffserv code point marking to be used when sending GTP-C messages originating from the session manager and SGTPC manager.
> CLI (SGTP Service Configuration Mode)
> gtpc ip qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef }
> default gtpc ip qos-dscp
> gtpp dictionary
> The custom33 keyword has been enabled to allow inclusion of the custom33 dictionary in the billing context configuration and to associate the dictionary with the GTPP server group for the billing context.
> CLI (Context Configuration Mode Commands)
> gtpp dictionary custom33
> CLI (GTPP Server Group Configuration Mode Commands)
> gtpp dictionary custom33
> gtpp storage-server local file
> New keyword "file-name-pattern" defines a pattern for the file name that will be used to match against the files to be purged.
> CLI (GTPP Server Group Configuration Mode Commands)
> gtpp storage-server local file purge-processed-files file-name-pattern <name_pattern>
> gtp send
> The rai keyword has been added to configure the SGSN to include the RAI of the SGSN in CPCQ and UPCQ messages to the GGSN.
> CLI (GTPP Server Group Configuration Mode Commands)
> gtp send { imeisv | ms-timezone | rai | rat | uli }
> [ no | remove ] gtp send rai
> hop-count
> The configurable number of hop counts for an SCCP network instance has been expanded to 15.
> CLI (SCCP-Network Configuration Mode)
> hop-count <1-15>
> imsi-range
> The description keyword has been added to the IMSI range configuration to clarify use of the ranges when Release 9.0 Operator Policy configurations are converted for use with the Operator Policy functionality of Release 12.0.
> CLI (SGSN-Global Configuration Mode Commands)
> imsi-range mcc <mcc> mnc <mnc> msin first <msin> last <msin> operator-policy <policy_name> description <description>
> link-aggregation redundancy
> New keywords enable the operator to provision port link aggregation across multiple side-by-side XGLCs -- horizontal link aggregation.
> CLI (Port Ethernet Configuration Mode Commands)
> link-aggregation redundancy { standard | switched } [ hold-time <seconds> ] [ preferred slot { none | <slot#>} ]
> link id <id> link-type {highspeed-narrowband | lowspeed-narrowband}
> Ranges and defaults for various MTP2 timers have been modified for ANSI and ITU variants for both SS7 lowspeed-narrowband and SS7 highspeed-narrowband links.
> CLI (Link Configuration Mode Commands)
> Lowspeed, ITU and ANSI; new defaults below:

> l | mtp2-tmr-t1 - ITU default value is 40s and ANSI default value is 13s

> l | mtp2-tmr-t2 - ITU default value is 5s, ANSI default value is 11.5s

> l | mtp2-tmr-t3 - ITU default value is 1.5s, ANSI default value is 11.5s

> l | mtp2-tmr-t4e - ITU default value is 500ms, ANSI default value is 600ms

> l | mtp2-tmr-t4n - ITU default value is 8.2s, ANSI default value is 2.3s

> Lowspeed, ITU and ANSI; new ranges below:

> l | mtp2-tmr-t1 - ITU & ANSI ranges are 120 - 500

> l | mtp2-tmr-t3 - ITU & ANSI ranges are 10 - 140

> l | mtp2-tmr-t4n - ITU & ANSI ranges are 20 - 95

> l | mtp2-tmr-t6 - ITU & ANSI ranges are 10 - 60

> Highspeed, ITU and ANSI; new defaults below:

> l | mtp2-tmr-t1 - ITU default value is 300s and ANSI default value is 170s

> l | mtp2-tmr-t2 - ITU default value is 5s, ANSI default value is 23s

> l | mtp2-tmr-t3 - ITU default value is 1.5s, ANSI default value is 11.5s

> l | mtp2-tmr-t4e - ITU default value is 500ms, ANSI default value is 5s

> Highspeed, ITU and ANSI; new ranges below:

> l | mtp2-tmr-t1 - ITU & ANSI ranges are 160 - 3500

> l | mtp2-tmr-t2 - ITU & ANSI ranges are 50 - 1500

> l | mtp2-tmr-t3 - ITU & ANSI ranges are 10 - 140

> l | mtp2-tmr-t4e - ITU & ANSI ranges are 4 - 60

> l | mtp2-tmr-t6 - ITU & ANSI ranges are 10 - 60

> network-initiated-pdp-activation
> In support of NRPCA, new keywords identify a predefined location area code list and define a GTPP failure cause code for inclusion in activation Reject messages.
> CLI (Call-Control Profile Configuration Mode)
> network-initiated-pdp-activation { allow { primary | secondary } | restrict { primary | secondary } } access type { gprs | umts } { all | location-area-list instance <instance> } failure-code <code>
> qos class
> New mbr-map-down and mbr-map-up keywords enable override mapping to replace a maximum bit rate (MBR) received from the HLR with locally configured MBR.
> CLI (APN-Profile Configuration Mode)
> qos class { background | conversational | interactive | streaming } [ mbr-map-down from from_kbps to to_kbps | mbr-map-up from from_kbps to to_kbps ]
> qos class
> The following keywords have been removed from the command:

> l | default

> l | no

> The following keywords have been added to the command:

> l | all-values

> l | arp

> l | mbr-map-down

> l | mbr-map-up

> l | thp

> l | remove

> CLI (APN-Profile Configuration Mode)
> [ remove ] qos class { background | conversational | interactive | streaming } [ all-values | arp | gbr-down | gbr-up | mbr-down | mbr-map-down | mbr-map-up | mbr-up | min-transfer-delay | residual-bit-error-rate | sdu | thp ]
> sctp-rto-min / sctp-sack-period
> Include this keyword with the following commands in the PSP configuration mode. Enter it before entering a value. This enables configuration with finer granuality - in 10 millisecond units.
> CLI (PSP Configuration Mode)
> sctp-rto-min units-10ms <1-500>
> sctp-sack-period units-10ms <1-500>
> sgsn offload
> Enable targeting an SGSN for offloading.
> CLI (Exec Mode)
> sgsn offload [ gprs-service srvc_name | sgsn-service srvc_name } srvc_name { activating | connecting [ nri-value <nri_value> | stop [ target-nri <target_nri> target-count <target_count> ] | t3312-timeout <seconds> [ target-nri <target_nri> target-count <target_count>] | target-nri <target_nri> target-count <target_count> }
> service timers changed
> Four timers have had changes to their ranges and two timers have had changes to their defaults:
> CLI (IuPS Service Configuration Mode)

> l | • reset ack-timeout range has been expanded from 5 - 10 to 5 - 60 seconds. Default has increased to 20 seconds.

> l | • reset guard-timeout range has been expanded from 5 - 10 to 5 - 60 seconds.

> l | • tigoc-timeout range has been expanded from 1 - 10 to 1 - 60 seconds

> l | • tintc-timeout range has been expanded from 1 - 10 to 1 - 60 seconds and the default has been increased to 30 seconds.

> sndcp reassembly-timeout
> The default (now 30 seconds) and maximum range of seconds (now 1 to 300) configurable for the SNDCP reassembly timer have been changed to facilitate support for the reordering of sub-network dependent convergence protocol N-PDU segments that arrive out-of-order.
> CLI (GPRS Service Configuration Mode)
> sndcp reassembly-timeout seconds
> default sndcp reassembly-timeout
> TPO Commands Modified in Release 12.0
> This section provides information on TPO commands modified in release 12.0.
> tcp fast-retransmit-dupacks
> This command specifies the number of duplicate ACKs required for fast retransmission. The dynamic keyword was added to this command. This enables to dynamically change the number of duplicate ACKs required for fast retransmission based on the number of in-flight packets (one-third of the in-flight packets, subject to a minimum of two). This enables to eliminate spurious retransmissions when packet reordering in the network is high.
> CLI (ACS TPO Profile Configuration Mode)
> tcp fast-retransmit-dupacks { duplicate_acks | dynamic }
> default tcp fast-retransmit-dupacks
> Obsoleted Commands
> This section identifies configuration commands that have been obsoleted in:

> l | Common Commands - Obsoleted in Release 12.0

> l | Application Detection and Control Commands - Obsoleted in Release 12.0

> l | Content Filtering Commands - Obsoleted in Release 12.0

> l | ECS Commands - Obsoleted in Release 12.0

> l | Firewall Commands - Obsoleted in Release 12.0

> l | GGSN Commands - Obsoleted in Release 12.0

> l | HA Commands - Obsoleted in Release 12.0

> l | Mobility Management Entity Commands - Obsoleted in Release 12.0

> l | PDSN Commands - Obsoleted in Release 12.0

> l | Session Control Manager Commands - Obsoleted in Release 12.0

> l | SGSN Commands - Obsoleted in Release 12.0

> Common Commands - Obsoleted in Release 12.0
> This section provides information on commands that are common to all products that were obsoleted in Release 12.0.
> None for this release.
> Application Detection and Control Commands - Obsoleted in Release 12.0
> This section provides information on new ADC commands available in Release 12.0.
> None for this release.
> Content Filtering Commands - Obsoleted in Release 12.0
> This section provides information on CF commands that were obsoleted in Release 12.0.
> None for this release.
> ECS Commands - Obsoleted in Release 12.0
> This section provides information on ECS commands that were obsoleted in Release 12.0.
> None for this release.
> Firewall Commands - Obsoleted in Release 12.0
> This section provides information on Stateful Firewall commands that were obsoleted in Release 12.0.
> None for this release.
> GGSN Commands - Obsoleted in Release 12.0
> This section provides information on GGSN commands that were obsoleted in Release 12.0.
> gtpu echo interval
> This command has been obsoleted in 12.0 release and now available in GTP-U service configuration mode.
> CLI (GGSN Service Configuration mode))
> gtpu echo-interval time_interval
> no gtpu echo-interval
> gtpu reorder
> This command has been obsoleted in 12.0 release.
> CLI (GGSN Service Configuration mode))
> gtpu reorder { context { ppp } | sequence-numbers { ipv4 | ppp | ipv4-ppp | ppp-ipv4 } | timeout time }
> [ no ] gtpu reorder { context | sequence-numbers { ipv4 | ppp | ipv4-ppp | ppp-ipv4 } }
> gtpu udp-checksum insert
> This command has been obsoleted in 12.0 release.
> CLI (GGSN Service Configuration mode))
> [ default | no ] gtpu udp-checksum insert
> HA Commands - Obsoleted in Release 12.0
> This section provides information on HA commands that were obsoleted in Release 12.0.
> None for this release.
> Mobility Management Entity Commands - Obsoleted in Release 12.0
> This section provides information on MME commands that were obsoleted in Release 12.0.
> mme-policy
> This command has been removed from the 12.0 release and replaced with the lte-policy command.
> CLI (Global Configuration Mode)
> mme-policy
> PDSN Commands - Obsoleted in Release 12.0
> This section provides information on PDSN commands that were obsoleted in Release 12.0.
> None for this release.
> Session Control Manager Commands - Obsoleted in Release 12.0
> This section provides information on SCM commands that were obsoleted in Release 12.0.
> authorization
> This command functionality has been moved to the CSCF PCRF-Policy-Control Configuration Mode and expanded.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> [ no ] authorization non-video
> policy
> This command functionality has been moved to the CSCF Service Configuration Mode and expanded.
> CLI (CSCF Policy Rules Configuration Mode)
> policy overload { redirect address1 [ weight weight1 ] [ address2 [ weight
> weight2 ] ] ... | reject [ use-reject-code { admin-prohibited | insufficient-resources } ] }
> default policy overload
> no policy overload redirect address1 [ address2 ] ...
> subscribe
> This command has been removed from the 12.0 release and replaced with the signaling-bearer-loss command in the CSCF PCRF-Policy-Control Configuration Mode.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> [ no ] subscribe signaling-bearer-loss
> SGSN Commands - Obsoleted in Release 12.0
> This section provides information on SGSN commands that were obsoleted in Release 12.0.
> ignore-remote-restart-counter
> This command, in the SGTP Service configuration mode, has been deprecated because the default behavior has been modified so that the SGSN verifies the remote restart counter changes observed in the PDP establishment messages and to ensure no mistaken configuration leads to genuine GGSN restarts being ignored. For information about the behavioral change, see the New Features section.
> GTPP Storage Server (GSS)
> This section provides information on GSS changes in Release 12.0.
> None for this release.
> This section provides information on GSS changes in Release 12.1
> None for this release.
> Web Element Manager Changes
> This section provides information on Web Element Manager changes in Release 12.0.
> This section provides information on Web Element Manager changes in Release 12.1.
> None for these releases.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883