> ASN QoS Descriptor Configuration Mode Commands
> Use the ASN QoS Descriptor Configuration mode to create and manage the Quality of Service Descriptor table for ASN GW service subscribers.
> dscp
> Use this command for DSCP marking of IP packets received on the ASNGW on a service flow basis.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> dscp [ be | af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | cs1 | cs2 | cs3 | cs4 | cs5 | cs6 | cs7 | ef ]
> be
> Best effort. This is the default.
> af11 through af43
> Specifies that the DSCP marking is AFnn.
> ef
> Specifies that the DSCP marking is EF.
> Usage
> DSCP marking can be done via AAA or the CLI. From the AAA, it is received as part of the QoS descriptor. In the CLI, the DSCP value is configured as part of the asn-qos-descriptor.
> Example
> The following example shows the inclusion of DSCP marking in the command.
> asn-qos-descriptor id 100 dscp af21
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> global-service-class-name
> Use this command to configure the global service class name within a QoS descriptor table.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> global-service-class-name svc_class_name
> no global-service-class-name
> no
> Deletes the configured global service class name from this QoS descriptor table.
> svc_class_name
> Specifies the global service class name in QoS descriptor table.
> svc_class_name must be an ASCII string of 6 characters in length.
> Usage
> Use this command to specify the global service class name (as per IEEE 802.16e standard) within a QoS descriptor table for an ASN GW service.
> The global service class name is similar in function to the Service Class Name except that (1) it may not be modified by a BS, (2) it remains consistent among all BSs, and 3) it is based on a rules-based naming system and contains referential QoS parameter codes.
> Example
> The following command specifies the global service class name g_svc1 in an ASN QoS descriptor table:
> global-service-class-name g_svc1
> schedule-type
> Use this command to configure the type of data delivery service identifier/type for an ASN GW service.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> schedule-type be [ max-sustained-traffic-rate max_sust_traffic_rate | traffic-priority priority_value ] +
> schedule-type ert-vr min-reserved-traffic-rate min_resd_traffic_rate max-latency dur_ms unsolicited-grant-interval dur_ms [ max-sustained-traffic-rate max_sust_traffic_rate | max-traffic-burst burst_size | tolerated-jitter dur_ms | traffic-priority priority_value ] +
> schedule-type nrt-vr min-reserved-traffic-rate min_resd_traffic_rate [ max-sustained-traffic-rate max_sust_traffic_rate | max-traffic-burst burst_size | traffic-priority priority_value ] +
> schedule-type rt-vr min-reserved-traffic-rate min_resd_traffic_rate max-latency dur_ms unsolicited-polling-interval dur_ms [ max-sustained-traffic-rate max_sust_traffic_rate | max-traffic-burst burst_size | traffic-priority priority_value ] +
> schedule-type ugs max-sustained-traffic-rate max-latency max-latency dur_ms unsolicited-grant-interval dur_ms [ sdu-size sdu_size | tolerated-jitter dur_ms | traffic-priority priority_value | min-reserved-traffic-rate min-latency ] +
> default schedule-type
> default
> Configures the data delivery service type to Best Effort (BE) service for a specific ASN GW service.
> be
> Configures the data delivery service type to Best Effort (BE) service for a specific ASN GW service.
> ert-vr
> Configures the data delivery service type to Extended Real-Time Variable Rate (ERT-VR) service for a specific ASN GW service.
> nrt-vr
> Configures the data delivery service type to Non-Real-Time Variable Rate (NRT-VR) service for specific ASN GW service.
> rt-vr
> Configures the data delivery service type to Real-Time Variable Rate (RT-VR) service for a specific ASN GW service.
> ugs
> Configures the data delivery service type to Unsolicited Grant Service (UGS) for a specific ASN GW service.
> max-sustained-traffic-rate max_resd_traffic_rate
> Specifies the maximum sustained traffic rate in bits per second, reserved for a service flow.
> For dur_ms, specify an integer between 0 and 65535. Maximum latency set to zero means no commitment is available for this service flow.
> max-latency dur_ms
> Specifies the maximum interval in milliseconds between the receipt of a packet to a BS or an SS on its network interface/Convergence Sublayer (CS), and the arrival of a packet to its RF interface or the peer device. This value represents a service commitment.
> For dur_ms, specify an integer between 0 and 65535. Maximum latency set to zero means no commitment is available for this service flow.
> min-reserved-traffic-rate min_resd_traffic_rate
> Default: 0 (disabled)
> Specifies the minimum traffic rates in bits per second, reserved for a service flow.
> min_resd_traffic_rate must be an integer between 0 and 65535. A minimum reserved traffic rate set to zero means no minimum traffic rate reservation is required for this service flow.
> max-sustained-traffic-rate max_sust_traffic_rate
> Configures the maximum sustained traffic rate in bits per second for traffic schedule.
> traffic_rate must be an integer between 1 and 65535.
> max-traffic-burst burst_size
> Default: 0 (disabled)
> Specifies the maximum burst size in bits that must be maintained for the service.
> For burst_size, specify an integer between 0 and 65535. A maximum traffic burst set to zero means no maximum traffic burst reservation is required for this service flow.
> sdu-size sdu_size
> Default: 49
> Specifies the length of the Service Data Unit (SDU) in bytes for a fixed-length SDU service flow.
> sdu_size must be an integer between 1 and 65535.
> Important: Use this parameter only if packing is on and the service flow is carrying fixed-length SDUs.
> tolerated-jitter dur_ms
> Specifies the maximum delay variation (jitter) allowed for the connection.
> dur_ms must be an integer between 1 and 65535.
> traffic-priority priority_value
> Default: 0 (disabled)
> This optional keyword specifies the traffic priority.
> priority_value must be an integer from 0 to 7.
> unsolicited-grant-interval dur_ms
> Specifies the nominal interval in millisecond between successive data grant opportunities for this service flow.
> dur_ms must be an integer value between 1 and 65535.
> unsolicited-polling-interval dur_ms
> Specifies the maximum nominal interval in millisecond between successive polling grants opportunities for this service flow.
> dur_ms must be an integer between 1 and 65535.
> Usage
> Use this command to configure type of data delivery service identifier within ASN GW service.
> Important: Only one data delivery service type, be, ert-vr, rt-vr, nrt-vr, or ugs is allowed within an ASN GW service.
> Example
> The following command configures the data delivery service type to Best Efforts (BE) service for an ASN GW service:
> default schedule-type
> service-class-name
> Use this command to configure the Service Class Name name within a specific QoS descriptor table.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> service-class-name svc_class_name
> no service-class-name
> no
> Deletes the configured global service class name from this QoS descriptor table.
> svc_class_name
> Specifies the service class name in QoS descriptor table.
> svc_class_name must be an ASCII string of from 2 through 128 characters.
> Usage
> A service class name is a group of QoS parameters defined at the BS that can be referenced by a service flow to apply certain QoS parameters. Use this command to specify a service class name (per IEEE 802.16 standard) within a specific QoS descriptor table for an ASN GW service
> Example
> The following command specifies the service class name ASN_Serv_class1 in a ASN QoS descriptor table:
> service-class-name ASN_Serv_class1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883