> VLAN Configuration Mode Commands
> The VLAN Configuration Mode is used to create and manage Virtual LANs and their bindings between contexts.
> bind interface
> Configures a virtual interface to context association for the current VLAN.
> Product
> PDSN, HA, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> bind interface interface_name context_name
> no bind interface interface_name context_name
> no
> Indicates the binding between the virtual interface specified and the context specified is to be unbound for the current VLAN.
> interface_name
> Specifies the name of the virtual interface to be bound to the context. interface_name must be from 1 to 79 alphanumeric characters.
> context_name
> Specifies the name of the context to be bound to the virtual interface. context_name must refer to a previously configured context.
> Usage
> Bind a virtual interface and context to allow the VLAN to provide service.
> Example
> bind interface sampleVirtual sampleContext
> no bind interface sampleVirtual sampleContext
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> ingress-mode
> This command toggles between enabling and disabling the port ingress mode.
> Product
> PDSN, HA, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ingress-mode
> Usage
> Use this command to enable or disable the ingress mode for the port.
> Example
> ingress-mode
> shutdown
> Disables/enables traffic over the current VLAN.
> Product
> PDSN, HA
> Privilege
> Security Administrator, Administrator
> Syntax
> shutdown
> no shutdown
> no
> Enables the VLAN. When omitted the VLAN is shutdown.
> Usage
> Shut down a VLAN.
> This command is necessary to bring a VLAN into service by enabling it via the no keyword.
> Example
> To disable a VLAN from sending or receiving network traffic use the following command:
> shutdown
> To enable a VLAN use the following command:
> no shutdown
> vlan-map
> This command sets a single next-hop IP address so that multiple vlans can use a single next-hop gateway. vlan-map is associated with a specific interface.
> Product
> PDSN, HA, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> vlan-map next-hop ip_address
> next-hop ip_address
> This keyword defines an IP address for the next-hop gateway.
> ip_address: Can be either an IPv4 or IPv6 address in standard format.
> Usage
> Use vlan-map to combine multiple vlan links to go through a single IP address. This feature is used in conjunction with nexthop forwarding and overlapping IP pools.
> After configuring the vlan-map, move to the Port Ethernet configuration mode to attach the vlan-map to a specific vlan.
> Example
> The following command sets an IPv4 for a next-hop gateway.
> vlan-map next-hop 123.123.123.1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883