> EAP Authentication Configuration Mode Commands
> The EAP Authentication Configuration Mode is used to configure the EAP authentication methods for the crypto template.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> eap-aka
> Configures shared key values for the EAP-AKA authentication method used by subscribers using this crypto template.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> eap-aka { encrypted key hex | key hex }
> encrypted key hex
> Specifies that the shared key is to be encrypted. hex must be a 16-character alpha and/or numeric string or a hexadecimal number beginning with “0x”.
> key hex
> Specifies that the shared key is to be transmitted in clear text. hex must be a 16-character alpha and/or numeric string or a hexadecimal number beginning with “0x”.
> Usage
> Use this command to set shared key parameters for subscribers using the EAP-AKA authentication method.
> Example
> The following command configures a clear-text shared key value for the EAP-AKA method:
> eap-aka key aa11223344556677
> eap-gtc
> Configures shared key values for the EAP-GTC authentication method used by subscribers using this crypto template.
> Product
> PDIF, ASN GW
> Privilege
> Security Administrator, Administrator
> Syntax
> eap-gtc { encrypted key value | key value }
> encrypted key value
> Specifies that the shared key is to be encrypted. value must be a 16-character alpha and/or numeric string.
> key value
> Specifies that the shared key is to be transmitted in clear text. value must be a 16-character alpha and/or numeric string.
> Usage
> Use this command to set shared key parameters for subscribers using the EAP-GTC authentication method.
> Example
> The following command configures a clear-text shared key value for the EAP-GTC method:
> eap-GTC key aa11223344556677
> eap-md5
> Configures shared key values for the EAP-MD5 authentication method used by subscribers using this crypto template.
> Product
> PDIF, ASN GW
> Privilege
> Security Administrator, Administrator
> Syntax
> eap-md5 { encrypted key value | key value }
> encrypted key value
> Specifies that the shared key is to be encrypted. value must be a 16-character alpha and/or numeric string.
> key value
> Specifies that the shared key is to be transmitted in clear text. value must be a 16-character alpha and/or numeric string.
> Usage
> Use this command to set shared key parameters for subscribers using the EAP-MD5 authentication method.
> Example
> The following command configures a clear-text shared key value for the EAP-MD5 method:
> eap-md5 key aa11223344556677
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec Mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the previous mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883