> Network Service Virtual Connection Configuration Mode Commands
> The Network Service Virtual Connection (NSVC) configuration mode is a sub-mode of the Network Service Entity (NSE) - Peer NSEI (for Frame Relay) configuration mode. The NSVC sub-mode creates a configuration instance for a specific NSVC, within the Gb interface, between a BSS and an SGSN in a 2.5G GPRSFrame Relay network connection.
> Upon accessing this mode, the prompt will appear similar to:
> [local]hostname(nse-fr-peer-nsei-<nse_id>-nsvci-<nsvc_id>)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the previous configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the network service entity - frame relay configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883