> show ipv6
> This chapter describes the outputs of the show ipv6 command.
> show ipv6 interface summary
> show ipv6 interface summary Command Output Descriptions

> Field | Description
> Intf name | Interface name
> Intf Type | Interface type
> Description
> Router Advertisement | Displays whether the system is sending router advertisements. Options are either enabled or disabled.
> IP State | Displays the IP state (UP/DOWN) and binding detail
> MTU | The subscriber’s maximum transmission unit (MTU) size in octets.
> IPv6 Link-Local Address: | Displays the IPv6 link-local address
> IPv6 Global Unicast Address: | Displays the ipv6 Global Unicast Address address

> ‌
> show ipv6 neighbors
> show ipv6 neighbors Command Output Descriptions

> Field | Description
> Address | IPv6 address from table
> Type | Interface type:
> • | Broadcast (Ethernet)
> • | Loopback
> Link address | MAC address
> Flags | One of the following flag codes:
> • | I = Incomplete
> • | R = Reachable
> • | M = Permanent
> • | S = Stale
> • | D = Delay
> • | P = Probe
> • | F = Failed
> Interface | Interface name

> ‌
> show ipv6 route
> show ipv6 route Command Output Descriptions

> Field | Description
> Destination | Designating ipv6 address prefix/length
> Next hop | Address of the directly connected next hop interface
> Protocol | Connected Unconnected
> Prec | Number of precedence bits set
> Cost | Number of router hops to destination address
> Interface | Name of the next hop interface
> Total Route Count | Total number of routes Number connected Number of static routes

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883